<?xml version="1.0" encoding= "UTF-8" ?>
<configuration name="MIMXRT1052xxxxB" xsi:schemaLocation="http://mcuxpresso.nxp.com/XSD/mex_configuration_12 http://mcuxpresso.nxp.com/XSD/mex_configuration_12.xsd" uuid="ea584181-55b7-4bac-96ba-c53df188dbf3" version="12" xmlns="http://mcuxpresso.nxp.com/XSD/mex_configuration_12" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">
   <common>
      <processor>MIMXRT1052xxxxB</processor>
      <package>MIMXRT1052DVL6B</package>
      <mcu_data>ksdk2_0</mcu_data>
      <cores selected="core0">
         <core name="Cortex-M7F" id="core0" description="M7 core"/>
      </cores>
      <description></description>
   </common>
   <preferences>
      <validate_boot_init_only>true</validate_boot_init_only>
      <generate_extended_information>false</generate_extended_information>
      <generate_code_modified_registers_only>false</generate_code_modified_registers_only>
      <update_include_paths>true</update_include_paths>
      <generate_registers_defines>false</generate_registers_defines>
   </preferences>
   <tools>
      <pins name="Pins" version="12.0" enabled="true" update_project_code="true">
         <generated_project_files>
            <file path="board/pin_mux.c" update_enabled="true"/>
            <file path="board/pin_mux.h" update_enabled="true"/>
         </generated_project_files>
         <pins_profile>
            <processor_version>12.0.0</processor_version>
            <pin_labels>
               <pin_label pin_num="C7" pin_signal="GPIO_EMC_41" label="LED_B" identifier="LED_R;LED_B"/>
               <pin_label pin_num="B12" pin_signal="GPIO_B1_07" label="LED_G" identifier="LED_G"/>
               <pin_label pin_num="A7" pin_signal="GPIO_EMC_40" label="LED_R" identifier="LED_B;LED_R"/>
               <pin_label pin_num="G14" pin_signal="GPIO_AD_B0_05" label="USDHC1_PWR" identifier="USDHC1_PWR"/>
               <pin_label pin_num="M11" pin_signal="GPIO_AD_B0_02" label="LCD_RST" identifier="LCD_RST"/>
               <pin_label pin_num="M14" pin_signal="GPIO_AD_B0_00" label="CSI_" identifier="CSI_;CSI_PDN"/>
               <pin_label pin_num="H10" pin_signal="GPIO_AD_B0_01" label="CSI_RST" identifier="CSI_RST"/>
               <pin_label pin_num="G11" pin_signal="GPIO_AD_B0_03" label="BUZZER" identifier="BUZZER"/>
               <pin_label pin_num="L6" pin_signal="WAKEUP" label="WAKEUP" identifier="WAKEUP"/>
            </pin_labels>
            <power_domains>
               <power_domain name="DCDC_IN" value="3.3"/>
               <power_domain name="DCDC_IN_Q" value="3.3"/>
               <power_domain name="DCDC_LP" value="1.25"/>
               <power_domain name="DCDC_PSWITCH" value="3.3"/>
               <power_domain name="DCDC_SENSE" value="1.25"/>
               <power_domain name="NVCC_EMC" value="3.3"/>
               <power_domain name="NVCC_GPIO" value="3.3"/>
               <power_domain name="NVCC_SD0" value="3.3"/>
               <power_domain name="NVCC_SD1" value="3.3"/>
               <power_domain name="VDDA_ADC_3P3" value="3.3"/>
               <power_domain name="VDD_HIGH_CAP" value="1.1"/>
               <power_domain name="VDD_HIGH_IN" value="3.3"/>
               <power_domain name="VDD_SNVS_CAP" value="1.1"/>
               <power_domain name="VDD_SNVS_IN" value="3.3"/>
               <power_domain name="VDD_SOC_IN" value="1.25"/>
               <power_domain name="VDD_USB_CAP" value="2.5"/>
            </power_domains>
         </pins_profile>
         <functions_list>
            <function name="BOARD_InitUARTDbgPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>true</callFromInitBoot>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="LPUART1" description="Peripheral LPUART1 is not initialized" problem_level="1" source="Pins:BOARD_InitUARTDbgPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitUARTDbgPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Pins initialization requires the IOMUXC Driver in the project." problem_level="2" source="Pins:BOARD_InitUARTDbgPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="LPUART1" signal="TX" pin_num="K14" pin_signal="GPIO_AD_B0_12"/>
                  <pin peripheral="LPUART1" signal="RX" pin_num="L14" pin_signal="GPIO_AD_B0_13"/>
               </pins>
            </function>
            <function name="BOARD_InitSWDPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>true</callFromInitBoot>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="JTAG" description="Peripheral JTAG is not initialized" problem_level="1" source="Pins:BOARD_InitSWDPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitSWDPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Pins initialization requires the IOMUXC Driver in the project." problem_level="2" source="Pins:BOARD_InitSWDPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="JTAG" signal="TMS" pin_num="E14" pin_signal="GPIO_AD_B0_06"/>
                  <pin peripheral="JTAG" signal="TCK" pin_num="F12" pin_signal="GPIO_AD_B0_07"/>
               </pins>
            </function>
            <function name="BOARD_InitFlexSPIPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>true</callFromInitBoot>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="FLEXSPI" description="Peripheral FLEXSPI is not initialized" problem_level="1" source="Pins:BOARD_InitFlexSPIPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitFlexSPIPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Pins initialization requires the IOMUXC Driver in the project." problem_level="2" source="Pins:BOARD_InitFlexSPIPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="FLEXSPI" signal="FLEXSPI_A_DATA0" pin_num="P3" pin_signal="GPIO_SD_B1_08"/>
                  <pin peripheral="FLEXSPI" signal="FLEXSPI_A_DATA1" pin_num="N4" pin_signal="GPIO_SD_B1_09"/>
                  <pin peripheral="FLEXSPI" signal="FLEXSPI_A_DATA2" pin_num="P4" pin_signal="GPIO_SD_B1_10"/>
                  <pin peripheral="FLEXSPI" signal="FLEXSPI_A_DATA3" pin_num="P5" pin_signal="GPIO_SD_B1_11"/>
                  <pin peripheral="FLEXSPI" signal="FLEXSPI_A_SS0_B" pin_num="L3" pin_signal="GPIO_SD_B1_06"/>
                  <pin peripheral="FLEXSPI" signal="FLEXSPI_A_SCLK" pin_num="L4" pin_signal="GPIO_SD_B1_07"/>
                  <pin peripheral="FLEXSPI" signal="FLEXSPI_A_DQS" pin_num="N3" pin_signal="GPIO_SD_B1_05"/>
               </pins>
            </function>
            <function name="BOARD_InituSDPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>false</callFromInitBoot>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="USDHC1" description="Peripheral USDHC1 is not initialized" problem_level="1" source="Pins:BOARD_InituSDPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InituSDPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Pins initialization requires the IOMUXC Driver in the project." problem_level="2" source="Pins:BOARD_InituSDPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.igpio" description="Pins initialization requires the IGPIO Driver in the project." problem_level="2" source="Pins:BOARD_InituSDPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="USDHC1" signal="usdhc_clk" pin_num="J3" pin_signal="GPIO_SD_B0_01"/>
                  <pin peripheral="USDHC1" signal="usdhc_cmd" pin_num="J4" pin_signal="GPIO_SD_B0_00"/>
                  <pin peripheral="USDHC1" signal="usdhc_data, 0" pin_num="J1" pin_signal="GPIO_SD_B0_02"/>
                  <pin peripheral="USDHC1" signal="usdhc_data, 1" pin_num="K1" pin_signal="GPIO_SD_B0_03"/>
                  <pin peripheral="USDHC1" signal="usdhc_data, 2" pin_num="H2" pin_signal="GPIO_SD_B0_04"/>
                  <pin peripheral="USDHC1" signal="usdhc_data, 3" pin_num="J2" pin_signal="GPIO_SD_B0_05"/>
                  <pin peripheral="GPIO1" signal="gpio_io, 05" pin_num="G14" pin_signal="GPIO_AD_B0_05">
                     <pin_features>
                        <pin_feature name="direction" value="OUTPUT"/>
                        <pin_feature name="gpio_init_state" value="true"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="USDHC1" signal="usdhc_vselect" pin_num="C14" pin_signal="GPIO_B1_14"/>
               </pins>
            </function>
            <function name="BOARD_InitSDWiFiPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>false</callFromInitBoot>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="USDHC2" description="Peripheral USDHC2 is not initialized" problem_level="1" source="Pins:BOARD_InitSDWiFiPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitSDWiFiPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Pins initialization requires the IOMUXC Driver in the project." problem_level="2" source="Pins:BOARD_InitSDWiFiPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="USDHC2" signal="usdhc_cmd" pin_num="N3" pin_signal="GPIO_SD_B1_05"/>
                  <pin peripheral="USDHC2" signal="usdhc_clk" pin_num="P2" pin_signal="GPIO_SD_B1_04"/>
                  <pin peripheral="USDHC2" signal="usdhc_data, 0" pin_num="M4" pin_signal="GPIO_SD_B1_03"/>
                  <pin peripheral="USDHC2" signal="usdhc_data, 1" pin_num="M3" pin_signal="GPIO_SD_B1_02"/>
                  <pin peripheral="USDHC2" signal="usdhc_data, 2" pin_num="M5" pin_signal="GPIO_SD_B1_01"/>
                  <pin peripheral="USDHC2" signal="usdhc_data, 3" pin_num="L5" pin_signal="GPIO_SD_B1_00"/>
               </pins>
            </function>
            <function name="BOARD_InitSEMCPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>false</callFromInitBoot>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="SEMC" description="Peripheral SEMC is not initialized" problem_level="1" source="Pins:BOARD_InitSEMCPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitSEMCPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Pins initialization requires the IOMUXC Driver in the project." problem_level="2" source="Pins:BOARD_InitSEMCPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="SEMC" signal="DATA, 00" pin_num="E3" pin_signal="GPIO_EMC_00"/>
                  <pin peripheral="SEMC" signal="DATA, 01" pin_num="F3" pin_signal="GPIO_EMC_01"/>
                  <pin peripheral="SEMC" signal="DATA, 02" pin_num="F4" pin_signal="GPIO_EMC_02"/>
                  <pin peripheral="SEMC" signal="DATA, 03" pin_num="G4" pin_signal="GPIO_EMC_03"/>
                  <pin peripheral="SEMC" signal="DATA, 04" pin_num="F2" pin_signal="GPIO_EMC_04"/>
                  <pin peripheral="SEMC" signal="DATA, 05" pin_num="G5" pin_signal="GPIO_EMC_05"/>
                  <pin peripheral="SEMC" signal="DATA, 06" pin_num="H5" pin_signal="GPIO_EMC_06"/>
                  <pin peripheral="SEMC" signal="DATA, 07" pin_num="H4" pin_signal="GPIO_EMC_07"/>
                  <pin peripheral="SEMC" signal="DATA, 08" pin_num="C6" pin_signal="GPIO_EMC_30"/>
                  <pin peripheral="SEMC" signal="DATA, 09" pin_num="C5" pin_signal="GPIO_EMC_31"/>
                  <pin peripheral="SEMC" signal="DATA, 10" pin_num="D5" pin_signal="GPIO_EMC_32"/>
                  <pin peripheral="SEMC" signal="DATA, 11" pin_num="C4" pin_signal="GPIO_EMC_33"/>
                  <pin peripheral="SEMC" signal="DATA, 12" pin_num="D4" pin_signal="GPIO_EMC_34"/>
                  <pin peripheral="SEMC" signal="DATA, 13" pin_num="E5" pin_signal="GPIO_EMC_35"/>
                  <pin peripheral="SEMC" signal="DATA, 14" pin_num="C3" pin_signal="GPIO_EMC_36"/>
                  <pin peripheral="SEMC" signal="DATA, 15" pin_num="E4" pin_signal="GPIO_EMC_37"/>
                  <pin peripheral="SEMC" signal="DM, 0" pin_num="H3" pin_signal="GPIO_EMC_08"/>
                  <pin peripheral="SEMC" signal="DM, 1" pin_num="D6" pin_signal="GPIO_EMC_38"/>
                  <pin peripheral="SEMC" signal="ADDR, 00" pin_num="C2" pin_signal="GPIO_EMC_09"/>
                  <pin peripheral="SEMC" signal="ADDR, 01" pin_num="G1" pin_signal="GPIO_EMC_10"/>
                  <pin peripheral="SEMC" signal="ADDR, 02" pin_num="G3" pin_signal="GPIO_EMC_11"/>
                  <pin peripheral="SEMC" signal="ADDR, 03" pin_num="H1" pin_signal="GPIO_EMC_12"/>
                  <pin peripheral="SEMC" signal="ADDR, 04" pin_num="A6" pin_signal="GPIO_EMC_13"/>
                  <pin peripheral="SEMC" signal="ADDR, 05" pin_num="B6" pin_signal="GPIO_EMC_14"/>
                  <pin peripheral="SEMC" signal="ADDR, 06" pin_num="B1" pin_signal="GPIO_EMC_15"/>
                  <pin peripheral="SEMC" signal="ADDR, 07" pin_num="A5" pin_signal="GPIO_EMC_16"/>
                  <pin peripheral="SEMC" signal="ADDR, 08" pin_num="A4" pin_signal="GPIO_EMC_17"/>
                  <pin peripheral="SEMC" signal="ADDR, 09" pin_num="B2" pin_signal="GPIO_EMC_18"/>
                  <pin peripheral="SEMC" signal="ADDR, 10" pin_num="G2" pin_signal="GPIO_EMC_23"/>
                  <pin peripheral="SEMC" signal="ADDR, 11" pin_num="B4" pin_signal="GPIO_EMC_19"/>
                  <pin peripheral="SEMC" signal="ADDR, 12" pin_num="A3" pin_signal="GPIO_EMC_20"/>
                  <pin peripheral="SEMC" signal="BA, 0" pin_num="C1" pin_signal="GPIO_EMC_21"/>
                  <pin peripheral="SEMC" signal="semc_cas" pin_num="D3" pin_signal="GPIO_EMC_24"/>
                  <pin peripheral="SEMC" signal="semc_ras" pin_num="D2" pin_signal="GPIO_EMC_25"/>
                  <pin peripheral="SEMC" signal="semc_we" pin_num="D1" pin_signal="GPIO_EMC_28"/>
                  <pin peripheral="SEMC" signal="semc_cke" pin_num="A2" pin_signal="GPIO_EMC_27"/>
                  <pin peripheral="SEMC" signal="semc_clk" pin_num="B3" pin_signal="GPIO_EMC_26"/>
                  <pin peripheral="SEMC" signal="semc_rdy" pin_num="A7" pin_signal="GPIO_EMC_40"/>
                  <pin peripheral="SEMC" signal="CS, 0" pin_num="E1" pin_signal="GPIO_EMC_29"/>
                  <pin peripheral="SEMC" signal="CSX, 0" pin_num="C7" pin_signal="GPIO_EMC_41"/>
                  <pin peripheral="SEMC" signal="BA, 1" pin_num="F1" pin_signal="GPIO_EMC_22"/>
               </pins>
            </function>
            <function name="BOARD_InitLCDPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>false</callFromInitBoot>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="LCDIF" description="Peripheral LCDIF is not initialized" problem_level="1" source="Pins:BOARD_InitLCDPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitLCDPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Pins initialization requires the IOMUXC Driver in the project." problem_level="2" source="Pins:BOARD_InitLCDPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.igpio" description="Pins initialization requires the IGPIO Driver in the project." problem_level="2" source="Pins:BOARD_InitLCDPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="LCDIF" signal="lcdif_clk" pin_num="D7" pin_signal="GPIO_B0_00"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 00" pin_num="C8" pin_signal="GPIO_B0_04"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 02" pin_num="A8" pin_signal="GPIO_B0_06"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 01" pin_num="B8" pin_signal="GPIO_B0_05"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 03" pin_num="A9" pin_signal="GPIO_B0_07"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 04" pin_num="B9" pin_signal="GPIO_B0_08"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 05" pin_num="C9" pin_signal="GPIO_B0_09"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 06" pin_num="D9" pin_signal="GPIO_B0_10"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 07" pin_num="A10" pin_signal="GPIO_B0_11"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 08" pin_num="C10" pin_signal="GPIO_B0_12"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 09" pin_num="D10" pin_signal="GPIO_B0_13"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 10" pin_num="E10" pin_signal="GPIO_B0_14"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 11" pin_num="E11" pin_signal="GPIO_B0_15"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 12" pin_num="A11" pin_signal="GPIO_B1_00"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 13" pin_num="B11" pin_signal="GPIO_B1_01"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 14" pin_num="C11" pin_signal="GPIO_B1_02"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 15" pin_num="D11" pin_signal="GPIO_B1_03"/>
                  <pin peripheral="LCDIF" signal="lcdif_enable" pin_num="E7" pin_signal="GPIO_B0_01"/>
                  <pin peripheral="LCDIF" signal="lcdif_hsync" pin_num="E8" pin_signal="GPIO_B0_02"/>
                  <pin peripheral="LCDIF" signal="lcdif_vsync" pin_num="D8" pin_signal="GPIO_B0_03"/>
                  <pin peripheral="GPIO1" signal="gpio_io, 02" pin_num="M11" pin_signal="GPIO_AD_B0_02">
                     <pin_features>
                        <pin_feature name="direction" value="OUTPUT"/>
                        <pin_feature name="gpio_init_state" value="true"/>
                     </pin_features>
                  </pin>
               </pins>
            </function>
            <function name="BOARD_InitCodecPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>false</callFromInitBoot>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="SAI1" description="Peripheral SAI1 is not initialized" problem_level="1" source="Pins:BOARD_InitCodecPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitCodecPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Pins initialization requires the IOMUXC Driver in the project." problem_level="2" source="Pins:BOARD_InitCodecPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="SAI1" signal="sai_tx_bclk" pin_num="G12" pin_signal="GPIO_AD_B1_14"/>
                  <pin peripheral="SAI1" signal="sai_tx_sync" pin_num="J14" pin_signal="GPIO_AD_B1_15"/>
                  <pin peripheral="SAI1" signal="sai_tx_data0" pin_num="H11" pin_signal="GPIO_AD_B1_13"/>
                  <pin peripheral="SAI1" signal="sai_rx_data0" pin_num="H12" pin_signal="GPIO_AD_B1_12"/>
                  <pin peripheral="SAI1" signal="sai_mclk" pin_num="M13" pin_signal="GPIO_AD_B1_09"/>
                  <pin peripheral="GPIO1" signal="gpio_io, 24" pin_num="H13" pin_signal="GPIO_AD_B1_08"/>
               </pins>
            </function>
            <function name="BOARD_InitCSIPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>false</callFromInitBoot>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="CSI" description="Peripheral CSI is not initialized" problem_level="1" source="Pins:BOARD_InitCSIPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitCSIPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Pins initialization requires the IOMUXC Driver in the project." problem_level="2" source="Pins:BOARD_InitCSIPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="CSI" signal="csi_data, 02" pin_num="J14" pin_signal="GPIO_AD_B1_15"/>
                  <pin peripheral="CSI" signal="csi_data, 03" pin_num="G12" pin_signal="GPIO_AD_B1_14"/>
                  <pin peripheral="CSI" signal="csi_data, 04" pin_num="H11" pin_signal="GPIO_AD_B1_13"/>
                  <pin peripheral="CSI" signal="csi_data, 05" pin_num="H12" pin_signal="GPIO_AD_B1_12"/>
                  <pin peripheral="CSI" signal="csi_data, 06" pin_num="J13" pin_signal="GPIO_AD_B1_11"/>
                  <pin peripheral="CSI" signal="csi_data, 07" pin_num="L13" pin_signal="GPIO_AD_B1_10"/>
                  <pin peripheral="CSI" signal="csi_data, 08" pin_num="M13" pin_signal="GPIO_AD_B1_09"/>
                  <pin peripheral="CSI" signal="csi_data, 09" pin_num="H13" pin_signal="GPIO_AD_B1_08"/>
                  <pin peripheral="CSI" signal="csi_hsync" pin_num="K10" pin_signal="GPIO_AD_B1_07"/>
                  <pin peripheral="CSI" signal="csi_vsync" pin_num="J12" pin_signal="GPIO_AD_B1_06"/>
                  <pin peripheral="CSI" signal="csi_mclk" pin_num="K12" pin_signal="GPIO_AD_B1_05"/>
                  <pin peripheral="CSI" signal="csi_pixclk" pin_num="D13" pin_signal="GPIO_B1_12"/>
                  <pin peripheral="GPIO1" signal="gpio_io, 00" pin_num="M14" pin_signal="GPIO_AD_B0_00">
                     <pin_features>
                        <pin_feature name="identifier" value="CSI_PDN"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="GPIO1" signal="gpio_io, 01" pin_num="H10" pin_signal="GPIO_AD_B0_01"/>
               </pins>
            </function>
            <function name="BOARD_InitSYSPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>false</callFromInitBoot>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="SUPPLY" description="Peripheral SUPPLY is not initialized" problem_level="1" source="Pins:BOARD_InitSYSPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="Peripheral" resourceId="CCM" description="Peripheral CCM is not initialized" problem_level="1" source="Pins:BOARD_InitSYSPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="Peripheral" resourceId="SNVS" description="Peripheral SNVS is not initialized" problem_level="1" source="Pins:BOARD_InitSYSPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="Peripheral" resourceId="SRC" description="Peripheral SRC is not initialized" problem_level="1" source="Pins:BOARD_InitSYSPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="Peripheral" resourceId="XTALOSC24M" description="Peripheral XTALOSC24M is not initialized" problem_level="1" source="Pins:BOARD_InitSYSPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitSYSPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Pins initialization requires the IOMUXC Driver in the project." problem_level="2" source="Pins:BOARD_InitSYSPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="SUPPLY" signal="DCDC_GND, 0" pin_num="N1" pin_signal="DCDC_GND0"/>
                  <pin peripheral="SUPPLY" signal="DCDC_GND, 1" pin_num="N2" pin_signal="DCDC_GND1"/>
                  <pin peripheral="SUPPLY" signal="DCDC_IN, 0" pin_num="L1" pin_signal="DCDC_IN0"/>
                  <pin peripheral="SUPPLY" signal="DCDC_IN, 1" pin_num="L2" pin_signal="DCDC_IN1"/>
                  <pin peripheral="SUPPLY" signal="dcdc_in_q" pin_num="K4" pin_signal="DCDC_IN_Q"/>
                  <pin peripheral="SUPPLY" signal="DCDC_LP, 0" pin_num="M1" pin_signal="DCDC_LP0"/>
                  <pin peripheral="SUPPLY" signal="DCDC_LP, 1" pin_num="M2" pin_signal="DCDC_LP1"/>
                  <pin peripheral="SUPPLY" signal="dcdc_pswitch" pin_num="K3" pin_signal="DCDC_PSWITCH"/>
                  <pin peripheral="SUPPLY" signal="dcdc_sense" pin_num="J5" pin_signal="DCDC_SENSE"/>
                  <pin peripheral="SUPPLY" signal="gpanaio" pin_num="N10" pin_signal="GPANAIO"/>
                  <pin peripheral="SUPPLY" signal="ngnd_kel0" pin_num="K9" pin_signal="NGND_KEL0"/>
                  <pin peripheral="SUPPLY" signal="NVCC_EMC, 0" pin_num="F5" pin_signal="NVCC_EMC0"/>
                  <pin peripheral="SUPPLY" signal="NVCC_EMC, 1" pin_num="E6" pin_signal="NVCC_EMC1"/>
                  <pin peripheral="SUPPLY" signal="NVCC_GPIO, 0" pin_num="E9" pin_signal="NVCC_GPIO0"/>
                  <pin peripheral="SUPPLY" signal="NVCC_GPIO, 1" pin_num="F10" pin_signal="NVCC_GPIO1"/>
                  <pin peripheral="SUPPLY" signal="NVCC_GPIO, 2" pin_num="J10" pin_signal="NVCC_GPIO2"/>
                  <pin peripheral="SUPPLY" signal="nvcc_pll" pin_num="P10" pin_signal="NVCC_PLL"/>
                  <pin peripheral="SUPPLY" signal="nvcc_sd0" pin_num="J6" pin_signal="NVCC_SD0"/>
                  <pin peripheral="SUPPLY" signal="nvcc_sd1" pin_num="K5" pin_signal="NVCC_SD1"/>
                  <pin peripheral="SUPPLY" signal="test_mode" pin_num="K6" pin_signal="TEST_MODE"/>
                  <pin peripheral="SUPPLY" signal="usb_otg1_chd_b" pin_num="N12" pin_signal="USB_OTG1_CHD_B"/>
                  <pin peripheral="SUPPLY" signal="usb_otg1_dn" pin_num="M8" pin_signal="USB_OTG1_DN"/>
                  <pin peripheral="SUPPLY" signal="usb_otg1_dp" pin_num="L8" pin_signal="USB_OTG1_DP"/>
                  <pin peripheral="SUPPLY" signal="usb_otg1_vbus" pin_num="N6" pin_signal="USB_OTG1_VBUS"/>
                  <pin peripheral="SUPPLY" signal="usb_otg2_dn" pin_num="N7" pin_signal="USB_OTG2_DN"/>
                  <pin peripheral="SUPPLY" signal="usb_otg2_dp" pin_num="P7" pin_signal="USB_OTG2_DP"/>
                  <pin peripheral="SUPPLY" signal="usb_otg2_vbus" pin_num="P6" pin_signal="USB_OTG2_VBUS"/>
                  <pin peripheral="SUPPLY" signal="VDD_HIGH_IN" pin_num="P12" pin_signal="VDD_HIGH_IN"/>
                  <pin peripheral="SUPPLY" signal="VDD_HIGH_CAP" pin_num="P8" pin_signal="VDD_HIGH_CAP"/>
                  <pin peripheral="SUPPLY" signal="VDD_SNVS_CAP" pin_num="M10" pin_signal="VDD_SNVS_CAP"/>
                  <pin peripheral="SUPPLY" signal="VDD_SNVS_IN" pin_num="M9" pin_signal="VDD_SNVS_IN"/>
                  <pin peripheral="SUPPLY" signal="VDD_SOC_IN, 0" pin_num="F6" pin_signal="VDD_SOC_IN0"/>
                  <pin peripheral="SUPPLY" signal="VDD_SOC_IN, 1" pin_num="G6" pin_signal="VDD_SOC_IN1"/>
                  <pin peripheral="SUPPLY" signal="VDD_SOC_IN, 2" pin_num="H6" pin_signal="VDD_SOC_IN2"/>
                  <pin peripheral="SUPPLY" signal="VDD_SOC_IN, 3" pin_num="F7" pin_signal="VDD_SOC_IN3"/>
                  <pin peripheral="SUPPLY" signal="VDD_SOC_IN, 4" pin_num="F8" pin_signal="VDD_SOC_IN4"/>
                  <pin peripheral="SUPPLY" signal="VDD_SOC_IN, 5" pin_num="F9" pin_signal="VDD_SOC_IN5"/>
                  <pin peripheral="SUPPLY" signal="VDD_SOC_IN, 6" pin_num="G9" pin_signal="VDD_SOC_IN6"/>
                  <pin peripheral="SUPPLY" signal="VDD_SOC_IN, 7" pin_num="H9" pin_signal="VDD_SOC_IN7"/>
                  <pin peripheral="SUPPLY" signal="VDD_SOC_IN, 8" pin_num="J9" pin_signal="VDD_SOC_IN8"/>
                  <pin peripheral="SUPPLY" signal="VDDA_ADC_3P3" pin_num="N14" pin_signal="VDDA_ADC_3P3"/>
                  <pin peripheral="SUPPLY" signal="VDD_USB_CAP" pin_num="K8" pin_signal="VDD_USB_CAP"/>
                  <pin peripheral="SUPPLY" signal="VSS, 0" pin_num="A1" pin_signal="VSS0"/>
                  <pin peripheral="SUPPLY" signal="VSS, 1" pin_num="P1" pin_signal="VSS1"/>
                  <pin peripheral="SUPPLY" signal="VSS, 2" pin_num="E2" pin_signal="VSS2"/>
                  <pin peripheral="SUPPLY" signal="VSS, 3" pin_num="K2" pin_signal="VSS3"/>
                  <pin peripheral="SUPPLY" signal="VSS, 4" pin_num="B5" pin_signal="VSS4"/>
                  <pin peripheral="SUPPLY" signal="VSS, 5" pin_num="N5" pin_signal="VSS5"/>
                  <pin peripheral="SUPPLY" signal="VSS, 6" pin_num="G7" pin_signal="VSS6"/>
                  <pin peripheral="SUPPLY" signal="VSS, 7" pin_num="H7" pin_signal="VSS7"/>
                  <pin peripheral="SUPPLY" signal="VSS, 8" pin_num="J7" pin_signal="VSS8"/>
                  <pin peripheral="SUPPLY" signal="VSS, 9" pin_num="G8" pin_signal="VSS9"/>
                  <pin peripheral="SUPPLY" signal="VSS, 10" pin_num="H8" pin_signal="VSS10"/>
                  <pin peripheral="SUPPLY" signal="VSS, 11" pin_num="J8" pin_signal="VSS11"/>
                  <pin peripheral="SUPPLY" signal="VSS, 12" pin_num="N8" pin_signal="VSS12"/>
                  <pin peripheral="SUPPLY" signal="VSS, 13" pin_num="L9" pin_signal="VSS13"/>
                  <pin peripheral="SUPPLY" signal="VSS, 14" pin_num="B10" pin_signal="VSS14"/>
                  <pin peripheral="SUPPLY" signal="VSS, 15" pin_num="E13" pin_signal="VSS15"/>
                  <pin peripheral="SUPPLY" signal="VSS, 16" pin_num="K13" pin_signal="VSS16"/>
                  <pin peripheral="SUPPLY" signal="VSS, 17" pin_num="A14" pin_signal="VSS17"/>
                  <pin peripheral="SUPPLY" signal="VSS, 18" pin_num="P14" pin_signal="VSS18"/>
                  <pin peripheral="CCM" signal="CLK1_N" pin_num="P13" pin_signal="CCM_CLK1_N"/>
                  <pin peripheral="CCM" signal="CLK1_P" pin_num="N13" pin_signal="CCM_CLK1_P"/>
                  <pin peripheral="SNVS" signal="snvs_pmic_on_req" pin_num="K7" pin_signal="PMIC_ON_REQ"/>
                  <pin peripheral="SRC" signal="RESET_B" pin_num="M6" pin_signal="ONOFF"/>
                  <pin peripheral="SRC" signal="POR_B" pin_num="M7" pin_signal="POR_B"/>
                  <pin peripheral="XTALOSC24M" signal="rtc_xtalo" pin_num="P9" pin_signal="RTC_XTALO"/>
                  <pin peripheral="XTALOSC24M" signal="rtc_xtali" pin_num="N9" pin_signal="RTC_XTALI"/>
                  <pin peripheral="XTALOSC24M" signal="xtali" pin_num="P11" pin_signal="XTALI"/>
                  <pin peripheral="XTALOSC24M" signal="xtalo" pin_num="N11" pin_signal="XTALO"/>
               </pins>
            </function>
            <function name="BOARD_InitENETPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>false</callFromInitBoot>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="ENET" description="Peripheral ENET is not initialized" problem_level="1" source="Pins:BOARD_InitENETPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitENETPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Pins initialization requires the IOMUXC Driver in the project." problem_level="2" source="Pins:BOARD_InitENETPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="ENET" signal="enet_mdc" pin_num="L12" pin_signal="GPIO_AD_B1_04"/>
                  <pin peripheral="ENET" signal="enet_mdio" pin_num="B14" pin_signal="GPIO_B1_15"/>
                  <pin peripheral="ENET" signal="enet_rx_data, 0" pin_num="E12" pin_signal="GPIO_B1_04"/>
                  <pin peripheral="ENET" signal="enet_rx_data, 1" pin_num="D12" pin_signal="GPIO_B1_05"/>
                  <pin peripheral="ENET" signal="enet_tx_data, 0" pin_num="B12" pin_signal="GPIO_B1_07"/>
                  <pin peripheral="ENET" signal="enet_tx_data, 1" pin_num="A12" pin_signal="GPIO_B1_08"/>
                  <pin peripheral="ENET" signal="enet_tx_en" pin_num="A13" pin_signal="GPIO_B1_09"/>
                  <pin peripheral="ENET" signal="enet_rx_er" pin_num="C13" pin_signal="GPIO_B1_11"/>
                  <pin peripheral="ENET" signal="enet_tx_clk" pin_num="B13" pin_signal="GPIO_B1_10"/>
                  <pin peripheral="ENET" signal="enet_rx_en" pin_num="C12" pin_signal="GPIO_B1_06"/>
               </pins>
            </function>
            <function name="BOARD_InitBasicIOPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>false</callFromInitBoot>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="GPIO5" description="Peripheral GPIO5 is not initialized" problem_level="1" source="Pins:BOARD_InitBasicIOPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitBasicIOPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Pins initialization requires the IOMUXC Driver in the project." problem_level="2" source="Pins:BOARD_InitBasicIOPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.igpio" description="Pins initialization requires the IGPIO Driver in the project." problem_level="2" source="Pins:BOARD_InitBasicIOPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="GPIO1" signal="gpio_io, 03" pin_num="G11" pin_signal="GPIO_AD_B0_03">
                     <pin_features>
                        <pin_feature name="direction" value="OUTPUT"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="GPIO5" signal="gpio_io, 00" pin_num="L6" pin_signal="WAKEUP">
                     <pin_features>
                        <pin_feature name="direction" value="INPUT"/>
                     </pin_features>
                  </pin>
               </pins>
            </function>
            <function name="BOARD_InitI2C1Pins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>false</callFromInitBoot>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="LPI2C1" description="Peripheral LPI2C1 is not initialized" problem_level="1" source="Pins:BOARD_InitI2C1Pins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitI2C1Pins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Pins initialization requires the IOMUXC Driver in the project." problem_level="2" source="Pins:BOARD_InitI2C1Pins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="LPI2C1" signal="SDA" pin_num="K11" pin_signal="GPIO_AD_B1_01"/>
                  <pin peripheral="LPI2C1" signal="SCL" pin_num="J11" pin_signal="GPIO_AD_B1_00"/>
               </pins>
            </function>
            <function name="BOARD_InitCAN2Pins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>false</callFromInitBoot>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="CAN2" description="Peripheral CAN2 is not initialized" problem_level="1" source="Pins:BOARD_InitCAN2Pins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitCAN2Pins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Pins initialization requires the IOMUXC Driver in the project." problem_level="2" source="Pins:BOARD_InitCAN2Pins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="CAN2" signal="RX" pin_num="L10" pin_signal="GPIO_AD_B0_15"/>
                  <pin peripheral="CAN2" signal="TX" pin_num="H14" pin_signal="GPIO_AD_B0_14"/>
               </pins>
            </function>
            <function name="BOARD_InitSPDIFPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>false</callFromInitBoot>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="SPDIF" description="Peripheral SPDIF is not initialized" problem_level="1" source="Pins:BOARD_InitSPDIFPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitSPDIFPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Pins initialization requires the IOMUXC Driver in the project." problem_level="2" source="Pins:BOARD_InitSPDIFPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="SPDIF" signal="spdif_in" pin_num="M12" pin_signal="GPIO_AD_B1_03"/>
                  <pin peripheral="SPDIF" signal="spdif_out" pin_num="L11" pin_signal="GPIO_AD_B1_02"/>
               </pins>
            </function>
         </functions_list>
      </pins>
      <clocks name="Clocks" version="10.0" enabled="true" update_project_code="true">
         <generated_project_files>
            <file path="board/clock_config.c" update_enabled="true"/>
            <file path="board/clock_config.h" update_enabled="true"/>
         </generated_project_files>
         <clocks_profile>
            <processor_version>12.0.0</processor_version>
         </clocks_profile>
         <clock_configurations>
            <clock_configuration name="Board_BootClockPLL600MHz" id_prefix="" prefix_user_defined="false">
               <description></description>
               <options/>
               <dependencies>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.xtali" description="&apos;XTALI&apos; (Pins tool id: XTALOSC24M.xtali, Clocks tool id: XTALOSC24M.XTALI) needs to be routed" problem_level="1" source="Clocks:Board_BootClockPLL600MHz">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.xtali" description="&apos;XTALI&apos; (Pins tool id: XTALOSC24M.xtali, Clocks tool id: XTALOSC24M.XTALI) needs to have &apos;INPUT&apos; direction" problem_level="1" source="Clocks:Board_BootClockPLL600MHz">
                     <feature name="direction" evaluation="">
                        <data>INPUT</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.xtalo" description="&apos;XTALO&apos; (Pins tool id: XTALOSC24M.xtalo, Clocks tool id: XTALOSC24M.XTALO) needs to be routed" problem_level="1" source="Clocks:Board_BootClockPLL600MHz">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.xtalo" description="&apos;XTALO&apos; (Pins tool id: XTALOSC24M.xtalo, Clocks tool id: XTALOSC24M.XTALO) needs to have &apos;OUTPUT&apos; direction" problem_level="1" source="Clocks:Board_BootClockPLL600MHz">
                     <feature name="direction" evaluation="">
                        <data>OUTPUT</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Clocks initialization requires the COMMON Driver in the project." problem_level="2" source="Clocks:Board_BootClockPLL600MHz">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Clocks initialization requires the IOMUXC Driver in the project." problem_level="2" source="Clocks:Board_BootClockPLL600MHz">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <clock_sources/>
               <clock_outputs>
                  <clock_output id="AHB_CLK_ROOT.outFreq" value="600 MHz" locked="false" accuracy=""/>
                  <clock_output id="CAN_CLK_ROOT.outFreq" value="2 MHz" locked="false" accuracy=""/>
                  <clock_output id="CLK_1M.outFreq" value="1 MHz" locked="false" accuracy=""/>
                  <clock_output id="CLK_24M.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="CSI_CLK_ROOT.outFreq" value="12 MHz" locked="false" accuracy=""/>
                  <clock_output id="ENET_125M_CLK.outFreq" value="2.4 MHz" locked="false" accuracy=""/>
                  <clock_output id="ENET_25M_REF_CLK.outFreq" value="1.2 MHz" locked="false" accuracy=""/>
                  <clock_output id="FLEXIO1_CLK_ROOT.outFreq" value="1.5 MHz" locked="false" accuracy=""/>
                  <clock_output id="FLEXIO2_CLK_ROOT.outFreq" value="1.5 MHz" locked="false" accuracy=""/>
                  <clock_output id="FLEXSPI_CLK_ROOT.outFreq" value="132 MHz" locked="false" accuracy=""/>
                  <clock_output id="GPT1_ipg_clk_highfreq.outFreq" value="5 MHz" locked="false" accuracy=""/>
                  <clock_output id="GPT2_ipg_clk_highfreq.outFreq" value="5 MHz" locked="false" accuracy=""/>
                  <clock_output id="IPG_CLK_ROOT.outFreq" value="150 MHz" locked="false" accuracy=""/>
                  <clock_output id="LCDIF_CLK_ROOT.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPI2C_CLK_ROOT.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPSPI_CLK_ROOT.outFreq" value="105.6 MHz" locked="false" accuracy=""/>
                  <clock_output id="LVDS1_CLK.outFreq" value="1.2 GHz" locked="false" accuracy=""/>
                  <clock_output id="MQS_MCLK.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="PERCLK_CLK_ROOT.outFreq" value="5 MHz" locked="false" accuracy=""/>
                  <clock_output id="PLL7_MAIN_CLK.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI1_CLK_ROOT.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI1_MCLK1.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI1_MCLK2.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI1_MCLK3.outFreq" value="1.5 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI2_CLK_ROOT.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI2_MCLK1.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI2_MCLK3.outFreq" value="1.5 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI3_CLK_ROOT.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI3_MCLK1.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI3_MCLK3.outFreq" value="1.5 MHz" locked="false" accuracy=""/>
                  <clock_output id="SEMC_CLK_ROOT.outFreq" value="132 MHz" locked="false" accuracy=""/>
                  <clock_output id="SPDIF0_CLK_ROOT.outFreq" value="1.5 MHz" locked="false" accuracy=""/>
                  <clock_output id="TRACE_CLK_ROOT.outFreq" value="88 MHz" locked="false" accuracy=""/>
                  <clock_output id="UART_CLK_ROOT.outFreq" value="4 MHz" locked="false" accuracy=""/>
                  <clock_output id="USDHC1_CLK_ROOT.outFreq" value="198 MHz" locked="false" accuracy=""/>
                  <clock_output id="USDHC2_CLK_ROOT.outFreq" value="198 MHz" locked="false" accuracy=""/>
               </clock_outputs>
               <clock_settings>
                  <setting id="CCM.ARM_PODF.scale" value="2" locked="true"/>
                  <setting id="CCM.FLEXSPI_PODF.scale" value="1" locked="false"/>
                  <setting id="CCM.LPSPI_PODF.scale" value="5" locked="false"/>
                  <setting id="CCM.PERCLK_PODF.scale" value="30" locked="false"/>
                  <setting id="CCM.SEMC_CLK_SEL.sel" value="CCM.SEMC_ALT_CLK_SEL" locked="false"/>
                  <setting id="CCM.SEMC_PODF.scale" value="3" locked="true"/>
                  <setting id="CCM_ANALOG.PLL1_BYPASS.sel" value="CCM_ANALOG.PLL1" locked="false"/>
                  <setting id="CCM_ANALOG.PLL1_PREDIV.scale" value="1" locked="true"/>
                  <setting id="CCM_ANALOG.PLL1_VDIV.scale" value="50" locked="true"/>
                  <setting id="CCM_ANALOG.PLL2.denom" value="1" locked="false"/>
                  <setting id="CCM_ANALOG.PLL2.num" value="0" locked="false"/>
                  <setting id="CCM_ANALOG.PLL2_BYPASS.sel" value="CCM_ANALOG.PLL2_OUT_CLK" locked="false"/>
                  <setting id="CCM_ANALOG.PLL2_PFD0_BYPASS.sel" value="CCM_ANALOG.PLL2_PFD0" locked="false"/>
                  <setting id="CCM_ANALOG.PLL2_PFD1_BYPASS.sel" value="CCM_ANALOG.PLL2_PFD1" locked="false"/>
                  <setting id="CCM_ANALOG.PLL2_PFD2_BYPASS.sel" value="CCM_ANALOG.PLL2_PFD2" locked="false"/>
                  <setting id="CCM_ANALOG.PLL2_PFD3_BYPASS.sel" value="CCM_ANALOG.PLL2_PFD3" locked="false"/>
               </clock_settings>
               <called_from_default_init>false</called_from_default_init>
            </clock_configuration>
            <clock_configuration name="Board_BootClockPLL480MHz" id_prefix="" prefix_user_defined="false">
               <description></description>
               <options/>
               <dependencies>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.xtali" description="&apos;XTALI&apos; (Pins tool id: XTALOSC24M.xtali, Clocks tool id: XTALOSC24M.XTALI) needs to be routed" problem_level="1" source="Clocks:Board_BootClockPLL480MHz">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.xtali" description="&apos;XTALI&apos; (Pins tool id: XTALOSC24M.xtali, Clocks tool id: XTALOSC24M.XTALI) needs to have &apos;INPUT&apos; direction" problem_level="1" source="Clocks:Board_BootClockPLL480MHz">
                     <feature name="direction" evaluation="">
                        <data>INPUT</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.xtalo" description="&apos;XTALO&apos; (Pins tool id: XTALOSC24M.xtalo, Clocks tool id: XTALOSC24M.XTALO) needs to be routed" problem_level="1" source="Clocks:Board_BootClockPLL480MHz">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.xtalo" description="&apos;XTALO&apos; (Pins tool id: XTALOSC24M.xtalo, Clocks tool id: XTALOSC24M.XTALO) needs to have &apos;OUTPUT&apos; direction" problem_level="1" source="Clocks:Board_BootClockPLL480MHz">
                     <feature name="direction" evaluation="">
                        <data>OUTPUT</data>
                     </feature>
                  </dependency>
               </dependencies>
               <clock_sources/>
               <clock_outputs>
                  <clock_output id="AHB_CLK_ROOT.outFreq" value="480 MHz" locked="false" accuracy=""/>
                  <clock_output id="CAN_CLK_ROOT.outFreq" value="2 MHz" locked="false" accuracy=""/>
                  <clock_output id="CLK_1M.outFreq" value="1 MHz" locked="false" accuracy=""/>
                  <clock_output id="CLK_24M.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="CSI_CLK_ROOT.outFreq" value="12 MHz" locked="false" accuracy=""/>
                  <clock_output id="ENET_125M_CLK.outFreq" value="2.4 MHz" locked="false" accuracy=""/>
                  <clock_output id="ENET_25M_REF_CLK.outFreq" value="1.2 MHz" locked="false" accuracy=""/>
                  <clock_output id="FLEXIO1_CLK_ROOT.outFreq" value="1.5 MHz" locked="false" accuracy=""/>
                  <clock_output id="FLEXIO2_CLK_ROOT.outFreq" value="1.5 MHz" locked="false" accuracy=""/>
                  <clock_output id="FLEXSPI_CLK_ROOT.outFreq" value="132 MHz" locked="false" accuracy=""/>
                  <clock_output id="GPT1_ipg_clk_highfreq.outFreq" value="4 MHz" locked="false" accuracy=""/>
                  <clock_output id="GPT2_ipg_clk_highfreq.outFreq" value="4 MHz" locked="false" accuracy=""/>
                  <clock_output id="IPG_CLK_ROOT.outFreq" value="120 MHz" locked="false" accuracy=""/>
                  <clock_output id="LCDIF_CLK_ROOT.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPI2C_CLK_ROOT.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPSPI_CLK_ROOT.outFreq" value="105.6 MHz" locked="false" accuracy=""/>
                  <clock_output id="LVDS1_CLK.outFreq" value="960 MHz" locked="false" accuracy=""/>
                  <clock_output id="MQS_MCLK.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="PERCLK_CLK_ROOT.outFreq" value="4 MHz" locked="false" accuracy=""/>
                  <clock_output id="PLL7_MAIN_CLK.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI1_CLK_ROOT.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI1_MCLK1.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI1_MCLK2.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI1_MCLK3.outFreq" value="1.5 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI2_CLK_ROOT.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI2_MCLK1.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI2_MCLK3.outFreq" value="1.5 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI3_CLK_ROOT.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI3_MCLK1.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI3_MCLK3.outFreq" value="1.5 MHz" locked="false" accuracy=""/>
                  <clock_output id="SEMC_CLK_ROOT.outFreq" value="132 MHz" locked="false" accuracy=""/>
                  <clock_output id="SPDIF0_CLK_ROOT.outFreq" value="1.5 MHz" locked="false" accuracy=""/>
                  <clock_output id="TRACE_CLK_ROOT.outFreq" value="88 MHz" locked="false" accuracy=""/>
                  <clock_output id="UART_CLK_ROOT.outFreq" value="4 MHz" locked="false" accuracy=""/>
                  <clock_output id="USDHC1_CLK_ROOT.outFreq" value="198 MHz" locked="false" accuracy=""/>
                  <clock_output id="USDHC2_CLK_ROOT.outFreq" value="198 MHz" locked="false" accuracy=""/>
               </clock_outputs>
               <clock_settings>
                  <setting id="CCM.ARM_PODF.scale" value="2" locked="true"/>
                  <setting id="CCM.FLEXSPI_PODF.scale" value="1" locked="false"/>
                  <setting id="CCM.LPSPI_PODF.scale" value="5" locked="false"/>
                  <setting id="CCM.PERCLK_PODF.scale" value="30" locked="false"/>
                  <setting id="CCM.SEMC_CLK_SEL.sel" value="CCM.SEMC_ALT_CLK_SEL" locked="false"/>
                  <setting id="CCM.SEMC_PODF.scale" value="3" locked="true"/>
                  <setting id="CCM_ANALOG.PLL1_BYPASS.sel" value="CCM_ANALOG.PLL1" locked="false"/>
                  <setting id="CCM_ANALOG.PLL1_PREDIV.scale" value="1" locked="true"/>
                  <setting id="CCM_ANALOG.PLL1_VDIV.scale" value="40" locked="true"/>
                  <setting id="CCM_ANALOG.PLL2.denom" value="1" locked="false"/>
                  <setting id="CCM_ANALOG.PLL2.num" value="0" locked="false"/>
                  <setting id="CCM_ANALOG.PLL2_BYPASS.sel" value="CCM_ANALOG.PLL2_OUT_CLK" locked="false"/>
                  <setting id="CCM_ANALOG.PLL2_PFD0_BYPASS.sel" value="CCM_ANALOG.PLL2_PFD0" locked="false"/>
                  <setting id="CCM_ANALOG.PLL2_PFD1_BYPASS.sel" value="CCM_ANALOG.PLL2_PFD1" locked="false"/>
                  <setting id="CCM_ANALOG.PLL2_PFD2_BYPASS.sel" value="CCM_ANALOG.PLL2_PFD2" locked="false"/>
                  <setting id="CCM_ANALOG.PLL2_PFD3_BYPASS.sel" value="CCM_ANALOG.PLL2_PFD3" locked="false"/>
               </clock_settings>
               <called_from_default_init>true</called_from_default_init>
            </clock_configuration>
            <clock_configuration name="BOARD_BootClockXT24MHz" id_prefix="" prefix_user_defined="false">
               <description></description>
               <options/>
               <dependencies>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.xtali" description="&apos;XTALI&apos; (Pins tool id: XTALOSC24M.xtali, Clocks tool id: XTALOSC24M.XTALI) needs to be routed" problem_level="1" source="Clocks:BOARD_BootClockXT24MHz">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.xtali" description="&apos;XTALI&apos; (Pins tool id: XTALOSC24M.xtali, Clocks tool id: XTALOSC24M.XTALI) needs to have &apos;INPUT&apos; direction" problem_level="1" source="Clocks:BOARD_BootClockXT24MHz">
                     <feature name="direction" evaluation="">
                        <data>INPUT</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.xtalo" description="&apos;XTALO&apos; (Pins tool id: XTALOSC24M.xtalo, Clocks tool id: XTALOSC24M.XTALO) needs to be routed" problem_level="1" source="Clocks:BOARD_BootClockXT24MHz">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.xtalo" description="&apos;XTALO&apos; (Pins tool id: XTALOSC24M.xtalo, Clocks tool id: XTALOSC24M.XTALO) needs to have &apos;OUTPUT&apos; direction" problem_level="1" source="Clocks:BOARD_BootClockXT24MHz">
                     <feature name="direction" evaluation="">
                        <data>OUTPUT</data>
                     </feature>
                  </dependency>
               </dependencies>
               <clock_sources/>
               <clock_outputs>
                  <clock_output id="AHB_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="CAN_CLK_ROOT.outFreq" value="2 MHz" locked="false" accuracy=""/>
                  <clock_output id="CLK_1M.outFreq" value="1 MHz" locked="false" accuracy=""/>
                  <clock_output id="CLK_24M.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="CSI_CLK_ROOT.outFreq" value="12 MHz" locked="false" accuracy=""/>
                  <clock_output id="ENET_125M_CLK.outFreq" value="2.4 MHz" locked="false" accuracy=""/>
                  <clock_output id="ENET_25M_REF_CLK.outFreq" value="1.2 MHz" locked="false" accuracy=""/>
                  <clock_output id="FLEXIO1_CLK_ROOT.outFreq" value="1.5 MHz" locked="false" accuracy=""/>
                  <clock_output id="FLEXIO2_CLK_ROOT.outFreq" value="1.5 MHz" locked="false" accuracy=""/>
                  <clock_output id="FLEXSPI_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="GPT1_ipg_clk_highfreq.outFreq" value="6 MHz" locked="false" accuracy=""/>
                  <clock_output id="GPT2_ipg_clk_highfreq.outFreq" value="6 MHz" locked="false" accuracy=""/>
                  <clock_output id="IPG_CLK_ROOT.outFreq" value="6 MHz" locked="false" accuracy=""/>
                  <clock_output id="LCDIF_CLK_ROOT.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPI2C_CLK_ROOT.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPSPI_CLK_ROOT.outFreq" value="6 MHz" locked="false" accuracy=""/>
                  <clock_output id="LVDS1_CLK.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="MQS_MCLK.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="PERCLK_CLK_ROOT.outFreq" value="6 MHz" locked="false" accuracy=""/>
                  <clock_output id="PLL7_MAIN_CLK.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI1_CLK_ROOT.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI1_MCLK1.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI1_MCLK2.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI1_MCLK3.outFreq" value="1.5 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI2_CLK_ROOT.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI2_MCLK1.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI2_MCLK3.outFreq" value="1.5 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI3_CLK_ROOT.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI3_MCLK1.outFreq" value="3 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI3_MCLK3.outFreq" value="1.5 MHz" locked="false" accuracy=""/>
                  <clock_output id="SEMC_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="SPDIF0_CLK_ROOT.outFreq" value="1.5 MHz" locked="false" accuracy=""/>
                  <clock_output id="TRACE_CLK_ROOT.outFreq" value="6 MHz" locked="false" accuracy=""/>
                  <clock_output id="UART_CLK_ROOT.outFreq" value="4 MHz" locked="false" accuracy=""/>
                  <clock_output id="USDHC1_CLK_ROOT.outFreq" value="12 MHz" locked="false" accuracy=""/>
                  <clock_output id="USDHC2_CLK_ROOT.outFreq" value="12 MHz" locked="false" accuracy=""/>
               </clock_outputs>
               <clock_settings>
                  <setting id="CCM.ARM_PODF.scale" value="1" locked="false"/>
                  <setting id="CCM.FLEXSPI_PODF.scale" value="1" locked="false"/>
                  <setting id="CCM.SEMC_PODF.scale" value="1" locked="false"/>
                  <setting id="CCM_ANALOG.PLL2.denom" value="1" locked="false"/>
                  <setting id="CCM_ANALOG.PLL2.num" value="0" locked="false"/>
                  <setting id="CCM_ANALOG_PLL_ARM_POWERDOWN_CFG" value="Yes" locked="false"/>
                  <setting id="CCM_ANALOG_PLL_SYS_POWERDOWN_CFG" value="Yes" locked="false"/>
               </clock_settings>
               <called_from_default_init>false</called_from_default_init>
            </clock_configuration>
         </clock_configurations>
      </clocks>
      <dcdx name="DCDx" version="3.0" enabled="true" update_project_code="true">
         <generated_project_files>
            <file path="board/dcd.c" update_enabled="true"/>
            <file path="board/dcd.h" update_enabled="true"/>
         </generated_project_files>
         <dcdx_profile>
            <processor_version>12.0.0</processor_version>
            <output_format>c_array</output_format>
         </dcdx_profile>
         <dcdx_configurations>
            <dcdx_configuration name="Device_configuration">
               <description></description>
               <options/>
               <command_groups/>
            </dcdx_configuration>
         </dcdx_configurations>
      </dcdx>
      <periphs name="Peripherals" version="11.0" enabled="true" update_project_code="true">
         <generated_project_files>
            <file path="board/peripherals.c" update_enabled="true"/>
            <file path="board/peripherals.h" update_enabled="true"/>
         </generated_project_files>
         <peripherals_profile>
            <processor_version>12.0.0</processor_version>
         </peripherals_profile>
         <functional_groups>
            <functional_group name="BOARD_InitPeripherals" uuid="19596643-a9d0-4000-b44d-6a0a05ec6830" called_from_default_init="true" id_prefix="" core="core0">
               <description></description>
               <options/>
               <dependencies/>
               <instances>
                  <instance name="NVIC" uuid="1ea08f7e-6d63-496f-a2f8-afb586fcebda" type="nvic" type_id="nvic_57b5eef3774cc60acaede6f5b8bddc67" mode="general" peripheral="NVIC" enabled="true" comment="" custom_name_enabled="false" editing_lock="false">
                     <config_set name="nvic">
                        <array name="interrupt_table"/>
                        <array name="interrupts"/>
                     </config_set>
                  </instance>
               </instances>
            </functional_group>
         </functional_groups>
         <components>
            <component name="system" uuid="15dd8f93-af91-460f-bf18-e4690cacdf7a" type_id="system_54b53072540eeeb8f8e9343e71f28176">
               <config_set_global name="global_system_definitions">
                  <setting name="user_definitions" value=""/>
                  <setting name="user_includes" value=""/>
               </config_set_global>
            </component>
            <component name="generic_enet" uuid="83ad6b24-4c84-45fd-82f6-36a320c6584f" type_id="generic_enet_74db5c914f0ddbe47d86af40cb77a619">
               <config_set_global name="global_enet"/>
            </component>
            <component name="gpio_adapter_common" uuid="d0ace3e4-b997-45d9-9572-66b0f4477747" type_id="gpio_adapter_common_57579b9ac814fe26bf95df0a384c36b6">
               <config_set_global name="global_gpio_adapter_common" quick_selection="default"/>
            </component>
            <component name="generic_uart" uuid="b3518c29-6dfa-44a7-b827-3e309f43befb" type_id="generic_uart_8cae00565451cf2346eb1b8c624e73a6">
               <config_set_global name="global_uart"/>
            </component>
            <component name="msg" uuid="e7a64295-f50c-465d-8bc3-2368a3aa31b2" type_id="msg_6e2baaf3b97dbeef01c0043275f9a0e7">
               <config_set_global name="global_messages"/>
            </component>
            <component name="uart_cmsis_common" uuid="d8a500d0-50a9-4f87-97c6-fda4e85c179e" type_id="uart_cmsis_common_9cb8e302497aa696fdbb5a4fd622c2a8">
               <config_set_global name="global_USART_CMSIS_common" quick_selection="default"/>
            </component>
            <component name="generic_can" uuid="4ecd0fd3-5bcc-4194-94d3-3736df7b752b" type_id="generic_can_1bfdd78b1af214566c1f23cf6a582d80">
               <config_set_global name="global_can"/>
            </component>
         </components>
      </periphs>
      <tee name="TEE" version="4.0" enabled="false" update_project_code="true">
         <generated_project_files/>
         <tee_profile>
            <processor_version>N/A</processor_version>
         </tee_profile>
      </tee>
   </tools>
</configuration>