(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 4.69)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" signal)
    (2 "In2.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 2" (type "prepreg") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 3" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints yes)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "VDDF")
  (net 2 "GND")
  (net 3 "/Sensor_Controller/LPC_~{RST}")
  (net 4 "Net-(C10-Pad1)")
  (net 5 "Net-(C11-Pad2)")
  (net 6 "VCC")
  (net 7 "/Power_Management/PS_SWITCH")
  (net 8 "/Power_Management/LED_A")
  (net 9 "VDD")
  (net 10 "Net-(C20-Pad1)")
  (net 11 "Net-(C22-Pad1)")
  (net 12 "Net-(C22-Pad2)")
  (net 13 "Net-(C23-Pad2)")
  (net 14 "Net-(C24-Pad2)")
  (net 15 "/WiFi_Display/PREVGH")
  (net 16 "/WiFi_Display/PREVGL")
  (net 17 "Net-(C27-Pad2)")
  (net 18 "Net-(C29-Pad2)")
  (net 19 "Net-(C30-Pad2)")
  (net 20 "Net-(C31-Pad2)")
  (net 21 "Net-(C32-Pad2)")
  (net 22 "Net-(D1-Pad2)")
  (net 23 "Net-(D1-Pad3)")
  (net 24 "Net-(D1-Pad4)")
  (net 25 "VBUS")
  (net 26 "unconnected-(J3-Pad3)")
  (net 27 "unconnected-(J3-Pad4)")
  (net 28 "/Power_Management/LED_K")
  (net 29 "unconnected-(J4-Pad1)")
  (net 30 "/WiFi_Display/GDR")
  (net 31 "/WiFi_Display/RESE")
  (net 32 "unconnected-(J4-Pad6)")
  (net 33 "unconnected-(J4-Pad7)")
  (net 34 "/WiFi_Display/EPD_BUSY")
  (net 35 "/WiFi_Display/EPD_~{RES}")
  (net 36 "/WiFi_Display/EPD_D{slash}~{C}")
  (net 37 "/WiFi_Display/EPD_CS")
  (net 38 "/WiFi_Display/EPD_SCLK")
  (net 39 "/WiFi_Display/EPD_SDI")
  (net 40 "/Sensor_Controller/LPC_~{ISP}")
  (net 41 "/Sensor_Controller/I2C_SDA")
  (net 42 "/Sensor_Controller/I2C_SCL")
  (net 43 "/Sensor_Controller/LPC_SWDIO")
  (net 44 "/Sensor_Controller/LPC_SWCLK")
  (net 45 "/Sensor_Controller/CAPT_X0")
  (net 46 "Net-(R10-Pad2)")
  (net 47 "Net-(R11-Pad1)")
  (net 48 "/Sensor_Controller/CAPT_X1")
  (net 49 "Net-(R13-Pad2)")
  (net 50 "Net-(R14-Pad2)")
  (net 51 "/Sensor_Controller/CAPT_X2")
  (net 52 "Net-(R16-Pad2)")
  (net 53 "Net-(R17-Pad2)")
  (net 54 "/Sensor_Controller/CAPT_X3")
  (net 55 "Net-(R19-Pad2)")
  (net 56 "Net-(R20-Pad2)")
  (net 57 "/Sensor_Controller/CAPT_X4")
  (net 58 "Net-(R22-Pad1)")
  (net 59 "/Power_Management/ADC_BAT")
  (net 60 "Net-(R27-Pad2)")
  (net 61 "Net-(J2-PadA5)")
  (net 62 "Net-(J2-PadB5)")
  (net 63 "/Sensor_Controller/CAPT_YH")
  (net 64 "/Sensor_Controller/LSM_A0")
  (net 65 "/Sensor_Controller/LSM_INT1")
  (net 66 "/Sensor_Controller/LSM_INT2")
  (net 67 "unconnected-(U1-Pad10)")
  (net 68 "unconnected-(U1-Pad11)")
  (net 69 "/Sensor_Controller/SPI_CS")
  (net 70 "/Power_Management/LED_PWM")
  (net 71 "/Sensor_Controller/ALS_INT")
  (net 72 "/Sensor_Controller/RTC_CLKO")
  (net 73 "/Sensor_Controller/RTC_INT")
  (net 74 "/Sensor_Controller/CAPT_YL")
  (net 75 "/Power_Management/DCDC_EN")
  (net 76 "/Power_Management/CHG_~{STBY}")
  (net 77 "/Power_Management/CHG_~{ACT}")
  (net 78 "/Sensor_Controller/SPI_~{INT}")
  (net 79 "/Sensor_Controller/SPI_MISO")
  (net 80 "Net-(U6-Pad2)")
  (net 81 "Net-(L1-Pad1)")
  (net 82 "Net-(L2-Pad1)")
  (net 83 "/WiFi_Display/USB_D+")
  (net 84 "/WiFi_Display/USB_D-")
  (net 85 "unconnected-(U12-Pad4)")
  (net 86 "unconnected-(U12-Pad7)")
  (net 87 "unconnected-(U12-Pad9)")
  (net 88 "unconnected-(U12-Pad10)")
  (net 89 "unconnected-(U12-Pad12)")
  (net 90 "unconnected-(U12-Pad15)")
  (net 91 "unconnected-(U12-Pad17)")
  (net 92 "Net-(SW3-Pad2)")
  (net 93 "unconnected-(U12-Pad24)")
  (net 94 "unconnected-(U12-Pad25)")
  (net 95 "unconnected-(U12-Pad28)")
  (net 96 "unconnected-(U12-Pad29)")
  (net 97 "/WiFi_Display/UART_RX")
  (net 98 "/WiFi_Display/UART_TX")
  (net 99 "unconnected-(U12-Pad32)")
  (net 100 "unconnected-(U12-Pad33)")
  (net 101 "unconnected-(U12-Pad34)")
  (net 102 "unconnected-(U12-Pad35)")
  (net 103 "Net-(BT1-Pad1)")
  (net 104 "unconnected-(J1-Pad6)")
  (net 105 "unconnected-(J1-Pad7)")
  (net 106 "unconnected-(J1-Pad8)")
  (net 107 "unconnected-(U4-Pad2)")

  (footprint "Touch_Sensor:CapTouch_Mutual_5X_Slider" (layer "F.Cu")
    (tedit 0) (tstamp 14df72c9-e155-4a3d-8347-b6e900e6bc7f)
    (at 151.125 154.875)
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/7fcaff45-24f7-4019-910f-2a69e797182e")
    (attr smd)
    (fp_text reference "T1" (at 0 -0.5 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cfffd5be-696c-4a75-b363-9f52da1ac285)
    )
    (fp_text value "Cap_Touch_Slider_5P" (at 0.1 1.35 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d9568371-27e2-456d-a11e-d19c902fc830)
    )
    (fp_text user "${REF}" (at 0 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a3cc1b42-4b3a-424a-aa5c-26acb897bc12)
    )
    (fp_line (start -36.5 -9.75) (end -8.75 -9.75) (layer "Dwgs.User") (width 0.1) (tstamp 7ba6a009-e643-40c7-893d-de2eea49a59e))
    (pad "1" smd custom (at -36.5 -5.75) (size 0 0) (layers "F.Cu")
      (net 45 "/Sensor_Controller/CAPT_X0") (pinfunction "X0") (pintype "passive")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0 4)
            (xy 0 -4)
            (xy 7 -4)
            (xy 1.4 -2)
            (xy 12.6 2)
            (xy 7 4)
          ) (width 0.1) (fill yes))
      ) (tstamp 57c27e7b-0707-4c7a-8eaa-c986dc5335cd))
    (pad "2" smd custom (at -28.5 -5.75) (size 0 0) (layers "F.Cu")
      (net 46 "Net-(R10-Pad2)") (pinfunction "X01A") (pintype "passive")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0 4)
            (xy 5.6 2)
            (xy -5.6 -2)
            (xy 0 -4)
            (xy 4.2 -4)
            (xy -1.4 -2)
            (xy 9.8 2)
            (xy 4.2 4)
          ) (width 0.1) (fill yes))
      ) (tstamp 6c688073-4cf2-44a3-ad15-cc81b4805281))
    (pad "3" smd custom (at -23.25 -5.75) (size 0 0) (layers "F.Cu")
      (net 47 "Net-(R11-Pad1)") (pinfunction "X01B") (pintype "passive")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0 4)
            (xy 5.6 2)
            (xy -5.6 -2)
            (xy 0 -4)
            (xy 4.2 -4)
            (xy -1.4 -2)
            (xy 9.8 2)
            (xy 4.2 4)
          ) (width 0.1) (fill yes))
      ) (tstamp ac2bc500-6b86-4596-84d4-f27a430de0a3))
    (pad "4" smd custom (at -18 -5.75) (size 0 0) (layers "F.Cu")
      (net 48 "/Sensor_Controller/CAPT_X1") (pinfunction "X1") (pintype "passive")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0 4)
            (xy 5.6 2)
            (xy -5.6 -2)
            (xy 0 -4)
            (xy 4.2 -4)
            (xy -1.4 -2)
            (xy 9.8 2)
            (xy 4.2 4)
          ) (width 0.1) (fill yes))
      ) (tstamp 671ce051-aed3-4bee-b25b-f4764bdb7dab))
    (pad "5" smd custom (at -12.75 -5.75) (size 0 0) (layers "F.Cu")
      (net 49 "Net-(R13-Pad2)") (pinfunction "X12A") (pintype "passive")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0 4)
            (xy 5.6 2)
            (xy -5.6 -2)
            (xy 0 -4)
            (xy 4.2 -4)
            (xy -1.4 -2)
            (xy 9.8 2)
            (xy 4.2 4)
          ) (width 0.1) (fill yes))
      ) (tstamp 33495e4c-870a-4d5f-ac75-4f5a7798799c))
    (pad "6" smd custom (at -7.5 -5.75) (size 0 0) (layers "F.Cu")
      (net 50 "Net-(R14-Pad2)") (pinfunction "X12B") (pintype "passive")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0 4)
            (xy 5.6 2)
            (xy -5.6 -2)
            (xy 0 -4)
            (xy 4.2 -4)
            (xy -1.4 -2)
            (xy 9.8 2)
            (xy 4.2 4)
          ) (width 0.1) (fill yes))
      ) (tstamp 9d34178c-3780-4616-9cd9-dd6bd15fc336))
    (pad "7" smd custom (at -2.25 -5.75) (size 0 0) (layers "F.Cu")
      (net 51 "/Sensor_Controller/CAPT_X2") (pinfunction "X2") (pintype "passive")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0 4)
            (xy 5.6 2)
            (xy -5.6 -2)
            (xy 0 -4)
            (xy 4.2 -4)
            (xy -1.4 -2)
            (xy 9.8 2)
            (xy 4.2 4)
          ) (width 0.1) (fill yes))
      ) (tstamp 3c2e30cf-c19f-4576-af9b-8733224f3ac8))
    (pad "8" smd custom (at 3 -5.75) (size 0 0) (layers "F.Cu")
      (net 52 "Net-(R16-Pad2)") (pinfunction "X23A") (pintype "passive")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0 4)
            (xy 5.6 2)
            (xy -5.6 -2)
            (xy 0 -4)
            (xy 4.2 -4)
            (xy -1.4 -2)
            (xy 9.8 2)
            (xy 4.2 4)
          ) (width 0.1) (fill yes))
      ) (tstamp fda40f44-f179-4a2d-817d-d95009283973))
    (pad "9" smd custom (at 8.25 -5.75) (size 0 0) (layers "F.Cu")
      (net 53 "Net-(R17-Pad2)") (pinfunction "X23B") (pintype "passive")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0 4)
            (xy 5.6 2)
            (xy -5.6 -2)
            (xy 0 -4)
            (xy 4.2 -4)
            (xy -1.4 -2)
            (xy 9.8 2)
            (xy 4.2 4)
          ) (width 0.1) (fill yes))
      ) (tstamp a3b967b2-5201-4494-a7f2-ec05d34f0df8))
    (pad "10" smd custom (at 13.5 -5.75) (size 0 0) (layers "F.Cu")
      (net 54 "/Sensor_Controller/CAPT_X3") (pinfunction "X3") (pintype "passive")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0 4)
            (xy 5.6 2)
            (xy -5.6 -2)
            (xy 0 -4)
            (xy 4.2 -4)
            (xy -1.4 -2)
            (xy 9.8 2)
            (xy 4.2 4)
          ) (width 0.1) (fill yes))
      ) (tstamp 72921563-3713-47a1-905d-8c7fb542b379))
    (pad "11" smd custom (at 18.75 -5.75) (size 0 0) (layers "F.Cu")
      (net 55 "Net-(R19-Pad2)") (pinfunction "X34A") (pintype "passive")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0 4)
            (xy 5.6 2)
            (xy -5.6 -2)
            (xy 0 -4)
            (xy 4.2 -4)
            (xy -1.4 -2)
            (xy 9.8 2)
            (xy 4.2 4)
          ) (width 0.1) (fill yes))
      ) (tstamp 6cdb8450-a8a3-43ec-9ba1-87eb59a8b3d0))
    (pad "12" smd custom (at 24 -5.75) (size 0 0) (layers "F.Cu")
      (net 56 "Net-(R20-Pad2)") (pinfunction "X34B") (pintype "passive")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0 4)
            (xy 5.6 2)
            (xy -5.6 -2)
            (xy 0 -4)
            (xy 4.2 -4)
            (xy -1.4 -2)
            (xy 9.8 2)
            (xy 4.2 4)
          ) (width 0.1) (fill yes))
      ) (tstamp 79d5e945-1469-430b-9eaa-ebf88e397ac7))
    (pad "13" smd custom (at 36.25 -5.75 180) (size 0 0) (layers "F.Cu")
      (net 57 "/Sensor_Controller/CAPT_X4") (pinfunction "X4") (pintype "passive")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0 4)
            (xy 0 -4)
            (xy 7 -4)
            (xy 1.4 -2)
            (xy 12.6 2)
            (xy 7 4)
          ) (width 0.1) (fill yes))
      ) (tstamp 43504a86-7a43-4f8f-9e63-19fed5a2d3e2))
    (pad "14" smd custom (at 36.25 -5.75 180) (size 0 0) (layers "B.Cu")
      (net 63 "/Sensor_Controller/CAPT_YH") (pinfunction "YH") (pintype "passive")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 0 4) (end 0 -4) (width 0.45))
        (gr_line (start 72 4) (end 0 4) (width 0.45))
        (gr_line (start 72 -4) (end 0 -4) (width 0.45))
        (gr_line (start 72 0) (end 0 0) (width 0.45))
      ) (tstamp f51aefec-3b86-41f1-91a4-91153e1e8d77))
    (zone (net 0) (net_name "") (layers *.Cu) (tstamp 85c0f213-9cad-4785-bf1b-62084759b464) (hatch edge 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254)
      (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 187.625 153.375)
          (xy 114.375 153.375)
          (xy 114.375 144.875)
          (xy 187.625 144.875)
        )
      )
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 1926dfd2-fa9a-459a-9831-251deda68485)
    (at 193.4 154.3)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/00dacdc9-2378-49a8-b5b4-fb10ee89b4a3")
    (attr smd)
    (fp_text reference "R30" (at 0 -1.17) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4c278fa2-e2c7-4088-aad5-34295374b8e1)
    )
    (fp_text value "5k1" (at 0 1.17) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 76b8d1b1-fb34-4a44-a70f-835a8c800651)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)))
      (tstamp 874acfff-5174-4f7d-8e28-1787542b91b5)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "F.SilkS") (width 0.12) (tstamp 414c03ba-82ad-4be2-99e8-e3e59b10f4e1))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "F.SilkS") (width 0.12) (tstamp ea5bc969-f012-40c1-a407-e262633f4e84))
    (fp_line (start -0.93 0.47) (end -0.93 -0.47) (layer "F.CrtYd") (width 0.05) (tstamp 1029d08e-05b6-4670-a745-8e219be9ce2e))
    (fp_line (start 0.93 -0.47) (end 0.93 0.47) (layer "F.CrtYd") (width 0.05) (tstamp 8380926f-b40d-4750-8030-17278e9fcffa))
    (fp_line (start 0.93 0.47) (end -0.93 0.47) (layer "F.CrtYd") (width 0.05) (tstamp 96a8b84f-53ba-4421-8070-869a580f98b9))
    (fp_line (start -0.93 -0.47) (end 0.93 -0.47) (layer "F.CrtYd") (width 0.05) (tstamp bab33f0e-b95d-49c9-9950-7069845fefeb))
    (fp_line (start 0.525 -0.27) (end 0.525 0.27) (layer "F.Fab") (width 0.1) (tstamp 292c7d73-8aa4-45c5-876a-c95d0603c9e3))
    (fp_line (start -0.525 -0.27) (end 0.525 -0.27) (layer "F.Fab") (width 0.1) (tstamp 9a66b406-c023-4005-8e79-4d7ad7bc268c))
    (fp_line (start -0.525 0.27) (end -0.525 -0.27) (layer "F.Fab") (width 0.1) (tstamp a344e292-2023-49dc-b9c2-b91cdb1b775b))
    (fp_line (start 0.525 0.27) (end -0.525 0.27) (layer "F.Fab") (width 0.1) (tstamp d47709da-cd12-45d8-a54a-9a32aab30ef4))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(J2-PadB5)") (pintype "passive") (tstamp b94abc15-0c7a-411f-9d01-e1b1f3279c81))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 1715e392-1094-48c5-bdbc-0fd8cc5243fe))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "LED_SMD:LED_Lumex_SML-LX0404SIUPGUSB" (layer "F.Cu")
    (tedit 5DDA4ABB) (tstamp 227d7d66-a27f-4daf-8f25-b3a33d60e86e)
    (at 195 107)
    (descr "Lumex RGB LED, clear, SMD, https://www.lumex.com/spec/SML-LX0404SIUPGUSB.pdf")
    (tags "LED RGB")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/b9b42071-a3cd-4576-9a71-5529d1a4b62d")
    (attr smd)
    (fp_text reference "D1" (at 0 -1.75) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d11255dc-72d0-4047-ae66-f096b8272334)
    )
    (fp_text value "FC-B1010RGBT-HG" (at 0 2.79) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1335ac4d-8eb2-410f-8026-d1a518e8be60)
    )
    (fp_text user "${REFERENCE}" (at 0 -1) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.1)))
      (tstamp 0b0d7583-29e0-4fc5-bdca-2702083504ef)
    )
    (fp_line (start -0.825 -0.825) (end -0.825 -0.25) (layer "F.SilkS") (width 0.1) (tstamp 54503d77-32e9-4efe-a95b-4fb4ad74efde))
    (fp_line (start -0.25 -0.825) (end -0.825 -0.825) (layer "F.SilkS") (width 0.1) (tstamp 5ddbd7ce-0731-4610-8519-caec22b01dc1))
    (fp_line (start 0.9 0.9) (end 0.9 -0.9) (layer "F.CrtYd") (width 0.05) (tstamp 44c37f3c-0075-40f7-8b23-6493941b7392))
    (fp_line (start -0.9 0.9) (end 0.9 0.9) (layer "F.CrtYd") (width 0.05) (tstamp 66544ef9-8bc2-40c4-a338-a1836641f0ca))
    (fp_line (start -0.9 -0.9) (end -0.9 0.9) (layer "F.CrtYd") (width 0.05) (tstamp 66618269-42ce-4ec2-b4af-a2b93d31703a))
    (fp_line (start 0.9 -0.9) (end -0.9 -0.9) (layer "F.CrtYd") (width 0.05) (tstamp 6bb06277-2884-46e3-a443-37bc1e518134))
    (fp_line (start 0.5 0.5) (end 0.5 -0.5) (layer "F.Fab") (width 0.1) (tstamp 53f54166-47e0-4ca1-aac6-da2217742358))
    (fp_line (start 0.5 -0.5) (end -0.25 -0.5) (layer "F.Fab") (width 0.1) (tstamp 67b1b279-e142-4020-9046-55d2843446c1))
    (fp_line (start -0.25 -0.5) (end -0.5 -0.25) (layer "F.Fab") (width 0.1) (tstamp c157df10-5482-4496-88b2-f6db41cee92b))
    (fp_line (start -0.5 -0.25) (end -0.5 0.5) (layer "F.Fab") (width 0.1) (tstamp efe69f82-2599-4af7-a698-7ba32b71683c))
    (fp_line (start -0.5 0.5) (end 0.5 0.5) (layer "F.Fab") (width 0.1) (tstamp f634123a-43a1-4757-9fb6-aa283060443d))
    (pad "1" smd roundrect (at -0.425 -0.425) (size 0.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pinfunction "A") (pintype "passive") (tstamp 098c9f7e-d0a1-4423-9452-6eb3b6c6ba89))
    (pad "2" smd roundrect (at 0.425 -0.425) (size 0.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(D1-Pad2)") (pinfunction "RK") (pintype "passive") (tstamp f440d6e5-291a-4ab2-8a6a-6be070c8146d))
    (pad "3" smd roundrect (at 0.425 0.425) (size 0.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(D1-Pad3)") (pinfunction "GK") (pintype "passive") (tstamp 5112af12-dcdd-4bb9-a9dc-1755363bf833))
    (pad "4" smd roundrect (at -0.425 0.425) (size 0.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(D1-Pad4)") (pinfunction "BK") (pintype "passive") (tstamp 0f043b1b-2189-44d9-8231-3e70097a7545))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_Lumex_SML-LX0404SIUPGUSB.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp f6c499bf-713a-4eae-8077-768814858d90)
    (at 193.4 153.3)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/601ad21f-7a43-42d7-951b-ab43a9658bba")
    (attr smd)
    (fp_text reference "R29" (at 0 -1.17) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 438b9b1b-5d6d-4ee9-8935-0391245734ae)
    )
    (fp_text value "5k1" (at 0 1.17) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a9fd1f24-7775-4107-a609-ce2e0d4e5739)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)))
      (tstamp f6321d6f-b783-475a-83a2-955ed39a82ef)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "F.SilkS") (width 0.12) (tstamp 94e6b51c-0d6b-4337-93ac-10c2c7caebfe))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "F.SilkS") (width 0.12) (tstamp ed702624-fc1e-4d8c-ac42-bbb6f4e312d3))
    (fp_line (start 0.93 0.47) (end -0.93 0.47) (layer "F.CrtYd") (width 0.05) (tstamp 59d2da2d-d564-41e2-a204-e51505f3be8d))
    (fp_line (start -0.93 -0.47) (end 0.93 -0.47) (layer "F.CrtYd") (width 0.05) (tstamp a864e3c7-c74a-4222-8c6f-acab6778da44))
    (fp_line (start 0.93 -0.47) (end 0.93 0.47) (layer "F.CrtYd") (width 0.05) (tstamp d504e502-d729-4a95-b5b5-ab5c5d33e344))
    (fp_line (start -0.93 0.47) (end -0.93 -0.47) (layer "F.CrtYd") (width 0.05) (tstamp fd6f898a-3479-4e50-9bce-87fc2ad1c8e4))
    (fp_line (start 0.525 0.27) (end -0.525 0.27) (layer "F.Fab") (width 0.1) (tstamp 055cbd53-fc55-453f-8612-add19b54906e))
    (fp_line (start 0.525 -0.27) (end 0.525 0.27) (layer "F.Fab") (width 0.1) (tstamp 0eca223e-fbce-437c-9375-ef149ba2d576))
    (fp_line (start -0.525 -0.27) (end 0.525 -0.27) (layer "F.Fab") (width 0.1) (tstamp 6d02d587-9303-4705-8868-de01a16d2afc))
    (fp_line (start -0.525 0.27) (end -0.525 -0.27) (layer "F.Fab") (width 0.1) (tstamp 9edbbd5f-057f-49bc-a2e4-a5b73351b3fc))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(J2-PadA5)") (pintype "passive") (tstamp 8465d87c-ccc1-4934-9008-a1f9727ef81c))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 2339b9d6-2414-4225-a6b9-f49dc110a56b))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_SO:MSOP-8_3x3mm_P0.65mm" (layer "B.Cu")
    (tedit 5E509FDD) (tstamp 034f9683-0fc4-4a40-b806-ad28dfb318ea)
    (at 164.6 136.2 180)
    (descr "MSOP, 8 Pin (https://www.jedec.org/system/files/docs/mo-187F.pdf variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "MSOP SO")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/f34a969a-2b53-42a3-8a58-dcfec9de65d9")
    (attr smd)
    (fp_text reference "U6" (at 0 2.45) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 3d239003-a982-42b2-96f2-cc87a2df6b86)
    )
    (fp_text value "PCF8563TS" (at 0 -2.45) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7f584bf8-05a6-47ae-9727-599edcb214da)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.75 0.75) (thickness 0.11)) (justify mirror))
      (tstamp 1e9047c5-4abd-4738-b89d-ac697fb155b6)
    )
    (fp_line (start 0 1.61) (end 1.5 1.61) (layer "B.SilkS") (width 0.12) (tstamp 70c66147-3203-4a50-a1c4-7e1ef7972096))
    (fp_line (start 0 -1.61) (end 1.5 -1.61) (layer "B.SilkS") (width 0.12) (tstamp 99ecfcdf-ccd1-432b-be17-8e1fc8c1ae74))
    (fp_line (start 0 1.61) (end -2.925 1.61) (layer "B.SilkS") (width 0.12) (tstamp e19e0098-16c6-4d7a-a489-33e040b0a0ea))
    (fp_line (start 0 -1.61) (end -1.5 -1.61) (layer "B.SilkS") (width 0.12) (tstamp e4aa84d1-c696-474d-937b-31469018d42f))
    (fp_line (start 3.18 1.75) (end -3.18 1.75) (layer "B.CrtYd") (width 0.05) (tstamp 3eacd064-0daf-48b2-ac37-2b03bb622197))
    (fp_line (start -3.18 1.75) (end -3.18 -1.75) (layer "B.CrtYd") (width 0.05) (tstamp 4a67c36a-f9e3-44ae-8ced-6a64e98c8259))
    (fp_line (start -3.18 -1.75) (end 3.18 -1.75) (layer "B.CrtYd") (width 0.05) (tstamp 54cdfb53-4090-4a09-b3fe-b47ef69b33bf))
    (fp_line (start 3.18 -1.75) (end 3.18 1.75) (layer "B.CrtYd") (width 0.05) (tstamp ff8cc47a-6056-42c0-a36b-78ac820375e8))
    (fp_line (start -0.75 1.5) (end 1.5 1.5) (layer "B.Fab") (width 0.1) (tstamp 087c3d89-10ef-43af-b16b-4ca34978f689))
    (fp_line (start 1.5 -1.5) (end -1.5 -1.5) (layer "B.Fab") (width 0.1) (tstamp 5b34678f-a230-4b26-92bf-36962adeee1c))
    (fp_line (start 1.5 1.5) (end 1.5 -1.5) (layer "B.Fab") (width 0.1) (tstamp b1fc3668-a718-44ef-98af-38f7653da7f1))
    (fp_line (start -1.5 0.75) (end -0.75 1.5) (layer "B.Fab") (width 0.1) (tstamp c8be6b47-48a4-4615-aaa6-b280a99459e5))
    (fp_line (start -1.5 -1.5) (end -1.5 0.75) (layer "B.Fab") (width 0.1) (tstamp f2b8d59c-82da-47a7-ab02-dcbb808d8bbc))
    (pad "1" smd roundrect (at -2.1125 0.975 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C11-Pad2)") (pinfunction "OSCI") (pintype "input") (tstamp 1b028326-3b4b-427d-aa8a-634f2aa774cb))
    (pad "2" smd roundrect (at -2.1125 0.325 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 80 "Net-(U6-Pad2)") (pinfunction "OSCO") (pintype "output") (tstamp 2300159b-b078-4250-b47c-762f2eeedeb3))
    (pad "3" smd roundrect (at -2.1125 -0.325 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 73 "/Sensor_Controller/RTC_INT") (pinfunction "~{INT}") (pintype "output") (tstamp 11d99526-4c54-410a-adb9-4941099e35a9))
    (pad "4" smd roundrect (at -2.1125 -0.975 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp fcf2ab7a-ab02-4c90-8a5a-073a64893796))
    (pad "5" smd roundrect (at 2.1125 -0.975 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 41 "/Sensor_Controller/I2C_SDA") (pinfunction "SDA") (pintype "bidirectional") (tstamp d67b858f-a429-46be-a47e-3089844f9a73))
    (pad "6" smd roundrect (at 2.1125 -0.325 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 42 "/Sensor_Controller/I2C_SCL") (pinfunction "SCL") (pintype "input") (tstamp 17c297bc-e69d-4c7a-a626-06b5946cc20c))
    (pad "7" smd roundrect (at 2.1125 0.325 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 72 "/Sensor_Controller/RTC_CLKO") (pinfunction "CLKO") (pintype "output") (tstamp 84d6a252-792d-4756-8d90-5bc49be5c649))
    (pad "8" smd roundrect (at 2.1125 0.975 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pinfunction "VDD") (pintype "power_in") (tstamp 39cd3654-bd60-47d1-b8ec-fc743ff8a937))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/MSOP-8_3x3mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 0636146e-9994-41c5-917b-a153fb5c4a01)
    (at 170.7 135.42 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/96e0fa9f-4507-4a4a-9ffb-5ab0c8bcb735")
    (attr smd)
    (fp_text reference "C11" (at 0 1.16 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp b42b7e53-8a93-4621-a1ee-d66a7f63b7ae)
    )
    (fp_text value "12pF" (at 0 -1.16 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 13155ded-fcfe-404e-9e67-5e03948ccb85)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
      (tstamp 7ca6a0ee-aa22-4a1b-9665-d9e2af80d75e)
    )
    (fp_line (start -0.107836 0.36) (end 0.107836 0.36) (layer "B.SilkS") (width 0.12) (tstamp 4af68891-d2f8-4ae0-a32e-ae9397bea0de))
    (fp_line (start -0.107836 -0.36) (end 0.107836 -0.36) (layer "B.SilkS") (width 0.12) (tstamp e3d66935-5a40-4671-98d1-42115a97498b))
    (fp_line (start -0.91 0.46) (end 0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 1655dc0e-ba48-432b-aac7-2f1979188896))
    (fp_line (start 0.91 0.46) (end 0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 6db2e7ab-c862-41c6-a36b-f006f4b39227))
    (fp_line (start 0.91 -0.46) (end -0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 9ea7b523-0f11-4833-ac5d-e7c07fb0cbe0))
    (fp_line (start -0.91 -0.46) (end -0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp f8966627-b967-4136-b063-bfbb96322ffb))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 106cb87d-df5d-4634-95da-e0f94baf6ba0))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 5d6d7ce9-5521-4d13-b9a4-6757692fdc81))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp d552cd7f-a889-46bc-94eb-b3882fdae4d3))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp ff786075-2d10-489e-9eb5-53ae274c23a6))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 0fa6e7d2-7806-427f-a852-c7ee6f764a8c))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C11-Pad2)") (pintype "passive") (tstamp 0d625222-a631-4b47-bf5e-5c9392850038))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 06379db1-87be-4496-965b-ca45806e0f0e)
    (at 180 154)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/4e156625-9fd4-4d5d-ad39-7ecbeed0c927")
    (attr smd)
    (fp_text reference "R21" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 8b1a72d4-167d-4b93-806a-8192a572b7b7)
    )
    (fp_text value "2.2k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp db4118ec-4a2d-41f8-9c7c-f4ed2ac071af)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp ecb0578b-34e7-4ce1-abfd-00d58ed5dee0)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 1be5c6fc-d915-413d-891a-30b8e50c9be4))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp f93d209e-ea37-4a3d-8f4f-c0d353046cea))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 3004f14d-f4a4-4d22-b55b-29ecf5f5c3f7))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 9617491b-fdc7-4c3f-bd75-defb5998ad2f))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp c404f95d-a41e-475e-8266-bcfab9203f28))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp fc3ed583-9ea3-46e0-b6a1-3801576595cf))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 4a05cffd-e671-4b09-85b7-bb37226e012a))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 4f81e6b7-c3f2-4c21-82d5-1cfe684b6518))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 92adb299-772f-4f05-8ae8-a9ded5622bda))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp dd2c9251-88e5-4c6f-bf09-160becb8edd6))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(R20-Pad2)") (pintype "passive") (tstamp 954575bd-b79d-4cde-b39f-aa8cddf4deff))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 57 "/Sensor_Controller/CAPT_X4") (pintype "passive") (tstamp 43e1f678-1f03-4674-b4c1-ebf99fbc881d))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 071cf0bb-fece-4c5d-b50e-b43ecc787a1a)
    (at 175 154)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/688f1d59-c60e-402d-83ce-d3f5c3a70b2a")
    (attr smd)
    (fp_text reference "R20" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp eba7e27b-fdee-4bb7-8329-f39435bec7e0)
    )
    (fp_text value "2.2k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 808274b0-c550-4631-a879-107223408191)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 8c1c88ff-f711-4d8d-87e3-130916c764cc)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 807c148d-2346-4f3f-bbe6-0b06a57598b5))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp ede66ab1-5f24-4387-ac33-a82f9244eab4))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 0840ab9f-a7c6-479a-ac35-0fccd3a5e62b))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 563efd66-2d08-4f8a-b63e-d97e79d747fa))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 58a65da6-62ef-4fab-93a3-86edec1bab76))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp c915f1f9-3d17-4204-8667-05d6ff67d542))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 6e8cb1f3-c089-4c09-81a8-3253e7cc07c6))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 74a2e861-ff4a-4874-99bf-0e79aa2216d2))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp c6fad81d-5142-4432-a964-41206306f381))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp f55c0b1a-9ab5-4018-a006-1fbd43976982))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(R19-Pad2)") (pintype "passive") (tstamp 42f80f86-ab21-43a2-8c3e-e4aea0ab0645))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(R20-Pad2)") (pintype "passive") (tstamp e85ae928-4688-46cf-9e29-6f941dc78bca))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 09a12715-75af-41d2-9ec8-fe0ad1b18df3)
    (at 167.4 125.3 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/8e358922-00a2-42cd-bd67-5db2e820b238")
    (attr smd)
    (fp_text reference "R35" (at 0 1.17 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 46fba4d7-c53e-4938-a271-1873c5f2358e)
    )
    (fp_text value "10k" (at 0 -1.17 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e750e191-00cf-42cc-a11f-089c18e29f52)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 1e598cab-89ef-4f29-bd8f-ba04c5798eb5)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 4320378c-5c3a-4941-9119-9ab9c1f4150e))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 7ccd8841-edf6-4c66-8cef-7e3bb10c77dd))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 779e3480-4fe9-4347-86ef-0cf40e9c43a8))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 9009b691-eea3-49c8-a3f2-3cca6b78566b))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp b531843f-5de1-4258-813f-3a0fe3fd696a))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp c271089f-6152-4848-9e08-8e84c7ce3ccc))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 69655ffe-8065-443f-bb9a-694b7b234499))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 71c98dc1-7646-47e7-b324-5cd8237df741))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 8f08e8db-ac93-4e56-aabe-50bdec0fe3a8))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 93af2d7c-0c2c-44af-967c-7345f4635565))
    (pad "1" smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 30 "/WiFi_Display/GDR") (pintype "passive") (tstamp a1b00e48-f621-4bf9-9120-0a7f608a0c3c))
    (pad "2" smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp f00596d9-cc74-4508-a73f-a3525e96bd65))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 0dd8d6eb-738f-4f1f-baf7-7e5a32fe166e)
    (at 120.2 127.4)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/385d375a-ca1a-4131-ba57-58095b1d80c5")
    (attr smd)
    (fp_text reference "R9" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 8a634fff-c68f-4053-91d2-8850406e7b45)
    )
    (fp_text value "100k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d5ef7cb5-37ff-4fea-aee3-948ce57b795e)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 16e753c0-0055-4662-82a8-779a0b5fd0df)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 50b983e5-549d-466b-881f-59a5dee158a9))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp e9382b42-60bd-425d-81f0-8e1190dda9f4))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 03c5b918-c4ff-411a-86b6-63372e8e6b5c))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 2240bb6f-e15c-45e5-88e2-c4407cd0fbcc))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 69efbcba-a79f-4ca1-968b-5e47164c8394))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 6dd24d57-fd0d-4f67-b520-9f8fc1436dfa))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 2123a139-da6c-4b72-b613-58220072f56f))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 4f2b2c4e-a302-476e-a6e1-8dbd39c6a4a6))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp e56d8dcf-6f9a-4dfc-bd44-cb020a612ccb))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp e7c23ad0-cc69-470f-af6e-9d00ce3e56da))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp 34c23e1f-f879-48c8-88ec-be92279cee8d))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 44 "/Sensor_Controller/LPC_SWCLK") (pintype "passive") (tstamp 8d9c660c-eebe-4c93-b4b5-28eb34030a55))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.62x3.51mm_ThermalVias" (layer "B.Cu")
    (tedit 5F7512B7) (tstamp 10440c11-568a-4a47-8c71-3eed2018c78f)
    (at 178.9 138.3)
    (descr "SOIC, 8 Pin (https://www.monolithicpower.com/en/documentview/productdocument/index/version/2/document_type/Datasheet/lang/en/sku/MP2303A/document_id/494#page=14), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/387129f7-eb5e-4379-8091-080031f64ead")
    (attr smd)
    (fp_text reference "U8" (at 0 3.4) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 54a899ff-ad4f-4cfe-b25c-0abda6c956b7)
    )
    (fp_text value "TP4056" (at 0 -3.4) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e65666f6-525d-4d0e-bb6b-c6ee4441b00d)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.98 0.98) (thickness 0.15)) (justify mirror))
      (tstamp 6792ce9b-932a-4e43-860b-adc5399d0a95)
    )
    (fp_line (start 0 2.56) (end 1.95 2.56) (layer "B.SilkS") (width 0.12) (tstamp 20391906-002b-4875-a0aa-60eaba8e7b62))
    (fp_line (start 0 -2.56) (end 1.95 -2.56) (layer "B.SilkS") (width 0.12) (tstamp 80df2173-1af2-422a-9488-2b7f7b2c7def))
    (fp_line (start 0 2.56) (end -3.45 2.56) (layer "B.SilkS") (width 0.12) (tstamp b2108ceb-33a9-4b0d-a067-a16bc681b3c8))
    (fp_line (start 0 -2.56) (end -1.95 -2.56) (layer "B.SilkS") (width 0.12) (tstamp b5a5a039-0040-40ee-8da9-b943d65ef2b3))
    (fp_line (start 3.7 -2.7) (end 3.7 2.7) (layer "B.CrtYd") (width 0.05) (tstamp 190ee863-7958-4f9f-a03a-b4a75b7eed28))
    (fp_line (start -3.7 2.7) (end -3.7 -2.7) (layer "B.CrtYd") (width 0.05) (tstamp 310e31e5-6dd2-4617-84c1-322287ff9c3e))
    (fp_line (start 3.7 2.7) (end -3.7 2.7) (layer "B.CrtYd") (width 0.05) (tstamp 9d57f103-95fa-4cb1-9eac-34c7068996de))
    (fp_line (start -3.7 -2.7) (end 3.7 -2.7) (layer "B.CrtYd") (width 0.05) (tstamp dc97a36b-52e8-4c24-b87e-eeb3ca58ed83))
    (fp_line (start -0.975 2.45) (end 1.95 2.45) (layer "B.Fab") (width 0.1) (tstamp 256e036b-061d-4734-82fd-b1d4f2ddb5ff))
    (fp_line (start 1.95 2.45) (end 1.95 -2.45) (layer "B.Fab") (width 0.1) (tstamp 3e78c855-3cdb-41d2-8b07-5d2d0f9e6540))
    (fp_line (start -1.95 -2.45) (end -1.95 1.475) (layer "B.Fab") (width 0.1) (tstamp 5a7ab131-b1d5-4ddb-b804-fe78bcb2de53))
    (fp_line (start -1.95 1.475) (end -0.975 2.45) (layer "B.Fab") (width 0.1) (tstamp 5e85febd-9696-4dc9-b92f-75a7ecda1cca))
    (fp_line (start 1.95 -2.45) (end -1.95 -2.45) (layer "B.Fab") (width 0.1) (tstamp a162bbc6-ff53-4a36-bbc0-8ef43793a5be))
    (pad "" smd roundrect (at -0.655 -0.875) (size 1.1 1.47) (layers "B.Paste") (roundrect_rratio 0.227273) (tstamp 478ecfbf-1fbe-4f3d-854b-e4a930a97d85))
    (pad "" smd roundrect (at 0.655 0.875) (size 1.1 1.47) (layers "B.Paste") (roundrect_rratio 0.227273) (tstamp b1fd67c7-7562-4864-aff5-e59b0780fe94))
    (pad "" smd roundrect (at -0.655 0.875) (size 1.1 1.47) (layers "B.Paste") (roundrect_rratio 0.227273) (tstamp b99aa3f1-6f17-464f-91bc-637ecfb641c1))
    (pad "" smd roundrect (at 0.655 -0.875) (size 1.1 1.47) (layers "B.Paste") (roundrect_rratio 0.227273) (tstamp c9e80e0c-c15a-4a4b-9d5e-2d11d9ad3f93))
    (pad "1" smd roundrect (at -2.48 1.905) (size 1.94 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "TEMP") (pintype "input") (tstamp c2229409-cfcc-4e4b-a52c-4487e48d0db7))
    (pad "2" smd roundrect (at -2.48 0.635) (size 1.94 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(R22-Pad1)") (pinfunction "PROG") (pintype "input") (tstamp 583a9ebe-e062-4005-bb11-e32cc800012c))
    (pad "3" smd roundrect (at -2.48 -0.635) (size 1.94 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp caa47198-c9dc-4ade-8890-4e40a7521549))
    (pad "4" smd roundrect (at -2.48 -1.905) (size 1.94 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "VBUS") (pinfunction "VCC") (pintype "power_in") (tstamp c3262c36-ed5a-4a65-87e9-766cabbe11aa))
    (pad "5" smd roundrect (at 2.48 -1.905) (size 1.94 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "VCC") (pinfunction "BAT") (pintype "power_out") (tstamp 5fbf29d2-98d0-4064-920a-3a3c0e1958de))
    (pad "6" smd roundrect (at 2.48 -0.635) (size 1.94 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "/Power_Management/CHG_~{STBY}") (pinfunction "~{STDBY}") (pintype "open_collector") (tstamp 507b5472-4f49-4970-b0a0-b63c3a3244bb))
    (pad "7" smd roundrect (at 2.48 0.635) (size 1.94 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "/Power_Management/CHG_~{ACT}") (pinfunction "~{CHRG}") (pintype "open_collector") (tstamp 1c2620d3-f95e-4a74-84b1-a3a79fe32254))
    (pad "8" smd roundrect (at 2.48 1.905) (size 1.94 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "VBUS") (pinfunction "CE") (pintype "input") (tstamp d176e24f-d29d-4e12-accc-39aff2519d45))
    (pad "9" smd rect (at 0 0) (size 1.9 2.5) (layers "F.Cu") (tstamp 0990f4a8-e3a1-4dcd-af14-447f19a10c87))
    (pad "9" thru_hole circle (at 0.7 1) (size 0.5 0.5) (drill 0.2) (layers *.Cu) (tstamp 8080f1db-9cde-45b1-86eb-d15ec7d44b75))
    (pad "9" smd rect (at 0 0) (size 2.62 3.51) (layers "B.Cu" "B.Mask") (tstamp 9434fffe-f6cf-4480-a723-ef0809ba5bef))
    (pad "9" thru_hole circle (at -0.7 -1) (size 0.5 0.5) (drill 0.2) (layers *.Cu) (tstamp a62cc872-f880-469f-b855-37b3cd39aaba))
    (pad "9" thru_hole circle (at 0.7 0) (size 0.5 0.5) (drill 0.2) (layers *.Cu) (tstamp ab59fc22-fa73-4c97-b864-7f4810b358c3))
    (pad "9" thru_hole circle (at -0.7 0) (size 0.5 0.5) (drill 0.2) (layers *.Cu) (tstamp b3667535-6582-44d8-bcf0-0987116cabc6))
    (pad "9" thru_hole circle (at -0.7 1) (size 0.5 0.5) (drill 0.2) (layers *.Cu) (tstamp c916b4a8-7588-4385-a524-c45237dcd1d8))
    (pad "9" thru_hole circle (at 0.7 -1) (size 0.5 0.5) (drill 0.2) (layers *.Cu) (tstamp eba00c27-f5df-4524-b44e-7ac90a243755))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.62x3.51mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958) (tstamp 1200001b-7938-4ba4-942e-434c7ab17c31)
    (at 157.25 118.5625 90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/bc3dd482-6ae8-4f1e-9fb1-4aba830a1ef6")
    (attr smd)
    (fp_text reference "Q1" (at 0 2.4 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7db79227-c6cc-4c38-9f58-2d3f41745a18)
    )
    (fp_text value "CJ3401" (at 0 -2.4 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 80439d74-7503-4d50-b522-97a686469980)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 0.32 0.32) (thickness 0.05)) (justify mirror))
      (tstamp e72d02f6-258a-4375-96bb-845c4b826956)
    )
    (fp_line (start 0 -1.56) (end -0.65 -1.56) (layer "B.SilkS") (width 0.12) (tstamp 339ccb93-723f-4891-9990-d64340a27477))
    (fp_line (start 0 1.56) (end 0.65 1.56) (layer "B.SilkS") (width 0.12) (tstamp cba17fab-102b-435e-90e7-8424743e195e))
    (fp_line (start 0 -1.56) (end 0.65 -1.56) (layer "B.SilkS") (width 0.12) (tstamp df66f786-4cf9-446c-bae7-d05984dfe223))
    (fp_line (start 0 1.56) (end -1.675 1.56) (layer "B.SilkS") (width 0.12) (tstamp e6f6a59a-5790-4c34-95bf-cb3bc15fb00b))
    (fp_line (start -1.92 1.7) (end -1.92 -1.7) (layer "B.CrtYd") (width 0.05) (tstamp 50b413c7-3fb9-46a2-8195-fa0cab725111))
    (fp_line (start 1.92 -1.7) (end 1.92 1.7) (layer "B.CrtYd") (width 0.05) (tstamp 7e28eddc-bf87-4e5d-9f31-4372cb68fabf))
    (fp_line (start 1.92 1.7) (end -1.92 1.7) (layer "B.CrtYd") (width 0.05) (tstamp f7b0a7aa-8ab0-4514-805e-1eeb80513b83))
    (fp_line (start -1.92 -1.7) (end 1.92 -1.7) (layer "B.CrtYd") (width 0.05) (tstamp f8d874a9-0dc2-475c-b45d-20a3da27240e))
    (fp_line (start -0.65 1.125) (end -0.325 1.45) (layer "B.Fab") (width 0.1) (tstamp 0543d8b7-6612-4c58-8ee3-69fe537e221b))
    (fp_line (start -0.325 1.45) (end 0.65 1.45) (layer "B.Fab") (width 0.1) (tstamp 0cd65df6-1e53-4083-9b3a-876203329400))
    (fp_line (start 0.65 -1.45) (end -0.65 -1.45) (layer "B.Fab") (width 0.1) (tstamp 4e6fa70a-292b-4053-881f-14ae48875bed))
    (fp_line (start -0.65 -1.45) (end -0.65 1.125) (layer "B.Fab") (width 0.1) (tstamp 56fe1c02-6d75-4f8c-a41d-9dc698f76b78))
    (fp_line (start 0.65 1.45) (end 0.65 -1.45) (layer "B.Fab") (width 0.1) (tstamp dbca82ca-8fb1-4103-93cb-d00aa6fa3979))
    (pad "1" smd roundrect (at -0.9375 0.95 90) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "VBUS") (pinfunction "G") (pintype "input") (tstamp 485904a6-19f5-4c0a-b9d9-782a40709cfb))
    (pad "2" smd roundrect (at -0.9375 -0.95 90) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "VCC") (pinfunction "S") (pintype "passive") (tstamp 501a54fe-678e-4abc-bfc4-4eaad23337f0))
    (pad "3" smd roundrect (at 0.9375 0 90) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "/Power_Management/PS_SWITCH") (pinfunction "D") (pintype "passive") (tstamp e9e58dc6-3984-4e30-a7d5-5bbfea5d1ea7))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 1321ba86-318b-4f01-9894-2bbcf57c791d)
    (at 174.9 124.1)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/7ecea5e6-cfca-4dab-b398-b484a5f246fd")
    (attr smd)
    (fp_text reference "C24" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 009f1259-0822-432f-8e12-89573ffcb0e1)
    )
    (fp_text value "1uF/50V" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 08352e74-c7fc-4f1b-96fe-0e1715ab86d0)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 31ff1ea2-2f7a-4c46-aec6-c631fb6927e1)
    )
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp 2dc75118-ec03-4635-9e70-fbf06de2be15))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp afe711da-4a8c-4bad-a474-68bba3075fba))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 1f9c378a-d8be-41eb-b681-07eebe943650))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 64b0ec6e-38bc-4c48-892c-84385b7c3491))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 7ca30736-3013-4b06-95a3-c379d6b3b17d))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 8e709239-d177-48eb-9978-8b63db34c477))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 4a97fd30-fb67-4afb-aa60-ea39d0f7f76f))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 7f73177d-ed87-4e79-81ce-379d48fed7b1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp b594bcc9-4930-429e-b6e0-7b20c6561a3b))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp e7e942dc-3511-4a3c-891d-ef583a3976cd))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp feeca604-5304-4a88-be73-448ae977ab3c))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(C24-Pad2)") (pintype "passive") (tstamp 7272484e-494d-49b3-a0f8-940d7814758b))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 14c67ec2-e7e0-46ef-bf26-7f59d45e273e)
    (at 138 154)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/852f2b59-4349-4ded-9ff8-40f442f4a468")
    (attr smd)
    (fp_text reference "R13" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp c324d956-ad69-4fd0-8ccf-935cf75b869a)
    )
    (fp_text value "2.2k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e8057a74-a353-4516-b452-d45e0aef1105)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 307fcbb5-2cfc-45ef-90a1-c6e4e50615c6)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 09e06a23-b16d-46c6-a340-db94caaef8b0))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 4cf31fa7-0823-4a72-bd69-ab03bcf50e1e))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 30eabeda-5b93-492d-b8de-47e94ba569e5))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 6d313a03-80d0-42d3-be68-d578ce583cc4))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp a6d85825-1790-4c6f-9e46-151bfbb9c889))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp e5264624-8c64-4d77-853d-a22ea99657d4))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 0ceb13ff-4416-4fd2-83bb-2cd26b7c2917))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 1009d022-b3ee-4c86-ba77-dc1d8836405e))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 2071bde3-0159-4622-a3e4-7e2a9c57ac67))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 6a9d4a18-ce9b-48b5-a900-d679ca87a850))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 48 "/Sensor_Controller/CAPT_X1") (pintype "passive") (tstamp e8ccba4c-7854-4a33-a7ab-d0de2c348177))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(R13-Pad2)") (pintype "passive") (tstamp de7aeb98-b2bc-42b8-a75b-4648a77771cf))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "B.Cu")
    (tedit 5F6F9B37) (tstamp 1e9924e2-d09c-41b6-b226-7c4b181ca046)
    (at 180.8 110.6 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/bc1119e7-c235-4e01-bcba-765c92c9171d")
    (attr smd)
    (fp_text reference "U9" (at 0 2.4 -270) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp decfe496-7ac0-4b52-9180-246d8b56e81e)
    )
    (fp_text value "PAM2804AAB010" (at 0 -2.4 -270) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 97508770-0e85-4e04-8781-80db62f74bd3)
    )
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp d6210ba9-9d0e-4dc1-a492-2a8cc0c649d2)
    )
    (fp_line (start 0 -1.56) (end -0.8 -1.56) (layer "B.SilkS") (width 0.12) (tstamp 28c5635f-bcde-46bf-8eac-111673b8dafc))
    (fp_line (start 0 1.56) (end -1.8 1.56) (layer "B.SilkS") (width 0.12) (tstamp 86fd2747-a482-4616-bc7f-f3d771a7edf9))
    (fp_line (start 0 1.56) (end 0.8 1.56) (layer "B.SilkS") (width 0.12) (tstamp 96b92b64-97bd-4af7-bedc-2cfbf22bbb1f))
    (fp_line (start 0 -1.56) (end 0.8 -1.56) (layer "B.SilkS") (width 0.12) (tstamp 9b108b5c-e631-48fa-b94a-4a189be1ab71))
    (fp_line (start -2.05 1.7) (end -2.05 -1.7) (layer "B.CrtYd") (width 0.05) (tstamp 2f8bf747-b18c-433b-b45a-1a5fe7bb53a8))
    (fp_line (start 2.05 -1.7) (end 2.05 1.7) (layer "B.CrtYd") (width 0.05) (tstamp 59418740-8dc4-45a2-a633-02865c67a53f))
    (fp_line (start -2.05 -1.7) (end 2.05 -1.7) (layer "B.CrtYd") (width 0.05) (tstamp 6f44e423-aa59-46f3-a09b-dcf1b222c3d5))
    (fp_line (start 2.05 1.7) (end -2.05 1.7) (layer "B.CrtYd") (width 0.05) (tstamp 8714d00b-98bc-4c62-ae1d-32281fb60c76))
    (fp_line (start 0.8 1.45) (end 0.8 -1.45) (layer "B.Fab") (width 0.1) (tstamp 0d4e988f-6beb-4920-be2a-e52d78a65fa4))
    (fp_line (start -0.8 -1.45) (end -0.8 1.05) (layer "B.Fab") (width 0.1) (tstamp 6153c9b9-4d7c-41e3-8f6d-13d153bd9877))
    (fp_line (start -0.4 1.45) (end 0.8 1.45) (layer "B.Fab") (width 0.1) (tstamp 6aba3f23-9a72-435a-b52e-f119586bcef4))
    (fp_line (start 0.8 -1.45) (end -0.8 -1.45) (layer "B.Fab") (width 0.1) (tstamp 74700514-f0bf-4f06-98dd-43e82d4a7035))
    (fp_line (start -0.8 1.05) (end -0.4 1.45) (layer "B.Fab") (width 0.1) (tstamp d4f7a701-2433-46e0-80f3-09ccc7ee357c))
    (pad "1" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 70 "/Power_Management/LED_PWM") (pinfunction "EN") (pintype "input") (tstamp 1fbbff41-f3ae-4a63-aafd-aca488af22c3))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 7f2b6590-31ee-4edc-9292-0de077ab8c1e))
    (pad "3" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 81 "Net-(L1-Pad1)") (pinfunction "SW") (pintype "power_out") (tstamp 7b10b0fb-78fa-4f00-9fbe-3282a1b659ca))
    (pad "4" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "/Power_Management/PS_SWITCH") (pinfunction "VIN") (pintype "power_in") (tstamp 1cf5385c-0a9e-4bfb-9af3-8e177327d2de))
    (pad "5" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 28 "/Power_Management/LED_K") (pinfunction "FB") (pintype "input") (tstamp 8b99292e-99a1-44af-a8e9-6f17f8956d51))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 217e1922-6758-4300-9065-183181884750)
    (at 174.6 139.6 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/72db94ec-ec8f-4f52-b14a-cad4ace8165c")
    (attr smd)
    (fp_text reference "R22" (at 0 1.17 -270) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 63919fdf-4f76-4612-a23e-24caf4651692)
    )
    (fp_text value "1.2k/1%" (at 0 -1.17 -270) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0dbd98e3-f380-420a-8980-062e99eeb227)
    )
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp fa66ce41-81c8-47c6-b260-581b6a50e02b)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 7195475c-46a6-46f9-a8b2-07be11e60ee1))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp ea191c79-ece6-4d65-829e-449535533f01))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 28f282b9-8683-4938-ac30-602cda7276ed))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp b94aa31d-8325-4d0c-86d4-a56c22c14a5a))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp d8999d6b-10e9-4293-a175-53a5d56940d7))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp e4bc7ada-072d-4c8b-a504-36c9c5415360))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 2561e86d-bd9e-49bc-86cf-50fd2bfe9879))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 4c4e906a-a31b-4c8a-b64f-41e629ae2948))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp a9e6caad-f9bf-4d42-a0eb-dbb0d47a89d4))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp ebfad4e6-93e3-420d-963b-06c58cce9c10))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(R22-Pad1)") (pintype "passive") (tstamp 19e863dc-0dce-475a-b6c3-b44c712b8b12))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 9bffa444-d5e8-4460-8a0c-af5acf071641))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 226393cd-22b5-4983-be87-3e20bc5f5e28)
    (at 155.4 141.8 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/45d7985c-1554-4487-86cc-8a66b6c5acbf")
    (attr smd)
    (fp_text reference "C12" (at 0 1.16) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 41840057-a5c6-4d10-8d67-734ffb8f616f)
    )
    (fp_text value "100nF" (at 0 -1.16) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4e6171df-0285-4054-b9ed-521c80c367c1)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
      (tstamp 472de63d-67a4-4f01-b7c9-8a19c3e4c2f6)
    )
    (fp_line (start -0.107836 -0.36) (end 0.107836 -0.36) (layer "B.SilkS") (width 0.12) (tstamp 6619f656-d6db-45b9-b056-dc8fc5bde40d))
    (fp_line (start -0.107836 0.36) (end 0.107836 0.36) (layer "B.SilkS") (width 0.12) (tstamp af6504c7-8ade-4819-acd9-c897b0faa00c))
    (fp_line (start -0.91 0.46) (end 0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 020bb31b-2d28-4f41-b8b0-13fbd99ec555))
    (fp_line (start 0.91 -0.46) (end -0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 300e8828-ea8d-42b1-b729-ababef1a1976))
    (fp_line (start -0.91 -0.46) (end -0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 663926df-5a4d-4a00-8f46-a12bc231da49))
    (fp_line (start 0.91 0.46) (end 0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp c3c96d2a-1999-4f84-b9af-f7dc68b0cfe4))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 2b9d5a16-b9d6-4870-a55a-348b713c794c))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 461cb3b1-fabf-4c9f-9c14-b0f8731efee8))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp adad789a-33f8-4f0d-b121-bd58eab931b5))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp eb2eb7ec-6bac-4f2a-918d-2602a00efcf5))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 63 "/Sensor_Controller/CAPT_YH") (pintype "passive") (tstamp 0959f107-6371-4c78-b9b9-7311cb488452))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 74 "/Sensor_Controller/CAPT_YL") (pintype "passive") (tstamp 2b72268e-c336-4c91-b986-01b20066c08a))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 244bc15e-3ae8-4870-bfa7-c97f8c79c39c)
    (at 130.8 113.4 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/b6fbb578-d9a9-41b6-94c1-87e986c95da5")
    (attr smd)
    (fp_text reference "R32" (at 0 1.17 -270) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 6ef62af6-0b3a-4f43-9b46-0302dc586129)
    )
    (fp_text value "10k" (at 0 -1.17 -270) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f0712750-74d9-4531-8453-432780b60d5f)
    )
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 7eabcb3f-61ef-48fc-b94b-7d08daad20d9)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 1d5de519-5468-486c-ae84-6f53c307fc64))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp d5d1dee7-dd17-489b-88ad-195d9656f347))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 32882d00-0786-40dd-9bf3-e215e00e32dc))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 6b4ecdea-3d21-468e-a254-707b75f31f9b))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 88f64c12-e6a7-4827-bd68-c7d0dd2e7e7b))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp ab7519fb-fa08-4e73-9af8-e224aee27e52))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 39c07f9d-98c0-4981-afa6-2afeab0abc8a))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 5b6c93bf-e610-4321-88c7-13f752b9788e))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 745dc813-72b2-49b5-8ef4-d40529dc0fb6))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 9f2ed64e-6d3b-46bd-9176-3a34622a8de1))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "VDD") (pintype "passive") (tstamp 5abcfa10-5fef-4172-930f-4b1017fc0b5b))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 35 "/WiFi_Display/EPD_~{RES}") (pintype "passive") (tstamp b87a3a50-d423-48ea-8987-f615be48113c))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 26394413-ed32-480a-afcf-831ead25ec12)
    (at 159 154)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/ff08df82-82e0-4f66-81d6-9361e8ff617f")
    (attr smd)
    (fp_text reference "R17" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp da103916-30f6-4d9e-bd80-72d95b00b726)
    )
    (fp_text value "2.2k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 97402c3d-c134-4aab-8950-3eb3030a5ddf)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp c32e4068-0bbb-4cbf-8426-66eb97e40e5c)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 1ae97f36-8b82-4cba-8ea9-f578959766fd))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 9f0857ff-458b-49c4-9e3e-529e1a0c08fa))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 167a9f0d-30b1-4b99-a270-2e64b34e1017))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 221869d1-02f8-4607-8bb7-37c5d7b48861))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 5a81c4f9-d660-493f-bbed-409e0343192b))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 831350e9-07a6-42e6-ada2-8095e0debd17))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 81bd237a-9bde-4705-a7d7-a99b367e10cf))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 9f3b88ac-71ba-445b-a9ed-e7019fc1fc0b))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp bc6ec194-af13-4709-a76f-4b2ecad0f2eb))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp d751e8a6-4117-419e-a949-849d7e17d914))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(R16-Pad2)") (pintype "passive") (tstamp 8de703ce-f09c-4742-9b4e-d5a9ef5b34ad))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(R17-Pad2)") (pintype "passive") (tstamp 1ba300a6-c588-4e7e-af84-16bdabb09857))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 26df824f-ac33-4e74-b441-fb2f5c05fd25)
    (at 122.5 154)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/225641de-f04d-4386-b398-c9e4eea312d2")
    (attr smd)
    (fp_text reference "R10" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 868a406a-0022-46a6-88a9-c65c24185b5a)
    )
    (fp_text value "2.2k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a982f870-0738-4390-a0ac-df25808c04d7)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp b3b71614-d96e-406f-94b3-98c46e7d9f71)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 5576b6fc-7b29-4cef-ba22-228822ea77aa))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 59297b19-632d-44f5-af15-44bc435a1738))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 53d4862b-849b-4a08-815c-b0a179fc03ef))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 67563aaf-d8a3-40f6-8578-af5c9e58def3))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 9d720ea2-baea-4ddd-a3aa-48a8d169a4a1))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp ef059274-f56f-4317-a5c7-bd10d9cfe8ae))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 52b9a64f-37ec-4bdf-a263-08dd68cd867a))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 9e0b8868-5f28-48d1-a9c2-4a10863171a7))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp d17a3e60-41f0-401f-a8c0-97bc5cc3bdee))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp d6d0cade-7956-4794-ae69-f04ac8df62e4))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "/Sensor_Controller/CAPT_X0") (pintype "passive") (tstamp d50d89ac-668e-4078-b987-41243b62c2ee))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(R10-Pad2)") (pintype "passive") (tstamp 42784d53-3bc1-45ed-ba43-0c9006c67ecc))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 279b4d26-74e0-4dd7-8c04-8045465f6bc5)
    (at 174.9 119.6)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/de5e0106-37c5-4989-9533-3c8be3a2ae94")
    (attr smd)
    (fp_text reference "C31" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f7562b17-fce9-4658-ac42-8e9e81658504)
    )
    (fp_text value "1uF/50V" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a47f679b-4aa7-42f5-b4c8-f1b0bac7b24e)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp bf4ca68a-f7fd-46d6-84ff-f09eaae6b91c)
    )
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp 4c96c2bf-be19-4bb5-8c72-a00c594b5fa9))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp 9e37d154-39c3-44a8-8476-e97241b7f32f))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp c8eac3dd-2e98-40a9-961f-020203e74a27))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp c958e914-9300-4007-bedb-ec66e3b39950))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp d22a5050-d3ee-4798-9975-c3b14f9bfd5d))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp f25cb490-2e58-4b4a-a002-7fcf2f2f4806))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 46c0cc17-413c-48aa-9fe0-1b2a692aa79d))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 6cfeaf3c-7a99-4681-a7bc-ddf6e7bd2d5e))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 87cd3a53-c294-42de-a9dd-a44501480e73))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp e606b722-953e-4eca-836d-864344e5f334))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp eed154e5-b8eb-4099-a0bf-5b245276ca03))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(C31-Pad2)") (pintype "passive") (tstamp 3eab41a1-4e00-4bc4-9a80-0cf32609574b))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (tedit 58645DC7) (tstamp 28f8e5f0-7257-44c2-bff6-a4c199377988)
    (at 169 120.8 180)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/a9a8016b-33a5-48af-954e-c479e1f25276")
    (attr smd)
    (fp_text reference "D4" (at 0 2) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp ab6aecf0-5474-4129-b2ff-249f5546d28b)
    )
    (fp_text value "RBR2MM30BTR" (at 0 -2.1) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 9e32adee-c7c6-4c1a-8cbc-143139bf04ba)
    )
    (fp_text user "${REFERENCE}" (at 0 2) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 9949b888-a918-4bd8-a370-334f5137d07c)
    )
    (fp_line (start -2.25 -1) (end 1.65 -1) (layer "B.SilkS") (width 0.12) (tstamp 65afe781-adf2-4144-88b7-117fc3fbbef6))
    (fp_line (start -2.25 1) (end -2.25 -1) (layer "B.SilkS") (width 0.12) (tstamp 737e34c4-9b80-4433-82cf-3940e9cbf3bd))
    (fp_line (start -2.25 1) (end 1.65 1) (layer "B.SilkS") (width 0.12) (tstamp 7b2f9605-b99b-4958-9464-cfd5e6f63e4c))
    (fp_line (start 2.35 1.15) (end 2.35 -1.15) (layer "B.CrtYd") (width 0.05) (tstamp 020e6e92-9ec3-46f4-95d7-f16bf33cf172))
    (fp_line (start -2.35 1.15) (end -2.35 -1.15) (layer "B.CrtYd") (width 0.05) (tstamp 04601928-da12-40e1-a158-b42168895cdd))
    (fp_line (start -2.35 1.15) (end 2.35 1.15) (layer "B.CrtYd") (width 0.05) (tstamp 3217d8f4-18b4-43e6-a000-f3524758ef7c))
    (fp_line (start 2.35 -1.15) (end -2.35 -1.15) (layer "B.CrtYd") (width 0.05) (tstamp 3493d6f3-768a-4fc6-8e15-7189c43cb1bc))
    (fp_line (start -1.4 -0.9) (end -1.4 0.9) (layer "B.Fab") (width 0.1) (tstamp 1eb39a27-b6fc-483f-afb1-7056edae9c75))
    (fp_line (start -1.4 0.9) (end 1.4 0.9) (layer "B.Fab") (width 0.1) (tstamp 2563eb79-bcbc-4435-8a85-452275ae8dd3))
    (fp_line (start -0.35 0) (end 0.25 0.4) (layer "B.Fab") (width 0.1) (tstamp 305c2a43-13af-4d42-9e98-45a7f86411a5))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4) (layer "B.Fab") (width 0.1) (tstamp 510d4455-4831-47f3-a9ae-510c0e077311))
    (fp_line (start 0.25 0) (end 0.75 0) (layer "B.Fab") (width 0.1) (tstamp 7c280c7b-3578-4408-b65b-2a7e5544cab1))
    (fp_line (start 0.25 -0.4) (end -0.35 0) (layer "B.Fab") (width 0.1) (tstamp 82cb542c-cc21-4d4d-a762-99b49416d096))
    (fp_line (start -0.75 0) (end -0.35 0) (layer "B.Fab") (width 0.1) (tstamp 8925b410-6d59-4c9d-9f9f-54581586ac3a))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer "B.Fab") (width 0.1) (tstamp 8957c93a-2fbb-4625-8b62-5ed03bdc663b))
    (fp_line (start 1.4 -0.9) (end -1.4 -0.9) (layer "B.Fab") (width 0.1) (tstamp 9601d96f-62c1-414d-b3d1-8609c10f6a6a))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer "B.Fab") (width 0.1) (tstamp e2432ebf-42d2-4085-825c-96524d254dbf))
    (fp_line (start 1.4 0.9) (end 1.4 -0.9) (layer "B.Fab") (width 0.1) (tstamp f9cae35d-35d1-4bc5-a36e-1f3c0f05324e))
    (pad "1" smd rect (at -1.65 0 180) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "K") (pintype "passive") (tstamp ea9fc206-662a-40e1-a27d-bfe2ebc24049))
    (pad "2" smd rect (at 1.65 0 180) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "Net-(C22-Pad1)") (pinfunction "A") (pintype "passive") (tstamp 06540d6f-ece8-408b-910f-a2aa61e9355d))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 2b259426-6943-4fac-a589-7602907648a5)
    (at 152.9 120.8 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/b0e1f2f9-8869-4117-9f57-9fc491871861")
    (attr smd)
    (fp_text reference "R28" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp fff79040-0349-4f57-9c14-ef3b7e61ff4d)
    )
    (fp_text value "5.1k/1%" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 605d48db-f266-4c76-90a7-ec225c25b0c5)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 4c2232c6-78dd-4cd5-87b2-67c9044a9930)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 3a7c9a3a-46ef-4c3c-b5c7-5dda1b723ba4))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp ca6a0032-eb9b-424c-b374-cb42f2a04e3d))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 5ae8e899-92cc-49ff-a192-205dd1465f54))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 9b625148-3472-4760-aacf-96617bad7980))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp bafbfa75-bda2-4f04-8d3b-e4b444af3acb))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp ea886d58-5152-4ba2-aadf-189c3fdf982b))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 22ba11d8-8a26-4eae-bf47-3e6188bf5852))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp a042d380-fd01-4702-afb3-817497801d4c))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp b20568c6-2d00-49c3-a0a2-7229b29305aa))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp bf5cca0d-1e23-4311-9db9-0cebf9bf8acb))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 60 "Net-(R27-Pad2)") (pintype "passive") (tstamp edc7daa6-9cd6-437f-95cc-d86fbd3b3c54))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 1b82510e-67a0-482f-a1c7-16065a1c2e88))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 2e68f97d-0bb4-491f-b3cd-5bea688cdb47)
    (at 154.7 118.3 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/7de2ce23-77a2-4da0-b343-e039cbb2217b")
    (attr smd)
    (fp_text reference "C18" (at 0 1.43 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp b252bcf7-83fa-4590-9671-7ce615bce521)
    )
    (fp_text value "4.7uF" (at 0 -1.43 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f131cc5a-2664-4742-8bac-17248283ba71)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp d61c54c4-c563-479b-9263-152fcfc7c590)
    )
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp 835bf769-a4a8-467e-8c83-9c768500bfe2))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp bb069eb0-fd6c-40a1-b68f-388af3f94d13))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 1c10b31f-b3db-4716-a69d-e9690d59a72e))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 5aaa20e6-1e77-44c4-b6cb-e42fc48a40f5))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 9f05fc03-f27b-438e-b822-452aac7d694b))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp d9b17df6-5ac0-494e-a5f2-bfca8d064f29))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 0254e687-80ef-45d3-beb9-7b7eb6761692))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 744226a9-08f1-4a4d-a55a-dea2dbaaefec))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp a1d482d4-aa48-46e3-ba5c-a9e825a85d46))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp aaaf0153-088b-4ada-92bf-f597b5a15ae6))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "/Power_Management/PS_SWITCH") (pintype "passive") (tstamp c96ddf13-ca31-47db-abad-b2401dbb45f3))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp eb3eac71-0c2f-455b-b3a5-69b08032c6f8))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (layer "B.Cu")
    (tedit 5A64794F) (tstamp 38127ad4-cca1-4c78-aee2-2e28b559f919)
    (at 195.7 132.2 90)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/9ca062cc-08da-433e-bffe-2c55fb0f798f")
    (attr exclude_from_pos_files)
    (fp_text reference "JP1" (at 0 1.8 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0d7664b5-1586-4e8b-b98d-88d1aa73994e)
    )
    (fp_text value "Jumper_2_Open" (at 0 -1.9 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 79cf566d-caed-4559-bf8b-a2ab7cc0cc5c)
    )
    (fp_line (start 1.4 -1) (end -1.4 -1) (layer "B.SilkS") (width 0.12) (tstamp 91a9af8f-3a58-43bd-ae78-a5400c39cd9f))
    (fp_line (start -1.4 -1) (end -1.4 1) (layer "B.SilkS") (width 0.12) (tstamp 964e2994-5538-404d-81cc-5c29debd4395))
    (fp_line (start -1.4 1) (end 1.4 1) (layer "B.SilkS") (width 0.12) (tstamp a4b011e3-b437-4c98-8707-906d2f1932e5))
    (fp_line (start 1.4 1) (end 1.4 -1) (layer "B.SilkS") (width 0.12) (tstamp df33c9e2-0097-4b83-86f1-90c82408441e))
    (fp_line (start -1.65 1.25) (end 1.65 1.25) (layer "B.CrtYd") (width 0.05) (tstamp d76fc4e8-7ba0-42e1-ab4c-e414582be8bb))
    (fp_line (start -1.65 1.25) (end -1.65 -1.25) (layer "B.CrtYd") (width 0.05) (tstamp e694fc6d-6452-44c3-817d-d848973fc169))
    (fp_line (start 1.65 -1.25) (end 1.65 1.25) (layer "B.CrtYd") (width 0.05) (tstamp f1e0bbcd-607c-44fc-8908-f558a33432d3))
    (fp_line (start 1.65 -1.25) (end -1.65 -1.25) (layer "B.CrtYd") (width 0.05) (tstamp fb8d5a2c-afe4-47f5-9e70-1e90c86e21b9))
    (pad "1" smd custom (at -0.725 0 90) (size 0.3 0.3) (layers "B.Cu" "B.Mask")
      (net 103 "Net-(BT1-Pad1)") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1 0)
            (xy 0.5 -0.75)
            (xy -0.5 -0.75)
            (xy -0.5 0.75)
            (xy 0.5 0.75)
          ) (width 0) (fill yes))
      ) (tstamp 83869a2f-1976-4b95-8777-0e71f675e57d))
    (pad "2" smd custom (at 0.725 0 90) (size 0.3 0.3) (layers "B.Cu" "B.Mask")
      (net 6 "VCC") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.5 -0.75)
            (xy -0.65 -0.75)
            (xy -0.15 0)
            (xy -0.65 0.75)
            (xy 0.5 0.75)
          ) (width 0) (fill yes))
      ) (tstamp e484df0b-90ea-4a13-b115-915b9b8f228e))
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 389bf5a5-a942-4c7c-9e24-cf86e886d331)
    (at 161 121.5 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/5098fb42-bc7c-42e8-9420-50e3b2cde494")
    (attr smd)
    (fp_text reference "R23" (at 0 1.17 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f31b7269-380f-4ffa-a522-13a349bb99d1)
    )
    (fp_text value "27.4k/1%" (at 0 -1.17 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 3ca5c00c-7751-48d9-b285-427e04f40740)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp d80b60cf-4925-4049-bd7c-e876aa70077b)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 98de562d-c708-4f10-8583-5c25bbb50169))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp e3dfa01e-3d6f-46b8-9b9b-d791fbfdeb0c))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 58da578b-95fc-453d-a2c2-61adad486303))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 5fa17f37-bdf9-44ee-8119-107cb867b887))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp c8e0090c-f40a-44a5-b96b-d8310ce9463d))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp d77b4982-23bb-449b-8442-0f585bf961ed))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 208d190b-7b86-4f37-ba8a-96afc27bd5e4))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp ba6ef5fb-63b5-4a89-9528-66b082c78529))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp c21c432c-9c02-4987-af4f-28c9765fdcf7))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp d7da7b58-2eaf-4646-b9cb-4ba565b06ada))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "VCC") (pintype "passive") (tstamp 76e6186d-f265-49e6-9c67-2bd1679127a4))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 59 "/Power_Management/ADC_BAT") (pintype "passive") (tstamp 3ee39d29-10da-4461-934c-8b97c1ba4139))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 3a8b6329-61e9-45be-9849-4b4d0f99dbeb)
    (at 174.9 125.8)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/59ed7485-a176-4f28-a203-6093f26603a7")
    (attr smd)
    (fp_text reference "C29" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4a03865e-4a35-4c58-8391-461821a80a03)
    )
    (fp_text value "1uF/50V" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5091702b-afbd-41d3-a6cb-75ae95bc37d9)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 50edf5b9-d54c-496c-93d0-f30645219324)
    )
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp 67d683cc-ab42-41d3-92fe-4f3d8cc05b03))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp 959ee9b8-bd33-4eb6-ba77-02dd4458c741))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 125f651a-b88c-4126-af4d-15b333ea8127))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 53d51f00-e51e-49d7-b5fb-43b536055a07))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 9e36483c-b79b-4aea-adb0-149aeb2ff12c))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp ccba2986-717c-4d0e-8691-061c9f4fd01d))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 0deee350-3ce8-43de-b2d0-5cd8d40cdcaa))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 39994704-4a55-4993-96e7-ce3ce3e9f098))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 98f87a6a-7cc8-4f89-95ae-31f3a30ea1e6))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp f8ce3691-1e38-41cb-8150-0c07230346a1))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 2800d593-d01c-4ff1-9542-380b8647eaf5))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(C29-Pad2)") (pintype "passive") (tstamp 117f8306-102c-4bcf-8da7-cfeb5751fc9a))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-666" (layer "B.Cu")
    (tedit 5A02FF57) (tstamp 3aff516b-5fe2-4568-b035-6f4a5297999f)
    (at 192.3 147.3 90)
    (descr "SOT666")
    (tags "SOT-666")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/b277339b-9993-4d9c-83f1-94c3e1969272")
    (attr smd)
    (fp_text reference "U11" (at 0 1.75 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 80c9154b-577d-4d26-abd2-6c2e768bad49)
    )
    (fp_text value "USBLC6-2P6" (at 0 -1.75 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 6a719da2-7d52-483a-9d0c-702376c392f0)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
      (tstamp 9dcf340c-c9e5-4832-b08e-7eb423a0a266)
    )
    (fp_line (start -0.8 -0.9) (end 0.8 -0.9) (layer "B.SilkS") (width 0.12) (tstamp 55c78095-0430-4058-b26a-4f03d7aadf68))
    (fp_line (start 0.8 0.9) (end -1.1 0.9) (layer "B.SilkS") (width 0.12) (tstamp ed625d72-292b-4204-9f50-a0488198d441))
    (fp_line (start -1.5 1.1) (end 1.5 1.1) (layer "B.CrtYd") (width 0.05) (tstamp 79d2bccc-e7b3-4d71-9155-a31a045ddb6a))
    (fp_line (start -1.5 -1.1) (end 1.5 -1.1) (layer "B.CrtYd") (width 0.05) (tstamp 9245cacd-ff6a-45ff-96bc-9853f8a04430))
    (fp_line (start -1.5 1.1) (end -1.5 -1.1) (layer "B.CrtYd") (width 0.05) (tstamp c5c0084d-82f8-40dc-98df-8f34eb71594c))
    (fp_line (start 1.5 -1.1) (end 1.5 1.1) (layer "B.CrtYd") (width 0.05) (tstamp e55f6686-f164-4c9d-b923-2ae183eda345))
    (fp_line (start 0.65 -0.85) (end -0.65 -0.85) (layer "B.Fab") (width 0.1) (tstamp 09ea0d68-2376-4ee5-b15b-e5fa7f7641db))
    (fp_line (start 0.65 0.85) (end -0.33 0.85) (layer "B.Fab") (width 0.1) (tstamp 7f9ea9d4-75ed-457c-8138-56eab532a2c8))
    (fp_line (start -0.65 0.53) (end -0.33 0.85) (layer "B.Fab") (width 0.1) (tstamp e3e8c907-2d96-4c29-ab8b-c7d6b367f76f))
    (fp_line (start -0.65 0.53) (end -0.65 -0.85) (layer "B.Fab") (width 0.1) (tstamp e889f87e-178f-4fdd-bfb4-f22e60cbb081))
    (fp_line (start 0.65 0.85) (end 0.65 -0.85) (layer "B.Fab") (width 0.1) (tstamp fbe6bcae-fd86-4649-b431-d1d8b3dfc067))
    (pad "1" smd rect (at -0.85 0.5375 90) (size 0.5 0.375) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 84 "/WiFi_Display/USB_D-") (pinfunction "I/O1") (pintype "passive") (tstamp ad80fb9b-2940-44a0-b984-5bb2ca7ded04))
    (pad "2" smd rect (at -0.925 0 90) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive") (tstamp a06e0270-f84e-4751-b217-be9cda5b6a8a))
    (pad "3" smd rect (at -0.85 -0.5375 90) (size 0.5 0.375) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 83 "/WiFi_Display/USB_D+") (pinfunction "I/O2") (pintype "passive") (tstamp 6b529606-7e7c-4c37-aa5d-230741ab0aaf))
    (pad "4" smd rect (at 0.85 -0.5375 90) (size 0.5 0.375) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 83 "/WiFi_Display/USB_D+") (pinfunction "I/O2") (pintype "passive") (tstamp 5e5abe92-b1c2-43bd-9010-138e3fbd8fa9))
    (pad "5" smd rect (at 0.925 0 90) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "VBUS") (pinfunction "VBUS") (pintype "passive") (tstamp 296f96c1-2f68-4990-8d78-5133994883ba))
    (pad "6" smd rect (at 0.85 0.5375 90) (size 0.5 0.375) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 84 "/WiFi_Display/USB_D-") (pinfunction "I/O1") (pintype "passive") (tstamp c02dae34-f334-48ec-bc33-4c24d0d98b3f))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-666.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 3c8f0ee5-2905-48f8-980d-16c50caf8473)
    (at 133 154 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/93a9dbdb-d19d-4957-b2bc-942977ecca26")
    (attr smd)
    (fp_text reference "R12" (at 0 -1.2) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d9403c5e-b9ef-4f90-916a-9042281fc480)
    )
    (fp_text value "2.2k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a3e21f03-1ee5-4d49-b818-1e22cac4a057)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 96eec8b7-1873-4d43-96d1-8b0cbc8c31ae)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 91ad4c4e-70d4-4f6f-8a6b-468e6043ae37))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp a21d7e60-eb90-426a-8727-b92d9cdfbd71))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 1306c618-e9d6-4f9c-8dad-aec4f3bb87d5))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 5c2e2978-61cb-4d5d-8d5d-b926f277264d))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 756d392d-24f3-44a4-8875-92f6c0d33701))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 9f32b52a-dd73-4334-bd99-4c792116ada8))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 2d51da5b-0ac2-4918-805d-a90d4fe8f82a))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 6da00c72-40c8-47bb-aeed-103373f111d9))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 95894ccb-e575-4bb8-9bfb-38b3b3d81345))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp d0bd9bbc-e966-415d-85bc-66b9fc85361d))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 48 "/Sensor_Controller/CAPT_X1") (pintype "passive") (tstamp b9a7fe8c-f6eb-4a3d-a00a-d08b7acfc10d))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 47 "Net-(R11-Pad1)") (pintype "passive") (tstamp fb03efd1-d65c-483a-afe9-87bf80f9617a))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Button_Switch_SMD:Panasonic_EVQPUJ_EVQPUA" (layer "B.Cu")
    (tedit 5A02FC95) (tstamp 3dc2effe-ce89-4859-b08e-4e141203499a)
    (at 158.4 107.4 180)
    (descr "http://industrial.panasonic.com/cdbs/www-data/pdf/ATV0000/ATV0000CE5.pdf")
    (tags "SMD SMT SPST EVQPUJ EVQPUA")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/50c3f9e1-72d8-4c24-85e0-c5f7d5eb3021")
    (attr smd)
    (fp_text reference "SW2" (at 0 4.5) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 85d355f7-a945-4b1e-a077-538eb0c48f8b)
    )
    (fp_text value "EVQPUA02K" (at 0 -3.5) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp c04c1663-475f-416f-8e67-791195f37492)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp cd204456-bcff-435b-ba6f-d2ad378dacc2)
    )
    (fp_line (start 2.35 1.85) (end 1.425 1.85) (layer "B.SilkS") (width 0.12) (tstamp 26a1224a-39f9-4d08-9082-44228cb235dd))
    (fp_line (start -1.425 1.85) (end -2.35 1.85) (layer "B.SilkS") (width 0.12) (tstamp aa852409-314a-43a5-a600-bbb2dfab0329))
    (fp_line (start 2.35 -1.85) (end -2.35 -1.85) (layer "B.SilkS") (width 0.12) (tstamp cc570866-967c-42e8-86fa-8584cabef770))
    (fp_line (start 2.45 -0.275) (end 2.45 0.275) (layer "B.SilkS") (width 0.12) (tstamp cf2c0af0-a2ee-4380-8361-76a2cd2557cb))
    (fp_line (start -2.45 -0.275) (end -2.45 0.275) (layer "B.SilkS") (width 0.12) (tstamp f0ad0976-65df-4f10-9373-49198dff5bcb))
    (fp_line (start -3.9 -2.25) (end -3.9 3.25) (layer "B.CrtYd") (width 0.05) (tstamp 32932905-014a-47d7-9d6e-8a1eae5f5f53))
    (fp_line (start 3.9 3.25) (end -3.9 3.25) (layer "B.CrtYd") (width 0.05) (tstamp 65dedb2b-88b3-4f64-8c77-18fd95549666))
    (fp_line (start 3.9 -2.25) (end -3.9 -2.25) (layer "B.CrtYd") (width 0.05) (tstamp 9f7251d2-b5d5-45c1-8475-8488fa04d943))
    (fp_line (start 3.9 -2.25) (end 3.9 3.25) (layer "B.CrtYd") (width 0.05) (tstamp d17035f7-ddd3-4cf3-b3b7-b6613923c3ed))
    (fp_line (start -2.35 -1.75) (end -2.35 1.75) (layer "B.Fab") (width 0.1) (tstamp 02074905-d2bb-4bb1-b4fb-2711cdcaa242))
    (fp_line (start -1.3 2.75) (end -1.3 1.75) (layer "B.Fab") (width 0.1) (tstamp 08300c1f-07c2-423c-b5d5-acd350ad8cc4))
    (fp_line (start 2.35 -1.75) (end -2.35 -1.75) (layer "B.Fab") (width 0.1) (tstamp 496c153f-cc7d-46cb-9886-6d37579ad345))
    (fp_line (start 1.3 2.75) (end -1.3 2.75) (layer "B.Fab") (width 0.1) (tstamp 828d1081-ff68-401f-8675-b8e6c41b3cbf))
    (fp_line (start 2.35 -1.75) (end 2.35 1.75) (layer "B.Fab") (width 0.1) (tstamp c172ce33-dbec-456e-8241-59be851364c7))
    (fp_line (start 1.3 2.75) (end 1.3 1.75) (layer "B.Fab") (width 0.1) (tstamp c8bead37-9359-43ab-aa40-129ef3102b6d))
    (fp_line (start 2.35 1.75) (end -2.35 1.75) (layer "B.Fab") (width 0.1) (tstamp e459ba3b-1fc9-4a81-b851-2b83e8a92b17))
    (pad "1" smd rect (at 2.625 0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive") (tstamp 0b1b5735-9cc7-4da7-8553-6c7863f044a4))
    (pad "1" smd rect (at -2.625 0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive") (tstamp fa8b2414-74f8-4a58-a79f-bd6912047b6a))
    (pad "2" smd rect (at -2.625 -0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "/Sensor_Controller/LPC_~{RST}") (pinfunction "2") (pintype "passive") (tstamp 2d1710b0-356c-49ae-8f46-927cf3960a5f))
    (pad "2" smd rect (at 2.625 -0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "/Sensor_Controller/LPC_~{RST}") (pinfunction "2") (pintype "passive") (tstamp f087bccb-ba96-484e-a94b-f944740d5db8))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/Panasonic_EVQPUJ_EVQPUA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (tedit 58645DC7) (tstamp 4668c841-f35f-41a7-b0b8-e2c693772000)
    (at 157.9 115.5)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/b5b31630-e16e-4c4b-a1c5-fb069ecbb43b")
    (attr smd)
    (fp_text reference "D2" (at 0 2) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 11e3dd5d-6d6e-4343-b74b-485a73d8cbd4)
    )
    (fp_text value "RBR2MM30BTR" (at 0 -2.1) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2229ca8b-d64e-49db-9bff-2694becb44e7)
    )
    (fp_text user "${REFERENCE}" (at 0 2) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a7d577d5-212c-48e7-aa1d-ccf87cf50704)
    )
    (fp_line (start -2.25 1) (end 1.65 1) (layer "B.SilkS") (width 0.12) (tstamp 1d3a726a-a4ad-449c-829e-1502ee89364d))
    (fp_line (start -2.25 1) (end -2.25 -1) (layer "B.SilkS") (width 0.12) (tstamp 5d5eedf7-c5d8-4e8a-b5e8-ddfa7cd166c9))
    (fp_line (start -2.25 -1) (end 1.65 -1) (layer "B.SilkS") (width 0.12) (tstamp ae125281-bfaf-40c0-ac4c-b32deea32bb8))
    (fp_line (start -2.35 1.15) (end -2.35 -1.15) (layer "B.CrtYd") (width 0.05) (tstamp 17ceaaba-7293-440c-9009-b98478a65106))
    (fp_line (start -2.35 1.15) (end 2.35 1.15) (layer "B.CrtYd") (width 0.05) (tstamp 29fcf295-31d9-42a4-80e4-265d500aea50))
    (fp_line (start 2.35 1.15) (end 2.35 -1.15) (layer "B.CrtYd") (width 0.05) (tstamp 8592dbb1-ff0e-4c75-9c63-6151e3d8747a))
    (fp_line (start 2.35 -1.15) (end -2.35 -1.15) (layer "B.CrtYd") (width 0.05) (tstamp e070a86c-ec43-473e-9414-62b5edb02e7a))
    (fp_line (start -1.4 -0.9) (end -1.4 0.9) (layer "B.Fab") (width 0.1) (tstamp 09c952b1-3558-40de-8887-7000fb598a15))
    (fp_line (start 1.4 -0.9) (end -1.4 -0.9) (layer "B.Fab") (width 0.1) (tstamp 218c9e41-606a-428f-bde7-17489acd9bdb))
    (fp_line (start -0.75 0) (end -0.35 0) (layer "B.Fab") (width 0.1) (tstamp 26bbc775-c329-4cd1-8531-056b4a7cb662))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer "B.Fab") (width 0.1) (tstamp 2e99ed41-787a-4f29-9e23-bf1df12058f8))
    (fp_line (start -0.35 0) (end 0.25 0.4) (layer "B.Fab") (width 0.1) (tstamp 79698fa1-a166-4089-9792-4d1086b7d9b6))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer "B.Fab") (width 0.1) (tstamp 7cacf749-8953-47ef-bf06-dfceeb90138d))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4) (layer "B.Fab") (width 0.1) (tstamp a83f1500-f8b8-4722-bb31-ae31e669c842))
    (fp_line (start 0.25 0) (end 0.75 0) (layer "B.Fab") (width 0.1) (tstamp b468c7fb-d6ca-48d9-94c5-3d4f1bb43ca1))
    (fp_line (start 0.25 -0.4) (end -0.35 0) (layer "B.Fab") (width 0.1) (tstamp b4b28668-08a8-46cb-a192-23847594ff01))
    (fp_line (start 1.4 0.9) (end 1.4 -0.9) (layer "B.Fab") (width 0.1) (tstamp c47249eb-ec06-45ed-8886-301bf6e3d1fa))
    (fp_line (start -1.4 0.9) (end 1.4 0.9) (layer "B.Fab") (width 0.1) (tstamp eab38140-0431-44f0-ab96-785055c12665))
    (pad "1" smd rect (at -1.65 0) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "/Power_Management/PS_SWITCH") (pinfunction "K") (pintype "passive") (tstamp 276987a2-7db4-478e-b9fc-234214692ec0))
    (pad "2" smd rect (at 1.65 0) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "VBUS") (pinfunction "A") (pintype "passive") (tstamp a4a54b82-2990-413b-ad01-08443415aa35))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 4ca10ff1-f91a-4098-893a-211fdfacb763)
    (at 159.7 122.9 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/2563902e-2890-4913-a645-9f387a8737a7")
    (attr smd)
    (fp_text reference "C13" (at 0 1.43 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 75a27c15-e306-4b35-af97-3e8621eef754)
    )
    (fp_text value "4.7uF" (at 0 -1.43 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 462d3d3d-bef3-4a79-81f2-12d19f233a7f)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp d3388eb4-5f64-4abb-8d8a-f1ee9714d83a)
    )
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp 0714c0c7-ac00-43e4-821d-22968f5fe521))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp bd1b0f34-2a0b-44c2-997b-abde9ec47a79))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 395cafc6-4f07-45db-853d-6af7f479eac7))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 6c9ce9c3-fe34-4563-81fe-15e97ba69b49))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp b0920a4a-059e-459e-ab05-12797cd696a7))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp fc713e09-ad5a-4b1b-a343-f9ac2ea14595))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 6b131d07-2e82-4329-9f1b-f715045c092c))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp d437a66c-7b61-4ba0-aaf8-71db44822adc))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp d5850f71-b966-418b-b3a8-9627dbbee18d))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp e7cc3828-f005-4c10-82f6-29fddd8c1855))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "VCC") (pintype "passive") (tstamp ea901b6f-c8bf-473d-b86b-ef25b9397be5))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp d98c1a08-e2ee-45ef-8a67-a1c3f0d821ce))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEF0) (tstamp 4d1ecefd-f385-4125-964f-8286276e15ed)
    (at 149.8 136.8)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/100c41f7-cf02-4b78-98a6-db06cc5ba264")
    (attr smd)
    (fp_text reference "FB1" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 994a0b94-e07b-43c2-b6f0-df42832b0306)
    )
    (fp_text value "1k/100MHz, ILBB0603ER102V" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 6e530789-b2b1-440b-80b2-98fd4a2293d3)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 4b5f09be-1b10-4374-b77b-d1d94193fd86)
    )
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer "B.SilkS") (width 0.12) (tstamp 8858c48a-8fbe-4332-a117-3fc927136158))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer "B.SilkS") (width 0.12) (tstamp f5502751-d91f-479b-b255-63e914f1043f))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 1a9a6307-8cb3-429a-bf7b-ef45d39168a4))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 42cda592-f41e-4a53-b7bc-9a1a96352ec4))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp abe903d6-f946-4ca1-8fb4-36df7245ec67))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp b7b99049-5165-401f-a190-d66720fcefc1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 16d567fb-626c-49d5-94e5-28fd162bca88))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp d7ab9f59-1fa2-4e01-9ff4-b7af966724ef))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp e3f3d6d9-4cf1-47be-bbf6-621f9514696a))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp ffb93eb7-2f89-431c-b1dc-62eb71e61617))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp c169c252-4a18-404f-bb85-4e45526b5ebd))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(C10-Pad1)") (pintype "passive") (tstamp fb30f8ba-c4e7-440d-9ba0-ecd7afdaa721))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 4e67c116-c710-44ef-aec1-fac3a78937fd)
    (at 129.9 140.4 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/a7e4c83d-2e2a-4884-9cc9-c0dadff5206a")
    (attr smd)
    (fp_text reference "C1" (at 0 1.16 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2eef7c4b-1d27-4e92-88a2-531e765eb7e0)
    )
    (fp_text value "100nF" (at 0 -1.16 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 46157b9c-be13-47f5-93e8-1cf79c472dbc)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
      (tstamp ee8b635b-6d41-4de1-99df-4ef5db127d52)
    )
    (fp_line (start -0.107836 -0.36) (end 0.107836 -0.36) (layer "B.SilkS") (width 0.12) (tstamp 02dff03a-f7c9-4675-91c1-2e955ec4714a))
    (fp_line (start -0.107836 0.36) (end 0.107836 0.36) (layer "B.SilkS") (width 0.12) (tstamp 983622b1-4773-40e8-ac36-a257cbd67873))
    (fp_line (start 0.91 -0.46) (end -0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 3ad2f333-55a7-4c13-b9cb-73970c108b0f))
    (fp_line (start -0.91 0.46) (end 0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp b9961134-5f10-40cf-9e9b-868e07781625))
    (fp_line (start 0.91 0.46) (end 0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp ccaeeb80-5fd3-4aab-8464-7df7076f30ac))
    (fp_line (start -0.91 -0.46) (end -0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp fa69e575-abfa-43e2-9610-c231da506d22))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 0c858c21-a1c4-41fc-b03e-95a7c4cbfa80))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 0d157f50-fe66-4c72-ac5b-ec5409cd32c2))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 3b90bf3c-2738-41e4-ab74-dd425eaae3ab))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp f5fe65a9-c0ab-4e9d-9f27-eb948c2ae389))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp 3ab2ee24-abd2-435f-b118-6b12bedfdac7))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp c5be0b92-13d7-4882-9edc-6f086268504b))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 560b91d7-8fff-4c42-b53d-2a72347b4061)
    (at 154.7 122.9 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/2147fc42-79ee-4a85-b8a6-66ccb58fff39")
    (attr smd)
    (fp_text reference "C14" (at 0 1.43 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d535d415-79ed-4288-9d84-3f6b4318ac5f)
    )
    (fp_text value "4.7uF" (at 0 -1.43 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 6a89deeb-7e10-484b-aa39-e882673e420a)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 61cbb8a1-0760-44dd-9217-8e53291fc157)
    )
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp 21bdd760-9ab4-4017-8c0b-afc91a6d0739))
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp 30e75019-a659-4a7e-875c-e69f4d80f518))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 003d3ecb-6910-49eb-9d60-52090432b203))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 3ed09a44-e7c7-40d4-90bd-8970975856ee))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 7127f945-01fc-4efc-8406-62122ca9a1f1))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp f120e6d1-82c5-4a8a-8ef7-c83fe9a36179))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 0cc5c9e9-770e-40e2-85ce-69ab9e9fedea))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 5f369b18-0ec6-466c-ad97-a47ce15979f8))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 884e2a48-1a60-4500-a4f0-3384bf5803d2))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp e40015f8-5e96-4940-8faf-931cae3c1b2b))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp e722cc4d-8b51-4679-927a-dd66c03f292c))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp ca69d446-e2a9-4d88-8a4d-409ccb109d36))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 5650ddff-c5f0-498f-8aaf-7c8cb67bab37)
    (at 174.9 130.4)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/8ade4f9a-b824-4c00-b090-a166074fdf98")
    (attr smd)
    (fp_text reference "C23" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp fd0e1af4-a735-4a1d-ab69-5269829e1c28)
    )
    (fp_text value "1uF/50V" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp df0a50bb-485a-4c7d-8316-f9469aad0b3f)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp b589158a-d0cd-40de-b311-c481a50048e6)
    )
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp 06f2039c-ff4a-4491-9889-3f314ea69b33))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp 2dae44fd-f9ab-43fe-97f1-560a21ddb070))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 0d77fed2-991d-4696-9ff2-c6c8c4e04154))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 17c6b762-6ff9-4930-9ae6-e309880a3fa2))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 25dc9c04-9e80-42cb-8912-23d2e04a041f))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp a39ec1e1-f288-48da-8ea7-ce9d35766421))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 06c5c09e-4114-41c8-a4f2-634075099364))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 8d048212-d735-46f1-9d8b-5d89c534730f))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp af44dc8a-aecc-4bf8-aa32-f05c27efffa7))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp d0064468-dee3-4a1e-83bf-5c074b9ab9ef))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp ef3ef5bc-ecec-475d-88df-5ac96930f274))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(C23-Pad2)") (pintype "passive") (tstamp 9b56fbb6-f886-47e5-8a18-f0396e5baf5e))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 57ba07f7-23d5-44c4-89f1-03be3d7fffbf)
    (at 159.5 118 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/5c56e763-eeb5-455b-8c25-846e8ddcc102")
    (attr smd)
    (fp_text reference "R25" (at 0 1.17 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5f6c1231-c9e7-46cb-b29e-0060e356637a)
    )
    (fp_text value "10k" (at 0 -1.17 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4bf96d01-75ce-409b-b1cd-297ff35af05d)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 2975b14e-41eb-452f-b2e7-2e65f286456e)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 1b764483-9ae0-46f1-b2e0-cb97482d2f91))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 64d5b7e2-dc41-4ea8-91d3-1c06d3b7eaeb))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 0377f5d3-2d4d-4c01-a126-cd0289a47881))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 3eba88c5-52bf-4c0b-8e3c-8f2c2fcebd21))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 9457f249-306a-4c43-8719-bd6a13f61ea9))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp a2baec2c-d5a9-48ab-aa84-852ce6e24430))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 10e49206-22dd-40b4-a900-b88d107a4138))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 5b446841-7ee8-4f79-9657-10a1e4335eb6))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 8b8425d2-e87b-4929-b8d8-daa1c986f18c))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp b009bb50-d6b0-41cd-b93d-3c9261de2ea8))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "VBUS") (pintype "passive") (tstamp 2268dc69-c8e4-4694-aad0-5fea790ae04e))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp fde958ab-7fcc-47ec-9bad-9059ac694027))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 58b88994-723e-40d2-8fb9-98403b8c0975)
    (at 174.9 127.3)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/35ed39c6-cb9d-4b31-9a1b-4646e6c39a13")
    (attr smd)
    (fp_text reference "C28" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 92085fdd-fea5-4fd6-93e4-af1a67aea759)
    )
    (fp_text value "1uF/50V" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5885999e-87e0-498b-b073-cf90c8e0aeaa)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 378173bf-93e8-46ac-a3fe-7bebd677bd57)
    )
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp 5ef6c2b9-03e5-4637-a8fd-782a5a83a1fa))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp 6ff332bb-9ab0-4ca4-b373-76c39b6c5bb6))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 3ba3f4e5-69d2-43dd-a2f4-faf75243f7f2))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 3f676555-2cf2-4426-a2c3-6c7a0db3a662))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 46e68a54-0094-4c83-b3a8-46b09a544863))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp beed6871-cd7c-4000-a34f-118b2ffa8512))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp a1c742dd-07ad-424d-aae9-3b434c47794a))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp c62fe7f8-bffe-49c8-a56d-84fddcab1c2b))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp ed53de20-2b83-4633-a775-83a71ea4ee0b))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp f34518ae-93cd-4054-a422-e20b64ea7989))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 847ae362-8fb9-411d-9827-f6c59422fb5c))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "VDD") (pintype "passive") (tstamp 46bc8e2f-ac0f-4da1-9183-efb8659c6cb5))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 684fb381-e33c-450b-9a80-3f3f79f82b15)
    (at 128.4 126.6875 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/6c6fb0a5-2807-42a3-bfcc-2ef023793f96")
    (attr smd)
    (fp_text reference "C4" (at 0 1.16) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d4e3a54f-0992-472f-8621-92781ce7ed6d)
    )
    (fp_text value "100nF" (at 0 -1.16) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 45f97375-a37e-4e2f-b80b-939efa51a81f)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
      (tstamp b70b2d94-e148-495a-80d9-1c059c36df51)
    )
    (fp_line (start -0.107836 0.36) (end 0.107836 0.36) (layer "B.SilkS") (width 0.12) (tstamp 712e5ace-a30f-487a-a185-0796f364566f))
    (fp_line (start -0.107836 -0.36) (end 0.107836 -0.36) (layer "B.SilkS") (width 0.12) (tstamp a9c26dc7-7ddb-4021-824d-30b18e0f604d))
    (fp_line (start -0.91 0.46) (end 0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 7ffe0ff6-19ce-415c-8d8d-5bb4d27c0961))
    (fp_line (start -0.91 -0.46) (end -0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 9970c24a-134f-48ee-ad8e-84f8fec74ee2))
    (fp_line (start 0.91 -0.46) (end -0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp b8bb9891-eb2d-4043-907c-a61560836213))
    (fp_line (start 0.91 0.46) (end 0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp d810e4dd-2052-4d4a-a828-8a42dff14833))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 15b6af81-8def-42fb-b174-981cba0d4d9a))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 2f8adfb7-2fe5-463c-b217-8c13e9757a86))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 96df8a23-1fe2-48d3-b8b4-f78b9d73b6df))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp af543cdc-a039-4d34-8e80-453d6dfb7626))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp 03c97026-d19a-4b58-8ea5-0b9b70b26339))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 03501c9f-8511-4bd0-bcc9-937842649bec))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-666" (layer "B.Cu")
    (tedit 5A02FF57) (tstamp 712f1fd6-029a-4525-8357-c07359d32f03)
    (at 195.4 147.2 -90)
    (descr "SOT666")
    (tags "SOT-666")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/977bde71-d79a-4262-9cc5-f31fae627590")
    (attr smd)
    (fp_text reference "U13" (at 0 1.75 -270) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 45d99599-3c2d-42a8-b0f8-e37470d726ff)
    )
    (fp_text value "USBLC6-2P6" (at 0 -1.75 -270) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 9a660cd2-2ef2-4a09-85b2-d5ad98c6de4c)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
      (tstamp f4571330-5106-4324-b234-eac6dcc29b72)
    )
    (fp_line (start -0.8 -0.9) (end 0.8 -0.9) (layer "B.SilkS") (width 0.12) (tstamp 39c1c1f5-71df-43bf-8c0b-1627587bb198))
    (fp_line (start 0.8 0.9) (end -1.1 0.9) (layer "B.SilkS") (width 0.12) (tstamp 46bdcdb3-2688-4f58-83f4-5e85992b6107))
    (fp_line (start -1.5 1.1) (end 1.5 1.1) (layer "B.CrtYd") (width 0.05) (tstamp 1677d044-bd63-48ff-b63b-b3feb2cebdc5))
    (fp_line (start -1.5 1.1) (end -1.5 -1.1) (layer "B.CrtYd") (width 0.05) (tstamp 427d398f-cb7f-437b-8c5e-2c8b667e8b8c))
    (fp_line (start 1.5 -1.1) (end 1.5 1.1) (layer "B.CrtYd") (width 0.05) (tstamp e34e48a9-d43e-4152-84f3-639fdb2a0569))
    (fp_line (start -1.5 -1.1) (end 1.5 -1.1) (layer "B.CrtYd") (width 0.05) (tstamp f3bc6ec1-440f-4235-ac85-9527c4d7b8fe))
    (fp_line (start 0.65 0.85) (end 0.65 -0.85) (layer "B.Fab") (width 0.1) (tstamp 202947b9-829e-4e83-8e97-6f7f967efc32))
    (fp_line (start 0.65 -0.85) (end -0.65 -0.85) (layer "B.Fab") (width 0.1) (tstamp 4914f67e-14f5-4bcf-9fc0-3a7fc5df2d1c))
    (fp_line (start -0.65 0.53) (end -0.33 0.85) (layer "B.Fab") (width 0.1) (tstamp bbc15ba6-9526-4c9e-886c-0b496b226dfd))
    (fp_line (start 0.65 0.85) (end -0.33 0.85) (layer "B.Fab") (width 0.1) (tstamp bced1dbc-0a69-4de6-85a1-1a4535d0c3e6))
    (fp_line (start -0.65 0.53) (end -0.65 -0.85) (layer "B.Fab") (width 0.1) (tstamp fab26335-5d26-4b23-836d-9f9f40818b33))
    (pad "1" smd rect (at -0.85 0.5375 270) (size 0.5 0.375) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 98 "/WiFi_Display/UART_TX") (pinfunction "I/O1") (pintype "passive") (tstamp a552f05e-f4fa-4331-8d0d-752b917d1742))
    (pad "2" smd rect (at -0.925 0 270) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive") (tstamp 8ef8d120-5af9-4314-ae99-6b1f7c0533e6))
    (pad "3" smd rect (at -0.85 -0.5375 270) (size 0.5 0.375) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 97 "/WiFi_Display/UART_RX") (pinfunction "I/O2") (pintype "passive") (tstamp 0ae43ca7-29d0-4e83-8e4e-9270453940fc))
    (pad "4" smd rect (at 0.85 -0.5375 270) (size 0.5 0.375) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 97 "/WiFi_Display/UART_RX") (pinfunction "I/O2") (pintype "passive") (tstamp 62101fdc-bd38-4430-8ede-f73287f451c5))
    (pad "5" smd rect (at 0.925 0 270) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "VBUS") (pinfunction "VBUS") (pintype "passive") (tstamp 56f08d1e-5db4-4282-b3c2-bb350253fde1))
    (pad "6" smd rect (at 0.85 0.5375 270) (size 0.5 0.375) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 98 "/WiFi_Display/UART_TX") (pinfunction "I/O1") (pintype "passive") (tstamp d668ab34-3c8e-4eb7-a5e7-d316c144ce7b))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-666.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 71ca6e8d-c1c6-4908-8bcc-cc05d65c76e7)
    (at 149.22 140 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/08a6c28a-e899-4622-bc28-0af06dccdee9")
    (attr smd)
    (fp_text reference "C7" (at 0 1.16) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 25360ba5-e32b-4cdb-933d-04e21f4bb1d9)
    )
    (fp_text value "10nF" (at 0 -1.16) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5851c52a-fba0-4500-9148-3ce5c2a4aef3)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
      (tstamp f85836b6-4782-42ec-8ad3-b52a43f8cc41)
    )
    (fp_line (start -0.107836 0.36) (end 0.107836 0.36) (layer "B.SilkS") (width 0.12) (tstamp 839abacf-dea3-494b-8026-3d2df30972a7))
    (fp_line (start -0.107836 -0.36) (end 0.107836 -0.36) (layer "B.SilkS") (width 0.12) (tstamp 896f9ccb-629a-4826-9943-0fd704921dd0))
    (fp_line (start 0.91 -0.46) (end -0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 02264127-ba56-421a-8871-e00b85c5e3cf))
    (fp_line (start -0.91 -0.46) (end -0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 5448c6a6-97a9-413c-b798-214141277b61))
    (fp_line (start -0.91 0.46) (end 0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 89e7f6f7-4f75-47ad-bf49-9da0f7692005))
    (fp_line (start 0.91 0.46) (end 0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp ef9f324c-70ff-4ec8-a527-760737a913b9))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 521e85da-da8f-4eb1-aff6-83ad369730af))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 7499d1d2-cc24-4f3c-8179-93710c423154))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 90240f78-9ae0-4f53-9a60-2074e695091c))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 971b9fba-4a75-405b-9b76-0b6f9a863bac))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp 84cf1403-408c-495e-9630-578f526ca15c))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp dc3168fd-3060-47ee-9c43-2c892df4bd4a))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 79eb008b-eb5c-4e26-93a2-6f5e1f9eb4fc)
    (at 174.9 117.9)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/b4770654-29c0-4fc2-8a72-b7b5e1e4d05a")
    (attr smd)
    (fp_text reference "C26" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0f2e3d82-7aa2-46df-8abc-7fa3ea4b9372)
    )
    (fp_text value "1uF/50V" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 926ebdce-e76c-4f7f-8a54-b345f5ff3927)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp a066fbb9-2e83-4439-8bc1-dc24f76b1294)
    )
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp d322dcb0-4b42-4fd1-86be-2478d332c9e1))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp ef8353fd-ef2e-4228-904c-d933425604dd))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 1efcbc3f-07ed-4ced-b535-cb78a798b5a9))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 80bbe12f-3695-4687-8ca2-94963df54481))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp cbbe1107-f3f7-45e7-a117-a707e40795ae))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp dcfd65f2-1ff8-45ec-bd9f-d3fa941f9e1b))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 25eb3656-9c65-4c12-bdab-4dfd45dee27f))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 4a75e7fb-5af5-429e-adf6-adf7c0aae4a8))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 9521df45-5bee-4b09-a2e3-5e9ea57fc33a))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp db0350ba-2e64-46cd-aeb6-50d299b4e91b))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 0aa95f6d-69d6-4c3d-9463-24537e3d1dd4))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 16 "/WiFi_Display/PREVGL") (pintype "passive") (tstamp c074c292-82f1-434d-92d7-99f37469dee0))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Button_Switch_SMD:Panasonic_EVQPUJ_EVQPUA" (layer "B.Cu")
    (tedit 5A02FC95) (tstamp 7c2a174f-35b6-4466-9b6a-e5a41813c832)
    (at 150.4 107.4 180)
    (descr "http://industrial.panasonic.com/cdbs/www-data/pdf/ATV0000/ATV0000CE5.pdf")
    (tags "SMD SMT SPST EVQPUJ EVQPUA")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/ad0ceda8-36a4-411d-8eb9-98e6845a3a17")
    (attr smd)
    (fp_text reference "SW1" (at 0 4.5) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp ab5c0926-48d9-4028-a4dc-6678d08e75af)
    )
    (fp_text value "EVQPUA02K" (at 0 -3.5) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4f0b6af4-b46e-4538-93d0-b7c5bb246083)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 8f717386-801b-48dc-82cd-f01b16584350)
    )
    (fp_line (start -2.45 -0.275) (end -2.45 0.275) (layer "B.SilkS") (width 0.12) (tstamp 03901ba5-96c2-4b22-ac48-ffa7763a5c94))
    (fp_line (start 2.45 -0.275) (end 2.45 0.275) (layer "B.SilkS") (width 0.12) (tstamp 2edb4960-2349-4b3d-bf55-2525f126a3f0))
    (fp_line (start 2.35 1.85) (end 1.425 1.85) (layer "B.SilkS") (width 0.12) (tstamp 3360c184-96a5-42a5-ba35-06618b3183e9))
    (fp_line (start 2.35 -1.85) (end -2.35 -1.85) (layer "B.SilkS") (width 0.12) (tstamp 4b60a8c8-b675-4d1d-bba3-92e0c459d8db))
    (fp_line (start -1.425 1.85) (end -2.35 1.85) (layer "B.SilkS") (width 0.12) (tstamp fc50ec4b-1f70-4d26-a8fd-2c58fbaba624))
    (fp_line (start 3.9 -2.25) (end -3.9 -2.25) (layer "B.CrtYd") (width 0.05) (tstamp 496c7c28-d9b7-43a2-9ab9-36dc0fdd7e00))
    (fp_line (start 3.9 -2.25) (end 3.9 3.25) (layer "B.CrtYd") (width 0.05) (tstamp 78a09d7d-7649-4d53-b555-f983a9a04f26))
    (fp_line (start -3.9 -2.25) (end -3.9 3.25) (layer "B.CrtYd") (width 0.05) (tstamp a9e45979-9029-41e0-b160-b709cad16e12))
    (fp_line (start 3.9 3.25) (end -3.9 3.25) (layer "B.CrtYd") (width 0.05) (tstamp f9af92dc-4bb1-47ae-a043-9d475a55ad5c))
    (fp_line (start 1.3 2.75) (end 1.3 1.75) (layer "B.Fab") (width 0.1) (tstamp 28d3166b-77b9-4ed3-8c67-e00b3e944b58))
    (fp_line (start 2.35 1.75) (end -2.35 1.75) (layer "B.Fab") (width 0.1) (tstamp 49aadf9a-fd81-4ab8-ace2-5ffb9da1ff01))
    (fp_line (start 1.3 2.75) (end -1.3 2.75) (layer "B.Fab") (width 0.1) (tstamp 5679d703-bf0d-4861-9fe9-28e2f857f62b))
    (fp_line (start 2.35 -1.75) (end 2.35 1.75) (layer "B.Fab") (width 0.1) (tstamp a70fafd5-3b5f-40be-a312-4e83d56d88bf))
    (fp_line (start 2.35 -1.75) (end -2.35 -1.75) (layer "B.Fab") (width 0.1) (tstamp b6105d0d-98d6-4b97-a2c8-d41e79693943))
    (fp_line (start -2.35 -1.75) (end -2.35 1.75) (layer "B.Fab") (width 0.1) (tstamp f7db98b9-1847-4d73-a874-96785b53cc78))
    (fp_line (start -1.3 2.75) (end -1.3 1.75) (layer "B.Fab") (width 0.1) (tstamp faf30b43-b2c3-4368-b67f-185783587590))
    (pad "1" smd rect (at 2.625 0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive") (tstamp b0939504-a2db-435a-bcc8-d6290025c73f))
    (pad "1" smd rect (at -2.625 0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive") (tstamp eda9caa4-66ac-4d86-a8a6-dcbfc9fe5903))
    (pad "2" smd rect (at 2.625 -0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "/Sensor_Controller/LPC_~{ISP}") (pinfunction "2") (pintype "passive") (tstamp 289727e8-1973-4f9c-9913-e8f2b620742c))
    (pad "2" smd rect (at -2.625 -0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "/Sensor_Controller/LPC_~{ISP}") (pinfunction "2") (pintype "passive") (tstamp 8314b4f5-250f-49e2-8a13-33d624c278c0))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/Panasonic_EVQPUJ_EVQPUA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Inductor_SMD:L_1210_3225Metric" (layer "B.Cu")
    (tedit 5F68FEF0) (tstamp 7d1fc2c2-7dac-402b-add3-fcd0eb27863a)
    (at 150.1 115.1 180)
    (descr "Inductor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/7a1f2c6b-9ca1-4af3-bf3c-5c9c2c2e3f32")
    (attr smd)
    (fp_text reference "L2" (at 0 2.28) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f96a6449-1179-4aab-bbd1-d29f43b19c20)
    )
    (fp_text value "2.2uH/1.5A, BRL3225T2R2M" (at 0 -2.28) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 169d5d1f-bb77-43e9-a4f7-7917ae665f8e)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.8 0.8) (thickness 0.12)) (justify mirror))
      (tstamp 77a7a142-bcdf-474d-b0a5-acc637b6f07a)
    )
    (fp_line (start -0.602064 1.36) (end 0.602064 1.36) (layer "B.SilkS") (width 0.12) (tstamp 06f35939-7af4-4739-9b87-69128d88932a))
    (fp_line (start -0.602064 -1.36) (end 0.602064 -1.36) (layer "B.SilkS") (width 0.12) (tstamp 418bb36c-4f60-4a3d-945a-e88bdbf30f81))
    (fp_line (start -2.28 1.58) (end 2.28 1.58) (layer "B.CrtYd") (width 0.05) (tstamp 3089e5ea-f3aa-4061-b626-7e16d2662243))
    (fp_line (start -2.28 -1.58) (end -2.28 1.58) (layer "B.CrtYd") (width 0.05) (tstamp 57551be9-437f-452c-9777-686b1051752d))
    (fp_line (start 2.28 1.58) (end 2.28 -1.58) (layer "B.CrtYd") (width 0.05) (tstamp 623cab55-76dd-41eb-8054-d9fb7c9b477d))
    (fp_line (start 2.28 -1.58) (end -2.28 -1.58) (layer "B.CrtYd") (width 0.05) (tstamp e50c6ed6-22ab-47b0-8848-9f971b8a41b4))
    (fp_line (start 1.6 -1.25) (end -1.6 -1.25) (layer "B.Fab") (width 0.1) (tstamp 4e495535-73a5-4f8b-b361-23597d9a85db))
    (fp_line (start -1.6 -1.25) (end -1.6 1.25) (layer "B.Fab") (width 0.1) (tstamp 50b92fcd-0a06-48c1-b706-197e62dc24a5))
    (fp_line (start 1.6 1.25) (end 1.6 -1.25) (layer "B.Fab") (width 0.1) (tstamp 565170d4-e506-4550-a149-0bdbcc9dc88a))
    (fp_line (start -1.6 1.25) (end 1.6 1.25) (layer "B.Fab") (width 0.1) (tstamp 8f719a75-21cd-4f20-8236-1fa4c5e41f81))
    (pad "1" smd roundrect (at -1.4 0 180) (size 1.25 2.65) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 82 "Net-(L2-Pad1)") (pinfunction "1") (pintype "passive") (tstamp 7b578300-4474-46d2-b8de-88f7e4013340))
    (pad "2" smd roundrect (at 1.4 0 180) (size 1.25 2.65) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 9 "VDD") (pinfunction "2") (pintype "passive") (tstamp bc359569-2635-4498-a0e3-6d841f11b36e))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 7d68677c-5326-4665-a3c5-ae55f8c3bb66)
    (at 153.6 133 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/61e7f132-cec4-465b-aa57-86a109c5fe88")
    (attr smd)
    (fp_text reference "R3" (at 0 1.17 -270) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp bb350d53-f544-4f52-8e80-331a4d5f04aa)
    )
    (fp_text value "4k7" (at 0 -1.17 -270) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 104b597b-4c43-4d47-8047-8a9b894da72e)
    )
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 754de932-970d-4847-ac83-f53dcf776cd2)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 33b43a2a-a5b2-4373-a0d6-19c05353209b))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 8e1dab39-df24-4681-890a-90a07f64259b))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 30a20e78-660d-4d6c-940c-9a783bd93c14))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 5de11ea8-2c1c-45f8-a53f-6f3feb433c0a))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 6791244d-40dc-4651-8880-8434053d17ba))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp f7a86f33-ee9e-48c0-a13c-0247dda4b98a))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 40ab2bf6-e76b-4f72-8007-cfb0eb36074f))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 7e30cfef-c526-46f8-9e80-1504afec1279))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp a37f1a71-d18d-443e-ba6a-278f2a4d1d6c))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp b7ad052e-9347-4728-8118-26d475bac57f))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp eaeda4e1-1b24-43c1-84b5-c312f9145342))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 42 "/Sensor_Controller/I2C_SCL") (pintype "passive") (tstamp 2c8a36e7-ca8b-45df-b76d-59de0b4e92da))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 7f9e53a4-b637-4449-8e34-b620debdb296)
    (at 128.4 141.9)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/d8468354-a2cc-4351-aa35-2e7bdee71071")
    (attr smd)
    (fp_text reference "C2" (at 0 1.16) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 04a1d56f-f939-4adb-ad80-d98fe6818e0c)
    )
    (fp_text value "100nF" (at 0 -1.16) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 92d4e39a-9db1-43b8-bdba-bdddc46963a5)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
      (tstamp 5001a481-bc3a-413f-acb7-9066a37098a9)
    )
    (fp_line (start -0.107836 -0.36) (end 0.107836 -0.36) (layer "B.SilkS") (width 0.12) (tstamp 93ae75bc-4328-4262-92e1-b5f6f1d4d255))
    (fp_line (start -0.107836 0.36) (end 0.107836 0.36) (layer "B.SilkS") (width 0.12) (tstamp ef0013d5-019e-4994-997d-469e8d298944))
    (fp_line (start 0.91 0.46) (end 0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 0ab0584a-1e00-417a-b0de-ae29f77273fd))
    (fp_line (start -0.91 0.46) (end 0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 197eb725-36cf-4295-b288-5d3d3e7ce5c8))
    (fp_line (start -0.91 -0.46) (end -0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 5848a774-adae-4bea-86a8-725647c734e8))
    (fp_line (start 0.91 -0.46) (end -0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp d0eb86b9-8c95-46cd-899e-69af84c7f11e))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 514ed829-4035-4325-8137-4ec90c9dd886))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 6b1a05b3-9634-4da3-8f94-365e2da6e703))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 7eef0b40-0096-4af8-886c-bd74ff80b00b))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp a9791ffc-8b0a-494f-9ef2-a1971fd8041b))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp 957f9e53-5ec3-459f-a470-3f0806b58ee8))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp ae342d38-bb03-4ffe-9632-3fecd496522e))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958) (tstamp 830f235c-cfb1-48de-9ca8-e2c2d9955dd9)
    (at 169.6 126.3 -90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/f27783ed-9efe-4703-8c28-0816eaad2c35")
    (attr smd)
    (fp_text reference "Q2" (at 0 2.4 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e42fe7d2-af11-4777-ad13-86bbab1ae9d9)
    )
    (fp_text value "SI1308EDL" (at 0 -2.4 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5421654f-13fd-4b21-a4fe-82869dc9ae54)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 0.32 0.32) (thickness 0.05)) (justify mirror))
      (tstamp 90771145-6a42-46db-9d25-7b17c27f80dd)
    )
    (fp_line (start 0 -1.56) (end -0.65 -1.56) (layer "B.SilkS") (width 0.12) (tstamp 4c610214-837a-417f-bb83-d760295b6f63))
    (fp_line (start 0 1.56) (end -1.675 1.56) (layer "B.SilkS") (width 0.12) (tstamp 4e189d1c-afb9-453c-976d-15248061a901))
    (fp_line (start 0 -1.56) (end 0.65 -1.56) (layer "B.SilkS") (width 0.12) (tstamp 50202cff-99ad-4375-b0d6-483aa7cee68b))
    (fp_line (start 0 1.56) (end 0.65 1.56) (layer "B.SilkS") (width 0.12) (tstamp 9d537d4c-a0c9-48ae-a8e5-f5ad53d64d86))
    (fp_line (start -1.92 1.7) (end -1.92 -1.7) (layer "B.CrtYd") (width 0.05) (tstamp 28da967a-58a0-442b-84c5-0c6bfe34dadf))
    (fp_line (start 1.92 1.7) (end -1.92 1.7) (layer "B.CrtYd") (width 0.05) (tstamp 64d09917-0a09-4334-8b14-0dcee4e3ac5e))
    (fp_line (start -1.92 -1.7) (end 1.92 -1.7) (layer "B.CrtYd") (width 0.05) (tstamp b6943e55-e8ed-41ca-948c-e9a4e160e91c))
    (fp_line (start 1.92 -1.7) (end 1.92 1.7) (layer "B.CrtYd") (width 0.05) (tstamp f7061b02-7da1-43e2-9593-b59a02f500a8))
    (fp_line (start 0.65 -1.45) (end -0.65 -1.45) (layer "B.Fab") (width 0.1) (tstamp 29fc5c75-e0f8-4d66-8b30-f1c5ebc0b2ec))
    (fp_line (start -0.325 1.45) (end 0.65 1.45) (layer "B.Fab") (width 0.1) (tstamp 6fa88215-bc1e-4d23-81c4-513e10d5aff5))
    (fp_line (start -0.65 -1.45) (end -0.65 1.125) (layer "B.Fab") (width 0.1) (tstamp a09326a6-f91e-4ff5-a7d5-fd6fd37ba303))
    (fp_line (start 0.65 1.45) (end 0.65 -1.45) (layer "B.Fab") (width 0.1) (tstamp d61e88ee-d8cd-4834-88f9-4274b691c3b5))
    (fp_line (start -0.65 1.125) (end -0.325 1.45) (layer "B.Fab") (width 0.1) (tstamp fe297dd7-73d4-401e-9102-3ef3240fb7da))
    (pad "1" smd roundrect (at -0.9375 0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 30 "/WiFi_Display/GDR") (pinfunction "G") (pintype "input") (tstamp 13e13a6f-8ea6-47eb-8887-a32e627143fe))
    (pad "2" smd roundrect (at -0.9375 -0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "/WiFi_Display/RESE") (pinfunction "S") (pintype "passive") (tstamp 0428e785-a8cc-4d06-9956-bcbeae17a743))
    (pad "3" smd roundrect (at 0.9375 0 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(C22-Pad2)") (pinfunction "D") (pintype "passive") (tstamp 0f481208-5023-4d75-b0f6-4619745df4aa))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 85db620f-0936-4015-b90f-7d195f73fece)
    (at 174.9 122.8)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/e62f2693-a028-431a-b2ab-4c5c401d17d0")
    (attr smd)
    (fp_text reference "C30" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4792c1ca-0755-4b46-82ac-8d2ce775705e)
    )
    (fp_text value "1uF/50V" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 653f71b2-30db-4798-a6a5-045ec65e1df5)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 534952b5-7fe3-4f62-bbea-5f9fd03a667c)
    )
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp 0952cd5d-15ac-4949-bf38-1e696debfa44))
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp 1d8db80b-b6ce-4eba-9498-dea9fe1fbf70))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 3d69bc7f-ae72-4fe9-94d7-d899f178bbfe))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 40c2d070-79bc-4fb9-9279-17c2f680f04e))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp bb6f2087-e894-4513-ad02-35ed08998bbc))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp c950d5d2-5e3c-4ab8-a4f4-56f6551c9558))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 90ba32c5-6410-4512-93ae-38b161bf6d3f))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp b1556e2c-c69e-49d6-8987-f213324313a2))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp ca30d885-c63d-44d5-8ad7-69844ae0dad8))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp e7ea066d-360d-483d-b7a8-9925a9671d45))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp d71eaf8d-17ed-4706-8f9c-eabb30363291))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(C30-Pad2)") (pintype "passive") (tstamp 3a55e3ee-ef19-45c7-81c3-0881f5d8530f))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "ESP32_Module:ESP32-C3-MINI-1" (layer "B.Cu")
    (tedit 0) (tstamp 87501285-62ab-4d19-824d-19f4277b0e70)
    (at 123.35 112.75 -90)
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/e999ee1a-2a83-42f5-928b-d28b8b805ac0")
    (attr smd)
    (fp_text reference "U12" (at -0.6 -7.1 -270 unlocked) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f06d5c4b-6886-4b63-b297-12250c38456e)
    )
    (fp_text value "ESP32-C3-Mini-1" (at 0 -1 -270 unlocked) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp bfde603e-e316-4731-93ed-07571bfb220c)
    )
    (fp_text user "${REF}" (at 0 -2.5 -270 unlocked) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e0b82b99-49b4-4f92-be3e-83d42cafb0d3)
    )
    (fp_line (start -6.6 5.6) (end -6.6 11) (layer "Dwgs.User") (width 0.1) (tstamp 42f7b6c7-b235-4337-af7c-74a950153d03))
    (fp_line (start -6.6 5.6) (end -6.6 -5.6) (layer "Dwgs.User") (width 0.1) (tstamp 53fd91bd-c64d-4af5-8350-fd0232b9315f))
    (fp_line (start 6.6 -5.6) (end 6.6 5.6) (layer "Dwgs.User") (width 0.1) (tstamp 7104a1ed-94c3-4cd8-a7bf-228f031c1d2d))
    (fp_line (start -6.6 -5.6) (end 6.6 -5.6) (layer "Dwgs.User") (width 0.1) (tstamp 715d3dbc-acd2-4756-85b0-44e1979db720))
    (fp_line (start 6.6 5.6) (end 6.6 11) (layer "Dwgs.User") (width 0.1) (tstamp 89e358c3-65bf-4f17-9044-becd3e4200e0))
    (fp_line (start 6.6 11) (end -6.6 11) (layer "Dwgs.User") (width 0.1) (tstamp a1c3590e-f145-4e7d-a255-70826f537ba1))
    (fp_line (start 6.6 5.6) (end -6.6 5.6) (layer "Dwgs.User") (width 0.1) (tstamp b797daa2-1186-4972-a823-94bc01d0ed38))
    (fp_line (start 6.6 11) (end -6.6 5.6) (layer "Dwgs.User") (width 0.1) (tstamp eb8730c1-84b9-4db0-abd4-ff9192c86b40))
    (pad "1" smd rect (at -5.9 4 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp cff1aad7-9b56-41b4-a3d5-13bbdf87b093))
    (pad "2" smd rect (at -5.9 3.2 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp fd516020-4377-4ff7-8c31-cb221bf5be6e))
    (pad "3" smd rect (at -5.9 2.4 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "VDD") (pinfunction "3V3") (pintype "power_in") (tstamp 96710aae-5380-4c5e-806e-f6019b40f3ee))
    (pad "4" smd rect (at -5.9 1.6 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 85 "unconnected-(U12-Pad4)") (pinfunction "NC") (pintype "no_connect") (tstamp 508710d6-b6f2-4918-bf27-5ccc2137b129))
    (pad "5" smd rect (at -5.9 0.8 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "/WiFi_Display/EPD_~{RES}") (pinfunction "IO2") (pintype "tri_state") (tstamp e3e034b3-276e-4c5e-b331-101621d904ee))
    (pad "6" smd rect (at -5.9 0 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 34 "/WiFi_Display/EPD_BUSY") (pinfunction "IO3") (pintype "tri_state") (tstamp 48eedbce-e092-4fa6-8c3c-8f6659b97f7d))
    (pad "7" smd rect (at -5.9 -0.8 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 86 "unconnected-(U12-Pad7)") (pinfunction "NC") (pintype "no_connect") (tstamp d393fe7b-421c-4973-952b-3e70a10d8aef))
    (pad "8" smd rect (at -5.9 -1.6 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 10 "Net-(C20-Pad1)") (pinfunction "EN") (pintype "input") (tstamp 764e8695-9cc5-495f-a278-c2225ea409f9))
    (pad "9" smd rect (at -5.9 -2.4 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 87 "unconnected-(U12-Pad9)") (pinfunction "NC") (pintype "no_connect") (tstamp 27beecaf-994e-49e0-8ff5-0797cd15bd39))
    (pad "10" smd rect (at -5.9 -3.2 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 88 "unconnected-(U12-Pad10)") (pinfunction "NC") (pintype "no_connect") (tstamp 94d9d8b4-042c-4ec1-a1ed-03e7eac8aa86))
    (pad "11" smd rect (at -5.9 -4 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp cb787e48-f293-4926-8cae-1d82f20e2004))
    (pad "12" smd rect (at -4.8 -4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 89 "unconnected-(U12-Pad12)") (pinfunction "IO0") (pintype "tri_state+no_connect") (tstamp 5d312589-0b24-41d1-afd5-af4498214dfd))
    (pad "13" smd rect (at -4 -4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 78 "/Sensor_Controller/SPI_~{INT}") (pinfunction "IO1") (pintype "tri_state") (tstamp 7aa827bf-0c69-45f9-86a0-c35929d3c6e1))
    (pad "14" smd rect (at -3.2 -4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp cea6f4eb-9ef5-451b-9c34-3b486f663a40))
    (pad "15" smd rect (at -2.4 -4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 90 "unconnected-(U12-Pad15)") (pinfunction "NC") (pintype "no_connect") (tstamp fbc434da-e162-4193-866e-adb61a0152f7))
    (pad "16" smd rect (at -1.6 -4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "/WiFi_Display/EPD_CS") (pinfunction "IO10") (pintype "tri_state") (tstamp 98ff7360-2f4d-41c4-b31d-fd299a99a037))
    (pad "17" smd rect (at -0.8 -4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 91 "unconnected-(U12-Pad17)") (pinfunction "NC") (pintype "no_connect") (tstamp f862175f-c138-49a5-a077-434074a19537))
    (pad "18" smd rect (at 0 -4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 38 "/WiFi_Display/EPD_SCLK") (pinfunction "IO4") (pintype "tri_state") (tstamp 02aef84a-a630-45d5-ac32-46c2d8753034))
    (pad "19" smd rect (at 0.8 -4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "/WiFi_Display/EPD_SDI") (pinfunction "IO5") (pintype "tri_state") (tstamp f6d6fde4-2ff3-423c-9880-d66b104212d5))
    (pad "20" smd rect (at 1.6 -4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 79 "/Sensor_Controller/SPI_MISO") (pinfunction "IO6") (pintype "tri_state") (tstamp f7a1d5fe-496c-4090-b078-b43b41e23dd0))
    (pad "21" smd rect (at 2.4 -4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 69 "/Sensor_Controller/SPI_CS") (pinfunction "IO7") (pintype "tri_state") (tstamp 8dd047ad-0c2c-4787-8f00-93f8e4a7591a))
    (pad "22" smd rect (at 3.2 -4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "/WiFi_Display/EPD_D{slash}~{C}") (pinfunction "IO8") (pintype "tri_state") (tstamp 513dec86-c952-4f8c-9e27-134ee70d3650))
    (pad "23" smd rect (at 4 -4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 92 "Net-(SW3-Pad2)") (pinfunction "IO9") (pintype "tri_state") (tstamp 4d8a535c-260c-4b8c-ac66-a8d204437ce1))
    (pad "24" smd rect (at 4.8 -4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 93 "unconnected-(U12-Pad24)") (pinfunction "NC") (pintype "no_connect") (tstamp 59a69132-8d5f-493e-9b7c-7d0b26c4d017))
    (pad "25" smd rect (at 5.9 -4 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 94 "unconnected-(U12-Pad25)") (pinfunction "NC") (pintype "no_connect") (tstamp 1dbc434a-9b34-4dab-bab5-3d1156eb2ae7))
    (pad "26" smd rect (at 5.9 -3.2 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 84 "/WiFi_Display/USB_D-") (pinfunction "IO18") (pintype "tri_state") (tstamp 3d2ddbd6-4364-4a4c-9060-079e7dc84a2d))
    (pad "27" smd rect (at 5.9 -2.4 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 83 "/WiFi_Display/USB_D+") (pinfunction "IO19") (pintype "tri_state") (tstamp ea17eaf1-4c6e-40c4-aac7-2dedd1365fca))
    (pad "28" smd rect (at 5.9 -1.6 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 95 "unconnected-(U12-Pad28)") (pinfunction "NC") (pintype "no_connect") (tstamp bbb1703b-483e-4697-b0dd-3bbab52b9173))
    (pad "29" smd rect (at 5.9 -0.8 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 96 "unconnected-(U12-Pad29)") (pinfunction "NC") (pintype "no_connect") (tstamp cd8d9d25-4747-47c1-83dc-ecf2558614d8))
    (pad "30" smd rect (at 5.9 0 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 97 "/WiFi_Display/UART_RX") (pinfunction "RXD0") (pintype "tri_state") (tstamp f4be51d4-436f-49ed-9b4f-eb06a1daec0a))
    (pad "31" smd rect (at 5.9 0.8 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 98 "/WiFi_Display/UART_TX") (pinfunction "TXD0") (pintype "tri_state") (tstamp 5dd662d0-c581-44d0-b1c3-3ae5f9d21dde))
    (pad "32" smd rect (at 5.9 1.6 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 99 "unconnected-(U12-Pad32)") (pinfunction "NC") (pintype "no_connect") (tstamp 8e0eab20-0b37-44db-97b4-4d7bc90b1317))
    (pad "33" smd rect (at 5.9 2.4 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 100 "unconnected-(U12-Pad33)") (pinfunction "NC") (pintype "no_connect") (tstamp 2adac89d-cb68-4fb8-bb8b-33707b4bf7df))
    (pad "34" smd rect (at 5.9 3.2 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 101 "unconnected-(U12-Pad34)") (pinfunction "NC") (pintype "no_connect") (tstamp d5ba88f5-7f66-4943-a441-270774ad8ea9))
    (pad "35" smd rect (at 5.9 4 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 102 "unconnected-(U12-Pad35)") (pinfunction "NC") (pintype "no_connect") (tstamp 4b940b5f-7b55-4c3f-bb48-e667b9cf8167))
    (pad "36" smd rect (at 4.8 4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp de973b81-adc5-4b39-a916-24f1b29bce2a))
    (pad "37" smd rect (at 4 4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 0cd886c8-2e62-41ec-b5f3-578e4fd5ffa7))
    (pad "38" smd rect (at 3.2 4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 87d21be9-e7b0-4bf9-a1b5-908eaf5777e0))
    (pad "39" smd rect (at 2.4 4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 03ed6c31-0861-46fd-90a2-705234bbf253))
    (pad "40" smd rect (at 1.6 4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp e2b605ab-2011-4f89-8272-e6d305b0ec53))
    (pad "41" smd rect (at 0.8 4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 4c924c44-3d4b-47a5-980a-7ab67b98dbc0))
    (pad "42" smd rect (at 0 4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 4c324237-9628-4b30-813f-9cb4039ada68))
    (pad "43" smd rect (at -0.8 4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 4d0743d9-e7b7-4d2d-9177-c39dd3566d11))
    (pad "44" smd rect (at -1.6 4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp d750b942-fee5-4f56-95e1-467c5ceab102))
    (pad "45" smd rect (at -2.4 4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp acaefc5e-cb01-424f-b6a2-416fadcbd8fd))
    (pad "46" smd rect (at -3.2 4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp d1c38329-8ca7-4745-b868-2402d8c46714))
    (pad "47" smd rect (at -4 4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 3f367c8b-e437-4a39-9372-8fad6af54d41))
    (pad "48" smd rect (at -4.8 4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp a83b5140-b738-49cc-bed4-d31417856f01))
    (pad "49" smd rect (at 0 1.975 270) (size 1.45 1.45) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 03911903-1c44-453e-83c1-3a8035c53a9b))
    (pad "49" smd rect (at 0 0 270) (size 1.45 1.45) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 26ad627a-4bb6-4def-857e-4b27333165a5))
    (pad "49" smd rect (at 1.975 1.975 180) (size 1.45 1.45) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 60ded7ac-3b08-4300-9936-2226080e45d9))
    (pad "49" smd rect (at 1.975 0 270) (size 1.45 1.45) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 7ea3d4c3-02a3-4f07-a556-c56a2615ef6e))
    (pad "49" smd rect (at -1.975 0 270) (size 1.45 1.45) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp aa1be952-04dd-447c-964c-b473bf3b5624))
    (pad "49" smd rect (at 1.975 -1.975 270) (size 1.45 1.45) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp b30fa555-136e-491c-bb09-810eb99acab6))
    (pad "49" smd rect (at -1.975 -1.975 270) (size 1.45 1.45) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp d5ea7269-4356-4671-994f-e2088f3ba2d8))
    (pad "49" smd roundrect (at -1.975 1.975 270) (size 1.45 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0)
      (chamfer_ratio 0.414) (chamfer bottom_left)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp d72e4bda-11c3-4e24-874c-0753a1fbb00e))
    (pad "49" smd rect (at 0 -1.975 270) (size 1.45 1.45) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp ddcde53d-9e57-49be-b17b-486eb68b5c8c))
    (pad "50" smd rect (at 5.95 4.95 270) (size 0.7 0.7) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 758f0efc-f8e3-4260-95ae-7a4c698684be))
    (pad "51" smd rect (at 5.95 -4.95 270) (size 0.7 0.7) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 5c34a94c-95f9-4f34-8896-9eefe7fb8c63))
    (pad "52" smd rect (at -5.95 -4.95 270) (size 0.7 0.7) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 1ed5f7e4-5c01-4e23-8be1-eaf328a84f94))
    (pad "53" smd rect (at -5.95 4.95 270) (size 0.7 0.7) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp f24c1f0d-0d72-4597-b045-71b218b3580c))
    (zone (net 0) (net_name "") (layers *.Cu "Dwgs.User") (tstamp dacb4ece-0a8f-4336-921c-254aaafb81ff) (hatch edge 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 117.75 119.35)
          (xy 117.75 106.15)
          (xy 112.35 106.15)
          (xy 112.35 119.35)
        )
      )
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 875f318c-ca2b-41d9-8455-86aa24bccdd8)
    (at 181.1 134.8 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/07ce96f0-ebcf-4468-9381-7d40b1b2a8d8")
    (attr smd)
    (fp_text reference "C15" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 59b87915-8700-4b78-82bb-93aa220310a0)
    )
    (fp_text value "4.7uF" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 830822dc-6c19-4aee-bbed-b42bd882f9df)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 60cc7178-87b8-4b14-ac75-02656e898c92)
    )
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp 345e650e-cab7-4f7c-8e23-a05d24685517))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp e790bb4f-9dff-4404-b663-07e29edeaeed))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 704c6497-67dc-4a16-9bcf-2962ec77d988))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp b76e5a12-e08f-4e98-8857-f987e760b41f))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp cef9d15e-689d-43e1-93d6-5b82b944a2c8))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp e04b0306-e349-4290-a4f4-969de632f7a7))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 9644d594-a1ff-48ac-8e51-3a42885e90ca))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp aa26397f-2c61-4c36-b526-44883c3a246c))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp cfb41a97-08cc-4b99-8529-6dc1b8d2d38e))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp ed0ba555-e6e4-43f1-8a65-2507c46d0243))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "VCC") (pintype "passive") (tstamp e8f2a94c-6ae6-48b5-84e1-f3f736a72d58))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 7a46462b-3f17-4fbd-a4b7-2b7ff0c165f3))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Inductor_SMD:L_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEF0) (tstamp 8ac28aef-b21c-4cbf-9b32-e308d2b47121)
    (at 165.8 122.6 90)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/d75d19d3-5b46-4b22-ae5d-4fe9be559e81")
    (attr smd)
    (fp_text reference "L3" (at 0 1.55 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 1a01a243-0538-4f32-bc4f-6e6d3a2b29b9)
    )
    (fp_text value "10uH, MLZ2012M100WTD25" (at 0 -1.55 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 38f6482f-0aaf-45ed-bc0f-e38c1774af8a)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp a3eecc3b-9693-4fba-9c8d-88827e35f56f)
    )
    (fp_line (start -0.399622 -0.56) (end 0.399622 -0.56) (layer "B.SilkS") (width 0.12) (tstamp 416cae2b-8f64-4020-a72c-29a7c6c6528f))
    (fp_line (start -0.399622 0.56) (end 0.399622 0.56) (layer "B.SilkS") (width 0.12) (tstamp c0583c07-405c-4673-b60d-8bafe03ee917))
    (fp_line (start 1.75 0.85) (end 1.75 -0.85) (layer "B.CrtYd") (width 0.05) (tstamp 234e5200-8ac4-4b3d-8553-93e8ec0a472b))
    (fp_line (start -1.75 0.85) (end 1.75 0.85) (layer "B.CrtYd") (width 0.05) (tstamp 84d568ff-21bb-4778-9ad5-ae603a21efca))
    (fp_line (start 1.75 -0.85) (end -1.75 -0.85) (layer "B.CrtYd") (width 0.05) (tstamp d6487cd5-1215-4561-a252-63a73f4469be))
    (fp_line (start -1.75 -0.85) (end -1.75 0.85) (layer "B.CrtYd") (width 0.05) (tstamp ffb3fcb7-37e2-46e1-bc6d-7fc06cf10451))
    (fp_line (start 1 0.45) (end 1 -0.45) (layer "B.Fab") (width 0.1) (tstamp 09222965-8dc7-4477-a769-e10b1a478704))
    (fp_line (start 1 -0.45) (end -1 -0.45) (layer "B.Fab") (width 0.1) (tstamp 0e2f7410-b777-4e95-bcc1-acb2df40bd76))
    (fp_line (start -1 0.45) (end 1 0.45) (layer "B.Fab") (width 0.1) (tstamp aa5166b2-88d1-4b0e-ad7d-f929d9e5acd3))
    (fp_line (start -1 -0.45) (end -1 0.45) (layer "B.Fab") (width 0.1) (tstamp c1e4c5ac-392a-4b2d-abac-8233bd6a10d0))
    (pad "1" smd roundrect (at -1.0625 0 90) (size 0.875 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "VDD") (pinfunction "1") (pintype "passive") (tstamp 41bfc507-4059-4be2-b39d-db68af57f2a9))
    (pad "2" smd roundrect (at 1.0625 0 90) (size 0.875 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(C22-Pad2)") (pinfunction "2") (pintype "passive") (tstamp 43b6599b-674e-4d0e-a909-f946dcb4e152))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_DFN_QFN:VQFN-32-1EP_5x5mm_P0.5mm_EP3.5x3.5mm_ThermalVias" (layer "B.Cu")
    (tedit 5DC5F6A8) (tstamp 8d4e399c-f677-4283-8935-ce15932c7076)
    (at 154.525 138.125 180)
    (descr "VQFN, 32 Pin (https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT4222H.pdf#page=40), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "VQFN NoLead")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/b5f834de-c7bf-4a4a-886f-7479a73ef33d")
    (attr smd)
    (fp_text reference "U5" (at 0 3.8) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 81b58340-3615-446f-bd2d-e2c9fb45f689)
    )
    (fp_text value "LPC804M101JHI33" (at 0 -3.8) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 1ea0601f-2b25-4c9c-9727-a0536b027d3c)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d78289a0-123a-4021-b5d0-b19f9bd4ec89)
    )
    (fp_line (start 2.61 -2.61) (end 2.61 -2.135) (layer "B.SilkS") (width 0.12) (tstamp 0a86c5b4-cab0-4951-9a04-8b3644547237))
    (fp_line (start 2.135 2.61) (end 2.61 2.61) (layer "B.SilkS") (width 0.12) (tstamp 36b371dc-6f64-47c0-bcd0-ba4657bcf187))
    (fp_line (start -2.61 -2.61) (end -2.61 -2.135) (layer "B.SilkS") (width 0.12) (tstamp 4034aff1-5049-48ca-b36a-e7cb54d38628))
    (fp_line (start 2.61 2.61) (end 2.61 2.135) (layer "B.SilkS") (width 0.12) (tstamp 9562f308-7d98-4081-b2e9-7acd2e53edcd))
    (fp_line (start 2.135 -2.61) (end 2.61 -2.61) (layer "B.SilkS") (width 0.12) (tstamp 97a665d9-00ae-43eb-8df6-4358ffa0d9aa))
    (fp_line (start -2.135 -2.61) (end -2.61 -2.61) (layer "B.SilkS") (width 0.12) (tstamp cd191336-45b2-4507-a30d-15f715df2f00))
    (fp_line (start -2.135 2.61) (end -2.61 2.61) (layer "B.SilkS") (width 0.12) (tstamp f910f391-c593-4e00-b6af-f1a415db2252))
    (fp_line (start 3.1 -3.1) (end 3.1 3.1) (layer "B.CrtYd") (width 0.05) (tstamp 4bc718e3-0dda-4cd7-9758-383baad8d602))
    (fp_line (start -3.1 3.1) (end -3.1 -3.1) (layer "B.CrtYd") (width 0.05) (tstamp 77443a9c-0d00-4bc2-a011-044a70edf3bb))
    (fp_line (start 3.1 3.1) (end -3.1 3.1) (layer "B.CrtYd") (width 0.05) (tstamp 7eb498f8-3ea7-4de6-9294-6c95d16d6b05))
    (fp_line (start -3.1 -3.1) (end 3.1 -3.1) (layer "B.CrtYd") (width 0.05) (tstamp ab80ae95-becf-4df3-b500-e9eb27ee5a69))
    (fp_line (start 2.5 -2.5) (end -2.5 -2.5) (layer "B.Fab") (width 0.1) (tstamp 0718ae16-c052-4435-8986-04c79eff36ff))
    (fp_line (start -1.5 2.5) (end 2.5 2.5) (layer "B.Fab") (width 0.1) (tstamp 1b24b644-34fd-49a9-b59c-abe20300f0b4))
    (fp_line (start 2.5 2.5) (end 2.5 -2.5) (layer "B.Fab") (width 0.1) (tstamp 2008c2c7-e713-48af-b3f9-4185630b35bf))
    (fp_line (start -2.5 -2.5) (end -2.5 1.5) (layer "B.Fab") (width 0.1) (tstamp 60d21545-7f8a-42ab-8eb3-ae6b05bdc437))
    (fp_line (start -2.5 1.5) (end -1.5 2.5) (layer "B.Fab") (width 0.1) (tstamp a60e2f43-13b8-45bb-953d-5feafe2717d1))
    (pad "" smd roundrect (at 0.875 -0.875 180) (size 1.46 1.46) (layers "B.Paste") (roundrect_rratio 0.171233) (tstamp 0867358d-8e73-414e-983f-1bd765f23dd0))
    (pad "" smd roundrect (at -0.875 -0.875 180) (size 1.46 1.46) (layers "B.Paste") (roundrect_rratio 0.171233) (tstamp 64df99fb-1e45-44f8-ab6b-8f66ba435516))
    (pad "" smd roundrect (at 0.875 0.875 180) (size 1.46 1.46) (layers "B.Paste") (roundrect_rratio 0.171233) (tstamp 861fbf20-22a7-4d6c-b256-ee2969680dd1))
    (pad "" smd roundrect (at -0.875 0.875 180) (size 1.46 1.46) (layers "B.Paste") (roundrect_rratio 0.171233) (tstamp c28d6b33-5ebc-4726-954c-d28f1747730f))
    (pad "1" smd roundrect (at -2.45 1.75 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 69 "/Sensor_Controller/SPI_CS") (pinfunction "PIO0_17/ADC_9") (pintype "tri_state") (tstamp 22251edf-dc68-4b2f-895d-e60c35544813))
    (pad "2" smd roundrect (at -2.45 1.25 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 70 "/Power_Management/LED_PWM") (pinfunction "PIO0_13/ADC_10") (pintype "tri_state") (tstamp 9a394f02-f4c9-4e9e-a35b-25d8d348013c))
    (pad "3" smd roundrect (at -2.45 0.75 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 40 "/Sensor_Controller/LPC_~{ISP}") (pinfunction "PIO0_12") (pintype "tri_state") (tstamp 583ea787-682f-4c0e-960b-39187d520ef5))
    (pad "4" smd roundrect (at -2.45 0.25 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/Sensor_Controller/LPC_~{RST}") (pinfunction "~{RESET}/PIO0_5") (pintype "tri_state") (tstamp fec7b2e2-1865-427f-bb89-da2b4032b804))
    (pad "5" smd roundrect (at -2.45 -0.25 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 71 "/Sensor_Controller/ALS_INT") (pinfunction "PIO0_4/ADC_11/TRSTN") (pintype "tri_state") (tstamp da047157-a0fe-4c80-8269-a34593421eec))
    (pad "6" smd roundrect (at -2.45 -0.75 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 44 "/Sensor_Controller/LPC_SWCLK") (pinfunction "SWCLK/PIO0_3/TCK") (pintype "tri_state") (tstamp 184ddae0-b65e-45be-9afd-e5be77bd26ab))
    (pad "7" smd roundrect (at -2.45 -1.25 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 43 "/Sensor_Controller/LPC_SWDIO") (pinfunction "SWDIO/PIO0_2/TMS") (pintype "tri_state") (tstamp 1bd692a3-1ee2-45ab-868b-df34ac55930b))
    (pad "8" smd roundrect (at -2.45 -1.75 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 72 "/Sensor_Controller/RTC_CLKO") (pinfunction "PIO0_11/ADC_6/WKTCLKIN") (pintype "tri_state") (tstamp a8b141cb-5408-4b57-8861-2f86502c64e9))
    (pad "9" smd roundrect (at -1.75 -2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 73 "/Sensor_Controller/RTC_INT") (pinfunction "PIO0_10/ADC_7") (pintype "tri_state") (tstamp 718fa5f6-68ec-4871-b5fb-3d878002568e))
    (pad "10" smd roundrect (at -1.25 -2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 63 "/Sensor_Controller/CAPT_YH") (pinfunction "PIO0_21/ACMP_I5") (pintype "tri_state") (tstamp c77dca70-51fe-4501-8a1b-d52e7a0f4494))
    (pad "11" smd roundrect (at -0.75 -2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 63 "/Sensor_Controller/CAPT_YH") (pinfunction "PIO0_29") (pintype "tri_state") (tstamp 17bc7786-adb4-4c8f-a72f-3b2580483235))
    (pad "12" smd roundrect (at -0.25 -2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 74 "/Sensor_Controller/CAPT_YL") (pinfunction "PIO0_28") (pintype "tri_state") (tstamp ea8cc298-006a-4cce-a6db-da84a05c12c9))
    (pad "13" smd roundrect (at 0.25 -2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 57 "/Sensor_Controller/CAPT_X4") (pinfunction "PIO0_27") (pintype "tri_state") (tstamp edae1377-8be7-43ca-b978-0191d68d7646))
    (pad "14" smd roundrect (at 0.75 -2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 54 "/Sensor_Controller/CAPT_X3") (pinfunction "PIO0_26") (pintype "tri_state") (tstamp 58809354-3508-40ed-a59e-3d84eaadc50e))
    (pad "15" smd roundrect (at 1.25 -2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 51 "/Sensor_Controller/CAPT_X2") (pinfunction "PIO0_20") (pintype "tri_state") (tstamp 66aea0da-01bd-4c71-843a-efab9ffc2410))
    (pad "16" smd roundrect (at 1.75 -2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 48 "/Sensor_Controller/CAPT_X1") (pinfunction "PIO0_15/ADC_8") (pintype "tri_state") (tstamp 27bc1461-5044-4d22-bc07-9b28fd61c7d0))
    (pad "17" smd roundrect (at 2.45 -1.75 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "/Sensor_Controller/CAPT_X0") (pinfunction "PIO0_1/ADC_0/ACMP_I2/TDI/CLKIN") (pintype "tri_state") (tstamp cd6b32e8-4005-4172-affa-bded613733b9))
    (pad "18" smd roundrect (at 2.45 -1.25 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 66 "/Sensor_Controller/LSM_INT2") (pinfunction "PIO0_9/ADC_4") (pintype "tri_state") (tstamp 4819db47-20fc-400d-ad88-2414d80ecaf8))
    (pad "19" smd roundrect (at 2.45 -0.75 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 65 "/Sensor_Controller/LSM_INT1") (pinfunction "PIO0_8/ADC_5") (pintype "tri_state") (tstamp 4eeb82c6-cf0e-4e50-887c-feb1b9da3349))
    (pad "20" smd roundrect (at 2.45 -0.25 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pinfunction "VDD") (pintype "power_in") (tstamp a6e50901-1d09-433f-a9ad-9187b741384a))
    (pad "21" smd roundrect (at 2.45 0.25 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 75 "/Power_Management/DCDC_EN") (pinfunction "PIO0_30") (pintype "tri_state") (tstamp a4b30c23-38df-41b0-9740-0be1a1fc9ee9))
    (pad "22" smd roundrect (at 2.45 0.75 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(C10-Pad1)") (pinfunction "PIO0_7/ADC_1/ACMPVREF") (pintype "tri_state") (tstamp 60c7a89f-cf38-4767-93ca-13362366ed3a))
    (pad "23" smd roundrect (at 2.45 1.25 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(C10-Pad1)") (pinfunction "VREFP") (pintype "power_in") (tstamp 86651daa-9530-4f84-8536-fcd5cdf84a1a))
    (pad "24" smd roundrect (at 2.45 1.75 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "/Power_Management/CHG_~{STBY}") (pinfunction "PIO0_0/ACMP_I1/TDO") (pintype "tri_state") (tstamp c50decdc-0569-428e-a532-0a06e3edd122))
    (pad "25" smd roundrect (at 1.75 2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 59 "/Power_Management/ADC_BAT") (pinfunction "PIO0_14/ADC_2/ACMP_I3") (pintype "tri_state") (tstamp 43f3ddd7-77ae-4ec0-ab1b-4b7e7aa8d056))
    (pad "26" smd roundrect (at 1.25 2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "/Power_Management/CHG_~{ACT}") (pinfunction "PIO0_19/DACOUT") (pintype "tri_state") (tstamp a85f74c0-f145-4bdf-9318-01572a9240b3))
    (pad "27" smd roundrect (at 0.75 2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 42 "/Sensor_Controller/I2C_SCL") (pinfunction "PIO0_25") (pintype "tri_state") (tstamp 0b863510-fed8-4696-94d5-d6bedbbeae7f))
    (pad "28" smd roundrect (at 0.25 2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 41 "/Sensor_Controller/I2C_SDA") (pinfunction "PIO0_24") (pintype "tri_state") (tstamp 6b776a7f-fddb-4482-9082-d5c542156fcd))
    (pad "29" smd roundrect (at -0.25 2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 78 "/Sensor_Controller/SPI_~{INT}") (pinfunction "PIO0_23") (pintype "tri_state") (tstamp 725bae75-512b-4205-8aba-a3c823ba4659))
    (pad "30" smd roundrect (at -0.75 2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 38 "/WiFi_Display/EPD_SCLK") (pinfunction "PIO0_22") (pintype "tri_state") (tstamp 72e58744-fb03-4138-9888-78c8d3cc9b81))
    (pad "31" smd roundrect (at -1.25 2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 79 "/Sensor_Controller/SPI_MISO") (pinfunction "PIO0_18") (pintype "tri_state") (tstamp 4a33fbae-d00e-4009-b2a2-49ae2db7e6f1))
    (pad "32" smd roundrect (at -1.75 2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 39 "/WiFi_Display/EPD_SDI") (pinfunction "PIO0_16/ADC_3/ACMP_I4") (pintype "tri_state") (tstamp 9e70ee1d-70a7-4a49-b89e-4a504423242a))
    (pad "33" thru_hole circle (at -1.45 0 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp 27c498d3-09f5-48f9-aa73-eca266251f87))
    (pad "33" smd rect (at 0 0 180) (size 3.5 3.5) (layers "B.Cu" "B.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp 28942866-840e-4447-a963-f9e1c307fbdf))
    (pad "33" thru_hole circle (at 0 -1.45 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp 2e575a2c-e28a-49ad-b2bf-6a96341b4ed1))
    (pad "33" thru_hole circle (at 0 1.45 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp 56c97341-29cc-4f56-9f57-422930246679))
    (pad "33" thru_hole circle (at 1.45 1.45 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp 5da56b94-3ac9-45a4-a7b4-d2be9a1d223b))
    (pad "33" thru_hole circle (at 1.45 0 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp c7823fe5-4edd-426e-b800-bdd338366f6b))
    (pad "33" thru_hole circle (at 0 0 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp cb4c0074-52e4-4a3c-9ec3-922e622a6c2f))
    (pad "33" thru_hole circle (at 1.45 -1.45 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp e026c0d4-6b22-427c-96dc-93f8cc050d35))
    (pad "33" smd rect (at 0 0 180) (size 3.5 3.5) (layers "F.Cu")
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp e2e76162-0f63-4528-bfa2-706ecb55eb99))
    (pad "33" thru_hole circle (at -1.45 1.45 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp e2f297ce-9ff5-4269-ae98-d9c591935d44))
    (pad "33" thru_hole circle (at -1.45 -1.45 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp ee19ae5b-4deb-4e6c-81fb-516765cef346))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/VQFN-32-1EP_5x5mm_P0.5mm_EP3.5x3.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 8ef911c1-1720-4804-8f8e-c0032d72a0d7)
    (at 169.5 154)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/4cdd1cf5-2bc6-4e6b-9649-5f3bff87da65")
    (attr smd)
    (fp_text reference "R19" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a90f10c4-07e5-40ee-b1de-881f775eabc0)
    )
    (fp_text value "2.2k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a357ae2b-9549-447d-9118-b80e31c33e94)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp cc66ca54-6cd2-4e82-b2c9-2547963aa97d)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 0e0324c4-9bb1-422a-95ad-5c3d31056f25))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 45ed7c4e-17fd-4568-83a0-55fe5d72907d))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 36434f13-46ef-4352-83a2-b52ebed7c1b3))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 53b63f0b-f6c4-47ba-af74-cfd4fcb4078b))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp d4a4300c-f188-47e1-9eb5-2fa413ab5622))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp dbcd69a0-abca-4178-900f-bdc15a8d94a1))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 5718dccd-2ed9-431a-aa44-42c071741664))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 82b96e40-67f7-483f-b8a4-7c075346ffc0))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp f698c811-94fb-461c-8f24-4dcf481c755b))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp fb80273d-7bda-4964-b81f-f7b9663c3c6e))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 54 "/Sensor_Controller/CAPT_X3") (pintype "passive") (tstamp 75a9da9e-0e56-4cfb-ae0e-bbe4eda743eb))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(R19-Pad2)") (pintype "passive") (tstamp bb3f4d73-2e8f-4038-a821-4a21959c4c6d))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_JST:JST_PH_B2B-PH-SM4-TB_1x02-1MP_P2.00mm_Vertical" (layer "B.Cu")
    (tedit 5B78AD87) (tstamp 930fcce0-6fc7-4bf8-a6f1-facc121e11cd)
    (at 193.2 138.6 -90)
    (descr "JST PH series connector, B2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH side entry")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/5065d46b-5f7e-440b-b3b9-6db133d83adc")
    (attr smd)
    (fp_text reference "BT1" (at 0 5.45 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4557fea1-fd2e-4aad-a7b8-267bd7c89807)
    )
    (fp_text value "Li-Po 1000-2000mAh" (at 0 -4.45 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 71d75b93-64d5-4253-b6b8-2a1496b5d333)
    )
    (fp_text user "${REFERENCE}" (at 0 1 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0112e727-824f-49e0-9a40-e702d6de2702)
    )
    (fp_line (start -4.085 -0.01) (end -4.085 -0.86) (layer "B.SilkS") (width 0.12) (tstamp 08f8ba10-d63f-468f-b8e1-cb14a0252f5e))
    (fp_line (start -4.085 4.36) (end 4.085 4.36) (layer "B.SilkS") (width 0.12) (tstamp 22191cb3-b2e0-4c39-9bdb-61eafbca46c7))
    (fp_line (start -4.085 -0.86) (end -1.76 -0.86) (layer "B.SilkS") (width 0.12) (tstamp 222e4d92-dc30-4f90-8a22-05f95edb1705))
    (fp_line (start 4.085 -0.01) (end 4.085 -0.86) (layer "B.SilkS") (width 0.12) (tstamp 29cd335a-6498-4b47-9f15-418b3ec2b96a))
    (fp_line (start 4.085 -0.86) (end 1.76 -0.86) (layer "B.SilkS") (width 0.12) (tstamp 2d6741bb-9af6-4c69-9e33-e533b4bb840e))
    (fp_line (start -4.085 3.51) (end -4.085 4.36) (layer "B.SilkS") (width 0.12) (tstamp 74682856-e109-4255-9b5f-957def300e18))
    (fp_line (start -1.76 -0.86) (end -1.76 -3.25) (layer "B.SilkS") (width 0.12) (tstamp 92be2371-21e6-4c97-8d62-fba82729df07))
    (fp_line (start 4.085 4.36) (end 4.085 3.51) (layer "B.SilkS") (width 0.12) (tstamp c6d6cf19-49d2-4c73-ba8b-833e4153581a))
    (fp_line (start -4.7 4.75) (end -4.7 -3.75) (layer "B.CrtYd") (width 0.05) (tstamp 0d0429e1-7734-426e-9078-4fa78512a0e7))
    (fp_line (start 4.7 4.75) (end -4.7 4.75) (layer "B.CrtYd") (width 0.05) (tstamp 35929fdb-cb3b-465e-93b5-f51df2dab10a))
    (fp_line (start 4.7 -3.75) (end 4.7 4.75) (layer "B.CrtYd") (width 0.05) (tstamp 5c24bbf4-6a9a-4b3f-ae0b-be7b6b99c1fb))
    (fp_line (start -4.7 -3.75) (end 4.7 -3.75) (layer "B.CrtYd") (width 0.05) (tstamp 8bff54a6-e951-4823-888c-8ff6dc803c5a))
    (fp_line (start -3.975 -0.75) (end -3.975 4.25) (layer "B.Fab") (width 0.1) (tstamp 15d776e6-0f79-4e3d-a1fc-1dd65697d6fa))
    (fp_line (start 0.75 2.75) (end 0.75 2.25) (layer "B.Fab") (width 0.1) (tstamp 1a25c20c-753f-472b-baff-d0729e88958f))
    (fp_line (start -3.975 -0.75) (end 3.975 -0.75) (layer "B.Fab") (width 0.1) (tstamp 1c5ed236-9011-4611-8680-0c3053caf3f6))
    (fp_line (start 1.25 2.25) (end 1.25 2.75) (layer "B.Fab") (width 0.1) (tstamp 25265eb2-9016-4950-a98f-4f7ffc33b7e0))
    (fp_line (start 3.975 -0.75) (end 3.975 4.25) (layer "B.Fab") (width 0.1) (tstamp 29c99fb1-f1a1-4ffc-99b1-e358a7d0a022))
    (fp_line (start -3.975 4.25) (end 3.975 4.25) (layer "B.Fab") (width 0.1) (tstamp 329cad0e-d28d-48c8-b974-78afbee64345))
    (fp_line (start -0.75 2.25) (end -0.75 2.75) (layer "B.Fab") (width 0.1) (tstamp 41851ac6-9e89-49c7-8276-842f9887a962))
    (fp_line (start -1.25 2.25) (end -0.75 2.25) (layer "B.Fab") (width 0.1) (tstamp 5ebe6b9f-8a90-4ccb-9577-e2812079b31c))
    (fp_line (start -0.75 2.75) (end -1.25 2.75) (layer "B.Fab") (width 0.1) (tstamp 6e53eed8-ab8a-4d38-a25a-f5d45c1b8afe))
    (fp_line (start 1.25 2.75) (end 0.75 2.75) (layer "B.Fab") (width 0.1) (tstamp 807c9bfa-f5c6-44f2-9fd3-13c350559ed2))
    (fp_line (start 0.75 2.25) (end 1.25 2.25) (layer "B.Fab") (width 0.1) (tstamp 811fc315-1729-455d-a206-8970e026fc4f))
    (fp_line (start -1 -0.042893) (end -0.5 -0.75) (layer "B.Fab") (width 0.1) (tstamp 82790e35-40a0-4535-9c90-301047013a68))
    (fp_line (start -1.25 2.75) (end -1.25 2.25) (layer "B.Fab") (width 0.1) (tstamp a9ecc861-373a-45c3-b907-2a56133fc9b3))
    (fp_line (start -1.5 -0.75) (end -1 -0.042893) (layer "B.Fab") (width 0.1) (tstamp cccea3e8-ab49-4b6d-b090-0022fc55c2af))
    (pad "1" smd roundrect (at -1 -0.5 270) (size 1 5.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 103 "Net-(BT1-Pad1)") (pinfunction "+") (pintype "passive") (tstamp 9e91f664-7223-4008-9717-4e3689f95dfc))
    (pad "2" smd roundrect (at 1 -0.5 270) (size 1 5.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "-") (pintype "passive") (tstamp cc6be4bc-28c0-4417-8da5-f265464b4484))
    (pad "MP" smd roundrect (at -3.4 1.75 270) (size 1.6 3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.15625) (tstamp 1133215f-620e-4913-95aa-e2529f5aa6b7))
    (pad "MP" smd roundrect (at 3.4 1.75 270) (size 1.6 3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.15625) (tstamp afbfa340-b350-4156-a9c7-08e55a3aa2fb))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_B2B-PH-SM4-TB_1x02-1MP_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 9b6cc922-a122-4c01-9443-bbdb32494d75)
    (at 127.5 154 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/77551999-4e6f-40be-807f-b54e7caa6297")
    (attr smd)
    (fp_text reference "R11" (at 0 -1.2) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 30141ae9-9c00-4fb9-b8d2-564d06112160)
    )
    (fp_text value "2.2k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 070b98c6-e821-49b7-ad2f-3a80e510a5f4)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp ecb3987a-4598-4873-aadd-ffcccac3f6d6)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 4b677dd3-1f4f-45f7-b3ba-30614b34fc1a))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp a3b59683-6558-4b2a-b676-96c90134ced4))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 1639d553-01fd-44d6-986c-ae8cbad1c6fb))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 4db1f014-8fce-4776-bb8f-29942e802774))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 7255e838-4065-475b-a781-bed8a0a56479))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 927bbdc9-2e59-4b10-9d50-6f4a18c9ba43))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp d1ec9174-1047-4198-bd53-d700926641a8))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp e08c4572-558f-4a24-b09a-857d914da1b2))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp e52aecdb-9f80-4d60-932b-23e752714d73))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp e65e1c99-cc43-4268-87fe-d67051a0fd2b))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 47 "Net-(R11-Pad1)") (pintype "passive") (tstamp d632f4ff-b47f-43d3-9359-ad6bf91be9cd))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(R10-Pad2)") (pintype "passive") (tstamp 4f7ed4af-60d4-4a30-8226-a2362e4048bd))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 9becb878-ef3d-4619-9b23-f622900f60fe)
    (at 174.9 128.9)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/c7529554-fb1b-436d-8376-0e1625341df0")
    (attr smd)
    (fp_text reference "C27" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 20d6da1d-577e-436d-a368-d51b990ccd1b)
    )
    (fp_text value "1uF/50V" (at 0 -1.93) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 23550477-115c-4637-a099-11311bfa30f9)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 3f131a9c-e592-49c4-88a8-3485f89e087e)
    )
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp 8617bc90-d39e-48cf-b7f3-54edf5c42dce))
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp a25620d1-8b35-4eb3-b2e7-65a938da6398))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 03a72157-a183-4a09-b582-1f3ff0110a96))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 2dd0df51-04af-4a8f-a20c-e0b96f6b822e))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp b0d5aecc-9dce-45b9-8a47-283124bcb7a3))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp dc77433c-904b-4874-89fd-74097aceb019))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 6e3a9079-b001-41a0-98b2-9b13d8b4c969))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 71d405ce-9c8a-4930-987b-f5151bc045d6))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 8719e39d-50bb-4d36-b596-ffd771f68842))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 8733df1d-4dfc-4dfe-9745-aa73cfd503ee))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 5f19aa1d-4005-4978-8b13-75236fdaa706))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(C27-Pad2)") (pintype "passive") (tstamp fd878961-2968-4646-adbe-0428c970fcfd))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 9fc61cda-71fb-47cf-bc26-abdb8ef0df6b)
    (at 154.6 133 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/137e690e-b61b-45c0-892e-e0c090818fe7")
    (attr smd)
    (fp_text reference "R2" (at 0 1.17 -270) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 338edc16-2ec8-4d79-9e78-eabd22957b10)
    )
    (fp_text value "4k7" (at 0 -1.17 -270) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 6e0e8737-a373-4be2-828f-1ab0c8f0d0f6)
    )
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 7dc055c1-ace0-4333-8fd7-f2a1d47ddf2d)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 052ca3e4-eae4-4fe6-9b53-f14d3283a085))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp e2f661d3-be51-4a35-ac6f-350d09fc0632))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 14abcc7d-f443-462d-8b98-463a28674fbf))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 2ffd4aaa-809c-48d6-a9cc-46e32c856318))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 3a18cc49-3d53-4786-bddf-cefee90b1b3c))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 68d19009-93e4-40e6-8f82-bbed402c3f24))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 4aabc145-70b2-452e-b551-64526e47fc8d))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 4c848b74-6f4a-4077-88fc-7fa36810aa3d))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp c812c830-0235-476d-bcb8-f4befa86a26a))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp e073dd7f-c811-478e-934d-75059605b0ba))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp a92192dd-b6a0-4632-8d84-e079276d1d31))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 41 "/Sensor_Controller/I2C_SDA") (pintype "passive") (tstamp 8106362f-b6a2-44f6-95c0-801e9ea94a6b))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_LGA:Bosch_LGA-8_2.5x2.5mm_P0.65mm_ClockwisePinNumbering" (layer "B.Cu")
    (tedit 5A0FA816) (tstamp 9fdfe07f-e16c-4e3e-bade-7f7e07316c4f)
    (at 127.9 139.8 180)
    (descr "LGA-8")
    (tags "lga land grid array")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/e686e57b-c43c-476c-b407-df572672ff85")
    (attr smd)
    (fp_text reference "U2" (at 0.015 2.465) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 1735f0dc-8fbb-45b6-83fa-c61e50b8f9a6)
    )
    (fp_text value "BME280" (at 0.015 -2.535) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 3031a0f7-e197-4fc6-bff1-5f0e2e0fe5db)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
      (tstamp 70cfbc53-845b-4e66-8b72-ecfab87e62b5)
    )
    (fp_line (start 1.35 -1.35) (end 1.35 -1.2) (layer "B.SilkS") (width 0.1) (tstamp 023db6ba-a1c3-49a5-8ac8-1460c670a066))
    (fp_line (start -1.35 -1.36) (end -1.2 -1.36) (layer "B.SilkS") (width 0.1) (tstamp 4dbbed8f-686a-4913-95d6-65280cded19a))
    (fp_line (start 1.35 -1.35) (end 1.2 -1.35) (layer "B.SilkS") (width 0.1) (tstamp 633df951-8c96-46f8-8f2d-42d58fda6ad5))
    (fp_line (start -1.35 -1.35) (end -1.35 -1.2) (layer "B.SilkS") (width 0.1) (tstamp 90f012bf-c1e7-4c83-af4a-6e77d0860faf))
    (fp_line (start 1.35 1.35) (end 1.35 1.2) (layer "B.SilkS") (width 0.1) (tstamp 929102ee-ecc3-4f5c-9d0b-435055047197))
    (fp_line (start 1.2 1.35) (end 1.35 1.35) (layer "B.SilkS") (width 0.1) (tstamp b78f4b2a-e94b-4200-8f5e-9fcc887a219d))
    (fp_line (start -1.35 1.2) (end -1.35 1.45) (layer "B.SilkS") (width 0.1) (tstamp c9b986ad-00c7-4718-b31d-8c003b17428f))
    (fp_line (start 1.41 -1.54) (end -1.41 -1.54) (layer "B.CrtYd") (width 0.05) (tstamp 107e39cb-16e0-4954-bcd3-8df3250ea398))
    (fp_line (start -1.41 -1.54) (end -1.41 1.54) (layer "B.CrtYd") (width 0.05) (tstamp 3b3f988a-6e80-4650-bac3-5bd97bfc41bd))
    (fp_line (start -1.41 1.54) (end 1.41 1.54) (layer "B.CrtYd") (width 0.05) (tstamp 4a71624e-cb7d-4123-ac22-6eb65fbcc371))
    (fp_line (start 1.41 1.54) (end 1.41 -1.54) (layer "B.CrtYd") (width 0.05) (tstamp 6941e982-ba9f-4892-b9d9-70f802acf8bf))
    (fp_line (start -1.25 0.5) (end -0.5 1.25) (layer "B.Fab") (width 0.1) (tstamp 01ccdcfb-4524-4845-9cfc-271852b93dfd))
    (fp_line (start 1.25 -1.25) (end -1.25 -1.25) (layer "B.Fab") (width 0.1) (tstamp 0ebfbe5e-bbec-4c7e-9fad-b578931fc372))
    (fp_line (start -1.25 -1.25) (end -1.25 0.5) (layer "B.Fab") (width 0.1) (tstamp 157167a0-592d-4872-b915-a643151b29ed))
    (fp_line (start -0.5 1.25) (end 1.25 1.25) (layer "B.Fab") (width 0.1) (tstamp dba90a98-b79c-43f9-a5c7-aa9f81e8729b))
    (fp_line (start 1.25 1.25) (end 1.25 -1.25) (layer "B.Fab") (width 0.1) (tstamp df17960c-3eae-4594-9c53-cc593181af82))
    (pad "1" smd rect (at -0.975 1.025 90) (size 0.5 0.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 16ac23ed-6ef2-41cc-953d-db115806a0e6))
    (pad "2" smd rect (at -0.325 1.025 90) (size 0.5 0.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "VDDF") (pinfunction "CSB") (pintype "input") (tstamp 27766c82-d132-4fec-a370-69da8457535a))
    (pad "3" smd rect (at 0.325 1.025 90) (size 0.5 0.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 41 "/Sensor_Controller/I2C_SDA") (pinfunction "SDI") (pintype "bidirectional") (tstamp 719c6679-3f8e-4db3-9ff2-270e3727f3c5))
    (pad "4" smd rect (at 0.975 1.025 90) (size 0.5 0.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 42 "/Sensor_Controller/I2C_SCL") (pinfunction "SCK") (pintype "input") (tstamp da848b1a-0e2d-4d5e-bade-3f5a03aa8d0f))
    (pad "5" smd rect (at 0.975 -1.025 90) (size 0.5 0.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "SDO") (pintype "bidirectional") (tstamp 36893633-982e-4401-ac2d-d6de11b53ec9))
    (pad "6" smd rect (at 0.325 -1.025 90) (size 0.5 0.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "VDDF") (pinfunction "VDDIO") (pintype "power_in") (tstamp 74901deb-88dc-45ad-8810-f5c6c327a334))
    (pad "7" smd rect (at -0.325 -1.025 90) (size 0.5 0.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 7b5fd1b1-844a-4e03-9554-cefb5f2c3782))
    (pad "8" smd rect (at -0.975 -1.025 90) (size 0.5 0.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "VDDF") (pinfunction "VDD") (pintype "power_in") (tstamp 9aca941e-8122-431e-ae0c-2425446d4ff3))
    (model "${KICAD6_3DMODEL_DIR}/Package_LGA.3dshapes/Bosch_LGA-8_2.5x2.5mm_P0.65mm_ClockwisePinNumbering.wrl"
      (offset (xyz 0.01500000025 -0.03500000059 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical_SMD" (layer "B.Cu")
    (tedit 59FED6E3) (tstamp a1bb3317-b16d-495e-91c3-219519108e5e)
    (at 116.9 123.1)
    (descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x05 1.27mm double row")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/d5ff02e9-b34c-4646-bb15-bf1695940209")
    (attr smd)
    (fp_text reference "J1" (at 0 4.235) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 256da29a-83e1-4192-8627-7b15c8bdc30c)
    )
    (fp_text value "Conn_02x05_Odd_Even" (at 0 -4.235) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 6d64b09d-0dfd-4a35-8b7e-3a5672be487b)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 9a5d72d3-41af-4cd7-897d-5d21e0585242)
    )
    (fp_line (start -1.765 -3.235) (end 1.765 -3.235) (layer "B.SilkS") (width 0.12) (tstamp 241fc6cd-adf3-4ef3-955f-65f983f27c81))
    (fp_line (start -1.765 3.235) (end -1.765 3.17) (layer "B.SilkS") (width 0.12) (tstamp 6e456bde-52d5-4145-a936-eb6fc0c9ea46))
    (fp_line (start -1.765 3.235) (end 1.765 3.235) (layer "B.SilkS") (width 0.12) (tstamp 8515203a-c19b-47d3-8197-0f24a236b636))
    (fp_line (start -3.09 3.17) (end -1.765 3.17) (layer "B.SilkS") (width 0.12) (tstamp a5d3355e-0247-4c34-a686-4c2ca8db2292))
    (fp_line (start -1.765 -3.17) (end -1.765 -3.235) (layer "B.SilkS") (width 0.12) (tstamp c7594c9d-4fbf-46c0-97b5-506ed456a419))
    (fp_line (start 1.765 -3.17) (end 1.765 -3.235) (layer "B.SilkS") (width 0.12) (tstamp da747909-ce6d-4ae0-80fa-724f0e494e72))
    (fp_line (start 1.765 3.235) (end 1.765 3.17) (layer "B.SilkS") (width 0.12) (tstamp f1e6a886-7b32-481a-bbfc-f668916f264c))
    (fp_line (start 4.3 3.7) (end -4.3 3.7) (layer "B.CrtYd") (width 0.05) (tstamp 31ddf1c5-8bd5-4213-b7c9-438dcf803146))
    (fp_line (start -4.3 -3.7) (end 4.3 -3.7) (layer "B.CrtYd") (width 0.05) (tstamp 4890fbba-5bd1-469a-90ea-a2b004b2be78))
    (fp_line (start 4.3 -3.7) (end 4.3 3.7) (layer "B.CrtYd") (width 0.05) (tstamp 8062717d-7552-4634-aaa1-f303f085c257))
    (fp_line (start -4.3 3.7) (end -4.3 -3.7) (layer "B.CrtYd") (width 0.05) (tstamp db5fae20-df74-4e62-b61a-98f365c2e7fe))
    (fp_line (start 1.705 -3.175) (end -1.705 -3.175) (layer "B.Fab") (width 0.1) (tstamp 06eb3590-5fa1-486b-8a49-0bad7e726cdd))
    (fp_line (start -2.75 0.2) (end -2.75 -0.2) (layer "B.Fab") (width 0.1) (tstamp 234df8d9-2ed5-4c60-9752-b7276ce9678d))
    (fp_line (start -1.705 1.47) (end -2.75 1.47) (layer "B.Fab") (width 0.1) (tstamp 309903aa-4411-4ca4-b9f5-75fbe3d0cd71))
    (fp_line (start 1.705 -2.34) (end 2.75 -2.34) (layer "B.Fab") (width 0.1) (tstamp 356aa333-3067-4f82-a36f-144123ef5833))
    (fp_line (start -2.75 2.74) (end -2.75 2.34) (layer "B.Fab") (width 0.1) (tstamp 40d3b5b1-0d9d-4290-af84-d7378f30b220))
    (fp_line (start -2.75 -0.2) (end -1.705 -0.2) (layer "B.Fab") (width 0.1) (tstamp 52c39cf7-9421-4b49-b359-dc5e409624cd))
    (fp_line (start 2.75 1.07) (end 1.705 1.07) (layer "B.Fab") (width 0.1) (tstamp 5d46253b-0b50-4329-9abf-132692c6cf0f))
    (fp_line (start -2.75 -1.47) (end -1.705 -1.47) (layer "B.Fab") (width 0.1) (tstamp 5f92b6ae-11fc-4b6a-8645-74415f553b4c))
    (fp_line (start 1.705 0.2) (end 2.75 0.2) (layer "B.Fab") (width 0.1) (tstamp 61b3f364-0bca-4c53-9945-2792515a445e))
    (fp_line (start -2.75 1.07) (end -1.705 1.07) (layer "B.Fab") (width 0.1) (tstamp 66e1b670-432a-4975-8302-aee6a9e44bf9))
    (fp_line (start 1.705 3.175) (end 1.705 -3.175) (layer "B.Fab") (width 0.1) (tstamp 6c71a5df-b30a-4824-8006-e81e5e97b857))
    (fp_line (start -1.27 3.175) (end 1.705 3.175) (layer "B.Fab") (width 0.1) (tstamp 70ed67df-9eda-4d18-a231-e4aa81a665c1))
    (fp_line (start 2.75 -0.2) (end 1.705 -0.2) (layer "B.Fab") (width 0.1) (tstamp 74493079-1000-4bf7-a893-9301fd73c9d9))
    (fp_line (start 2.75 -1.47) (end 1.705 -1.47) (layer "B.Fab") (width 0.1) (tstamp 776917fe-62a0-484d-b928-4055ced2ac90))
    (fp_line (start 2.75 -2.74) (end 1.705 -2.74) (layer "B.Fab") (width 0.1) (tstamp 79a96bd2-adba-40b8-bd4f-100a61f1f50e))
    (fp_line (start 1.705 1.47) (end 2.75 1.47) (layer "B.Fab") (width 0.1) (tstamp 7bd310c5-b6ed-4ad1-bd5b-b475825a4947))
    (fp_line (start -1.705 2.74) (end -1.27 3.175) (layer "B.Fab") (width 0.1) (tstamp 8145c8bb-ea6f-408a-89ef-da8a99e84090))
    (fp_line (start -1.705 -2.34) (end -2.75 -2.34) (layer "B.Fab") (width 0.1) (tstamp 91b384dd-5f28-464e-b640-37097fad3d4f))
    (fp_line (start 2.75 -1.07) (end 2.75 -1.47) (layer "B.Fab") (width 0.1) (tstamp 92d17004-8f0f-4437-959e-aea791efa5d5))
    (fp_line (start 2.75 -2.34) (end 2.75 -2.74) (layer "B.Fab") (width 0.1) (tstamp 97023a0d-6da9-431a-a4de-08f59e0646e1))
    (fp_line (start -1.705 -3.175) (end -1.705 2.74) (layer "B.Fab") (width 0.1) (tstamp 9ec8979b-383e-4012-b0a8-a197d46dba71))
    (fp_line (start 1.705 -1.07) (end 2.75 -1.07) (layer "B.Fab") (width 0.1) (tstamp aa88c50b-9bf0-4d9e-a265-8a4daabd70aa))
    (fp_line (start 2.75 2.74) (end 2.75 2.34) (layer "B.Fab") (width 0.1) (tstamp ae637d19-ae9c-486c-be46-9762a736e77e))
    (fp_line (start -2.75 2.34) (end -1.705 2.34) (layer "B.Fab") (width 0.1) (tstamp b15287f7-ce5f-42ce-9495-2b51379f2698))
    (fp_line (start -2.75 1.47) (end -2.75 1.07) (layer "B.Fab") (width 0.1) (tstamp ba44e59f-fee4-4cd7-aae3-ee2237360d10))
    (fp_line (start -1.705 -1.07) (end -2.75 -1.07) (layer "B.Fab") (width 0.1) (tstamp bcb6aea3-dc8c-447b-8874-dc05037dedba))
    (fp_line (start 2.75 1.47) (end 2.75 1.07) (layer "B.Fab") (width 0.1) (tstamp c28d2a67-906d-466c-962a-ae27f3f5269d))
    (fp_line (start 2.75 0.2) (end 2.75 -0.2) (layer "B.Fab") (width 0.1) (tstamp d53f060a-61a9-4462-a1a2-6bdc06bfec00))
    (fp_line (start -1.705 0.2) (end -2.75 0.2) (layer "B.Fab") (width 0.1) (tstamp ef90ccd3-c683-4981-97be-fce66c169c45))
    (fp_line (start -1.705 2.74) (end -2.75 2.74) (layer "B.Fab") (width 0.1) (tstamp f316167a-74ae-414e-8058-816ced75cf20))
    (fp_line (start 2.75 2.34) (end 1.705 2.34) (layer "B.Fab") (width 0.1) (tstamp f32efb9a-0057-4100-8b1b-7d0a211e2fa2))
    (fp_line (start -2.75 -2.74) (end -1.705 -2.74) (layer "B.Fab") (width 0.1) (tstamp f3337f69-290b-4abe-acec-b255ec312c2c))
    (fp_line (start 1.705 2.74) (end 2.75 2.74) (layer "B.Fab") (width 0.1) (tstamp f434dad9-059c-4e8b-ab00-1fea3512e9b5))
    (fp_line (start -2.75 -2.34) (end -2.75 -2.74) (layer "B.Fab") (width 0.1) (tstamp f61b25bf-560f-4fc3-97fc-370fec898f5a))
    (fp_line (start -2.75 -1.07) (end -2.75 -1.47) (layer "B.Fab") (width 0.1) (tstamp fa3b63e3-3bb6-441d-9e65-7c92584435d7))
    (pad "1" smd rect (at -1.95 2.54) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "VDDF") (pinfunction "Pin_1") (pintype "passive") (tstamp 39321b80-f8d2-4fc2-9206-0b8cfe47530a))
    (pad "2" smd rect (at 1.95 2.54) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 43 "/Sensor_Controller/LPC_SWDIO") (pinfunction "Pin_2") (pintype "passive") (tstamp 47022f3b-bc70-46f5-8e63-23533616b3e4))
    (pad "3" smd rect (at -1.95 1.27) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive") (tstamp 762037a1-880e-4f8d-95ef-bf65edab381a))
    (pad "4" smd rect (at 1.95 1.27) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 44 "/Sensor_Controller/LPC_SWCLK") (pinfunction "Pin_4") (pintype "passive") (tstamp 18d28863-9273-4508-81a8-5aefbf9962d0))
    (pad "5" smd rect (at -1.95 0) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Pin_5") (pintype "passive") (tstamp 4cb6b8d3-02f3-46c9-9aa8-74327bddd986))
    (pad "6" smd rect (at 1.95 0) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 104 "unconnected-(J1-Pad6)") (pinfunction "Pin_6") (pintype "passive+no_connect") (tstamp 979512d8-cd76-4c28-add8-42cd3094bb70))
    (pad "7" smd rect (at -1.95 -1.27) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 105 "unconnected-(J1-Pad7)") (pinfunction "Pin_7") (pintype "passive+no_connect") (tstamp 85193aea-ae77-45f0-92e7-ac2eff0eeb7d))
    (pad "8" smd rect (at 1.95 -1.27) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 106 "unconnected-(J1-Pad8)") (pinfunction "Pin_8") (pintype "passive+no_connect") (tstamp 6371f893-89cf-4e7a-913b-3dc95b6ad9a9))
    (pad "9" smd rect (at -1.95 -2.54) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Pin_9") (pintype "passive") (tstamp bfa4e90a-6fcf-4d7e-acbe-87c5273076f9))
    (pad "10" smd rect (at 1.95 -2.54) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "/Sensor_Controller/LPC_~{RST}") (pinfunction "Pin_10") (pintype "passive") (tstamp a738a243-6f85-4732-bc0c-761a0f7794bb))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical_SMD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "KiCAD_Mods:Connector_FPC_FFC_JS_AFC07-S24ECA-00" (layer "B.Cu")
    (tedit 60028AE1) (tstamp a7809bd2-2991-4911-98e9-a5d4b79b7761)
    (at 178.425 124.65 -90)
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/3a1a01f4-238a-4b56-a295-7725401edea8")
    (attr smd)
    (fp_text reference "J4" (at 0 -1.8 -270) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f74f86b1-b7c5-4d6e-b63f-f2c1aa50eb19)
    )
    (fp_text value "AFC07-S24ECA-00" (at 0 -4.9 -270) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5356db46-9624-4ffc-a0ab-b525257511e2)
    )
    (fp_text user "1" (at 7.5 0.15 -270) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f2e0ee48-89ba-41d6-aaff-fe246dd6fba9)
    )
    (fp_line (start -6 0.83) (end 6 0.83) (layer "B.SilkS") (width 0.12) (tstamp 025cb963-110b-42a9-bf59-81b0d381a587))
    (fp_line (start -8.76 -3.97) (end -8.76 -0.61) (layer "B.SilkS") (width 0.12) (tstamp 032fcc36-4046-4e0c-b48e-41ca81fff7b0))
    (fp_line (start -6 -0.83) (end -6 -3.97) (layer "B.SilkS") (width 0.12) (tstamp 0c3d915e-2d65-4232-9fc5-d6654103c05f))
    (fp_line (start 6 -0.61) (end 6 0.83) (layer "B.SilkS") (width 0.12) (tstamp 3c5eb6e0-e290-4d64-bafe-0b25f3ec8eaa))
    (fp_line (start 8.76 -3.97) (end 8.76 -0.61) (layer "B.SilkS") (width 0.12) (tstamp 50610d67-636c-442a-bbd0-d92b0be12b60))
    (fp_line (start -8.76 -0.61) (end -6 -0.61) (layer "B.SilkS") (width 0.12) (tstamp 67f66976-b98a-45f6-bede-42f032a54862))
    (fp_line (start -6 -3.97) (end -8.76 -3.97) (layer "B.SilkS") (width 0.12) (tstamp 7190449d-e958-40d1-af0b-9e4d50e3db42))
    (fp_line (start 6 -3.97) (end 8.76 -3.97) (layer "B.SilkS") (width 0.12) (tstamp a79e90f6-7851-4ac0-80d8-160004bcc08e))
    (fp_line (start -6 -0.83) (end 6 -0.83) (layer "B.SilkS") (width 0.12) (tstamp b9ef4c0e-99f9-4688-bba4-0630e7171bec))
    (fp_line (start -6 -0.61) (end -6 0.83) (layer "B.SilkS") (width 0.12) (tstamp c6d36843-190c-4170-9d7d-a000ff22db8f))
    (fp_line (start 6 -0.83) (end 6 -3.97) (layer "B.SilkS") (width 0.12) (tstamp cb7f21a9-7edc-419d-a575-716d31a2076e))
    (fp_line (start 8.76 -0.61) (end 6 -0.61) (layer "B.SilkS") (width 0.12) (tstamp fd9c701c-1915-4e5e-b8a0-7ee8d4480d01))
    (fp_poly (pts
        (xy 6.6 -0.6)
        (xy 6 -0.6)
        (xy 6 0)
      ) (layer "B.SilkS") (width 0.1) (fill solid) (tstamp e9b5d04e-4223-4b25-868d-e10038e00748))
    (fp_line (start 9 1.05) (end 9 -4.2) (layer "B.CrtYd") (width 0.05) (tstamp 64d7488c-adc3-4c77-a4da-ce84cbf14188))
    (fp_line (start -9 -4.2) (end 9 -4.2) (layer "B.CrtYd") (width 0.05) (tstamp 808f0c2a-1abd-462a-8a95-d01a31c44532))
    (fp_line (start -9 1.05) (end 9 1.05) (layer "B.CrtYd") (width 0.05) (tstamp 8867963c-2e90-42e2-bc5f-f4076d85b975))
    (fp_line (start -9 1.05) (end -9 -4.2) (layer "B.CrtYd") (width 0.05) (tstamp ae770fd8-be83-47eb-ac60-0c0e3e9a23aa))
    (pad "1" smd rect (at 5.75 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "unconnected-(J4-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect") (tstamp bdf9ebea-bbb7-4637-955f-dd15c4b20e8d))
    (pad "2" smd rect (at 5.25 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 30 "/WiFi_Display/GDR") (pinfunction "Pin_2") (pintype "passive") (tstamp 237d3841-5d1f-465d-97c8-57de4d21ad20))
    (pad "3" smd rect (at 4.75 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 31 "/WiFi_Display/RESE") (pinfunction "Pin_3") (pintype "passive") (tstamp f18622d4-98c4-475e-8ec7-40e52c4b178a))
    (pad "4" smd rect (at 4.25 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "Net-(C23-Pad2)") (pinfunction "Pin_4") (pintype "passive") (tstamp cf3cf7d4-071e-4621-8f34-dc3e515688b7))
    (pad "5" smd rect (at 3.75 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "Net-(C27-Pad2)") (pinfunction "Pin_5") (pintype "passive") (tstamp f70b5b4b-1f8c-4c6f-9538-574ab420dba6))
    (pad "6" smd rect (at 3.25 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 32 "unconnected-(J4-Pad6)") (pinfunction "Pin_6") (pintype "passive+no_connect") (tstamp 278f916e-4447-44d1-b865-885e99cf15d0))
    (pad "7" smd rect (at 2.75 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "unconnected-(J4-Pad7)") (pinfunction "Pin_7") (pintype "passive+no_connect") (tstamp 8e5c3ace-092b-42e5-9047-8eed0daec53f))
    (pad "8" smd rect (at 2.25 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Pin_8") (pintype "passive") (tstamp d8d7f49b-1b23-437e-8249-f58773828103))
    (pad "9" smd rect (at 1.75 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 34 "/WiFi_Display/EPD_BUSY") (pinfunction "Pin_9") (pintype "passive") (tstamp 700055f7-359e-46f8-a89b-f3896e2b5dbc))
    (pad "10" smd rect (at 1.25 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "/WiFi_Display/EPD_~{RES}") (pinfunction "Pin_10") (pintype "passive") (tstamp 0e152cf3-24c0-466e-b9db-95d4426e6de7))
    (pad "11" smd rect (at 0.75 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "/WiFi_Display/EPD_D{slash}~{C}") (pinfunction "Pin_11") (pintype "passive") (tstamp 45adee83-97bc-4e26-ac68-86b31b4c7466))
    (pad "12" smd rect (at 0.25 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "/WiFi_Display/EPD_CS") (pinfunction "Pin_12") (pintype "passive") (tstamp 928ee37c-0cb6-413d-9f51-629f33a6ba0b))
    (pad "13" smd rect (at -0.25 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 38 "/WiFi_Display/EPD_SCLK") (pinfunction "Pin_13") (pintype "passive") (tstamp a39ecece-979f-4f5c-aff3-83e5c4280482))
    (pad "14" smd rect (at -0.75 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "/WiFi_Display/EPD_SDI") (pinfunction "Pin_14") (pintype "passive") (tstamp a0ae1e37-0c56-454d-9d9d-ef5045a97ce8))
    (pad "15" smd rect (at -1.25 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "VDD") (pinfunction "Pin_15") (pintype "passive") (tstamp 38b1daaf-8dd8-45a8-b42b-0b38a8893fed))
    (pad "16" smd rect (at -1.75 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "VDD") (pinfunction "Pin_16") (pintype "passive") (tstamp e102e0ed-c731-4751-a432-c3583b7c9a1f))
    (pad "17" smd rect (at -2.25 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Pin_17") (pintype "passive") (tstamp e021bed0-e5ac-4cf4-9b2e-a0e07aafd52d))
    (pad "18" smd rect (at -2.75 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "Net-(C29-Pad2)") (pinfunction "Pin_18") (pintype "passive") (tstamp a6f4f86a-5b80-4e6f-bdbf-36599fb28daf))
    (pad "19" smd rect (at -3.25 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "Net-(C24-Pad2)") (pinfunction "Pin_19") (pintype "passive") (tstamp 15b815b0-6456-4221-be25-0e020c8ddd67))
    (pad "20" smd rect (at -3.75 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "Net-(C30-Pad2)") (pinfunction "Pin_20") (pintype "passive") (tstamp 453a2347-3353-4215-9c4d-46177ae3dc2c))
    (pad "21" smd rect (at -4.25 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "/WiFi_Display/PREVGH") (pinfunction "Pin_21") (pintype "passive") (tstamp 832608e3-3c1e-4061-9c00-b068f3eb3d62))
    (pad "22" smd rect (at -4.75 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "Net-(C31-Pad2)") (pinfunction "Pin_22") (pintype "passive") (tstamp 4d547913-abc4-4606-90a7-2eed61bbb55e))
    (pad "23" smd rect (at -5.25 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "/WiFi_Display/PREVGL") (pinfunction "Pin_23") (pintype "passive") (tstamp 17c715c4-c689-4e34-a12f-08cb598fc967))
    (pad "24" smd rect (at -5.75 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "Net-(C32-Pad2)") (pinfunction "Pin_24") (pintype "passive") (tstamp 8d48f40c-8178-498b-8803-b1b6e7434f9a))
    (pad "MP" smd rect (at -7.4 -2.35 270) (size 2 3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "MountPin") (pintype "passive") (tstamp 495827f0-5b44-4444-a781-edc2547faaee))
    (pad "MP" smd rect (at 7.4 -2.35 270) (size 2 3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "MountPin") (pintype "passive") (tstamp 6232f840-56ce-4f2a-9ed5-eb5bbe05647d))
  )

  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp a98105ab-00fb-497a-b386-34dd4b968be3)
    (at 131.4 110.2 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/7d8b0c60-4781-4aae-a53d-c586cbf927ed")
    (attr smd)
    (fp_text reference "C20" (at 0 1.16) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp ce171eab-a480-4ce9-969e-540871619188)
    )
    (fp_text value "100nF" (at 0 -1.16) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 997c2b86-e823-445e-9560-ab4d47aa2c19)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
      (tstamp 8a9e0411-442c-4a5e-a3ea-38c656c77b22)
    )
    (fp_line (start -0.107836 0.36) (end 0.107836 0.36) (layer "B.SilkS") (width 0.12) (tstamp 5a6a08ce-d607-46ba-9076-0b266002b2ec))
    (fp_line (start -0.107836 -0.36) (end 0.107836 -0.36) (layer "B.SilkS") (width 0.12) (tstamp a749317a-6047-4d75-92cf-45ed130d88c9))
    (fp_line (start -0.91 -0.46) (end -0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 7880aeac-7156-4df1-87d5-21b0aee450fe))
    (fp_line (start 0.91 -0.46) (end -0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp d98db492-254c-468d-ab85-f09e70938da9))
    (fp_line (start 0.91 0.46) (end 0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp ddf15e8d-3103-4c27-ba61-27ff64d5bb66))
    (fp_line (start -0.91 0.46) (end 0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp fae61bc3-41da-45d5-a79e-fe85b507ebf6))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 1dfc0f58-20bc-484b-af3a-b109a9c844ee))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 4c4e6c83-2bbe-4579-af24-b59d284256a9))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 6338ebc0-33fd-4463-afb0-3cba177a64c0))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 9afae567-0717-4ae1-98b7-b3ce4e60e6a0))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(C20-Pad1)") (pintype "passive") (tstamp 65d7769a-f785-44e4-9069-f47a76d16a33))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp c68639ab-ac48-4c2c-b10a-fbe7b2c7a174))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp a9cd9147-a9b6-41cd-81b9-a24e33a9227d)
    (at 178.3 111.2 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/2615342f-3cc9-47ef-8bcb-532586fcdd97")
    (attr smd)
    (fp_text reference "R26" (at 0 1.43 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e7709e1e-d553-4f25-9c48-3d38e60ca0d8)
    )
    (fp_text value "2R/0.5%" (at 0 -1.43 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e5d003f7-8e88-4216-95e1-4ce79308ddcf)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp ae7b7483-33ce-4b51-a09f-5cf1847ca0dd)
    )
    (fp_line (start -0.237258 -0.5225) (end 0.237258 -0.5225) (layer "B.SilkS") (width 0.12) (tstamp 5af1ba78-751b-45a4-b81f-2acc639b6451))
    (fp_line (start -0.237258 0.5225) (end 0.237258 0.5225) (layer "B.SilkS") (width 0.12) (tstamp a0d01b50-4bd3-45ba-b2d8-6b6ca69916f0))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 3c80a748-6a0c-4510-85f1-455029d19a86))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 781cd9cb-a5f4-4d74-8d28-6f3c9b19b1b3))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 7a3c6bb1-e643-4ae8-b7bb-2cd8786467b6))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 8fe31c17-4ffb-4a9a-b5c2-abc618648b08))
    (fp_line (start 0.8 0.4125) (end 0.8 -0.4125) (layer "B.Fab") (width 0.1) (tstamp 514ebca3-be25-4279-902b-9fbddc053051))
    (fp_line (start 0.8 -0.4125) (end -0.8 -0.4125) (layer "B.Fab") (width 0.1) (tstamp 5d225da1-77f1-4c3c-8fe3-b050ed0f29a0))
    (fp_line (start -0.8 -0.4125) (end -0.8 0.4125) (layer "B.Fab") (width 0.1) (tstamp 5fe89951-89c4-4325-970a-50525f0a0e8f))
    (fp_line (start -0.8 0.4125) (end 0.8 0.4125) (layer "B.Fab") (width 0.1) (tstamp 6e354681-82bd-40fc-87d6-f32aa59933da))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 28 "/Power_Management/LED_K") (pintype "passive") (tstamp e4be497d-ecea-4503-be1f-d889729ebb75))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 78f98a21-5734-4d4b-98bb-8a740223bce3))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp aa78f927-42d8-4ba7-b3ae-f1bcdf880f70)
    (at 148.9 118.3 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/6c84cf61-52c7-4b7a-9c9e-ec40be31c6d8")
    (attr smd)
    (fp_text reference "C19" (at 0 1.43 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 07f03192-3ebb-4e88-a680-1a00758dbfda)
    )
    (fp_text value "10uF" (at 0 -1.43 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 9ac2d23a-cedf-42e1-a18a-b3ac5218f97a)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 1739d637-947d-4642-aff2-fe8088ebadef)
    )
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp 7d02a602-fa8d-4815-a50b-194d18067601))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp 9ec8b252-ceb0-452d-9593-36c933a32592))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 055c38a3-3c92-476f-af5e-7a4de2926680))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 4826952e-9a7c-469e-a126-4250d3de3a4a))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 64fdb7fe-1fbd-4c9e-b07b-20c53d43468f))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp e7a98667-41e4-4dbd-8606-5398de23bf4f))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp b4b7038c-5265-46ab-ad83-aadc2d9e5e8a))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp ea0fffa4-b48b-4624-908d-d36cfb3d1ec6))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp fe08190e-8cd1-4535-80e3-b3a8b22efde0))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp fee7ada3-70b7-4a0f-818e-b4db437411e2))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "VDD") (pintype "passive") (tstamp c475a6fb-1936-4569-a182-ca9a79efae63))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 6b247820-a2e0-4240-ad14-c6a7ee767403))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp abc34439-9b02-4022-a81e-62a8cd8854da)
    (at 155.4 111.2)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/5bb8fc73-3b84-4fec-a5b9-236b7a12debc")
    (attr smd)
    (fp_text reference "R4" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 3e026644-7cd5-4619-871f-c201838e1d58)
    )
    (fp_text value "100k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 253d4a1b-4d38-401d-8530-f379c84e1ac6)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp fc0b3927-d4fe-4397-aef5-2d521568c534)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 6f2943e6-f5a8-4522-9c81-5250a5cca95b))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp ed7115b3-29a6-4eac-9244-b2c273a72de7))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 0199e30d-eb6f-4e4f-8aac-41d14eb6770f))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 1a834adc-0fd8-4ed9-8089-5d245415ae13))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp d727613f-be10-405d-bd08-19267bede21b))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp dba114bf-98e9-4f5b-a9dc-02193cc39000))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 4372a5e2-085e-4816-a52a-36848a533cff))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 712b8bd1-a02e-4272-b3f2-f2be0b71d11f))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp c414cc05-0852-4dec-821d-2c79c61fed3c))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp e4620475-5ddc-4219-977b-796ed2eed581))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp 12dd37ba-4fb9-4cf9-bb3b-c5e34558af6d))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/Sensor_Controller/LPC_~{RST}") (pintype "passive") (tstamp 616010f7-b11e-4a11-b933-942f4e186999))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp b0453f78-a608-49a3-b8b3-288a0dfc0552)
    (at 152.9 121.8)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/bb143e55-5b21-48df-8ac4-9dd5a084e89f")
    (attr smd)
    (fp_text reference "R27" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 575bd10e-6bc2-4b0f-aca9-9c3f2d87fcdd)
    )
    (fp_text value "22.8k/1%" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 876c22fe-2498-44d7-98f2-d9aff4eabb0c)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp a5d08036-df94-457d-a2d1-78d7f017d5b3)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 339d8b78-c73a-409d-a04b-42e84cfb1eb9))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp ad47806f-7d4d-49f2-b32a-e5aaca29e374))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 251ee8ea-d8e2-437b-889a-b17bbf8d0cf2))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 35aba278-1584-4fa5-b0de-d9d13621c627))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp c6bbe283-68b2-4dcf-a953-ee33c6ef2331))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp eb6236b9-4f1f-415b-b261-b822f433a05d))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 5dc2f7b8-a63b-41c0-9cd6-5bc7b0edc6c9))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 938e3f21-dbc5-4e6f-a01e-076aab60d9b4))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp cd0b3cdc-99c0-4430-a1a0-2f450fba1953))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp fb37a393-c5ef-4707-a19d-417c0818921d))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "VDD") (pintype "passive") (tstamp 27d37ada-0f4c-4967-a2b8-23829ff4d071))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 60 "Net-(R27-Pad2)") (pintype "passive") (tstamp d402f73e-9894-4c4b-a929-a1c5d12b078b))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp b59d7c25-3678-43d4-8a78-9fb304e6c001)
    (at 121.8 124.6 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/f7622d79-b5a7-44a2-937d-b5c487b37ebf")
    (attr smd)
    (fp_text reference "R8" (at 0 1.17 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 726ea5ff-c760-4444-a2ad-2b4f51b697ea)
    )
    (fp_text value "100k" (at 0 -1.17 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 409a88b2-b7e7-483c-8337-a0b3101146fd)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 7850b36e-9f11-48fc-be5a-466fc700edd5)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 24bbe7b3-2794-400a-adc4-226cde27db2d))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp a4e348c2-8730-4d2a-b857-790d252e414f))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 2dad0fa6-bffb-4f7d-a4b8-2ba94d358685))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 443b6076-53d6-41f7-9647-4652df201587))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 91a026ae-7f2f-4fd9-8819-f2a059abf8f0))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp e0440ffa-460d-4d10-8f86-243d346eba59))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 07affaa3-1124-46a9-aeb2-ba645cf02e42))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 1831d5d9-90b5-4f4f-8363-81cf0508da46))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 354528e9-5e4e-45eb-b00d-12c6fc0f3eb3))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp b91d9cc8-6c02-4975-98c6-328a1d85ed41))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp b4b0f20a-6548-41d6-bccc-9ed9bc0c8b92))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 43 "/Sensor_Controller/LPC_SWDIO") (pintype "passive") (tstamp 25e4deaf-7a4d-4afe-aace-591f6b9d57b3))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_USB:USB_C_Receptacle_XKB_U262-16XN-4BVC11" (layer "B.Cu")
    (tedit 5E1305FC) (tstamp b7f70fd6-816a-4b8b-b891-5d04a3af75d5)
    (at 192.9 154.2 -90)
    (descr "USB Type C, right-angle, SMT, https://datasheet.lcsc.com/szlcsc/1811141824_XKB-Enterprise-U262-161N-4BVC11_C319148.pdf")
    (tags "USB C Type-C Receptacle SMD")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/42c410e1-c833-4f75-9dc0-4b6bca6833e1")
    (attr smd)
    (fp_text reference "J2" (at 0 5.715 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5c4dbd5a-14bc-4f3b-bc0f-d83b7b081c93)
    )
    (fp_text value "XKB-U262-161N-4BS165" (at 0 -4.935 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp aa1554d4-4f73-4f1c-8bc6-54506943dc8f)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 99393fdd-d9e9-45ed-8f76-b7e0c80f8d9d)
    )
    (fp_line (start 4.58 -3.785) (end -4.58 -3.785) (layer "B.SilkS") (width 0.12) (tstamp 375b2832-e9b5-43d4-9a34-673e25b14962))
    (fp_line (start 4.58 -2.08) (end 4.58 -3.785) (layer "B.SilkS") (width 0.12) (tstamp 74c81772-684b-4abf-bde0-12994031e7f6))
    (fp_line (start 4.58 -0.07) (end 4.58 1.85) (layer "B.SilkS") (width 0.12) (tstamp b0a6865c-d709-4d1c-83a1-ad74081e3062))
    (fp_line (start -4.58 1.85) (end -4.58 -0.07) (layer "B.SilkS") (width 0.12) (tstamp df3916ea-4b4f-4a3d-a393-37a053aea798))
    (fp_line (start -4.58 -3.785) (end -4.58 -2.08) (layer "B.SilkS") (width 0.12) (tstamp ecddc703-16b3-43fd-97bb-af4b6db2c3a8))
    (fp_line (start -5.32 -4.18) (end -5.32 4.75) (layer "B.CrtYd") (width 0.05) (tstamp 2f909e82-e446-4d1a-bbb5-d35f65bb1fb7))
    (fp_line (start 5.32 -4.18) (end -5.32 -4.18) (layer "B.CrtYd") (width 0.05) (tstamp 38bbcad3-1ee2-444f-89bd-b15e087075e6))
    (fp_line (start -5.32 4.75) (end 5.32 4.75) (layer "B.CrtYd") (width 0.05) (tstamp 68cedb9a-8f82-4d47-b55f-99e44b9ca86d))
    (fp_line (start 5.32 4.75) (end 5.32 -4.18) (layer "B.CrtYd") (width 0.05) (tstamp d747c55e-b310-40ac-b572-02fb97a04fd6))
    (fp_line (start 4.47 -3.675) (end 4.47 3.675) (layer "B.Fab") (width 0.1) (tstamp 35efb65d-9b6b-4c63-bdd4-a8d6a1d5f041))
    (fp_line (start -4.47 3.675) (end -4.47 -3.675) (layer "B.Fab") (width 0.1) (tstamp b7b8ba21-fe4f-4afb-b9cb-713eeb02910f))
    (fp_line (start -4.47 3.675) (end 4.47 3.675) (layer "B.Fab") (width 0.1) (tstamp d8770668-a851-40d2-bf03-7056e4c36bd1))
    (fp_line (start -4.47 -3.675) (end 4.47 -3.675) (layer "B.Fab") (width 0.1) (tstamp ee6cbbd4-e29e-4d6b-8ed5-1ccd7b42a8d0))
    (pad "" np_thru_hole circle (at 2.89 2.605 270) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask) (tstamp 9368da43-3947-4055-9870-ec822283eff6))
    (pad "" np_thru_hole circle (at -2.89 2.605 270) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask) (tstamp f967adad-9500-405b-ac60-ecb143e524fd))
    (pad "A1" smd rect (at -3.35 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive") (tstamp 08d82666-e741-4e31-a0fb-9e5a2bca0769))
    (pad "A4" smd rect (at -2.55 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "VBUS") (pinfunction "VBUS") (pintype "passive") (tstamp c05a0ec3-fbf8-41ac-aa18-480168705788))
    (pad "A5" smd rect (at -1.25 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "Net-(J2-PadA5)") (pinfunction "CC1") (pintype "bidirectional") (tstamp acbf36aa-611d-4f06-a181-d8d43dd89c22))
    (pad "A6" smd rect (at -0.25 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 83 "/WiFi_Display/USB_D+") (pinfunction "D+") (pintype "bidirectional") (tstamp c74b463c-d943-4ce5-85ab-0a86a5370994))
    (pad "A7" smd rect (at 0.25 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 84 "/WiFi_Display/USB_D-") (pinfunction "D-") (pintype "bidirectional") (tstamp 9c33fbec-276d-4929-af11-b9bbd4453b76))
    (pad "A8" smd rect (at 1.25 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 97 "/WiFi_Display/UART_RX") (pinfunction "SBU1") (pintype "bidirectional") (tstamp a4e663d1-908e-40a8-b408-28ee0f79a882))
    (pad "A9" smd rect (at 2.55 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "VBUS") (pinfunction "VBUS") (pintype "passive") (tstamp e3b7a090-8536-4322-9158-0c23192e8bd6))
    (pad "A12" smd rect (at 3.35 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive") (tstamp 347092df-520a-4304-bce1-0b546f56ceaf))
    (pad "B1" smd rect (at 3.05 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive") (tstamp ca89f65e-e30f-49f2-8616-15c5ddb4bfbc))
    (pad "B4" smd rect (at 2.25 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "VBUS") (pinfunction "VBUS") (pintype "passive") (tstamp 919aa72a-5cdd-4e47-8834-99557c6742a4))
    (pad "B5" smd rect (at 1.75 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 62 "Net-(J2-PadB5)") (pinfunction "CC2") (pintype "bidirectional") (tstamp 45f54814-05ec-4929-bb16-c4fd314dd07c))
    (pad "B6" smd rect (at 0.75 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 83 "/WiFi_Display/USB_D+") (pinfunction "D+") (pintype "bidirectional") (tstamp 606ff535-0c7c-41f0-b6dd-4bc7d807146b))
    (pad "B7" smd rect (at -0.75 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 84 "/WiFi_Display/USB_D-") (pinfunction "D-") (pintype "bidirectional") (tstamp 78b2b580-612b-4e2f-8fdc-f04e6080572a))
    (pad "B8" smd rect (at -1.75 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 98 "/WiFi_Display/UART_TX") (pinfunction "SBU2") (pintype "bidirectional") (tstamp 8e3267b9-f86b-4212-9570-237be7cdc9f7))
    (pad "B9" smd rect (at -2.25 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "VBUS") (pinfunction "VBUS") (pintype "passive") (tstamp 9fd37cf2-0e7b-4c81-8b12-88fc1bd4abdd))
    (pad "B12" smd rect (at -3.05 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive") (tstamp 237108a2-a73b-4e83-8ad0-871ad2a9d59e))
    (pad "S1" thru_hole oval (at 4.32 -1.075 270) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive") (tstamp 0c5cdebb-154c-4f4a-8ce7-a029b1f7db98))
    (pad "S1" thru_hole oval (at 4.32 3.105 270) (size 1 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive") (tstamp 2b5339b6-5264-4f38-b713-c1872113fa99))
    (pad "S1" thru_hole oval (at -4.32 3.105 270) (size 1 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive") (tstamp adbb9b3b-cc5b-4215-9bee-0e03177f3698))
    (pad "S1" thru_hole oval (at -4.32 -1.075 270) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive") (tstamp b0ca2fa4-f91d-4492-b244-c92b3f1ad2ec))
    (model "${KICAD6_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_XKB_U262-16XN-4BVC11.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_SO:MSOP-8_3x3mm_P0.65mm" (layer "B.Cu")
    (tedit 5E509FDD) (tstamp bc04bda0-beeb-4a95-ab89-10189cc0f580)
    (at 164.6 139.7 180)
    (descr "MSOP, 8 Pin (https://www.jedec.org/system/files/docs/mo-187F.pdf variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "MSOP SO")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/5e31b07e-6edf-49dd-8861-29f3783f96cd")
    (attr smd)
    (fp_text reference "U3" (at 0 2.45) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 455e28d1-4e8d-4772-8f23-fea0d6086aa6)
    )
    (fp_text value "BL24C256A-SFRC" (at 0 -2.45) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f2e1a211-0a00-4015-aad3-e01187629cbb)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.75 0.75) (thickness 0.11)) (justify mirror))
      (tstamp c0ec6b07-f6a0-45db-8719-f14db3ebd5d5)
    )
    (fp_line (start 0 1.61) (end 1.5 1.61) (layer "B.SilkS") (width 0.12) (tstamp 97b6051f-adaa-4771-85a7-f92a46668f23))
    (fp_line (start 0 -1.61) (end -1.5 -1.61) (layer "B.SilkS") (width 0.12) (tstamp aeb293c5-8472-4d12-b4a4-40674335df21))
    (fp_line (start 0 1.61) (end -2.925 1.61) (layer "B.SilkS") (width 0.12) (tstamp d349f801-6410-4b6f-9bfd-d178b825c942))
    (fp_line (start 0 -1.61) (end 1.5 -1.61) (layer "B.SilkS") (width 0.12) (tstamp ed7f323a-9a83-4f55-bc0e-ed9216e11cb1))
    (fp_line (start -3.18 1.75) (end -3.18 -1.75) (layer "B.CrtYd") (width 0.05) (tstamp 272f8220-b7bc-49b2-a347-8fa9938bec47))
    (fp_line (start 3.18 1.75) (end -3.18 1.75) (layer "B.CrtYd") (width 0.05) (tstamp 30ad2469-2625-4b2b-a99a-b796d50866de))
    (fp_line (start -3.18 -1.75) (end 3.18 -1.75) (layer "B.CrtYd") (width 0.05) (tstamp a1424326-750b-4088-9fe5-7fa64ce71460))
    (fp_line (start 3.18 -1.75) (end 3.18 1.75) (layer "B.CrtYd") (width 0.05) (tstamp c89eeb5a-d0b8-4936-b71d-a40c8bbf13d7))
    (fp_line (start -0.75 1.5) (end 1.5 1.5) (layer "B.Fab") (width 0.1) (tstamp 4ccd8e5d-acb3-4bc8-aa0f-08b449537fa2))
    (fp_line (start -1.5 -1.5) (end -1.5 0.75) (layer "B.Fab") (width 0.1) (tstamp 5338764b-7f7a-4f22-8037-4cdaf8f59161))
    (fp_line (start 1.5 1.5) (end 1.5 -1.5) (layer "B.Fab") (width 0.1) (tstamp 550f4f34-b804-42da-a740-0e221644f4cd))
    (fp_line (start -1.5 0.75) (end -0.75 1.5) (layer "B.Fab") (width 0.1) (tstamp c6727eb7-7f49-4efa-9e85-2bd615951340))
    (fp_line (start 1.5 -1.5) (end -1.5 -1.5) (layer "B.Fab") (width 0.1) (tstamp e206a525-d827-4059-8706-1551a778b857))
    (pad "1" smd roundrect (at -2.1125 0.975 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "A0") (pintype "input") (tstamp c71f0662-f7ee-4c2e-a23e-8f8bf8836425))
    (pad "2" smd roundrect (at -2.1125 0.325 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "A1") (pintype "input") (tstamp 4ec37775-b337-4eb3-95f4-b43bbc03f14c))
    (pad "3" smd roundrect (at -2.1125 -0.325 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "A2") (pintype "input") (tstamp 731ce20a-5584-4181-b2df-933b2be41657))
    (pad "4" smd roundrect (at -2.1125 -0.975 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 454cf39f-5076-489c-b17c-93499213524e))
    (pad "5" smd roundrect (at 2.1125 -0.975 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 41 "/Sensor_Controller/I2C_SDA") (pinfunction "SDA") (pintype "bidirectional") (tstamp 2336c947-65cf-409b-86b1-e13b16834329))
    (pad "6" smd roundrect (at 2.1125 -0.325 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 42 "/Sensor_Controller/I2C_SCL") (pinfunction "SCL") (pintype "input") (tstamp 95971152-5d60-4f70-81e1-016073990cd5))
    (pad "7" smd roundrect (at 2.1125 0.325 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "WP") (pintype "input") (tstamp fe3f84ae-b0d3-4c07-9af6-ab27ca704eba))
    (pad "8" smd roundrect (at 2.1125 0.975 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pinfunction "VCC") (pintype "power_in") (tstamp ecdbe1ee-e4aa-49c9-8aa8-3daf8b3a620c))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/MSOP-8_3x3mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp bc7df6c8-11c9-4287-8edb-a0a9670ba4dd)
    (at 178.3 108.2 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/9c3337a3-b1d9-42c7-b871-ae280cc7c859")
    (attr smd)
    (fp_text reference "C17" (at 0 1.43 -270) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e5d20853-ef6e-4ff6-84df-4840c254d4c6)
    )
    (fp_text value "10uF" (at 0 -1.43 -270) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 15d19ea4-2ed4-4099-969c-8367dc310697)
    )
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp a0b414ac-f98d-4991-ac82-f86e0c53a215)
    )
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp 0fd825f9-b38e-45a6-a176-4dd8b159ebc2))
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp 866d035a-16af-48f8-8a39-63218a4a8cae))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 9f244187-5856-4e32-bd71-b2acb861d950))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp be42f4cb-53be-44f9-8ad7-b8b9c564666b))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp bfb18f7d-01c8-4f78-bdb8-2f8904e462e6))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp ede81694-6810-4c22-9f13-19703ec80b12))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 21a29a99-46e4-4295-b8c0-acef8865107c))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 5510f931-ba0c-47c4-a00c-9ad1c5b3979c))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 8d197a8c-1ed9-4a72-96cd-6968203b4d19))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp afc50c62-6dce-4002-a19d-cca66d2277a9))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/Power_Management/LED_A") (pintype "passive") (tstamp 681eb4eb-f03c-4174-b8ed-3f71bd63a62c))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 8780721f-f8db-4b65-9b1a-947e65eb9436))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp be58c61b-9ebb-4fd7-9c53-227358ce1677)
    (at 126.5 126.6875 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/568992a3-2d20-4370-8147-67be49b51947")
    (attr smd)
    (fp_text reference "C3" (at 0 1.16) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp b8bb1f14-d2e5-404e-81c7-12d70e5a7fb2)
    )
    (fp_text value "100nF" (at 0 -1.16) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a97e9da6-2ed8-4f5d-9c32-78d88cf03d94)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
      (tstamp 5078d587-0602-483e-bb0c-cdf618404d19)
    )
    (fp_line (start -0.107836 -0.36) (end 0.107836 -0.36) (layer "B.SilkS") (width 0.12) (tstamp 26159000-0b5c-4630-b159-6b032ca54cb5))
    (fp_line (start -0.107836 0.36) (end 0.107836 0.36) (layer "B.SilkS") (width 0.12) (tstamp 754ff76f-39f4-4f3b-86e3-eb1699bb5b73))
    (fp_line (start 0.91 -0.46) (end -0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 14700925-69e9-410f-94ef-0ffcebcf535f))
    (fp_line (start -0.91 -0.46) (end -0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 31a73d5f-3b51-4d23-80bc-eceb1f4be525))
    (fp_line (start -0.91 0.46) (end 0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 58c35daf-6b69-4560-89a2-fa494b78862d))
    (fp_line (start 0.91 0.46) (end 0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 9cacdd15-1e28-4310-9f56-548afa63c61d))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 893d6e3f-84c4-4a3f-8138-5bee4b6a0b33))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 94de779f-e6f7-4cde-a971-37d0c61150a3))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp aa18482a-1c96-4fc9-948c-4696fcafdf50))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp c98c3e74-722a-44b4-a012-1ac944523d3c))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp 6ab25c23-43df-4d21-b98b-af7ad986d0fd))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 6a1e4fa7-6a6d-4658-a371-e823c77ec520))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_LGA:LGA-14_3x2.5mm_P0.5mm_LayoutBorder3x4y" (layer "B.Cu")
    (tedit 5D9F7937) (tstamp bedb2d63-7071-4452-9cee-8fa66de5b0f1)
    (at 128.4 124.6875 180)
    (descr "LGA, 14 Pin (http://www.st.com/resource/en/datasheet/lsm6ds3.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "LGA NoLead")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/06e56a77-f6fa-4386-b7c1-79cf55ed810a")
    (attr smd)
    (fp_text reference "U1" (at 0 2.2) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp b6a76da6-b7b9-46e1-9b5e-860c2d2f07b1)
    )
    (fp_text value "LSM6DS3" (at 0 -2.2) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f9c7ece3-c077-4b01-b5a0-8ce8ab1cb937)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.75 0.75) (thickness 0.11)) (justify mirror))
      (tstamp 183a4388-85a1-45b6-b94c-ae2299be7ce1)
    )
    (fp_line (start -0.96 -1.36) (end -1.61 -1.36) (layer "B.SilkS") (width 0.12) (tstamp 23297984-5a74-4021-a865-1dea68fea909))
    (fp_line (start 0.96 -1.36) (end 1.61 -1.36) (layer "B.SilkS") (width 0.12) (tstamp 8851f350-c031-42d4-b5cb-a80ea78d2a4a))
    (fp_line (start -0.96 1.36) (end -1.61 1.36) (layer "B.SilkS") (width 0.12) (tstamp 8ef68c83-cde6-4d1f-8c90-1f0347409c3c))
    (fp_line (start -1.61 -1.36) (end -1.61 -1.21) (layer "B.SilkS") (width 0.12) (tstamp 98971603-1f92-4710-83e0-efd3d91c36e1))
    (fp_line (start 1.61 1.36) (end 1.61 1.21) (layer "B.SilkS") (width 0.12) (tstamp 9e52bf7f-8541-4eea-8cac-7f043ef74d4d))
    (fp_line (start 1.61 -1.36) (end 1.61 -1.21) (layer "B.SilkS") (width 0.12) (tstamp ab4898f6-ec0a-4974-9cfb-bd6a0357bfdf))
    (fp_line (start 0.96 1.36) (end 1.61 1.36) (layer "B.SilkS") (width 0.12) (tstamp fb75f1f3-6ed6-4808-9dbe-bc66a95a093e))
    (fp_line (start -1.75 -1.5) (end 1.75 -1.5) (layer "B.CrtYd") (width 0.05) (tstamp 34130493-82ca-4e99-a5ac-cb51224ad304))
    (fp_line (start 1.75 -1.5) (end 1.75 1.5) (layer "B.CrtYd") (width 0.05) (tstamp 6e02743f-ff1d-4d30-9a24-5823fa3ae574))
    (fp_line (start 1.75 1.5) (end -1.75 1.5) (layer "B.CrtYd") (width 0.05) (tstamp 856f1b3a-d2c9-4de4-8113-81a128eed687))
    (fp_line (start -1.75 1.5) (end -1.75 -1.5) (layer "B.CrtYd") (width 0.05) (tstamp d80d5d83-348e-444e-b669-de0293714ca3))
    (fp_line (start -1.5 -1.25) (end -1.5 0.625) (layer "B.Fab") (width 0.1) (tstamp 322e78d1-e3ce-4886-97b7-2b737a1e22cc))
    (fp_line (start 1.5 1.25) (end 1.5 -1.25) (layer "B.Fab") (width 0.1) (tstamp 4660cd09-2f17-46c2-aaf8-a2a8cc253eb4))
    (fp_line (start -1.5 0.625) (end -0.875 1.25) (layer "B.Fab") (width 0.1) (tstamp 8d182b79-1a63-453f-817c-37863dc281cb))
    (fp_line (start 1.5 -1.25) (end -1.5 -1.25) (layer "B.Fab") (width 0.1) (tstamp a7611074-070b-4af3-9627-e74c77580f76))
    (fp_line (start -0.875 1.25) (end 1.5 1.25) (layer "B.Fab") (width 0.1) (tstamp dcb0b219-61c7-49e0-9069-3a695bc6af58))
    (pad "1" smd custom (at -1.1625 0.75 180) (size 0.223223 0.223223) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 64 "/Sensor_Controller/LSM_A0") (pinfunction "SDO/SA0") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.2375 -0.081066)
            (xy 0.2375 -0.125)
            (xy -0.2375 -0.125)
            (xy -0.2375 0.125)
            (xy 0.031434 0.125)
          ) (width 0.15) (fill yes))
      ) (tstamp 994f531d-d3e5-40db-92b6-cd52c7bf32c7))
    (pad "2" smd roundrect (at -1.1625 0.25 180) (size 0.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "SDX") (pintype "bidirectional") (tstamp 301e9ba3-d757-4d65-8442-c56aef0d5d9d))
    (pad "3" smd roundrect (at -1.1625 -0.25 180) (size 0.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "SCX") (pintype "input") (tstamp 81c88955-83cc-4e3d-b1df-9bf574602497))
    (pad "4" smd custom (at -1.1625 -0.75 180) (size 0.223223 0.223223) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 65 "/Sensor_Controller/LSM_INT1") (pinfunction "INT1") (pintype "output")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.2375 0.081066)
            (xy 0.031434 -0.125)
            (xy -0.2375 -0.125)
            (xy -0.2375 0.125)
            (xy 0.2375 0.125)
          ) (width 0.15) (fill yes))
      ) (tstamp 07eab6db-6493-4ba2-99f6-f9759ab1b8c0))
    (pad "5" smd custom (at -0.5 -0.9125 180) (size 0.223223 0.223223) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "VDDF") (pinfunction "VDDIO") (pintype "power_in")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.125 -0.2375)
            (xy -0.125 -0.2375)
            (xy -0.125 0.031434)
            (xy 0.081066 0.2375)
            (xy 0.125 0.2375)
          ) (width 0.15) (fill yes))
      ) (tstamp 6b4a3c60-cf1a-4507-834d-8587eeda1bb0))
    (pad "6" smd roundrect (at 0 -0.9125 180) (size 0.4 0.625) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 37169c03-3ee2-443d-8f34-7b8ee69867f8))
    (pad "7" smd custom (at 0.5 -0.9125 180) (size 0.223223 0.223223) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.125 0.031434)
            (xy 0.125 -0.2375)
            (xy -0.125 -0.2375)
            (xy -0.125 0.2375)
            (xy -0.081066 0.2375)
          ) (width 0.15) (fill yes))
      ) (tstamp 4dc9509d-45f1-4148-9426-81720d1301c7))
    (pad "8" smd custom (at 1.1625 -0.75 180) (size 0.223223 0.223223) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "VDDF") (pinfunction "VDD") (pintype "power_in")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.2375 -0.125)
            (xy -0.031434 -0.125)
            (xy -0.2375 0.081066)
            (xy -0.2375 0.125)
            (xy 0.2375 0.125)
          ) (width 0.15) (fill yes))
      ) (tstamp 3d64f3ed-5957-4107-a249-b281801ed4ae))
    (pad "9" smd roundrect (at 1.1625 -0.25 180) (size 0.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 66 "/Sensor_Controller/LSM_INT2") (pinfunction "INT2") (pintype "output") (tstamp f37710d1-3c6d-49db-a557-89f92f9c6633))
    (pad "10" smd roundrect (at 1.1625 0.25 180) (size 0.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 67 "unconnected-(U1-Pad10)") (pinfunction "NC") (pintype "no_connect") (tstamp 2210e876-16ba-43a5-a245-979513e1c7aa))
    (pad "11" smd custom (at 1.1625 0.75 180) (size 0.223223 0.223223) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 68 "unconnected-(U1-Pad11)") (pinfunction "NC") (pintype "no_connect")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.2375 -0.125)
            (xy -0.2375 -0.125)
            (xy -0.2375 -0.081066)
            (xy -0.031434 0.125)
            (xy 0.2375 0.125)
          ) (width 0.15) (fill yes))
      ) (tstamp 80cfcaf7-0915-4f80-bfab-9c8365808da4))
    (pad "12" smd custom (at 0.5 0.9125 180) (size 0.223223 0.223223) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "VDDF") (pinfunction "CS") (pintype "input")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.125 -0.031434)
            (xy -0.081066 -0.2375)
            (xy -0.125 -0.2375)
            (xy -0.125 0.2375)
            (xy 0.125 0.2375)
          ) (width 0.15) (fill yes))
      ) (tstamp c5fef5b8-569a-4bab-a419-ac0b4062a936))
    (pad "13" smd roundrect (at 0 0.9125 180) (size 0.4 0.625) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 42 "/Sensor_Controller/I2C_SCL") (pinfunction "SCL") (pintype "input") (tstamp a5e34a11-ccd5-4bff-9ab3-aa46eb01f715))
    (pad "14" smd custom (at -0.5 0.9125 180) (size 0.223223 0.223223) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 41 "/Sensor_Controller/I2C_SDA") (pinfunction "SDA") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.125 -0.2375)
            (xy 0.081066 -0.2375)
            (xy -0.125 -0.031434)
            (xy -0.125 0.2375)
            (xy 0.125 0.2375)
          ) (width 0.15) (fill yes))
      ) (tstamp 339b5a7b-145b-4619-87d5-9920c0ca7dfd))
    (model "${KICAD6_3DMODEL_DIR}/Package_LGA.3dshapes/LGA-14_3x2.5mm_P0.5mm_LayoutBorder3x4y.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp c18d8f0d-9434-4bfc-bce5-9a4623ea1a5b)
    (at 154 154)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/6e1caec3-a6d0-4a90-9938-6cdd78bb7478")
    (attr smd)
    (fp_text reference "R16" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 83eccd2c-7eca-4030-b440-86dbb3c124c4)
    )
    (fp_text value "2.2k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0345edad-18ee-4c71-bc5d-bb13e9ef823e)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp e8412301-7691-4904-bd9b-8a0fe7b98b4f)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 3c7ac3a4-3b70-4458-b1db-6904a1fadc07))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 84638afd-94ec-4c2a-a87b-c394319e87c3))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 2aed225d-6d7c-4abd-9715-f66423df9118))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 3e1bd748-7cf3-4faf-ad0c-74dc6a9e4eb5))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 5a5523fd-be7e-4e81-a706-2721e820b560))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 7e462183-f4bc-44c5-a69d-f57eca835bd3))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 03781969-6d2e-46ac-88e1-e6cab9bae4be))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 1145946f-b9ce-463a-9fe2-d568af4360be))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 427575de-17d3-4f65-b48a-ecb3d1a28788))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp df4049e8-e0ca-404a-8dc0-bb6845153bd3))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 51 "/Sensor_Controller/CAPT_X2") (pintype "passive") (tstamp f586b135-26dd-4e27-8219-c0bf441648a9))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(R16-Pad2)") (pintype "passive") (tstamp 2c87135e-8ae7-4048-ba8d-f5f66ad911d8))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp c1e82e01-95b3-4e5c-969d-4587a2c9043f)
    (at 143 154)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/c7843172-09e9-4c84-8d8b-9e36fed5d8f0")
    (attr smd)
    (fp_text reference "R14" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp eadea057-473d-4e37-8985-65cdacde671d)
    )
    (fp_text value "2.2k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp ea663bf3-e968-4c88-b337-83185d522047)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 1d3504e6-02f4-407c-b644-8efdec39ba86)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 8806d6ae-19e3-4465-bf3b-a891d10384a6))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 94de928d-f43a-4cc4-bdc3-3168b525cfd7))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 1def6cf0-628c-48e2-abd4-7a201774f452))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 8e1873ce-ccb4-421e-a2a8-783371ca06f1))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 9f128694-0ceb-4581-80d7-81d95cb6f4b5))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp cf748d95-1c1b-4de5-8bc5-8df4c53a2a56))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 360777eb-2a87-4139-b94a-4f0fc45ef2c7))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 491dee5f-f83e-4d78-baac-750faabd4c4c))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 5de8362f-ae7c-4017-ade5-1b7775a84cec))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp a8623c18-8e18-4f84-bcbf-600cb0aed4e8))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(R13-Pad2)") (pintype "passive") (tstamp 07f662b5-c20f-4a5d-8cd9-77f31c4a447d))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(R14-Pad2)") (pintype "passive") (tstamp d9a27493-8ac5-4645-84bb-9e6847f47e4b))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Crystal:Crystal_SMD_MicroCrystal_CM9V-T1A-2Pin_1.6x1.0mm" (layer "B.Cu")
    (tedit 5D24C13B) (tstamp c42b5006-f4b0-409d-a515-1873d308e6ee)
    (at 169 135.4)
    (descr "SMD Crystal MicroCrystal CM9V-T1A series https://www.microcrystal.com/fileadmin/Media/Products/32kHz/Datasheet/CM9V-T1A.pdf, 1.6x1.0mm^2 package")
    (tags "SMD SMT crystal")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/3188079d-fd99-4090-8af4-8f4aa53c565d")
    (attr smd)
    (fp_text reference "Y1" (at 0 1.7) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 1837caf3-7fe3-483e-a7a9-2ea5ee517e80)
    )
    (fp_text value "32768Hz" (at 0 -1.7) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 1f247c34-0a27-44b5-aa54-7a3039ed43bd)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
      (tstamp 1b9cd306-1bd3-4644-ac3d-7b40cdd0974f)
    )
    (fp_line (start -0.1 -0.7) (end 0.1 -0.7) (layer "B.SilkS") (width 0.12) (tstamp 76bea174-0ea1-455a-b021-16c7cf6e3bc2))
    (fp_line (start -1.1 0.6) (end -1.1 -0.6) (layer "B.SilkS") (width 0.12) (tstamp 81464acb-805b-48c5-9131-2ab11c5c292a))
    (fp_line (start -0.1 0.7) (end 0.1 0.7) (layer "B.SilkS") (width 0.12) (tstamp ae2f132c-21fc-4cfe-8fba-deb49d04c627))
    (fp_line (start 1.2 -0.9) (end 1.2 0.9) (layer "B.CrtYd") (width 0.05) (tstamp 4896135f-9a21-4f0e-99a0-9a09d992db8e))
    (fp_line (start -1.2 0.9) (end -1.2 -0.9) (layer "B.CrtYd") (width 0.05) (tstamp 54a2fa9f-8b45-4429-9d76-23e167da01bc))
    (fp_line (start 1.2 0.9) (end -1.2 0.9) (layer "B.CrtYd") (width 0.05) (tstamp 853cc42e-4723-4367-a57e-f72273ac6389))
    (fp_line (start -1.2 -0.9) (end 1.2 -0.9) (layer "B.CrtYd") (width 0.05) (tstamp ae37a442-db3a-4a90-985a-05feac7170e8))
    (fp_line (start 0.8 -0.5) (end 0.8 0.5) (layer "B.Fab") (width 0.1) (tstamp 18d89673-0571-4f04-89b6-d7ed63ec8164))
    (fp_line (start -0.8 -0.5) (end 0.8 -0.5) (layer "B.Fab") (width 0.1) (tstamp 6158f42f-3f5b-4820-a484-a5bc69e61e4b))
    (fp_line (start 0.8 0.5) (end -0.8 0.5) (layer "B.Fab") (width 0.1) (tstamp 8c7ebcd7-e2bb-4cca-a405-6c030c5d891e))
    (fp_line (start -0.8 0.5) (end -0.8 -0.5) (layer "B.Fab") (width 0.1) (tstamp 94b1d9af-e849-4f22-ad49-e9f2163877cf))
    (fp_line (start -0.8 0) (end -0.3 -0.5) (layer "B.Fab") (width 0.1) (tstamp ecbe5f54-693f-4ab5-b548-c2f66f8d341a))
    (pad "1" smd rect (at -0.6 0) (size 0.6 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 80 "Net-(U6-Pad2)") (pinfunction "1") (pintype "passive") (tstamp 43dcb3e3-c7e3-402d-9650-d76d5cd4637f))
    (pad "2" smd rect (at 0.6 0) (size 0.6 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "Net-(C11-Pad2)") (pinfunction "2") (pintype "passive") (tstamp 0781190d-9e86-4489-bf64-a4508c48e1a4))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_MicroCrystal_CM9V-T1A-2Pin_1.6x1.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp c5e08c7e-db3c-4398-bb52-ecff9aea122e)
    (at 149.2 138 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/aabae4df-ada0-49e1-88d2-524812bcc349")
    (attr smd)
    (fp_text reference "C10" (at 0 1.16) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 04226619-25f5-4888-ad27-e1ebd9da7260)
    )
    (fp_text value "100nF" (at 0 -1.16) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d083ab07-0b7a-4d2d-9631-f25534bebe9e)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
      (tstamp 485114c1-473b-44c4-b2c7-1b46300051b6)
    )
    (fp_line (start -0.107836 -0.36) (end 0.107836 -0.36) (layer "B.SilkS") (width 0.12) (tstamp 2bef97ab-35cf-4bab-8774-fc1dcdf02834))
    (fp_line (start -0.107836 0.36) (end 0.107836 0.36) (layer "B.SilkS") (width 0.12) (tstamp 4b185791-e04f-4147-b794-5389e8cab64c))
    (fp_line (start -0.91 -0.46) (end -0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 09696426-25b8-45d9-a69c-d73c34f7e8ba))
    (fp_line (start 0.91 0.46) (end 0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 715e7338-ee11-482b-8bbe-7a1c583ac087))
    (fp_line (start 0.91 -0.46) (end -0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp ae0a5aac-80d1-434a-b9a2-e0d87beb49dd))
    (fp_line (start -0.91 0.46) (end 0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp ff967518-0d0f-40b5-85e0-af862e63a8f0))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 31d3294e-f4ae-43cf-aa10-681044030ef3))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 352dc4da-0e58-47e3-b153-c8b56067ffd2))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 60fc4256-83b7-4913-8120-741d1d08a0d5))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 8c1546ff-b5ee-439e-b839-0bd6a7697aa5))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(C10-Pad1)") (pintype "passive") (tstamp 1a64fe25-350c-4fbb-a989-e104f0d518f7))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 611414ed-8ef1-44b2-b12c-f94b55c49730))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (tedit 58645DC7) (tstamp c75ce1de-807a-44c9-add0-7205ae600acb)
    (at 169 123.2 180)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/88ac2693-582e-4101-9907-13f627fe32f7")
    (attr smd)
    (fp_text reference "D5" (at 0 2) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7412f750-3d49-4737-ae2a-dae74cc1fde4)
    )
    (fp_text value "RBR2MM30BTR" (at 0 -2.1) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e7d40930-f99e-46a7-915f-6ae6f35b2eb3)
    )
    (fp_text user "${REFERENCE}" (at 0 2) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2ddf2e49-d6e6-4406-b45d-dc3efd97a102)
    )
    (fp_line (start -2.25 1) (end 1.65 1) (layer "B.SilkS") (width 0.12) (tstamp 1c5e42be-34db-45a1-9748-c7f7944bea97))
    (fp_line (start -2.25 -1) (end 1.65 -1) (layer "B.SilkS") (width 0.12) (tstamp 1d717c38-c9c8-4f04-bd0d-8538b865d85a))
    (fp_line (start -2.25 1) (end -2.25 -1) (layer "B.SilkS") (width 0.12) (tstamp 5b50c1cd-8e32-4f17-94a9-fc98ee0f2a17))
    (fp_line (start -2.35 1.15) (end -2.35 -1.15) (layer "B.CrtYd") (width 0.05) (tstamp 2bbcee5a-a3cb-48b8-b971-055d0fbc7081))
    (fp_line (start 2.35 -1.15) (end -2.35 -1.15) (layer "B.CrtYd") (width 0.05) (tstamp 8c0a52d0-5d42-48eb-a8b2-f041ab492944))
    (fp_line (start -2.35 1.15) (end 2.35 1.15) (layer "B.CrtYd") (width 0.05) (tstamp b344164d-174c-4758-9a87-4f78e2b0bb7b))
    (fp_line (start 2.35 1.15) (end 2.35 -1.15) (layer "B.CrtYd") (width 0.05) (tstamp bd31f8c3-1cf5-4d35-a4ed-c60d2400f006))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4) (layer "B.Fab") (width 0.1) (tstamp 006c1a0a-6d96-449f-aca8-a7e2526f70e5))
    (fp_line (start 1.4 -0.9) (end -1.4 -0.9) (layer "B.Fab") (width 0.1) (tstamp 1268c09a-b5f5-4801-95ea-be5482da7274))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer "B.Fab") (width 0.1) (tstamp 1ffebe54-5632-47f3-85de-665491e33338))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer "B.Fab") (width 0.1) (tstamp 40f67971-dc80-4dc6-921c-ac4074511bae))
    (fp_line (start -0.35 0) (end 0.25 0.4) (layer "B.Fab") (width 0.1) (tstamp 5695161b-5f5b-48d1-b529-defa0d0623ae))
    (fp_line (start 0.25 0) (end 0.75 0) (layer "B.Fab") (width 0.1) (tstamp 600e5226-9f72-46c4-9a9d-1d4e2f2db054))
    (fp_line (start -1.4 -0.9) (end -1.4 0.9) (layer "B.Fab") (width 0.1) (tstamp 699f3ad0-b286-4f56-ad18-4aebda3518a3))
    (fp_line (start -1.4 0.9) (end 1.4 0.9) (layer "B.Fab") (width 0.1) (tstamp 9665d5ce-4f48-4042-9653-f3b3bed29351))
    (fp_line (start -0.75 0) (end -0.35 0) (layer "B.Fab") (width 0.1) (tstamp a813361c-d52a-4e2f-84a3-bf1b7719099d))
    (fp_line (start 0.25 -0.4) (end -0.35 0) (layer "B.Fab") (width 0.1) (tstamp ae79e0af-e3bd-4feb-82b5-ab99d3ab4c99))
    (fp_line (start 1.4 0.9) (end 1.4 -0.9) (layer "B.Fab") (width 0.1) (tstamp c0c3716f-78e8-4f8b-b67c-d926f80f3bf7))
    (pad "1" smd rect (at -1.65 0 180) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "/WiFi_Display/PREVGH") (pinfunction "K") (pintype "passive") (tstamp 71607f2e-2e25-4173-9e4e-9f171084a245))
    (pad "2" smd rect (at 1.65 0 180) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "Net-(C22-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 01338a16-3eb3-4d7a-b3a2-e8ec3c9e669c))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958) (tstamp cc0cb76a-7a54-4836-bcc4-75c47c58b45d)
    (at 157.2 122.5 90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/eeea116b-6c1f-4db6-8810-b1e60195ce6b")
    (attr smd)
    (fp_text reference "U7" (at 0 2.4 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp fd6a64fc-725b-45dc-b039-b5d77f88d379)
    )
    (fp_text value "AP2138N-3.3" (at 0 -2.4 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 3c2ed0de-9147-4227-af97-946ece1c5fc8)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 0.32 0.32) (thickness 0.05)) (justify mirror))
      (tstamp 67d8dd9c-3958-4867-b14d-9b577f0bd180)
    )
    (fp_line (start 0 -1.56) (end 0.65 -1.56) (layer "B.SilkS") (width 0.12) (tstamp 06e4180b-088b-4718-82eb-ce07a002ac15))
    (fp_line (start 0 1.56) (end 0.65 1.56) (layer "B.SilkS") (width 0.12) (tstamp 0ede8e28-6ea3-42ae-a4f7-bbf4d3023452))
    (fp_line (start 0 -1.56) (end -0.65 -1.56) (layer "B.SilkS") (width 0.12) (tstamp b604785c-0f88-488a-be35-b335f9e37e7d))
    (fp_line (start 0 1.56) (end -1.675 1.56) (layer "B.SilkS") (width 0.12) (tstamp f7158098-7385-4521-a8aa-1256ec2df9eb))
    (fp_line (start 1.92 1.7) (end -1.92 1.7) (layer "B.CrtYd") (width 0.05) (tstamp 17712ddd-9c13-4f33-a7be-a2a6ec6b3f95))
    (fp_line (start -1.92 1.7) (end -1.92 -1.7) (layer "B.CrtYd") (width 0.05) (tstamp 5135e8df-7e74-46a8-a777-167dccb5d542))
    (fp_line (start -1.92 -1.7) (end 1.92 -1.7) (layer "B.CrtYd") (width 0.05) (tstamp d590fe94-46f0-42cd-ae08-feeb91d4fcda))
    (fp_line (start 1.92 -1.7) (end 1.92 1.7) (layer "B.CrtYd") (width 0.05) (tstamp e50f7fc6-6235-4df8-a06d-4588fd9842c0))
    (fp_line (start -0.65 -1.45) (end -0.65 1.125) (layer "B.Fab") (width 0.1) (tstamp 1cb99dfe-879c-4279-b59d-81ee3ebcd546))
    (fp_line (start -0.325 1.45) (end 0.65 1.45) (layer "B.Fab") (width 0.1) (tstamp 29e23020-4261-4dff-9564-ee74ffecedd2))
    (fp_line (start 0.65 1.45) (end 0.65 -1.45) (layer "B.Fab") (width 0.1) (tstamp 869c96a1-994b-4d7e-b943-4a145aa54793))
    (fp_line (start -0.65 1.125) (end -0.325 1.45) (layer "B.Fab") (width 0.1) (tstamp 88451ac7-ac41-458b-8c5e-66275395cb88))
    (fp_line (start 0.65 -1.45) (end -0.65 -1.45) (layer "B.Fab") (width 0.1) (tstamp d9ab9d33-f471-414f-aab8-462fe935985c))
    (pad "1" smd roundrect (at -0.9375 0.95 90) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp ea49a98d-c682-40c1-9215-465120995447))
    (pad "2" smd roundrect (at -0.9375 -0.95 90) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pinfunction "VO") (pintype "power_out") (tstamp 581b4931-b434-45d1-bde8-5177d004138c))
    (pad "3" smd roundrect (at 0.9375 0 90) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "VCC") (pinfunction "VI") (pintype "power_in") (tstamp cd8be2eb-2a57-448a-83c3-8ad6ec8f7570))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp d0779e40-520e-471b-89ac-ea7040f7e1f6)
    (at 149.83 135.35 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/ebb9c173-6f5b-447b-9537-a03e95b5677a")
    (attr smd)
    (fp_text reference "C9" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e7884167-8512-44e0-8819-30d4880b187c)
    )
    (fp_text value "10uF" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 11ad9709-4518-4ce2-b71c-41f4fcb4a3c2)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp e1f49355-a385-46cb-96a2-f204758ad01e)
    )
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp a8ce6962-d18e-4b6e-a1cd-4d75be3fce5a))
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp f81be49b-b844-42a1-b180-26bf994c9d31))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 00f125db-bace-4121-aa8f-d61623e2b433))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 264b94b2-4432-4f33-973d-adc7c58da56c))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 61b171d2-3162-49f2-92c2-ce03705d7f2c))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp e090a7e0-a0b5-44a3-bc31-9aac2b32e7d0))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 78d97ed3-3636-4d3a-97f2-342386f91e83))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 9db60c82-1e52-4b96-bfdc-c49b0d234743))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp d5db6cb4-d6d4-47fe-b3f4-2dcca45bd784))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp ec0b01de-f3f3-48b8-bcac-9f46e8a9c824))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(C10-Pad1)") (pintype "passive") (tstamp a1bf8cfd-8cf4-48a7-839c-a9bc64c2e5de))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp fd39150e-2916-4d5e-a06e-7355538ba587))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp d1d46201-6542-4bb3-a935-ea07874f4acb)
    (at 183.3 111.125 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/15b9af59-26c6-4279-a932-10b52b9e4eb4")
    (attr smd)
    (fp_text reference "C16" (at 0 1.43 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d70b983b-fe61-46ff-9258-5f01b1bfce01)
    )
    (fp_text value "10uF" (at 0 -1.43 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 76f95e66-2ea2-4a9f-b41a-9257f6564053)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 5e01e43c-22fa-4067-aef5-9b242a08ae00)
    )
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp 254cb0c1-7628-4809-8254-8de90637ac9d))
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp e6ea6861-273e-424d-8094-6e3dd7db728e))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 419d302c-1e81-498d-a4f8-af5b8b59e608))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 57306889-91e8-485d-b426-eed7c5dbeac7))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp c95a8a1f-7d66-46f1-9963-e9557edc6d98))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp e51c4103-4a88-41a2-9da7-b6a7dbce4efb))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 49620c81-8b74-41c2-9d73-8306fb818b6b))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 53d2145d-8f41-431d-93ff-d610536b2ae8))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 8700df72-060a-4218-ac1b-a077b6586b1b))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp fc812942-17d7-48dc-bd0a-61cfe4f36591))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "/Power_Management/PS_SWITCH") (pintype "passive") (tstamp 79d816c2-bbf5-4dc8-9aeb-a81ae29f8762))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 007c816b-5017-488f-bb66-0810c1b00510))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "OptoDevice:Lite-On_LTR-303ALS-01" (layer "B.Cu")
    (tedit 5B870A3B) (tstamp d92555c6-6ec1-43cc-a6f9-7f05df037f76)
    (at 134 140)
    (descr "ambient light sensor, i2c interface, 6-pin chipled package, http://optoelectronics.liteon.com/upload/download/DS86-2013-0004/LTR-303ALS-01_DS_V1.pdf")
    (tags "ambient light sensor chipled")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/2794166c-ea3e-4417-9ece-5f24c5d9bfc2")
    (attr smd)
    (fp_text reference "U4" (at 0 2.025) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 3e47b3b8-8822-4ee9-b73e-cce87ac4c009)
    )
    (fp_text value "LTR-303ALS-01" (at 0 -2.025) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2d93b6bf-c885-477b-b193-1bd3cc24142d)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 2c598f4c-b0e8-409f-be3f-dc73c089fb73)
    )
    (fp_line (start -1.2 1.1) (end 1 1.1) (layer "B.SilkS") (width 0.12) (tstamp 59a6a3bd-1fb7-407e-b593-866a86265055))
    (fp_line (start -0.98 -1.1) (end 0.99 -1.1) (layer "B.SilkS") (width 0.12) (tstamp c7bebe46-a021-415d-8fb9-06b9206f747a))
    (fp_line (start -1.48 -1.25) (end 1.48 -1.25) (layer "B.CrtYd") (width 0.05) (tstamp 011d08ed-b717-4d5d-874c-5d976b6b0ee9))
    (fp_line (start -1.48 1.25) (end -1.48 -1.25) (layer "B.CrtYd") (width 0.05) (tstamp 6f6d251d-d120-4eff-9fae-23747d5a5353))
    (fp_line (start 1.48 1.25) (end -1.48 1.25) (layer "B.CrtYd") (width 0.05) (tstamp 8dafb58f-473e-4973-9048-c82590b8ca04))
    (fp_line (start 1.48 -1.25) (end 1.48 1.25) (layer "B.CrtYd") (width 0.05) (tstamp bd7aeb04-726e-4c38-9fa8-137ad93094a2))
    (fp_line (start -1 0.5) (end -0.5 1) (layer "B.Fab") (width 0.1) (tstamp 737a4484-60ea-4c83-9301-e4790c8b687b))
    (fp_line (start -0.5 1) (end 1 1) (layer "B.Fab") (width 0.1) (tstamp 8a7df68a-5011-43d3-a205-2b5fc1c9d3d0))
    (fp_line (start 1 -1) (end -1 -1) (layer "B.Fab") (width 0.1) (tstamp 99981404-ba5a-4953-84c8-f98edaa0002c))
    (fp_line (start -1 -1) (end -1 0.5) (layer "B.Fab") (width 0.1) (tstamp dc09973f-454c-4bf8-8be9-ddbcb601c462))
    (fp_line (start 1 1) (end 1 -1) (layer "B.Fab") (width 0.1) (tstamp de7d253c-b7e9-4cb2-adc1-891f593a32ac))
    (pad "1" smd roundrect (at -0.9 0.65) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pinfunction "VDD") (pintype "power_in") (tstamp af9a8237-0ee1-4977-864e-dc474f959004))
    (pad "2" smd roundrect (at -0.9 0) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 107 "unconnected-(U4-Pad2)") (pinfunction "NC") (pintype "no_connect") (tstamp 05881c8c-4a37-4b18-8f37-a81ebb0d0a32))
    (pad "3" smd roundrect (at -0.9 -0.65) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 76dbeade-c98c-47c1-984c-3b33096292e7))
    (pad "4" smd roundrect (at 0.9 -0.65) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 42 "/Sensor_Controller/I2C_SCL") (pinfunction "SCL") (pintype "input") (tstamp 843cd14d-b528-4fb5-ab9a-69203f7a8a29))
    (pad "5" smd roundrect (at 0.9 0) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 71 "/Sensor_Controller/ALS_INT") (pinfunction "INT") (pintype "open_collector") (tstamp 60975524-5518-4d46-bf75-20cc6f4bf38b))
    (pad "6" smd roundrect (at 0.9 0.65) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 41 "/Sensor_Controller/I2C_SDA") (pinfunction "SDA") (pintype "bidirectional") (tstamp 3dd0f7fe-153c-43f9-a771-dbc2c1a86da7))
    (model "${KICAD6_3DMODEL_DIR}/OptoDevice.3dshapes/Lite-On_LTR-303ALS-01.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp db0cad29-d5b4-4042-923f-90eb33243281)
    (at 149.22 139 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/4587f5f5-a764-48df-9175-19439dd1a2f8")
    (attr smd)
    (fp_text reference "C8" (at 0 1.16) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 105b8712-cfab-4472-80f6-459c303252c1)
    )
    (fp_text value "100nF" (at 0 -1.16) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 93e163fb-67b5-424a-a27b-a1f598441601)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
      (tstamp 6f66347e-c936-47e1-9ed0-a7df9871bfc8)
    )
    (fp_line (start -0.107836 -0.36) (end 0.107836 -0.36) (layer "B.SilkS") (width 0.12) (tstamp cf0ae319-a225-4172-9f72-ae0344622c78))
    (fp_line (start -0.107836 0.36) (end 0.107836 0.36) (layer "B.SilkS") (width 0.12) (tstamp dd64d6cd-8a39-427d-b861-81a487d95394))
    (fp_line (start 0.91 0.46) (end 0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 2ef3d7b8-7f1e-40d4-9c64-fee4bf73042a))
    (fp_line (start 0.91 -0.46) (end -0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 4834122e-48f3-4be3-90ec-5d1e539ff2dd))
    (fp_line (start -0.91 0.46) (end 0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 74bff41b-4382-4d73-a6cf-dcff051783dc))
    (fp_line (start -0.91 -0.46) (end -0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp f46cd10b-5e28-4d28-b932-c32e08c63720))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 07dad92f-d0dd-4932-9d92-95fae53cb41a))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 4789d63c-ad71-4bbf-92e0-2202cc4c3ed7))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 4aa58b94-1219-4578-bda1-6477cea774aa))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp c5563eac-9a46-4da5-a1ff-e4b5398c34f3))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp cd37aaf7-ead1-4f22-b9dc-cc73bf95816a))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 95da2d17-9cf9-4e8a-8324-2fcb5e131bc0))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp dbd9500c-3387-426f-8a3e-f88ba54b2224)
    (at 131.4 111.2)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/8ae4a0ac-8d10-4bb4-a45e-465633fe5f14")
    (attr smd)
    (fp_text reference "R33" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f6445a46-cbbd-4944-ace4-a17dd0475aec)
    )
    (fp_text value "10k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 225a58dd-172c-4fe1-a01a-ec8834ec00f0)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 42225565-0bfa-442f-a4c3-d64d32d3a082)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 113a24ff-1cfa-4394-8b37-8bc4f9f9cc45))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp d3c4b7cc-5681-4ce3-aa61-8971052412d5))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 1792e912-a152-47e1-90bd-37c9599c96e6))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 20beee87-1207-4f3c-a036-92e7b4f4e154))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 4b1e0c77-14f6-4012-82db-919482bf2b13))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 8b9270d9-f54a-4c3f-a57a-1781c65bda88))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 4f3ffe5a-2bcd-49dd-a3cf-e46ccce1d7e9))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 7705c5c7-26ca-478e-8861-26e123043306))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp c14b0969-c100-40d4-ac02-407ec9867b7c))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp f5101fb9-f8b3-4a9c-b89c-d6d8b3578a24))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "VDD") (pintype "passive") (tstamp dfe05bf8-d140-4c15-aadb-5cb8176a244c))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(C20-Pad1)") (pintype "passive") (tstamp 3cb7e6f3-fcfa-472d-a245-cb7d2568c70e))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp dc48003d-04ce-4b15-9fdb-e4e9d720db75)
    (at 155.4 110.2 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/b08657b1-8687-4bb6-a8ff-1c55f5e08bd1")
    (attr smd)
    (fp_text reference "C5" (at 0 1.16) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f5478b06-d44e-422c-9c4b-89061deb1e93)
    )
    (fp_text value "100nF" (at -0.1 -1.7) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7364e5e5-fdb5-488d-9ead-a9c83b1e6a31)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.04)))
      (tstamp dfec3404-1d8e-426d-9ffb-4206644d9c41)
    )
    (fp_line (start -0.107836 0.36) (end 0.107836 0.36) (layer "B.SilkS") (width 0.12) (tstamp 636051ce-38ed-49b1-9883-6f874a85c68a))
    (fp_line (start -0.107836 -0.36) (end 0.107836 -0.36) (layer "B.SilkS") (width 0.12) (tstamp cfce1db3-bca9-4728-8f4f-38d502f6ae88))
    (fp_line (start 0.91 -0.46) (end -0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 0d8c772e-a203-48c5-82e1-d6d79a17c36b))
    (fp_line (start 0.91 0.46) (end 0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 35102d9f-338a-4d5b-8d08-f29263f73e95))
    (fp_line (start -0.91 -0.46) (end -0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 817e0100-922b-48d4-8370-42f0a140842b))
    (fp_line (start -0.91 0.46) (end 0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp cdc5493e-d7fc-4a95-8fd1-fa52d9d20c87))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 21102843-5fec-49d8-97c0-f3b1d0191941))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 3fcb6bb1-8d0c-4b8b-bd6a-3a62aef4be56))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 6a964822-311f-4986-8c1b-90e9f956ae6f))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 9458a226-eab3-4562-935c-18b82fbea34c))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/Sensor_Controller/LPC_~{RST}") (pintype "passive") (tstamp ea9aa488-a527-4455-a981-f359550b1e1e))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp a98fd498-72ac-4c65-b5d0-62aefab99587))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp de29cb86-9ec3-47d2-84f9-ba1975e2c788)
    (at 148.5 154)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/835995d5-bcf4-4fa4-aa55-eb4b8b467ea5")
    (attr smd)
    (fp_text reference "R15" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 237b1e1d-800f-47e4-b02d-a342d4463833)
    )
    (fp_text value "2.2k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 079a7835-1b5d-4d2f-8184-31c5030c4f00)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 54163ee5-172c-4924-a381-5503bb612140)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 2d13ece1-6bc8-45e9-8c2c-aff107caec15))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 4f2eebc9-3f64-4151-a32e-e77a983875e7))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 4833f014-e8bc-411b-9735-cc15eadac5ba))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 71d89df0-b80a-4225-9d48-96eb71055456))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp a76aeba2-e9da-4392-97fe-e42d4c901582))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp ac24a6d4-c63b-451b-917e-8fdcd8b0ffbe))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 3393f562-549c-4e8a-b48a-f0054a9f6f63))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 798ea727-f919-4a63-af49-99dd7560d47e))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 8aec5469-eca5-4f03-b735-ba228cc2567f))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp fc6fa1f6-a65c-43ed-aecf-0e80f0996805))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(R14-Pad2)") (pintype "passive") (tstamp 80fe6ff0-fb09-4fb5-b386-dbddefde99cf))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 51 "/Sensor_Controller/CAPT_X2") (pintype "passive") (tstamp ee796564-42f2-4766-a508-475bc6da402c))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp df91479e-4e3f-4f38-bc03-f13c316483d8)
    (at 174.9 121.1)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/4fe6e85d-d828-45ba-aa29-de22abbbb051")
    (attr smd)
    (fp_text reference "C25" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 615335ff-6dbf-4cbc-863b-f85fe38fc0b6)
    )
    (fp_text value "1uF/50V" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7558174c-9e6a-4309-9eb2-2e147989eb76)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 76c49579-17c4-4617-8117-7d8981ea4281)
    )
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp 573e52aa-45ce-4870-b566-61e59995b965))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp 9fe72bb8-d82d-4f9a-9c5e-caada695b36f))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 3bf00323-9d51-415b-9f41-7305e307ec56))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 4595c635-c085-4465-81f5-59224451cfd7))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 89866b86-9ebf-4c11-993d-58acea924933))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp dd9f5f84-18b0-461c-90d1-a9f154c4cefd))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 05ef6d66-f7d6-486c-8be8-87e79a36479c))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 634081fa-dcd1-41e7-8ab4-1a6738a8a264))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 959ff910-dd52-4d4e-b87a-d074bff99352))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp ccf2b39e-41e4-4dbd-9233-411fb27459a7))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp c66dd5f4-171e-4a35-afd5-bd69b4401e61))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 15 "/WiFi_Display/PREVGH") (pintype "passive") (tstamp 0f46cb1b-0601-4d84-9a9b-bc9616b2f62f))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (tedit 58645DC7) (tstamp e3d497ac-5ccc-4dfb-ac5d-446d2c8ecdc0)
    (at 169 118.4)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/803517bf-0db0-45b4-8f88-724fa4a8ce2c")
    (attr smd)
    (fp_text reference "D3" (at 0 2) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp dd178ae8-35fe-46c3-9c19-73f010517636)
    )
    (fp_text value "RBR2MM30BTR" (at 0 -2.1) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp eee3e58d-2199-4ece-a41a-5e2e9f19677a)
    )
    (fp_text user "${REFERENCE}" (at 0 2) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 92725e63-c029-4318-94a9-6b6fa365334e)
    )
    (fp_line (start -2.25 1) (end -2.25 -1) (layer "B.SilkS") (width 0.12) (tstamp 44730429-ec5f-416f-b29c-ffc21bb20ae3))
    (fp_line (start -2.25 1) (end 1.65 1) (layer "B.SilkS") (width 0.12) (tstamp 6e84eb4c-3f7e-4120-b8a6-a476e065ece7))
    (fp_line (start -2.25 -1) (end 1.65 -1) (layer "B.SilkS") (width 0.12) (tstamp c9e9ed2a-4bcb-46d1-9f26-b0d1c271bd0a))
    (fp_line (start 2.35 1.15) (end 2.35 -1.15) (layer "B.CrtYd") (width 0.05) (tstamp 2f9632a5-2ee0-46fc-8c8b-f6798022cf03))
    (fp_line (start -2.35 1.15) (end -2.35 -1.15) (layer "B.CrtYd") (width 0.05) (tstamp 5a9fcad6-3bc1-4fdd-b744-9589f3304922))
    (fp_line (start -2.35 1.15) (end 2.35 1.15) (layer "B.CrtYd") (width 0.05) (tstamp 9e1c60e4-2d91-42cd-8243-cb7a543ec049))
    (fp_line (start 2.35 -1.15) (end -2.35 -1.15) (layer "B.CrtYd") (width 0.05) (tstamp ef2d9b3b-9c3a-4cbc-8fda-0529dabc4622))
    (fp_line (start -0.35 0) (end 0.25 0.4) (layer "B.Fab") (width 0.1) (tstamp 0ef09064-c5a3-4ad1-a766-68544e4876d0))
    (fp_line (start 1.4 0.9) (end 1.4 -0.9) (layer "B.Fab") (width 0.1) (tstamp 17dba404-b339-4694-a399-d16f126e4711))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4) (layer "B.Fab") (width 0.1) (tstamp 21d0f766-77fc-475f-be80-91803ce874b8))
    (fp_line (start 1.4 -0.9) (end -1.4 -0.9) (layer "B.Fab") (width 0.1) (tstamp 21fb1250-dfa4-4016-8f6a-2f5507e99478))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer "B.Fab") (width 0.1) (tstamp 3df36ddf-35f5-45c0-b9b1-9d8de0bbd39a))
    (fp_line (start -1.4 -0.9) (end -1.4 0.9) (layer "B.Fab") (width 0.1) (tstamp 5d2feb08-36eb-4fb3-bbf3-b990b000c871))
    (fp_line (start 0.25 0) (end 0.75 0) (layer "B.Fab") (width 0.1) (tstamp 65aacbd9-45c7-470f-9c5b-d1da638d9b27))
    (fp_line (start -0.75 0) (end -0.35 0) (layer "B.Fab") (width 0.1) (tstamp 6f7f023b-ae5b-4cc2-b52f-d53115880909))
    (fp_line (start 0.25 -0.4) (end -0.35 0) (layer "B.Fab") (width 0.1) (tstamp 72428f87-4d65-4a2c-a9ac-2b0f9a5b9bcc))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer "B.Fab") (width 0.1) (tstamp c12f57c0-16e0-4778-b255-dd9c227bf43c))
    (fp_line (start -1.4 0.9) (end 1.4 0.9) (layer "B.Fab") (width 0.1) (tstamp eaad3188-ac86-426a-a6f1-4ef6f8f61924))
    (pad "1" smd rect (at -1.65 0) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "Net-(C22-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 5af199ff-0acb-46e0-8827-2362706c5b63))
    (pad "2" smd rect (at 1.65 0) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "/WiFi_Display/PREVGL") (pinfunction "A") (pintype "passive") (tstamp c0e5446b-fe43-4faf-b34d-ff77a8c740c2))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp e49bb379-7a56-4797-b30b-8b170deba133)
    (at 161 123.45 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/85017d16-d3bb-44bf-aadb-a6eda059e74e")
    (attr smd)
    (fp_text reference "R24" (at 0 1.17 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp eb431cdf-d560-4bad-b676-37ca4bf27eab)
    )
    (fp_text value "100k/1%" (at 0 -1.17 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e8f0f4d7-7b6b-435e-b4d2-414f7adb3b81)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp acc3db9c-55fe-4748-a33c-248ec85d059c)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp aa3a7e91-f166-4fb4-bbf8-3a831f57e355))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp edab3239-79f2-4f60-872b-7b97dc512b2c))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 0f1a85f6-1a5f-46ea-8d0e-0665cf7e429e))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 7aecbfaa-345f-4b06-88aa-e1026e14f953))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp af2e2197-9b5b-4988-8f99-a5f54b292204))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp fc818b09-5cf6-44b3-b29e-180e1008d870))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 17794b82-7fdd-47b2-b3c7-e248cf949241))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 7afb269d-e672-43b5-87d0-a4dac4788177))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 803a35aa-4565-451a-97cb-c90792002c3d))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp ef89a8de-a294-42bb-a5ea-78fd00ed3860))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 59 "/Power_Management/ADC_BAT") (pintype "passive") (tstamp 3efc3c21-4727-494e-a82d-02c17e8cdc9b))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 02a7582e-565b-41fa-98a7-4f51033fd776))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp e5f9678e-717c-40e3-ad3a-730d36c2169e)
    (at 174.9 116.4)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/5a64bddd-8972-49cf-93e2-52fb528d00cd")
    (attr smd)
    (fp_text reference "C32" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7f05cb7d-9b3c-4a20-9aef-9e06f672fb00)
    )
    (fp_text value "1uF/50V" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp c453cb26-d4a1-4172-a7e0-9171a28f3191)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp b2b5cebf-6b5d-4ee4-9d99-5eda6fae18d4)
    )
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp 130ab62f-6513-4e4b-97ed-77ceacd5341c))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp f205fc23-e243-43e4-8bba-8a3bed145bc8))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 0f7932f8-4229-4827-b836-13689fd08d9d))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 8a42ec5d-36a4-41b1-ac2b-b6825ea68cdb))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp de4cd396-6459-42cf-8968-f2c3d97e239b))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp ffb433d3-768a-439f-88c6-ce530b8c354e))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 0cae9b3c-c631-4af1-9a77-44a92170611c))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 3e07c77e-a28c-4fcb-a6c6-5e604eed3be5))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp df7c98df-1594-400a-9c3c-4b16c630ccb3))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp e2f166fd-6468-43d6-8b3e-2157a088b59f))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp f0b71bc9-bf8e-4e6e-b6b9-67a2fa4187a1))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(C32-Pad2)") (pintype "passive") (tstamp d9bd8f67-b983-47e6-84ef-7c72a882a883))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp e7357d35-7fcf-49cb-8a5f-057ca79309e6)
    (at 167.1 127.8 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/7f9dfaad-2be6-41c1-a167-4ccb4287e8d1")
    (attr smd)
    (fp_text reference "C21" (at 0 1.43 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 04cc55be-ab45-4b31-9e10-41456aac48e3)
    )
    (fp_text value "4.7uF" (at 0 -1.43 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a16cd7f7-8f55-4f19-b8c3-49e5c217510c)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp aad3eaf6-5324-4782-868e-17f9ab91e63a)
    )
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp 274fa3eb-85d7-4199-b2b0-fe2457891cf0))
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp d91812d1-f8ee-40e0-baa4-a7e45f4ed8b2))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 7b9bb1e8-87bf-4fb4-a604-5d4f2d8c859e))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 8e1bf26b-f3cf-4f87-805e-98a2abf976e3))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp b883cb68-98c1-4d09-85a2-783c7c50cc39))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp e2140fcd-b0ec-4724-830b-6988c9eae874))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 6b49e2c3-c7cf-48fa-b15a-0024c51fb02e))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp a2934e60-f7f2-4afa-8648-b887bffc8556))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp bcb2b53a-b6cc-40e8-bf3a-7676efb243a4))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp dc2ddfbd-54b4-4b74-ae4e-ea5d769aa23b))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "VDD") (pintype "passive") (tstamp efc1a00e-835b-4294-96b1-74b95182f22d))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 7c6a9e2b-7dc4-43e1-9215-ac630e359a1d))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp e8d95a4b-4e79-4665-9cd0-526fa97605fe)
    (at 165.8 119.3 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/349bfb54-48d8-41e2-b24c-d550bd415c38")
    (attr smd)
    (fp_text reference "C22" (at 0 1.43 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d62ef6e7-2947-42de-92e0-07d662b95ece)
    )
    (fp_text value "4.7uF/50V" (at 0 -1.43 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7e37d067-abad-4c7f-a073-e6038a14f7f2)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp afd29a84-a551-4a13-85bf-b0a0df79c45b)
    )
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp 0c4a3a74-710d-49bc-83db-ea1e9e14b1aa))
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp ea9c60b1-04fd-4bcb-bc53-87e42bf89dd8))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 15ecc3e0-f2d9-4b23-92f8-7542608740e6))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 7f494ad1-052a-4629-9a38-e059f1b86cf0))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp ae7bae80-ca24-4255-9efd-49e58cf75470))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp ef725b0d-6086-4969-be0c-9f96b1136583))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 1c3c37df-b2af-424e-b329-2311b9f6ceb3))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 6a2ae24b-989a-478a-a7af-fca8cdd572d2))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp a1296481-78c3-4459-9b1a-79eb4c946d28))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp d4b40bc3-cbb2-451a-b8b5-590a1865577d))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(C22-Pad1)") (pintype "passive") (tstamp c6c40cbf-24f1-4e78-9a8a-5696843a00c8))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(C22-Pad2)") (pintype "passive") (tstamp 7e2a1501-856e-476f-baa3-ff983bd28457))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp ebf8f570-88fc-4fd3-a501-cf28d4c817f3)
    (at 131.8 113.4 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/b86b9743-ef60-4657-98d6-63d95505d5e0")
    (attr smd)
    (fp_text reference "R31" (at 0 1.17 -270) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 96e848eb-cbb2-4e80-96aa-35920b23b692)
    )
    (fp_text value "10k" (at 0 -1.17 -270) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 1d4aa064-1faa-4873-a896-12f258279489)
    )
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 679e3123-f95e-476d-bed6-7a0a1c134dcf)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 2a1d940d-5d66-4861-a624-7f78bfc642a7))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp b29caf03-1a0f-4fb9-b116-0e6e41e05789))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 2c55f1e5-a766-4fbc-9e90-94d73ace501c))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 8a48a987-eccb-43b9-abc2-acdc30b7657b))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp d7521d5d-b3bb-4219-b362-e2f941108ad3))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp eac61aa0-c45d-44f4-94dd-7f58476b69ab))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 160d9f9f-bb8d-4313-b3c4-5712bb774fb8))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp b6113dd7-922a-4996-ae0c-775cbebc95a1))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp b87b3739-db9b-4692-9412-e5536f3eaaae))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp efa35552-45f4-4371-85c6-f1db360f7ab4))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "VDD") (pintype "passive") (tstamp 68aff084-5e59-4fd7-a170-f6995ef3e057))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "/WiFi_Display/EPD_D{slash}~{C}") (pintype "passive") (tstamp e9e4a1f1-1b6e-4f9c-bda1-7517144f2086))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp ebfb83f2-7f6a-48c0-aa12-324afcc3906a)
    (at 147.4 110.2)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/d520198b-2a40-455f-b648-af30bd40d0f3")
    (attr smd)
    (fp_text reference "R1" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5585e71f-19d2-41aa-b745-9015f24da9f1)
    )
    (fp_text value "100k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp b3f3204d-9da3-45f8-96ce-aba013599c74)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 58ec57e6-30f3-4898-9c94-a25039367e20)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 6a51d1cb-fe05-40b3-909d-40ef54b3a2ff))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 9f4861ba-74d9-400e-b7b0-093976c80ffd))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 08341754-4e3b-47a1-bee9-33ed00e29609))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 5b9a2ad0-27f4-4aba-9005-bc9d50b1903d))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp b857ba1e-2b45-4ab0-a721-ef9e56debfb5))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp f55662c9-ee3c-4471-ba9d-3c288d24f8ef))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 656533d3-9085-4585-92ff-aea2556ed9f5))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 8b911e8b-b489-41ed-8b13-f8ec364984ba))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 9d67ca75-27e4-46e6-b240-3423a91212c5))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp c89cd3c9-aee1-49d1-9483-7d6bc600aff3))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp 1cf79173-a21a-4ac5-94c6-e6b42bad8105))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 40 "/Sensor_Controller/LPC_~{ISP}") (pintype "passive") (tstamp 0c8ddc40-9c23-4bbb-be73-53f68312212f))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "B.Cu")
    (tedit 5F6F9B37) (tstamp ec092202-beea-46c9-800c-b66ce60e1791)
    (at 151.8 118.5)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/c8699d74-e891-4979-9162-ae2cd3da4c96")
    (attr smd)
    (fp_text reference "U10" (at 0 2.4) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp cb115414-1d88-46d3-9cc0-79b493a94487)
    )
    (fp_text value "TLV62568DBV" (at 0 -2.4) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7ae9ecc6-e30b-4e0a-a592-54b15cd9a9ec)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 78a41668-797b-4bc5-8ab3-c859b354fc63)
    )
    (fp_line (start 0 1.56) (end 0.8 1.56) (layer "B.SilkS") (width 0.12) (tstamp 11b9a787-fa42-477f-ab08-82e42f31c5a1))
    (fp_line (start 0 -1.56) (end -0.8 -1.56) (layer "B.SilkS") (width 0.12) (tstamp 613fde20-4257-4023-8467-093f42ed08de))
    (fp_line (start 0 -1.56) (end 0.8 -1.56) (layer "B.SilkS") (width 0.12) (tstamp ab73cb86-4065-4324-a54e-f95cf7c4bcc9))
    (fp_line (start 0 1.56) (end -1.8 1.56) (layer "B.SilkS") (width 0.12) (tstamp e6d9a129-40b7-4668-9a0a-b97394c23b61))
    (fp_line (start 2.05 -1.7) (end 2.05 1.7) (layer "B.CrtYd") (width 0.05) (tstamp 1e322f88-8d85-4bf0-9ce9-53d9a259c804))
    (fp_line (start 2.05 1.7) (end -2.05 1.7) (layer "B.CrtYd") (width 0.05) (tstamp 3aed1516-e9bd-4433-b979-d7f5857dc1da))
    (fp_line (start -2.05 -1.7) (end 2.05 -1.7) (layer "B.CrtYd") (width 0.05) (tstamp 5716862c-f02b-4b9b-ae46-feeaf91cd555))
    (fp_line (start -2.05 1.7) (end -2.05 -1.7) (layer "B.CrtYd") (width 0.05) (tstamp 80f6533a-62a4-4221-a03c-3ae80458636c))
    (fp_line (start -0.4 1.45) (end 0.8 1.45) (layer "B.Fab") (width 0.1) (tstamp 0937f0fa-9288-4efa-b18c-6b669dea8e7e))
    (fp_line (start 0.8 -1.45) (end -0.8 -1.45) (layer "B.Fab") (width 0.1) (tstamp 1ef20350-baca-4310-86ac-a0fc06dddc61))
    (fp_line (start 0.8 1.45) (end 0.8 -1.45) (layer "B.Fab") (width 0.1) (tstamp 87517563-5c5f-4d97-a050-41cdfaff7901))
    (fp_line (start -0.8 1.05) (end -0.4 1.45) (layer "B.Fab") (width 0.1) (tstamp bf11e403-5e7a-457a-bb5c-1ead516bfdc3))
    (fp_line (start -0.8 -1.45) (end -0.8 1.05) (layer "B.Fab") (width 0.1) (tstamp d10b8a2b-09df-4362-99de-7de739c35570))
    (pad "1" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 75 "/Power_Management/DCDC_EN") (pinfunction "EN") (pintype "input") (tstamp 3af36875-e1eb-437c-92f4-43adcad9be09))
    (pad "2" smd roundrect (at -1.1375 0) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp c2fc7f49-f56c-4e2f-a7f1-5f631b469775))
    (pad "3" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 82 "Net-(L2-Pad1)") (pinfunction "SW") (pintype "power_out") (tstamp 59a02827-d8b5-47d4-85d2-dc9f101a4d04))
    (pad "4" smd roundrect (at 1.1375 -0.95) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "/Power_Management/PS_SWITCH") (pinfunction "VIN") (pintype "power_in") (tstamp 5ce56aa5-cc59-4c39-b7c0-abc5838aab3b))
    (pad "5" smd roundrect (at 1.1375 0.95) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 60 "Net-(R27-Pad2)") (pinfunction "FB") (pintype "input") (tstamp bac226e1-e794-4824-8e4e-426fcf793a71))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp ec2e5c35-338b-4597-90f7-ca2929cbada6)
    (at 132 140.3 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/2e594ab1-4a99-4203-a5cc-e5c18959b1aa")
    (attr smd)
    (fp_text reference "C6" (at 0 1.16 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp fad4eecb-dc34-4615-999e-982028b89509)
    )
    (fp_text value "100nF" (at 0 -1.16 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f6da8172-f49e-4776-b23e-6436ed66f1c2)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
      (tstamp 9c3a1f32-ffe3-4744-bc4e-181903d775b7)
    )
    (fp_line (start -0.107836 0.36) (end 0.107836 0.36) (layer "B.SilkS") (width 0.12) (tstamp 09e20f31-1ca4-4e74-8acd-3e8e06c64a0b))
    (fp_line (start -0.107836 -0.36) (end 0.107836 -0.36) (layer "B.SilkS") (width 0.12) (tstamp 98d46e2c-1df6-4d63-a728-d33ab5e4047e))
    (fp_line (start 0.91 0.46) (end 0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 1f46248a-9695-4a68-93db-8e6169a1afdb))
    (fp_line (start 0.91 -0.46) (end -0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 46729c0a-dc6e-495d-9b5e-5d10cf19a0f7))
    (fp_line (start -0.91 0.46) (end 0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 952e7e7d-0ed6-4db3-96c2-972b248d94b6))
    (fp_line (start -0.91 -0.46) (end -0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp b04c81d3-f33b-4b11-ad93-ead91a3394fb))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 0ab5a12c-73a4-4481-bd69-27a0234781ff))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 112e69c5-e151-4b3e-b4f6-4290e8e0331a))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 13203af3-54b0-46aa-a995-7bf4ecaf7717))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp ec67697d-a698-44d2-8d0d-3fbd690e281c))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp 18137bf6-21e8-4eab-9c78-0b597edf0c9a))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 85520cf8-1112-41ef-92a9-80dc38e3bdd1))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp f43b9359-857e-4768-aefb-fbc77e8c5bce)
    (at 164.5 154)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/154b2b1b-f7bb-4fa8-8160-bc69fc4cb438")
    (attr smd)
    (fp_text reference "R18" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0b7fb85b-a072-4fcd-befd-3ea532afdf9b)
    )
    (fp_text value "2.2k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5961691b-180e-47bf-8a4e-e9657e479f34)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp a1d1dfb9-51b3-481c-a88e-41c49dc0bf2c)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 311f6c4a-294a-441b-a560-ac3491c7cb1e))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 8ffb7691-4dc2-4737-8f97-60f7cbc405d9))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 2b42e69f-f89a-42cf-a55c-0769c8c07b29))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 2e018315-787f-4a80-9c3b-e34d9840b6d3))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 4f4fc170-56c3-4e85-8dc0-d2038f232da3))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp cd28e71e-c994-43a1-b1e3-2c15cdb96716))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 5ffdfc1c-88f0-4f40-898d-52e01ec09286))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp d307b2a8-1e32-4572-8ed5-506b1d8615cc))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp db380dc8-f8b8-48c9-82cc-eef66980a9ec))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp df790381-cca8-4fe4-9ae5-2069aa52e7e1))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(R17-Pad2)") (pintype "passive") (tstamp f4c198df-bbd2-4bb1-b71c-1a5e4eddd0ff))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 54 "/Sensor_Controller/CAPT_X3") (pintype "passive") (tstamp 705ccafc-8293-418b-b385-f80269af9823))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp f53ef5e2-00a3-48ce-9544-8754764f1379)
    (at 171.8 125.3 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/e5fa1235-e15c-437f-b421-f08c168cc4c8")
    (attr smd)
    (fp_text reference "R34" (at 0 1.17 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e81271ea-8563-481e-896c-8668080e77da)
    )
    (fp_text value "2R2" (at 0 -1.17 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp cc1741a3-5bc8-4fc1-b725-b7332e241cd5)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 9efe1901-2b5b-4c95-b9ae-273fda0dcc56)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp e6cf4ff7-6502-4449-97ea-963ad9494e4b))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp e8fb340f-be19-4de1-8b9c-a40986fee97c))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 04636ec1-1951-47d8-bcd2-f0b05f1d5b91))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 13e54bc4-4061-422a-a82a-d97d5746d058))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp cd474a7e-8a8f-4461-90ed-f9f5760c3768))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp ebd8b1c8-28c8-4f36-a21a-4190a3a3acb9))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 46409daa-1802-4f79-8233-36629136b911))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 9b0be282-2f14-4006-990c-b8afc9debbfe))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 9d779d83-361b-4eb5-98cd-0f94f207aa1f))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp f42c8f76-027b-4d93-b4e7-741e764a4325))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "/WiFi_Display/RESE") (pintype "passive") (tstamp 67065ca4-ad04-45fc-9671-12948c7d5861))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 65bdce80-000c-444d-86dc-50d9a69900cc))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Button_Switch_SMD:Panasonic_EVQPUJ_EVQPUA" (layer "B.Cu")
    (tedit 5A02FC95) (tstamp f87f1538-9f33-494f-b7b3-fd491638b700)
    (at 142.4 107.4 180)
    (descr "http://industrial.panasonic.com/cdbs/www-data/pdf/ATV0000/ATV0000CE5.pdf")
    (tags "SMD SMT SPST EVQPUJ EVQPUA")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/a50f8db5-02b5-4d54-8a5b-d177fb2e3369")
    (attr smd)
    (fp_text reference "SW3" (at 0 4.5) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 8e5bf5b6-ab0d-4c10-99a6-66a869ef4ddb)
    )
    (fp_text value "EVQPUA02K" (at 0 -3.5) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 67bd2d66-095c-4208-a5da-6514a13def95)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp ee693f9a-2358-451f-ae36-8d5a7d561e97)
    )
    (fp_line (start -1.425 1.85) (end -2.35 1.85) (layer "B.SilkS") (width 0.12) (tstamp 037b5100-d0ab-4175-89a7-de47eb19572a))
    (fp_line (start 2.35 -1.85) (end -2.35 -1.85) (layer "B.SilkS") (width 0.12) (tstamp 04d67115-8487-4533-931a-8c62b677703f))
    (fp_line (start 2.35 1.85) (end 1.425 1.85) (layer "B.SilkS") (width 0.12) (tstamp 7454b6a8-b36e-437b-85db-9d9105d67284))
    (fp_line (start 2.45 -0.275) (end 2.45 0.275) (layer "B.SilkS") (width 0.12) (tstamp c04c2d5f-1f8d-4b25-9371-60485cd21fb5))
    (fp_line (start -2.45 -0.275) (end -2.45 0.275) (layer "B.SilkS") (width 0.12) (tstamp ebbc8062-991d-41c3-918c-79bbc961da3d))
    (fp_line (start 3.9 3.25) (end -3.9 3.25) (layer "B.CrtYd") (width 0.05) (tstamp 6d1507b2-e297-43a1-bc95-746fdb0b7a81))
    (fp_line (start 3.9 -2.25) (end -3.9 -2.25) (layer "B.CrtYd") (width 0.05) (tstamp 9bdfae59-deda-4d9d-ae1d-7822becf4854))
    (fp_line (start -3.9 -2.25) (end -3.9 3.25) (layer "B.CrtYd") (width 0.05) (tstamp a2bdec57-7a71-4a9b-ad3a-0cbb0e029415))
    (fp_line (start 3.9 -2.25) (end 3.9 3.25) (layer "B.CrtYd") (width 0.05) (tstamp d84c25aa-914a-4f96-93f2-3538a9645b51))
    (fp_line (start -1.3 2.75) (end -1.3 1.75) (layer "B.Fab") (width 0.1) (tstamp 03304a63-91a4-4b8d-bc74-206813b90c0a))
    (fp_line (start 2.35 1.75) (end -2.35 1.75) (layer "B.Fab") (width 0.1) (tstamp 07e249bf-f3bb-4438-a179-4da2fc4962eb))
    (fp_line (start 2.35 -1.75) (end -2.35 -1.75) (layer "B.Fab") (width 0.1) (tstamp 3b993a29-53b3-47d8-a7d2-97fafac0b1ef))
    (fp_line (start -2.35 -1.75) (end -2.35 1.75) (layer "B.Fab") (width 0.1) (tstamp 5b8dd6b4-bbb5-42a1-8062-6d5f367aae4f))
    (fp_line (start 1.3 2.75) (end 1.3 1.75) (layer "B.Fab") (width 0.1) (tstamp 91f8cd54-9ecb-494b-bf61-49d5041dcb54))
    (fp_line (start 1.3 2.75) (end -1.3 2.75) (layer "B.Fab") (width 0.1) (tstamp c289c873-3c00-47c4-8967-822d88216321))
    (fp_line (start 2.35 -1.75) (end 2.35 1.75) (layer "B.Fab") (width 0.1) (tstamp fd39594d-c8a6-461a-a3b4-228e9a0e2719))
    (pad "1" smd rect (at 2.625 0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive") (tstamp ed8ae13c-e62b-432c-b712-08ade7e209c4))
    (pad "1" smd rect (at -2.625 0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive") (tstamp f5eae70a-f52c-4328-9214-c3554ff628c3))
    (pad "2" smd rect (at -2.625 -0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 92 "Net-(SW3-Pad2)") (pinfunction "2") (pintype "passive") (tstamp 4267da53-13d8-47c0-960f-7b4459b0589b))
    (pad "2" smd rect (at 2.625 -0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 92 "Net-(SW3-Pad2)") (pinfunction "2") (pintype "passive") (tstamp a5fc1014-3082-465a-9f5b-283849b985f1))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/Panasonic_EVQPUJ_EVQPUA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Button_Switch_SMD:Panasonic_EVQPUJ_EVQPUA" (layer "B.Cu")
    (tedit 5A02FC95) (tstamp f9007fab-2e08-4532-9f22-40a0d60ceb70)
    (at 134.4 107.4 180)
    (descr "http://industrial.panasonic.com/cdbs/www-data/pdf/ATV0000/ATV0000CE5.pdf")
    (tags "SMD SMT SPST EVQPUJ EVQPUA")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/d89521b4-2b5f-4235-a4df-eae3d9fa2f04")
    (attr smd)
    (fp_text reference "SW4" (at 0 4.5) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp fab67ee8-a980-4270-a2c1-e911a56e453e)
    )
    (fp_text value "EVQPUA02K" (at 0 -3.5) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 55b1d32c-eccf-49f4-a90c-b398c03d8bac)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 833a34f8-b4db-45d9-9cbf-61d0f533f7cc)
    )
    (fp_line (start 2.45 -0.275) (end 2.45 0.275) (layer "B.SilkS") (width 0.12) (tstamp 23778edf-794c-4ff8-98d5-053d18fa5fd6))
    (fp_line (start -1.425 1.85) (end -2.35 1.85) (layer "B.SilkS") (width 0.12) (tstamp 2c1872ae-c97a-4951-9bfd-516fedc3d25c))
    (fp_line (start 2.35 1.85) (end 1.425 1.85) (layer "B.SilkS") (width 0.12) (tstamp 46c7a4b1-451e-40da-b6ec-1a119e375ddc))
    (fp_line (start 2.35 -1.85) (end -2.35 -1.85) (layer "B.SilkS") (width 0.12) (tstamp 56864517-629b-48de-9331-a01814d41fd9))
    (fp_line (start -2.45 -0.275) (end -2.45 0.275) (layer "B.SilkS") (width 0.12) (tstamp 70dc2e91-d9a9-4f37-94bb-26180ae68ce7))
    (fp_line (start 3.9 3.25) (end -3.9 3.25) (layer "B.CrtYd") (width 0.05) (tstamp 8b282d21-7c9a-4416-bec1-156c96375126))
    (fp_line (start 3.9 -2.25) (end 3.9 3.25) (layer "B.CrtYd") (width 0.05) (tstamp 9a0dda58-c117-49cc-b60c-ce510450d8c3))
    (fp_line (start 3.9 -2.25) (end -3.9 -2.25) (layer "B.CrtYd") (width 0.05) (tstamp dc2ccffc-45e8-4ed5-ae8d-655de2cfbd0a))
    (fp_line (start -3.9 -2.25) (end -3.9 3.25) (layer "B.CrtYd") (width 0.05) (tstamp ff1e80aa-5240-47a2-b700-e665f5f65b33))
    (fp_line (start 1.3 2.75) (end -1.3 2.75) (layer "B.Fab") (width 0.1) (tstamp 0da8d618-1786-47d0-8962-ca473cfa683c))
    (fp_line (start 2.35 -1.75) (end 2.35 1.75) (layer "B.Fab") (width 0.1) (tstamp 13a5edc3-9ba7-4935-8b00-b14ca8c9aafe))
    (fp_line (start 2.35 -1.75) (end -2.35 -1.75) (layer "B.Fab") (width 0.1) (tstamp 27e90440-f79d-4ae8-a709-3436349c4b97))
    (fp_line (start -2.35 -1.75) (end -2.35 1.75) (layer "B.Fab") (width 0.1) (tstamp 3bb9c5ab-0788-4979-9582-6f25a31909e8))
    (fp_line (start -1.3 2.75) (end -1.3 1.75) (layer "B.Fab") (width 0.1) (tstamp 708f28dd-1380-4191-b8c2-c33049c5b933))
    (fp_line (start 2.35 1.75) (end -2.35 1.75) (layer "B.Fab") (width 0.1) (tstamp 9436e234-4a73-4f25-8aa2-c383381e1bf9))
    (fp_line (start 1.3 2.75) (end 1.3 1.75) (layer "B.Fab") (width 0.1) (tstamp db43c00c-23d1-4dc2-8267-d16ee24c989a))
    (pad "1" smd rect (at 2.625 0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive") (tstamp 0ca9703b-4035-4655-8a27-cd9af7ec606d))
    (pad "1" smd rect (at -2.625 0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive") (tstamp 59f73f8e-fbd6-40d2-8786-3054233a8c57))
    (pad "2" smd rect (at -2.625 -0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 10 "Net-(C20-Pad1)") (pinfunction "2") (pintype "passive") (tstamp 83f0fbbb-e940-495d-8031-32c0e51ee852))
    (pad "2" smd rect (at 2.625 -0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 10 "Net-(C20-Pad1)") (pinfunction "2") (pintype "passive") (tstamp d13be004-795b-45f9-a9be-28410246a219))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/Panasonic_EVQPUJ_EVQPUA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Inductor_SMD:L_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEF0) (tstamp f92bf2e3-54c1-4ee4-8754-6ecb60d99de8)
    (at 180.8 107.6 180)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/ed113c5b-a828-44f6-9de0-3b3524d9275b")
    (attr smd)
    (fp_text reference "L1" (at 0 1.55) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp eba3525c-37e9-4ac4-af86-6fa63049cf98)
    )
    (fp_text value "10uH/350mA, MLZ2012M100WTD25" (at 0 -2.59) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp bffbeeb7-c21d-471b-9054-e91d1a0e6bc9)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 18300a02-4268-4041-b7ae-afea6ed878ab)
    )
    (fp_line (start -0.399622 0.56) (end 0.399622 0.56) (layer "B.SilkS") (width 0.12) (tstamp 57084240-42b8-4bb3-9caf-7abf068fd7a7))
    (fp_line (start -0.399622 -0.56) (end 0.399622 -0.56) (layer "B.SilkS") (width 0.12) (tstamp 890cecdb-5856-4d31-856a-51d80cfc3558))
    (fp_line (start 1.75 -0.85) (end -1.75 -0.85) (layer "B.CrtYd") (width 0.05) (tstamp 54ef8946-52ed-4d16-bd90-c5040c126bf8))
    (fp_line (start -1.75 0.85) (end 1.75 0.85) (layer "B.CrtYd") (width 0.05) (tstamp 74530a27-2fb0-428a-8469-ecccf5090423))
    (fp_line (start 1.75 0.85) (end 1.75 -0.85) (layer "B.CrtYd") (width 0.05) (tstamp c81fe176-32a5-41ba-b76e-040bbd6749ce))
    (fp_line (start -1.75 -0.85) (end -1.75 0.85) (layer "B.CrtYd") (width 0.05) (tstamp dfa11587-5d4f-458f-ba0e-88db0dfa6d07))
    (fp_line (start 1 0.45) (end 1 -0.45) (layer "B.Fab") (width 0.1) (tstamp 0a578e3f-dde5-4919-9d3d-3b4880f1cc17))
    (fp_line (start 1 -0.45) (end -1 -0.45) (layer "B.Fab") (width 0.1) (tstamp a1408923-877f-47da-b45f-9f240c77b0b1))
    (fp_line (start -1 -0.45) (end -1 0.45) (layer "B.Fab") (width 0.1) (tstamp b4ab520b-baa6-4cb7-9970-9eedfd1b537c))
    (fp_line (start -1 0.45) (end 1 0.45) (layer "B.Fab") (width 0.1) (tstamp dc0129be-a6bc-4c2a-937a-9000638f2fd3))
    (pad "1" smd roundrect (at -1.0625 0 180) (size 0.875 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 81 "Net-(L1-Pad1)") (pinfunction "1") (pintype "passive") (tstamp 82f3619a-5174-430c-9ab4-fcb24b9aad0c))
    (pad "2" smd roundrect (at 1.0625 0 180) (size 0.875 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/Power_Management/LED_A") (pinfunction "2") (pintype "passive") (tstamp 13d648bd-d67d-4b9b-bad8-99dd05e606b5))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_HDGC:0.5K-1.5-6PWB" (layer "B.Cu")
    (tedit 0) (tstamp fe2fb94b-8a50-4f8e-b213-7ce150b35a2a)
    (at 165.425 110.05 -90)
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/44a9183e-289d-4f05-a8c0-8458fc7f1cd8")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.05 -270) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2579ac89-0f84-4d09-859b-c3e2ad95bc7e)
    )
    (fp_text value "0.5K-1.5-6PWB" (at 0 -3.2 -270) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7526d798-b7e6-4c94-8281-8961c889a56e)
    )
    (fp_line (start -1.75 0) (end -1.75 0.75) (layer "B.SilkS") (width 0.12) (tstamp 40cfb16b-41db-4f2f-afe5-4a090b3769c8))
    (fp_line (start -1.75 0) (end -4.25 0) (layer "B.SilkS") (width 0.12) (tstamp ce63eb8f-38e0-4f81-848d-e737592353a3))
    (fp_line (start -4.55 -4.55) (end 4.55 -4.55) (layer "B.CrtYd") (width 0.05) (tstamp 6e35aa7d-765e-46f0-9707-f40191181384))
    (fp_line (start 4.55 1.3) (end 4.55 -4.55) (layer "B.CrtYd") (width 0.05) (tstamp 88c20351-cfc9-4706-a398-84544aff0f33))
    (fp_line (start -4.55 1.3) (end -4.55 -4.55) (layer "B.CrtYd") (width 0.05) (tstamp c9bffa16-3766-4929-87bc-1ecae6aa93f1))
    (fp_line (start -4.55 1.3) (end 4.55 1.3) (layer "B.CrtYd") (width 0.05) (tstamp f0c12028-a0f1-427b-a86d-ed9a05639cce))
    (pad "1" smd rect (at -1.25 0 270) (size 0.3 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 28 "/Power_Management/LED_K") (pinfunction "Pin_1") (pintype "passive") (tstamp e1a9d088-e77e-4872-aeb8-fabb23a7b225))
    (pad "2" smd rect (at -0.75 0 270) (size 0.3 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 28 "/Power_Management/LED_K") (pinfunction "Pin_2") (pintype "passive") (tstamp e6754f11-8753-47ce-a8ac-2019a2d38416))
    (pad "3" smd rect (at -0.25 0 270) (size 0.3 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 26 "unconnected-(J3-Pad3)") (pinfunction "Pin_3") (pintype "passive+no_connect") (tstamp 23d5cb36-b1da-4db7-b8cb-344522731d53))
    (pad "4" smd rect (at 0.25 0 270) (size 0.3 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 27 "unconnected-(J3-Pad4)") (pinfunction "Pin_4") (pintype "passive+no_connect") (tstamp eb3decee-0b88-40c0-907c-749ae4e8f2dd))
    (pad "5" smd rect (at 0.75 0 270) (size 0.3 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "/Power_Management/LED_A") (pinfunction "Pin_5") (pintype "passive") (tstamp 27c5163e-fb99-4bdf-b265-52fe7dee0afc))
    (pad "6" smd rect (at 1.25 0 270) (size 0.3 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "/Power_Management/LED_A") (pinfunction "Pin_6") (pintype "passive") (tstamp 22470dd4-d9f6-4921-96f0-5f282763d2c2))
    (pad "MP" smd rect (at -3.4 -3.15 270) (size 1.1 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "MountPin") (pintype "passive") (tstamp 47980a62-849d-4634-b212-2f8c247b21aa))
    (pad "MP" smd rect (at 3.4 -3.15 270) (size 1.1 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "MountPin") (pintype "passive") (tstamp bcc062d7-12a9-4df5-9293-dbdcf0446704))
  )

  (gr_rect locked (start 112.5 106.3) (end 191.5 143) (layer "Dwgs.User") (width 0.15) (fill none) (tstamp 3a959ea3-664f-4552-8653-c6e4dcdb715d))
  (gr_line (start 112.5 124.15) (end 191.5 124.15) (layer "Dwgs.User") (width 0.15) (tstamp 88d4e556-1df4-4ec6-8ebf-f46650e267f2))
  (gr_line (start 168.1 111.8) (end 191.5 111.8) (layer "Dwgs.User") (width 0.15) (tstamp b7337c66-9018-416f-ba81-c31151777b59))
  (gr_line (start 168.1 108.3) (end 168.1 111.8) (layer "Dwgs.User") (width 0.15) (tstamp d70287ac-f4b0-4f3f-aecd-335f31ed676c))
  (gr_line (start 191.5 108.3) (end 168.1 108.3) (layer "Dwgs.User") (width 0.15) (tstamp ed19b09f-82d9-4562-b578-d2198bc4f8d5))
  (gr_line (start 112 159.4) (end 197 159.4) (layer "Edge.Cuts") (width 0.1) (tstamp 0c9ca2e1-32e2-4bef-a1a4-7e3dd0070393))
  (gr_arc (start 192 111.4) (mid 191 112.4) (end 190 111.4) (layer "Edge.Cuts") (width 0.1) (tstamp 39b2434a-4f98-45b5-b3aa-9979da5b3973))
  (gr_line (start 192 132) (end 192 117) (layer "Edge.Cuts") (width 0.1) (tstamp 7bac970f-c349-4622-87c8-62f913c75d16))
  (gr_line (start 112 105.4) (end 112 159.4) (layer "Edge.Cuts") (width 0.1) (tstamp 7f546b4f-3242-4f45-bfc3-d7b15c1923be))
  (gr_arc (start 190 117) (mid 191 116) (end 192 117) (layer "Edge.Cuts") (width 0.1) (tstamp 8f07758b-1c3d-4dc7-b517-d263d15ea273))
  (gr_line (start 190 117) (end 190 132) (layer "Edge.Cuts") (width 0.1) (tstamp b4509015-f66f-4ee7-816a-4afd8a7704f1))
  (gr_line (start 197 159.4) (end 197 105.4) (layer "Edge.Cuts") (width 0.1) (tstamp ba32ba7f-8217-4b48-b727-569440c3f6e5))
  (gr_line (start 197 105.4) (end 112 105.4) (layer "Edge.Cuts") (width 0.1) (tstamp bfd41b31-5bd3-4d0a-ae20-1e1fed6828c8))
  (gr_arc (start 192 132) (mid 191 133) (end 190 132) (layer "Edge.Cuts") (width 0.1) (tstamp d2b4f581-9b50-4e03-a29b-793980edda7e))
  (gr_line (start 190 108.6) (end 190 111.4) (layer "Edge.Cuts") (width 0.1) (tstamp ddcf24c1-57c5-45c0-8415-c9c0f89fcfa0))
  (gr_line (start 192 108.6) (end 192 111.4) (layer "Edge.Cuts") (width 0.1) (tstamp df501692-480b-49d2-bf80-6b4ff0bff4be))
  (gr_arc (start 190 108.6) (mid 191 107.6) (end 192 108.6) (layer "Edge.Cuts") (width 0.1) (tstamp f836eaa5-c33a-4040-8328-3e57efb08912))
  (dimension (type aligned) (layer "Dwgs.User") (tstamp 038d57ef-ffab-4d2e-8f36-264c7d3688cd)
    (pts (xy 168.1 108.3) (xy 191.5 108.3))
    (height -3.6)
    (gr_text "23.4000 mm" (at 179.8 103.55) (layer "Dwgs.User") (tstamp 038d57ef-ffab-4d2e-8f36-264c7d3688cd)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp 0d48a53d-1f92-479a-ac00-6cb633e66acb)
    (pts (xy 112.5 106.3) (xy 112.5 143))
    (height 3.5)
    (gr_text "36.7000 mm" (at 107.85 124.65 90) (layer "Dwgs.User") (tstamp 0d48a53d-1f92-479a-ac00-6cb633e66acb)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp 2cd37e26-39f9-4e64-9daf-7287929a872a)
    (pts (xy 191.5 106.3) (xy 191.5 108.3))
    (height -8)
    (gr_text "2.0000 mm" (at 198.35 107.3 90) (layer "Dwgs.User") (tstamp 2cd37e26-39f9-4e64-9daf-7287929a872a)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp 3af81ae6-5c97-4c41-94c3-443993ba5f0b)
    (pts (xy 180.8 133.65) (xy 191.5 133.65))
    (height 11.6)
    (gr_text "10.7000 mm" (at 186.15 144.1) (layer "Dwgs.User") (tstamp 3af81ae6-5c97-4c41-94c3-443993ba5f0b)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp 836dc643-f787-436e-988d-4283e65f8fa8)
    (pts (xy 112.5 106.3) (xy 191.5 106.3))
    (height -3.799993)
    (gr_text "79.0000 mm" (at 152 101.350007) (layer "Dwgs.User") (tstamp 836dc643-f787-436e-988d-4283e65f8fa8)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp d8d81214-7453-47b8-822e-91257695a217)
    (pts (xy 191.5 109.34) (xy 191.5 112.84))
    (height -10.3)
    (gr_text "3.5000 mm" (at 200.65 111.09 90) (layer "Dwgs.User") (tstamp d8d81214-7453-47b8-822e-91257695a217)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp e2a9f3de-2a71-4e63-a781-c051be424d3b)
    (pts (xy 112.5 106.3) (xy 112.5 124.65))
    (height 1.55)
    (gr_text "18.3500 mm" (at 109.8 115.475 90) (layer "Dwgs.User") (tstamp e2a9f3de-2a71-4e63-a781-c051be424d3b)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )

  (segment (start 193.725 106.575) (end 193.7 106.6) (width 0.25) (layer "F.Cu") (net 1) (tstamp 5b9728b4-38a5-472f-8ad7-2a355545dbf0))
  (segment (start 194.575 106.575) (end 193.725 106.575) (width 0.25) (layer "F.Cu") (net 1) (tstamp b2938052-f325-4400-92cb-c8cadd206580))
  (via (at 119 127.4) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 1) (tstamp 27d76ae9-3f78-4614-9fa6-26581671e844))
  (via (at 154.6 131.8) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 1) (tstamp 2f6a160a-b290-4469-8efe-d73d35968eaa))
  (via (at 153.6 131.8) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 1) (tstamp 4f498090-e505-4b42-9971-89137d886cac))
  (via (at 161 135.2) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 1) (tstamp 98042410-37fe-4752-9813-4d136aae66c4))
  (via (at 113.2 125.6) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 1) (tstamp a5e5eb56-9fed-4c66-a4c7-42ca97829b5e))
  (via (at 160.994609 138.783828) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 1) (tstamp af2055b8-d315-4648-b0d3-41ee0656a796))
  (via (at 121.8 123.4) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 1) (tstamp b3bd6c3d-d982-45b4-90f9-818945368ab5))
  (via (at 193.7 106.6) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 1) (tstamp d0826d8a-249f-40e1-a42c-9a08b3cb3d83))
  (via (at 147.8 136.8) (size 0.6) (drill 0.4) (layers "F.Cu" "B.Cu") (net 1) (tstamp e5bcc47d-c0ca-4537-9f49-eb69ff89592d))
  (via (at 150.539317 138.4) (size 0.6) (drill 0.4) (layers "F.Cu" "B.Cu") (net 1) (tstamp ee1b375f-f603-48bb-923e-bd28b71dc110))
  (segment (start 161.025 135.225) (end 161 135.2) (width 0.1524) (layer "B.Cu") (net 1) (tstamp 01608157-68f4-47cf-9dc8-cc925a66e53a))
  (segment (start 119.69 127.4) (end 119 127.4) (width 0.1524) (layer "B.Cu") (net 1) (tstamp 097c2782-cf04-4ee6-b01e-309bf0fbaa41))
  (segment (start 154.6 132.49) (end 154.6 131.8) (width 0.1524) (layer "B.Cu") (net 1) (tstamp 0f167d7c-0467-4724-9c1c-160d4fd3172b))
  (segment (start 149.7 140) (end 149.7 139) (width 0.25) (layer "B.Cu") (net 1) (tstamp 1bde5233-9660-466e-a029-36d5041aceca))
  (segment (start 161.053437 138.725) (end 160.994609 138.783828) (width 0.1524) (layer "B.Cu") (net 1) (tstamp 1cdf3456-3341-4cd8-a410-ebcb6f1e4920))
  (segment (start 153.6 132.49) (end 153.6 131.8) (width 0.1524) (layer "B.Cu") (net 1) (tstamp 44d4ebfc-1b7f-4689-a6c9-ee10ad470f77))
  (segment (start 121.8 124.09) (end 121.8 123.4) (width 0.1524) (layer "B.Cu") (net 1) (tstamp 452841ae-f9be-4b5f-92cb-2c3aff908a78))
  (segment (start 149.0125 136.8) (end 147.8 136.8) (width 0.25) (layer "B.Cu") (net 1) (tstamp 49a455c4-14a1-4a50-903a-1880797dfa92))
  (segment (start 113.24 125.64) (end 113.2 125.6) (width 0.1524) (layer "B.Cu") (net 1) (tstamp 580c58e7-a5af-4162-95fe-2ea4968eb6bd))
  (segment (start 150.269659 138.4) (end 150.539317 138.4) (width 0.25) (layer "B.Cu") (net 1) (tstamp 7d13c152-dba6-43ef-8222-be1fe3ce23be))
  (segment (start 162.4875 135.225) (end 161.025 135.225) (width 0.1524) (layer "B.Cu") (net 1) (tstamp 7e062289-8e78-4436-9a44-c116b3b46e8b))
  (segment (start 149.7 139) (end 149.7 138.969659) (width 0.25) (layer "B.Cu") (net 1) (tstamp 8ec6d48f-ed66-43e3-b754-2a67a6183c85))
  (segment (start 151.034024 138.399299) (end 151.033323 138.4) (width 0.25) (layer "B.Cu") (net 1) (tstamp 8f7003c1-616e-41b5-b2ff-4a26dd4588de))
  (segment (start 149.7 138.969659) (end 150.269659 138.4) (width 0.25) (layer "B.Cu") (net 1) (tstamp 942b7fff-dd6e-4439-8ecd-104da0e1261f))
  (segment (start 152.075 138.375) (end 152.050701 138.399299) (width 0.25) (layer "B.Cu") (net 1) (tstamp 9f970d72-75e8-4c35-b403-56f6743e6e32))
  (segment (start 151.033323 138.4) (end 150.539317 138.4) (width 0.25) (layer "B.Cu") (net 1) (tstamp ad3b679f-4d2b-44c9-ade2-ba251ee49c22))
  (segment (start 152.050701 138.399299) (end 151.034024 138.399299) (width 0.25) (layer "B.Cu") (net 1) (tstamp bbcd0d30-5264-4cd4-b437-36e49a51dc1f))
  (segment (start 162.4875 138.725) (end 161.053437 138.725) (width 0.1524) (layer "B.Cu") (net 1) (tstamp ea7ecd6c-f8a5-48de-9fcc-d89167b9bd7f))
  (segment (start 114.95 125.64) (end 113.24 125.64) (width 0.1524) (layer "B.Cu") (net 1) (tstamp f8569f7c-d7f6-48fb-b34f-402d01eaba95))
  (via (at 161.2 139.4) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 2) (tstamp 787489f3-149b-484b-9cb3-4c4e9309c1e1))
  (segment (start 162.4875 139.375) (end 161.225 139.375) (width 0.1524) (layer "B.Cu") (net 2) (tstamp 5f80f8ea-3567-4f68-b71c-7b556223a5b3))
  (segment (start 161.225 139.375) (end 161.2 139.4) (width 0.1524) (layer "B.Cu") (net 2) (tstamp e78bf2d0-dcab-43ef-9e68-8c445871e1e4))
  (segment (start 163.2 125.297663) (end 163.2 116) (width 0.1524) (layer "F.Cu") (net 3) (tstamp 103b7a3a-a127-44c0-ba95-6fb21a70a412))
  (segment (start 157.6 130.897663) (end 163.2 125.297663) (width 0.1524) (layer "F.Cu") (net 3) (tstamp 4502828e-dacc-4e16-bd4b-265e69bbcfd5))
  (segment (start 158.8 132.2) (end 158.097664 132.2) (width 0.1524) (layer "F.Cu") (net 3) (tstamp 77698c1c-4821-4f6e-84a1-5b7058d22502))
  (segment (start 163.2 116) (end 158.4 111.2) (width 0.1524) (layer "F.Cu") (net 3) (tstamp 8106f626-8f44-4b36-a975-c9f66be85e7b))
  (segment (start 158.4 111.2) (end 156.6 111.2) (width 0.1524) (layer "F.Cu") (net 3) (tstamp 9ae1de5d-6858-4b91-9d9d-f90d4221528e))
  (segment (start 157.6 131.702336) (end 157.6 130.897663) (width 0.1524) (layer "F.Cu") (net 3) (tstamp 9edcf993-241a-4c58-bb77-f509307a4186))
  (segment (start 158.097664 132.2) (end 157.6 131.702336) (width 0.1524) (layer "F.Cu") (net 3) (tstamp f536fdb9-269b-4ee3-ac01-c410fb4153dd))
  (via (at 158.8 132.2) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 3) (tstamp 0994c8b1-b1ee-4ba7-b89b-7ab8e1a38c95))
  (segment (start 158.9483 136.447732) (end 157.521032 137.875) (width 0.1524) (layer "B.Cu") (net 3) (tstamp 29c54e5c-57d0-4638-a468-68db3a89fb74))
  (segment (start 158.9483 132.3483) (end 158.9483 136.447732) (width 0.1524) (layer "B.Cu") (net 3) (tstamp 561fcd9b-b35e-45c2-8930-9b57516a059f))
  (segment (start 158.8 132.2) (end 158.9483 132.3483) (width 0.1524) (layer "B.Cu") (net 3) (tstamp 5d353dfa-ce71-4e90-b534-098ade40d94e))
  (segment (start 157.521032 137.875) (end 156.975 137.875) (width 0.1524) (layer "B.Cu") (net 3) (tstamp 5e578f7c-8afa-4cd7-8867-07393b482849))
  (segment (start 150.605 135.35) (end 150.605 136.7825) (width 0.25) (layer "B.Cu") (net 4) (tstamp 208ab4fa-9e8c-459f-9344-cfd73fa22cb6))
  (segment (start 152.075 137.375) (end 151.375 137.375) (width 0.25) (layer "B.Cu") (net 4) (tstamp 5191a31b-d83c-4d03-8429-9e21c75335ab))
  (segment (start 152.075 136.875) (end 150.6625 136.875) (width 0.25) (layer "B.Cu") (net 4) (tstamp 577c0053-037e-48e8-8315-1d37d985d28d))
  (segment (start 150.5875 137.0925) (end 149.68 138) (width 0.25) (layer "B.Cu") (net 4) (tstamp 6143fefd-7965-483f-b073-19ee85d7be8d))
  (segment (start 150.605 136.7825) (end 150.5875 136.8) (width 0.25) (layer "B.Cu") (net 4) (tstamp 692e70cf-3141-4f14-a4ae-50db595edf11))
  (segment (start 151.375 137.375) (end 150.8 136.8) (width 0.25) (layer "B.Cu") (net 4) (tstamp 6c3db197-4baa-4511-99cd-19790a301f68))
  (segment (start 150.6625 136.875) (end 150.5875 136.8) (width 0.25) (layer "B.Cu") (net 4) (tstamp 755083b6-7210-4b99-9776-9eba7012e6aa))
  (segment (start 150.8 136.8) (end 150.5875 136.8) (width 0.25) (layer "B.Cu") (net 4) (tstamp 7fdc96e4-e129-4e29-8677-1d10bdb38cf2))
  (segment (start 150.5875 136.8) (end 150.5875 137.0925) (width 0.25) (layer "B.Cu") (net 4) (tstamp f2240139-31b6-4efd-bb0d-905a4264a3de))
  (segment (start 169.6 135.1) (end 169.6 135.4) (width 0.25) (layer "B.Cu") (net 5) (tstamp 295ae101-8923-44f1-8ff8-97406ff9c246))
  (segment (start 166.7125 135.225) (end 167.4625 134.475) (width 0.25) (layer "B.Cu") (net 5) (tstamp 7ed8f25f-18b0-48c8-8f56-7eb23011c3eb))
  (segment (start 167.4625 134.475) (end 168.975 134.475) (width 0.25) (layer "B.Cu") (net 5) (tstamp 852a552d-6836-49d0-ba8a-9a5804bcdbc5))
  (segment (start 170.1 135.9) (end 170.7 135.9) (width 0.25) (layer "B.Cu") (net 5) (tstamp 8695ce4d-e917-4d02-9ba3-58156db32e65))
  (segment (start 169.6 135.4) (end 170.1 135.9) (width 0.25) (layer "B.Cu") (net 5) (tstamp b7b48860-6d23-4c59-b333-a7116ba32f95))
  (segment (start 168.975 134.475) (end 169.6 135.1) (width 0.25) (layer "B.Cu") (net 5) (tstamp dc393316-1a95-4e33-9d2c-f1c2f3509df9))
  (via (at 195.7 129.8) (size 1) (drill 0.6) (layers "F.Cu" "B.Cu") (net 6) (tstamp 83cfa84f-d318-41dd-8e92-33790f5b572e))
  (segment (start 195.7 131.475) (end 195.7 129.8) (width 0.5) (layer "B.Cu") (net 6) (tstamp bc969c06-aef9-41bb-8ef5-4a592820ba51))
  (segment (start 147.2 120.6) (end 147.2 117.6) (width 0.25) (layer "F.Cu") (net 9) (tstamp 0bc9bc17-3416-4939-901f-7f358270b581))
  (segment (start 151.5 121.8) (end 148.4 121.8) (width 0.25) (layer "F.Cu") (net 9) (tstamp 1110c232-f341-48cc-b84d-ba90ca04337b))
  (segment (start 148.4 121.8) (end 147.3 120.7) (width 0.25) (layer "F.Cu") (net 9) (tstamp 49b88b1c-5693-4acb-be36-44710154839a))
  (segment (start 147.3 120.7) (end 147.2 120.6) (width 0.25) (layer "F.Cu") (net 9) (tstamp ee444db6-8ea7-406d-9333-affcc0134eb8))
  (via (at 147.2 117.6) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 9) (tstamp 059ba0e7-f558-47c3-bb2e-0e1423cb7741))
  (via (at 151.5 121.8) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 9) (tstamp adbaacb2-b567-44d5-acff-6ec885896993))
  (segment (start 152.39 121.8) (end 151.5 121.8) (width 0.25) (layer "B.Cu") (net 9) (tstamp 01065175-7c01-4368-8779-bb35965f6cb4))
  (segment (start 178.425 123.4) (end 177.600609 123.4) (width 0.25) (layer "B.Cu") (net 9) (tstamp 4b96f560-6dcf-4cca-a43b-0468fb4b68ae))
  (segment (start 176.9 124.100609) (end 176.9 126.075) (width 0.25) (layer "B.Cu") (net 9) (tstamp d5b8f3f7-0ae5-44e5-86e7-169036ed3aaf))
  (segment (start 178.425 122.9) (end 178.425 123.4) (width 0.25) (layer "B.Cu") (net 9) (tstamp e4d430f1-aa2f-46cd-8e4a-e3ba5369d27f))
  (segment (start 177.600609 123.4) (end 176.9 124.100609) (width 0.25) (layer "B.Cu") (net 9) (tstamp e745cce9-733b-45db-8224-4f486a380c4c))
  (segment (start 176.9 126.075) (end 175.675 127.3) (width 0.25) (layer "B.Cu") (net 9) (tstamp f75a9585-0f82-4a79-b88d-7decee414af9))
  (segment (start 167.35 120.8) (end 167.35 118.4) (width 0.25) (layer "B.Cu") (net 11) (tstamp 2f378c6f-f18f-4c66-9753-794a022a2d1a))
  (segment (start 167.225 118.525) (end 167.35 118.4) (width 0.25) (layer "B.Cu") (net 11) (tstamp 8c772c61-d554-403b-98d8-5282799e44fa))
  (segment (start 165.8 118.525) (end 167.225 118.525) (width 0.25) (layer "B.Cu") (net 11) (tstamp cddb359b-5e2d-4db8-a801-1efcf3cb13b9))
  (segment (start 169.6 124.75) (end 168.05 123.2) (width 0.25) (layer "B.Cu") (net 12) (tstamp 3894feb2-d959-441e-8138-6a9710daced1))
  (segment (start 167.35 123.2) (end 167.35 123.0875) (width 0.25) (layer "B.Cu") (net 12) (tstamp 3cc573c2-c61b-45a1-86ed-220ae91a1124))
  (segment (start 165.8 121.5375) (end 165.8 120.075) (width 0.25) (layer "B.Cu") (net 12) (tstamp 77f1482e-236d-4d4c-9c80-d2803869bff2))
  (segment (start 168.05 123.2) (end 167.35 123.2) (width 0.25) (layer "B.Cu") (net 12) (tstamp a16c5616-6548-4f23-83d2-5fc6032e5d07))
  (segment (start 169.6 127.2375) (end 169.6 124.75) (width 0.25) (layer "B.Cu") (net 12) (tstamp ab4b99e4-3366-49dd-a39e-16a4f9b75601))
  (segment (start 167.35 123.0875) (end 165.8 121.5375) (width 0.25) (layer "B.Cu") (net 12) (tstamp e6b8ff48-0ab6-4e97-ae07-9e0d7bd5fce6))
  (segment (start 178.425 128.9) (end 177.172952 128.9) (width 0.29337) (layer "B.Cu") (net 13) (tstamp 090cf6e3-d26c-4fa9-81f5-57863d223692))
  (segment (start 175.675 130.397952) (end 175.675 130.4) (width 0.29337) (layer "B.Cu") (net 13) (tstamp 5ae3d1d1-686b-45f2-83f2-244b86394aa1))
  (segment (start 177.172952 128.9) (end 175.675 130.397952) (width 0.29337) (layer "B.Cu") (net 13) (tstamp 800acced-691e-4c01-b725-4bd4fd53fa18))
  (segment (start 177.33931 121.4) (end 176.45 122.28931) (width 0.25) (layer "B.Cu") (net 14) (tstamp 0e7696e7-bbbe-439a-b9de-16bbfc339548))
  (segment (start 176.000499 123.727318) (end 176.000499 123.774501) (width 0.25) (layer "B.Cu") (net 14) (tstamp 33b38e96-c1d3-4eb9-b2b1-804cd9b0517b))
  (segment (start 178.425 121.4) (end 177.33931 121.4) (width 0.25) (layer "B.Cu") (net 14) (tstamp 49e68c02-b2f8-4442-a37a-5e59dcf48f0e))
  (segment (start 176.45 123.277817) (end 176.000499 123.727318) (width 0.25) (layer "B.Cu") (net 14) (tstamp 5776ed68-a531-49df-92cc-24aad4433786))
  (segment (start 176.45 122.28931) (end 176.45 123.277817) (width 0.25) (layer "B.Cu") (net 14) (tstamp fa083e88-f15d-41ee-996a-5fdd0d3ce915))
  (segment (start 176.000499 123.774501) (end 175.675 124.1) (width 0.25) (layer "B.Cu") (net 14) (tstamp fe0591a7-5605-4429-b06a-abb2888dc103))
  (segment (start 175.675 121.1) (end 174.875 121.9) (width 0.25) (layer "B.Cu") (net 15) (tstamp 1d68a395-034d-4bdc-b5e3-437ed37c8cf5))
  (segment (start 178.425 120.4) (end 176.375 120.4) (width 0.25) (layer "B.Cu") (net 15) (tstamp 2ff7b5aa-c160-4a13-9d8c-78928611cae9))
  (segment (start 171.95 121.9) (end 170.65 123.2) (width 0.25) (layer "B.Cu") (net 15) (tstamp 85b7c076-b0c1-4378-b71e-6db943a2540b))
  (segment (start 174.875 121.9) (end 171.95 121.9) (width 0.25) (layer "B.Cu") (net 15) (tstamp 9dd63b23-a18c-416d-9dc4-c7fdbb16a909))
  (segment (start 176.375 120.4) (end 175.675 121.1) (width 0.25) (layer "B.Cu") (net 15) (tstamp bc9f6ab0-6dc8-4ae2-af1d-5d0dce9b27a7))
  (segment (start 178.425 119.4) (end 177.175 119.4) (width 0.25) (layer "B.Cu") (net 16) (tstamp 1fb593fc-cf91-442b-81d7-ae586bc6856d))
  (segment (start 175.675 117.9) (end 174.775 118.8) (width 0.25) (layer "B.Cu") (net 16) (tstamp 4d99d23d-66c7-4de2-8d31-e271fe857f5b))
  (segment (start 174.775 118.8) (end 171.05 118.8) (width 0.25) (layer "B.Cu") (net 16) (tstamp 7a56350c-f115-460d-949f-f78f40ad5b67))
  (segment (start 177.175 119.4) (end 175.675 117.9) (width 0.25) (layer "B.Cu") (net 16) (tstamp 9e3539e2-883b-4b53-a2ab-e22fc9d271b2))
  (segment (start 171.05 118.8) (end 170.65 118.4) (width 0.25) (layer "B.Cu") (net 16) (tstamp db1d2e21-cbcb-43f0-9bb3-693f3269a091))
  (segment (start 176.175 128.4) (end 175.675 128.9) (width 0.29337) (layer "B.Cu") (net 17) (tstamp 1476bb43-e32e-4d16-a95a-7e4e2639dafe))
  (segment (start 178.425 128.4) (end 176.175 128.4) (width 0.29337) (layer "B.Cu") (net 17) (tstamp c9ba0cde-3e29-45a3-846b-01ef141ce025))
  (segment (start 175.675 125.352817) (end 175.675 125.8) (width 0.25) (layer "B.Cu") (net 18) (tstamp 28756625-4fb3-4389-bb98-aa8837ab8570))
  (segment (start 177.475 121.9) (end 176.9 122.475) (width 0.25) (layer "B.Cu") (net 18) (tstamp 96d947b7-e479-4efc-a5f0-478d09370ecd))
  (segment (start 176.9 122.475) (end 176.9 123.464213) (width 0.25) (layer "B.Cu") (net 18) (tstamp 975e6513-65bb-4a7a-aa90-7d453cfd0d0f))
  (segment (start 176.45 124.577817) (end 175.675 125.352817) (width 0.25) (layer "B.Cu") (net 18) (tstamp 9af1d5d3-5970-4e54-8b26-09859d33325f))
  (segment (start 178.425 121.9) (end 177.475 121.9) (width 0.25) (layer "B.Cu") (net 18) (tstamp c963fe56-1200-4d2b-b297-f376189538f0))
  (segment (start 176.9 123.464213) (end 176.45 123.914213) (width 0.25) (layer "B.Cu") (net 18) (tstamp d0960fea-05eb-48ca-9b57-da458459bd72))
  (segment (start 176.45 123.914213) (end 176.45 124.577817) (width 0.25) (layer "B.Cu") (net 18) (tstamp f72a87b1-bb46-4bb0-8c5f-fb4248ae6f9e))
  (segment (start 175.675 122.8) (end 175.675 122.42862) (width 0.25) (layer "B.Cu") (net 19) (tstamp 17cfa7d9-0474-4b05-9cf1-1d8327d9692a))
  (segment (start 175.675 122.42862) (end 177.20362 120.9) (width 0.25) (layer "B.Cu") (net 19) (tstamp 74a02fd6-4cba-4584-aaff-8b88b58c0f8a))
  (segment (start 177.20362 120.9) (end 178.425 120.9) (width 0.25) (layer "B.Cu") (net 19) (tstamp b07edd09-fe60-4632-a006-fba4efb33b61))
  (segment (start 176.9 119.9) (end 178.425 119.9) (width 0.25) (layer "B.Cu") (net 20) (tstamp 2f1a35f9-448f-4c94-8793-447e5a39aafe))
  (segment (start 175.675 119.6) (end 176.6 119.6) (width 0.25) (layer "B.Cu") (net 20) (tstamp 3509d26b-a92c-48e0-9f86-a81b99eadcf5))
  (segment (start 176.6 119.6) (end 176.9 119.9) (width 0.25) (layer "B.Cu") (net 20) (tstamp 51c33008-4c15-40ed-9d7f-4f54f43b489e))
  (segment (start 177.4 118.9) (end 178.425 118.9) (width 0.25) (layer "B.Cu") (net 21) (tstamp 18b6d40c-bdd0-41b8-892f-53982a6dcae4))
  (segment (start 175.675 116.4) (end 177 117.725) (width 0.25) (layer "B.Cu") (net 21) (tstamp 32d43225-1f69-4d7c-8b0b-de21786d6b30))
  (segment (start 177 118.5) (end 177.4 118.9) (width 0.25) (layer "B.Cu") (net 21) (tstamp 62b83e32-64fd-411e-900d-cc2a77e44a4e))
  (segment (start 177 117.725) (end 177 118.5) (width 0.25) (layer "B.Cu") (net 21) (tstamp a6a44d43-79ec-42d9-86a4-acae2cab39a5))
  (segment (start 195.425 106.575) (end 196 107.15) (width 0.25) (layer "F.Cu") (net 22) (tstamp 035ff1c5-8fed-47e5-abc2-61a0009748ff))
  (segment (start 196 107.15) (end 196 108.1) (width 0.25) (layer "F.Cu") (net 22) (tstamp a641e468-32b1-48b3-a0e7-85bb5e54a1f6))
  (via (at 196 108.1) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 22) (tstamp 27a17c73-e86a-43aa-a0dc-35921a70646f))
  (segment (start 196 109.78) (end 196 108.1) (width 0.25) (layer "B.Cu") (net 22) (tstamp 632cc496-246c-4492-9c85-941e2ba39421))
  (segment (start 195.425 107.675) (end 195 108.1) (width 0.25) (layer "F.Cu") (net 23) (tstamp c2d74581-96c9-4498-a110-4a3d949102b0))
  (segment (start 195.425 107.425) (end 195.425 107.675) (width 0.25) (layer "F.Cu") (net 23) (tstamp de47c38d-a4de-4fdd-845a-35c935c0970d))
  (via (at 195 108.1) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 23) (tstamp ed7eb29e-557f-49bd-8dec-5cabb605becd))
  (segment (start 195 109.78) (end 195 108.1) (width 0.25) (layer "B.Cu") (net 23) (tstamp a0f58411-2083-4cf1-9364-d6857b5803e9))
  (segment (start 194.575 107.425) (end 194 108) (width 0.25) (layer "F.Cu") (net 24) (tstamp 3aab3db2-33f4-46f8-b9fa-b1a372ef61ff))
  (segment (start 194 108) (end 194 108.1) (width 0.25) (layer "F.Cu") (net 24) (tstamp 5ee3ed42-01d0-48d5-a7d0-8a9115fff735))
  (via (at 194 108.1) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 24) (tstamp e506ef0a-ad46-4211-b3dd-94ecf6f701a7))
  (segment (start 194 109.78) (end 194 108.1) (width 0.25) (layer "B.Cu") (net 24) (tstamp da2ba35b-6fd7-4aa9-976c-6e7caa2820a4))
  (segment (start 177.475 129.9) (end 178.425 129.9) (width 0.25) (layer "B.Cu") (net 30) (tstamp 1ac4c5e2-1c77-4d11-9e1f-7abd7f7d39fe))
  (segment (start 173.513811 131.849501) (end 176.114007 131.8495) (width 0.25) (layer "B.Cu") (net 30) (tstamp 20a982ec-2848-49e4-9ee0-fa010047793b))
  (segment (start 168.65 125.3625) (end 168.65 127.696751) (width 0.25) (layer "B.Cu") (net 30) (tstamp 49424e60-c0f5-4350-8d1f-1421fd50da8d))
  (segment (start 167.4 125.81) (end 168.2025 125.81) (width 0.25) (layer "B.Cu") (net 30) (tstamp 8a9a7cfd-f4e9-465a-9e98-9a7f8720d5a5))
  (segment (start 168.65 127.696751) (end 169.389438 128.436189) (width 0.25) (layer "B.Cu") (net 30) (tstamp 9ea4eb1e-4b86-4f26-8dbb-f17713f0dbca))
  (segment (start 169.389438 128.436189) (end 170.100499 128.436189) (width 0.25) (layer "B.Cu") (net 30) (tstamp ba9cffcf-0c58-40cd-a555-6b63701418bd))
  (segment (start 176.9 131.063507) (end 176.9 130.475) (width 0.25) (layer "B.Cu") (net 30) (tstamp d28ef401-4fdd-43d8-ad4c-424390aac1b9))
  (segment (start 176.9 130.475) (end 177.475 129.9) (width 0.25) (layer "B.Cu") (net 30) (tstamp da7b9c7c-0b3b-4599-8221-a81b63acd71e))
  (segment (start 176.114007 131.8495) (end 176.9 131.063507) (width 0.25) (layer "B.Cu") (net 30) (tstamp dc42bdcb-6b7f-462f-9a3c-cde7f45986f2))
  (segment (start 170.100499 128.436189) (end 173.513811 131.849501) (width 0.25) (layer "B.Cu") (net 30) (tstamp e4413827-c745-425e-9048-0e278b22639d))
  (segment (start 168.2025 125.81) (end 168.65 125.3625) (width 0.25) (layer "B.Cu") (net 30) (tstamp fd1721db-408b-4828-85df-3e97cab50992))
  (segment (start 170.55 125.3625) (end 171.2275 125.3625) (width 0.25) (layer "B.Cu") (net 31) (tstamp 16edcfa1-e1e0-44da-82a8-48b11c20db52))
  (segment (start 173.7 131.4) (end 170.55 128.25) (width 0.25) (layer "B.Cu") (net 31) (tstamp 23804988-efae-4695-a484-40f3fb37a3f1))
  (segment (start 171.2275 125.3625) (end 171.8 124.79) (width 0.25) (layer "B.Cu") (net 31) (tstamp 43a19ee4-771c-46a9-a87c-3eac81b7e6b4))
  (segment (start 170.55 128.25) (end 170.55 125.3625) (width 0.25) (layer "B.Cu") (net 31) (tstamp 514c3edb-dede-490d-bbab-693bd8df3b24))
  (segment (start 175.927817 131.4) (end 173.7 131.4) (width 0.25) (layer "B.Cu") (net 31) (tstamp 6c28dff5-5a96-4b5e-8fef-b1dd53807670))
  (segment (start 176.450499 130.288811) (end 176.450499 130.877318) (width 0.25) (layer "B.Cu") (net 31) (tstamp 82e4041d-7de2-4555-b27f-285bce837448))
  (segment (start 178.425 129.4) (end 177.33931 129.4) (width 0.25) (layer "B.Cu") (net 31) (tstamp 8eb1225f-21ba-4e78-a501-ef46de988ed0))
  (segment (start 177.33931 129.4) (end 176.450499 130.288811) (width 0.25) (layer "B.Cu") (net 31) (tstamp 9dca3ea0-4e1d-4e08-a3b3-828596ef96db))
  (segment (start 176.450499 130.877318) (end 175.927817 131.4) (width 0.25) (layer "B.Cu") (net 31) (tstamp df23738a-ca7e-4f0d-b2b3-0509e99d33df))
  (segment (start 155.275 135.023368) (end 155.9524 134.345968) (width 0.1524) (layer "B.Cu") (net 38) (tstamp 1bf02830-d82b-42a6-bd4e-f1ece4c0ed2d))
  (segment (start 155.275 135.675) (end 155.275 135.023368) (width 0.1524) (layer "B.Cu") (net 38) (tstamp 359bf4bb-dcce-4801-acaa-9c3cdfb39170))
  (segment (start 155.9524 134.345968) (end 155.9524 131.1524) (width 0.1524) (layer "B.Cu") (net 38) (tstamp 74d5eeef-5c8d-4f8d-9924-b8e3a5d4aa58))
  (segment (start 155.9524 131.1524) (end 155.8 131) (width 0.1524) (layer "B.Cu") (net 38) (tstamp fe42e04e-f2a3-4938-acdf-a027333cbf95))
  (segment (start 156.275 135.675) (end 156.6572 135.2928) (width 0.1524) (layer "B.Cu") (net 39) (tstamp 51a9ce66-b56f-475f-b8b2-547cfe87f673))
  (segment (start 156.6572 135.2928) (end 156.6572 130.758831) (width 0.1524) (layer "B.Cu") (net 39) (tstamp 576dfa3f-f94e-4605-8168-53df520038ae))
  (segment (start 156.6572 130.758831) (end 156.249184 130.350815) (width 0.1524) (layer "B.Cu") (net 39) (tstamp 9e590085-735a-4462-8da9-e8809e548d69))
  (segment (start 162.8476 116.2476) (end 158.2 111.6) (width 0.1524) (layer "F.Cu") (net 40) (tstamp 09ef7405-2302-4b2c-9143-4d36289443de))
  (segment (start 158.4 133) (end 157.2 131.8) (width 0.1524) (layer "F.Cu") (net 40) (tstamp 13b4c27d-f7a2-46cd-b660-26e91c87a523))
  (segment (start 162.8476 125.1524) (end 162.8476 116.2476) (width 0.1524) (layer "F.Cu") (net 40) (tstamp 5d25b13d-ecf5-4c2f-b725-be22bd1fe3c2))
  (segment (start 158.2 111.6) (end 150.2 111.6) (width 0.1524) (layer "F.Cu") (net 40) (tstamp 5fc3effd-e679-4fe6-9755-e2df23dfda63))
  (segment (start 157.2 131.8) (end 157.2 130.8) (width 0.1524) (layer "F.Cu") (net 40) (tstamp 69f5d545-184d-47b6-a8c4-2de116442b0f))
  (segment (start 158.4476 133) (end 158.4 133) (width 0.1524) (layer "F.Cu") (net 40) (tstamp 6e1b04e5-360e-48b6-a322-4ffdc379a167))
  (segment (start 150.2 111.6) (end 148.8 110.2) (width 0.1524) (layer "F.Cu") (net 40) (tstamp 93d8a105-0606-48e7-8e84-d1f443dec7ec))
  (segment (start 157.2 130.8) (end 162.8476 125.1524) (width 0.1524) (layer "F.Cu") (net 40) (tstamp e1f32cfb-c5e5-431c-8ccb-491972ca4dad))
  (via (at 158.4476 133) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 40) (tstamp ccbad806-97cc-431d-82ef-209d09a2c9b2))
  (segment (start 158.5959 133.1483) (end 158.5959 136.302468) (width 0.1524) (layer "B.Cu") (net 40) (tstamp 327fc2e0-9af3-4428-9db7-01c9a8d65bb7))
  (segment (start 157.523368 137.375) (end 156.975 137.375) (width 0.1524) (layer "B.Cu") (net 40) (tstamp 59f639d3-0852-42ca-a230-2b2884fad057))
  (segment (start 158.4476 133) (end 158.5959 133.1483) (width 0.1524) (layer "B.Cu") (net 40) (tstamp 73fc1987-4628-4da1-8e93-09d6fca668b5))
  (segment (start 158.5959 136.302468) (end 157.523368 137.375) (width 0.1524) (layer "B.Cu") (net 40) (tstamp e8eb1969-5b02-4e19-8902-de40a95827b5))
  (segment (start 160.854049 137.054049) (end 158.105426 134.305426) (width 0.1524) (layer "F.Cu") (net 41) (tstamp 0139e0d0-5cd5-46fd-bdda-0a5e29fdd901))
  (segment (start 154.284217 134.305426) (end 154.278091 134.2993) (width 0.1524) (layer "F.Cu") (net 41) (tstamp 84d8e826-f64f-41c8-a6c0-3e3066d53db7))
  (segment (start 158.105426 134.305426) (end 154.284217 134.305426) (width 0.1524) (layer "F.Cu") (net 41) (tstamp f9c7c550-b0d5-4b6f-b0d1-59a8d5ef2505))
  (via (at 154.278091 134.2993) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 41) (tstamp 60a6b63f-8418-46f2-bde4-5bbbae028ea4))
  (via (at 160.854049 137.054049) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 41) (tstamp a64df761-2798-42ce-80cf-a3af13dfdbc2))
  (segment (start 154.6 133.51) (end 154.278091 133.831909) (width 0.1524) (layer "B.Cu") (net 41) (tstamp 196d918b-6d32-4ff7-9f54-077ce08213f0))
  (segment (start 160.975 137.175) (end 160.854049 137.054049) (width 0.1524) (layer "B.Cu") (net 41) (tstamp 53bdf2ce-58b6-4d4d-b299-78dfa6d09033))
  (segment (start 154.275 135.675) (end 154.275 134.302391) (width 0.1524) (layer "B.Cu") (net 41) (tstamp 589abf06-f32f-436f-8dc3-c5e5af424e13))
  (segment (start 154.278091 133.831909) (end 154.278091 134.2993) (width 0.1524) (layer "B.Cu") (net 41) (tstamp 5bb51dbc-bcdc-4437-b9ba-b6cf2ff3300d))
  (segment (start 160.4 139.308097) (end 160.4 137.508098) (width 0.1524) (layer "B.Cu") (net 41) (tstamp 5ccc6eab-d201-4d34-94c2-168654e1e50f))
  (segment (start 160.4 137.508098) (end 160.854049 137.054049) (width 0.1524) (layer "B.Cu") (net 41) (tstamp 68249225-2a90-4b43-bee1-8d997befea6a))
  (segment (start 162.4875 140.675) (end 161.766903 140.675) (width 0.1524) (layer "B.Cu") (net 41) (tstamp aa4c7998-57d8-4f3d-a61d-4b7034edca35))
  (segment (start 162.4875 137.175) (end 160.975 137.175) (width 0.1524) (layer "B.Cu") (net 41) (tstamp ba6e40d4-c42b-4887-b1df-ff8b075db177))
  (segment (start 154.275 134.302391) (end 154.278091 134.2993) (width 0.1524) (layer "B.Cu") (net 41) (tstamp d244f13e-7dd2-4afb-803d-e2fa086d3286))
  (segment (start 161.766903 140.675) (end 160.4 139.308097) (width 0.1524) (layer "B.Cu") (net 41) (tstamp dc921dfa-d6be-4f08-a8f2-8ddf95de25b3))
  (segment (start 154.640621 133.953026) (end 154.485695 133.7981) (width 0.1524) (layer "F.Cu") (net 42) (tstamp 06ddc828-40d6-4843-8937-050bed94e9bc))
  (segment (start 161.313317 136.594781) (end 161.103585 136.594781) (width 0.1524) (layer "F.Cu") (net 42) (tstamp 351295bb-408b-4e8d-a98d-01c2237d0caf))
  (segment (start 153.669294 134.2) (end 153.6 134.2) (width 0.1524) (layer "F.Cu") (net 42) (tstamp 47cc228c-472d-4c79-8124-40b6177291cf))
  (segment (start 158.251394 133.953026) (end 154.640621 133.953026) (width 0.1524) (layer "F.Cu") (net 42) (tstamp 58e6d63f-a071-44df-b689-fce0b9db5c60))
  (segment (start 161.061653 136.552849) (end 160.851217 136.552849) (width 0.1524) (layer "F.Cu") (net 42) (tstamp 5fabb1db-9dad-4256-ac58-af56c88892d6))
  (segment (start 154.071194 133.7981) (end 153.669294 134.2) (width 0.1524) (layer "F.Cu") (net 42) (tstamp 6dd6356d-89f0-4d64-b66c-80a486e61047))
  (segment (start 154.485695 133.7981) (end 154.071194 133.7981) (width 0.1524) (layer "F.Cu") (net 42) (tstamp 94e89460-d47e-4cfb-a7f5-c9d02d839587))
  (segment (start 161.103585 136.594781) (end 161.061653 136.552849) (width 0.1524) (layer "F.Cu") (net 42) (tstamp bd3d158d-1246-480c-ba81-15c1985260cf))
  (segment (start 160.851217 136.552849) (end 158.251394 133.953026) (width 0.1524) (layer "F.Cu") (net 42) (tstamp e5d56774-8832-41fe-a983-d9161d646c5f))
  (via (at 161.313317 136.594781) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 42) (tstamp 2721eecd-5fbb-43d4-9fb0-ab91a7dcd29a))
  (via (at 153.6 134.2) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 42) (tstamp 4cb29675-2735-461c-b583-74231c50e40c))
  (segment (start 163.5762 139.630827) (end 163.182027 140.025) (width 0.1524) (layer "B.Cu") (net 42) (tstamp 19386b99-87e4-4d78-8929-557de1b1f673))
  (segment (start 161.313317 136.594781) (end 161.383098 136.525) (width 0.1524) (layer "B.Cu") (net 42) (tstamp 19495647-11a6-4c75-8ff6-0c4f7f800f17))
  (segment (start 153.6 133.51) (end 153.6 134.2) (width 0.1524) (layer "B.Cu") (net 42) (tstamp 2c6b0f16-ec15-43f9-8bd1-1f1ab0f35819))
  (segment (start 161.383098 136.525) (end 162.4875 136.525) (width 0.1524) (layer "B.Cu") (net 42) (tstamp 315c3feb-ef81-49b0-9ffe-b330d677d78c))
  (segment (start 163.182027 140.025) (end 162.4875 140.025) (width 0.1524) (layer "B.Cu") (net 42) (tstamp 4c195b1d-8157-427e-af85-88732575ec60))
  (segment (start 163.182027 136.525) (end 163.5762 136.919173) (width 0.1524) (layer "B.Cu") (net 42) (tstamp 5d1179d8-98d6-4c1a-a198-5db402e66eee))
  (segment (start 153.6 134.491903) (end 153.775 134.666903) (width 0.1524) (layer "B.Cu") (net 42) (tstamp 63fa6847-b9cc-4ea9-89ac-875ff4038582))
  (segment (start 153.775 134.666903) (end 153.775 135.675) (width 0.1524) (layer "B.Cu") (net 42) (tstamp caafe1ff-0fbb-4764-8af6-d287b2732f3d))
  (segment (start 153.6 134.2) (end 153.6 134.491903) (width 0.1524) (layer "B.Cu") (net 42) (tstamp cb16c8df-8e92-433f-b652-f7af2ecdfde0))
  (segment (start 162.4875 136.525) (end 163.182027 136.525) (width 0.1524) (layer "B.Cu") (net 42) (tstamp f2878d80-4926-4cf6-b589-6cd0247a0dc0))
  (segment (start 163.5762 136.919173) (end 163.5762 139.630827) (width 0.1524) (layer "B.Cu") (net 42) (tstamp f3f4852b-8eac-40d1-9d49-1ee0e6b76731))
  (segment (start 121.24 125.64) (end 118.85 125.64) (width 0.1524) (layer "B.Cu") (net 43) (tstamp 37cbaf4c-f0db-43c5-bd91-8c52f25d16ae))
  (segment (start 159.6476 138.850768) (end 159.6476 138.850064) (width 0.1524) (layer "B.Cu") (net 43) (tstamp 4a953b17-8c34-448b-aeb4-07ca9e89bf2e))
  (segment (start 124.8 129.2) (end 121.24 125.64) (width 0.1524) (layer "B.Cu") (net 43) (tstamp 55388e83-ac5b-4376-b852-290eadc84d72))
  (segment (start 157.2 129.2) (end 124.8 129.2) (width 0.1524) (layer "B.Cu") (net 43) (tstamp 5729caad-b236-4fb2-ad59-5ba8f3d40add))
  (segment (start 159.6476 138.850064) (end 159.652601 138.845062) (width 0.1524) (layer "B.Cu") (net 43) (tstamp 879f0c31-2409-4a16-bcf6-bdc0405e161e))
  (segment (start 121.8 125.11) (end 121.255 125.655) (width 0.1524) (layer "B.Cu") (net 43) (tstamp 93e99410-15bc-4f73-a3be-29d5d087e3bb))
  (segment (start 159.123368 139.375) (end 159.6476 138.850768) (width 0.1524) (layer "B.Cu") (net 43) (tstamp ba5c3169-3d67-4546-816a-9937574689df))
  (segment (start 156.975 139.375) (end 159.123368 139.375) (width 0.1524) (layer "B.Cu") (net 43) (tstamp d137450d-7e1c-460b-872f-880d40bae56f))
  (segment (start 159.652601 131.652601) (end 157.2 129.2) (width 0.1524) (layer "B.Cu") (net 43) (tstamp da1d2ed1-a457-4f76-9f89-f1a5bc630706))
  (segment (start 121.255 125.655) (end 121.4 125.8) (width 0.1524) (layer "B.Cu") (net 43) (tstamp da1fb129-0b60-4fd4-9050-20b8cb3dc2c4))
  (segment (start 159.652601 138.845062) (end 159.652601 131.652601) (width 0.1524) (layer "B.Cu") (net 43) (tstamp ea47c93e-1930-4b1d-b7c2-f52b451b9cc8))
  (segment (start 121.51 126.6) (end 121.6 126.6) (width 0.1524) (layer "B.Cu") (net 44) (tstamp 21690dff-1fdb-4ebf-8bde-52c7aa159dcd))
  (segment (start 157.101632 129.6) (end 124.6 129.6) (width 0.1524) (layer "B.Cu") (net 44) (tstamp 35c57777-11c0-43da-a5f9-fca032fa4883))
  (segment (start 117 126.2) (end 117 125.39) (width 0.1524) (layer "B.Cu") (net 44) (tstamp 6f93b294-52b2-431e-88b1-b54ad33e4532))
  (segment (start 159.3007 138.6993) (end 159.3007 131.799068) (width 0.1524) (layer "B.Cu") (net 44) (tstamp 81341c95-8dab-40b4-bbc9-f447d6ab9bd1))
  (segment (start 120.71 127.4) (end 121.51 126.6) (width 0.1524) (layer "B.Cu") (net 44) (tstamp a62c901e-5ef0-4c1a-aa6c-145383cab223))
  (segment (start 117 125.39) (end 118.02 124.37) (width 0.1524) (layer "B.Cu") (net 44) (tstamp a88551ff-c148-465b-9bf0-add41f4dc428))
  (segment (start 124.6 129.6) (end 121.6 126.6) (width 0.1524) (layer "B.Cu") (net 44) (tstamp ba51db60-9773-4de5-818c-8392b5c85e0d))
  (segment (start 121.6 126.6) (end 117.4 126.6) (width 0.1524) (layer "B.Cu") (net 44) (tstamp bc317e58-3996-4ff6-a2c8-c5f61aa3b4cc))
  (segment (start 118.02 124.37) (end 118.85 124.37) (width 0.1524) (layer "B.Cu") (net 44) (tstamp e443763d-00f4-43f5-97d2-b371ba55864d))
  (segment (start 159.125 138.875) (end 159.3007 138.6993) (width 0.1524) (layer "B.Cu") (net 44) (tstamp e6c542c6-a635-4ae7-ab1a-2173c9edf18f))
  (segment (start 156.975 138.875) (end 159.125 138.875) (width 0.1524) (layer "B.Cu") (net 44) (tstamp ef4d2776-4e3a-4fa9-a335-54694c70deab))
  (segment (start 117.4 126.6) (end 117 126.2) (width 0.1524) (layer "B.Cu") (net 44) (tstamp fdc87dbc-6a8b-4421-8f78-66684cc3ad34))
  (segment (start 159.3007 131.799068) (end 157.101632 129.6) (width 0.1524) (layer "B.Cu") (net 44) (tstamp ff648b36-bc9c-440f-bb41-71695068a70a))
  (segment (start 118.1 144.2) (end 118.1 145.2) (width 0.25) (layer "F.Cu") (net 45) (tstamp 94eb1a78-6acb-417c-bf8f-ded8f5be195e))
  (segment (start 121.2 154) (end 121.2 153.2) (width 0.25) (layer "F.Cu") (net 45) (tstamp e73363f4-86fd-4838-9624-00508ee91667))
  (via (at 121.2 154) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 45) (tstamp 335fda18-ef08-4a69-8611-3277cdf2ee69))
  (via (at 118.1 144.2) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 45) (tstamp a52b6ce0-00d7-457d-9115-da924dd7bfcf))
  (segment (start 121.99 154) (end 121.2 154) (width 0.25) (layer "B.Cu") (net 45) (tstamp 013f6bf1-9f9c-4e0b-a976-8e3328240f17))
  (segment (start 152.075 139.875) (end 151.502111 139.875) (width 0.25) (layer "B.Cu") (net 45) (tstamp 272ba19c-76b7-48c8-a7b7-80a5817f0d4a))
  (segment (start 151.2 143.2) (end 150.8 143.6) (width 0.25) (layer "B.Cu") (net 45) (tstamp 6b420b47-0277-43a2-a631-728047c5b235))
  (segment (start 151.502111 139.875) (end 151.2 140.177111) (width 0.25) (layer "B.Cu") (net 45) (tstamp 8d9fd5fe-60e0-4cad-9ca5-c3e5bb451c8c))
  (segment (start 118.7 143.6) (end 118.1 144.2) (width 0.25) (layer "B.Cu") (net 45) (tstamp 983bc9da-70b7-416d-b32d-170ab878b0db))
  (segment (start 151.2 140.177111) (end 151.2 143.2) (width 0.25) (layer "B.Cu") (net 45) (tstamp ab5b104f-714d-41fa-94ac-30a47a77f188))
  (segment (start 150.8 143.6) (end 118.7 143.6) (width 0.25) (layer "B.Cu") (net 45) (tstamp c755ef27-8b64-4efd-8b5d-1c34dce969d3))
  (segment (start 126.2 154) (end 126.2 153.2) (width 0.25) (layer "F.Cu") (net 46) (tstamp 44a7b275-1b92-4721-b4ad-3f4bb9ded1bc))
  (segment (start 123.7 154) (end 123.7 153.2) (width 0.25) (layer "F.Cu") (net 46) (tstamp 48c5b635-df05-4e03-9a32-35193f21e5c7))
  (via (at 123.7 154) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 46) (tstamp 8a333905-d7bf-4d29-9c0a-0835579d88cd))
  (via (at 126.2 154) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 46) (tstamp def6625a-c3f2-42db-89a5-ac2a0bd83a88))
  (segment (start 123.01 154) (end 123.7 154) (width 0.25) (layer "B.Cu") (net 46) (tstamp 6e81a8c9-ee9a-4947-9008-c5477dba1e29))
  (segment (start 126.99 154) (end 126.2 154) (width 0.25) (layer "B.Cu") (net 46) (tstamp e5a0090f-3a1c-4c6c-a3d7-34895a9521ad))
  (segment (start 129 154) (end 129 153.2) (width 0.25) (layer "F.Cu") (net 47) (tstamp 6e6b4cc6-4f59-4b74-86fc-a576f8305d37))
  (segment (start 131.8 154) (end 131.8 153.2) (width 0.25) (layer "F.Cu") (net 47) (tstamp ea3d5bfb-1f4b-48b3-a38d-47d062ca727c))
  (via (at 129 154) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 47) (tstamp 84d1a211-7ab7-4d86-a82a-00103e19b8c9))
  (via (at 131.8 154) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 47) (tstamp ef51f86d-7378-44ea-97b1-121a8ca6010c))
  (segment (start 132.49 154) (end 131.8 154) (width 0.25) (layer "B.Cu") (net 47) (tstamp c13490bd-eee2-4099-802e-068956eaa306))
  (segment (start 128.01 154) (end 129 154) (width 0.25) (layer "B.Cu") (net 47) (tstamp f7ed1e22-3cb2-42a4-8615-28a4a449af61))
  (segment (start 134.4 154) (end 134.4 153.2) (width 0.25) (layer "F.Cu") (net 48) (tstamp 4e0d8c30-0803-4073-825a-f477d3e4763d))
  (segment (start 134.6 144.7) (end 133.583912 145.716088) (width 0.25) (layer "F.Cu") (net 48) (tstamp 6d901d0d-4ee5-40e0-b24e-0e994f9cfb80))
  (segment (start 134.6 144.2) (end 134.6 144.7) (width 0.25) (layer "F.Cu") (net 48) (tstamp ca3ca87e-8632-4222-b54f-87f3c4b06dd3))
  (segment (start 133.583912 145.716088) (end 133.125 145.716088) (width 0.25) (layer "F.Cu") (net 48) (tstamp faa19e06-4d85-4341-af5d-5fa648939473))
  (segment (start 136.6 154) (end 136.6 153.2) (width 0.25) (layer "F.Cu") (net 48) (tstamp fc9458a6-4482-4765-add6-fb9cbcfbbb75))
  (via (at 134.6 144.2) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 48) (tstamp 7b88c455-9d91-4788-aaae-19787fbdcf5b))
  (via (at 136.6 154) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 48) (tstamp b23f7b4b-13d5-42e4-bc23-922a28f4e35a))
  (via (at 134.4 154) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 48) (tstamp ca1473a6-171a-4fcb-ad8c-4390bc616a82))
  (segment (start 134.7 144.1) (end 134.6 144.2) (width 0.25) (layer "B.Cu") (net 48) (tstamp 0d430d2c-4121-4e96-a1e4-98d5129a9088))
  (segment (start 151.1 144.1) (end 134.7 144.1) (width 0.25) (layer "B.Cu") (net 48) (tstamp 31634e94-db6f-4f64-af03-0b47631c5285))
  (segment (start 137.49 154) (end 136.6 154) (width 0.25) (layer "B.Cu") (net 48) (tstamp 7773cb8c-866d-41b9-bf0c-0f565233fa3c))
  (segment (start 152.775 142.425) (end 151.1 144.1) (width 0.25) (layer "B.Cu") (net 48) (tstamp a0806127-a545-492a-9c0f-6dd7f9c260d1))
  (segment (start 133.51 154) (end 134.4 154) (width 0.25) (layer "B.Cu") (net 48) (tstamp c50aba9f-0441-466c-b02c-3e420db0b102))
  (segment (start 152.775 140.575) (end 152.775 142.425) (width 0.25) (layer "B.Cu") (net 48) (tstamp dba9459e-b3b5-42b5-99a7-78858b129818))
  (segment (start 141.6 154) (end 141.6 153.2) (width 0.25) (layer "F.Cu") (net 49) (tstamp 0a3fd235-fd78-44be-a8ef-688e852cdf28))
  (segment (start 139.4 154) (end 139.4 153.2) (width 0.25) (layer "F.Cu") (net 49) (tstamp 2e4b9f13-f54b-4b61-bac5-1541c778391f))
  (via (at 139.4 154) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 49) (tstamp 3400d1df-59b2-44ec-b7de-1547deed1401))
  (via (at 141.6 154) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 49) (tstamp 3dac8cbf-9875-4933-802d-e5bf46ba4375))
  (segment (start 142.49 154) (end 141.6 154) (width 0.25) (layer "B.Cu") (net 49) (tstamp 08ccc58a-8e5e-4c0d-a0ae-c0b4835101a6))
  (segment (start 138.51 154) (end 139.4 154) (width 0.25) (layer "B.Cu") (net 49) (tstamp b5fd5b68-2abe-4dd5-a4eb-388bcfd38d36))
  (segment (start 144.4 154) (end 144.4 153.2) (width 0.25) (layer "F.Cu") (net 50) (tstamp 3a642489-6f0e-4b9b-a894-bb93b121cb13))
  (segment (start 147.2 154) (end 147.2 153.2) (width 0.25) (layer "F.Cu") (net 50) (tstamp b2468319-dffb-4bd8-99fc-a86483cdefc0))
  (via (at 144.4 154) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 50) (tstamp 16e1ddd9-3615-4d27-a96a-a40d85f0919d))
  (via (at 147.2 154) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 50) (tstamp 1a623483-804d-4094-8209-6166b64d482b))
  (segment (start 147.99 154) (end 147.2 154) (width 0.25) (layer "B.Cu") (net 50) (tstamp 1d1cd0fe-86e0-4bd5-afb6-ab133b4eb073))
  (segment (start 143.51 154) (end 144.4 154) (width 0.25) (layer "B.Cu") (net 50) (tstamp 65f27d31-d517-48ee-a252-42eb727522b8))
  (segment (start 149.8 154) (end 149.8 153.2) (width 0.25) (layer "F.Cu") (net 51) (tstamp 4963ccac-7272-4f69-87ba-475554ac1ae9))
  (segment (start 150.106568 145.870544) (end 151.538556 144.438556) (width 0.25) (layer "F.Cu") (net 51) (tstamp 4adc2695-81e1-4756-ac94-5a2a9abe80ca))
  (segment (start 152.6 154) (end 152.6 153.2) (width 0.25) (layer "F.Cu") (net 51) (tstamp 7e30fd41-8014-49d2-a4dd-89d115dc7485))
  (segment (start 149.029456 145.870544) (end 150.106568 145.870544) (width 0.25) (layer "F.Cu") (net 51) (tstamp ccb0a483-9e51-4549-8731-e34c260b68e9))
  (via (at 149.8 154) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 51) (tstamp 101a275f-6888-4301-80cd-74aede690dc0))
  (via (at 152.6 154) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 51) (tstamp f94a3319-72d2-4af8-8261-dcbbebc4281c))
  (via (at 151.538556 144.438556) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 51) (tstamp f9641beb-855f-4c18-81c1-01b3ecc6a4a4))
  (segment (start 153.275 142.725) (end 151.561444 144.438556) (width 0.25) (layer "B.Cu") (net 51) (tstamp 083bc72d-809c-4117-a3bf-96f5839e3130))
  (segment (start 153.275 140.575) (end 153.275 142.725) (width 0.25) (layer "B.Cu") (net 51) (tstamp 3afb0bf0-6478-4f5c-8dd4-5fedcf06db96))
  (segment (start 149.01 154) (end 149.8 154) (width 0.25) (layer "B.Cu") (net 51) (tstamp 44a00d9b-e351-4af2-89e9-f357930c2cd4))
  (segment (start 151.561444 144.438556) (end 151.538556 144.438556) (width 0.25) (layer "B.Cu") (net 51) (tstamp 804ba6b3-51ec-459b-93de-3664cf9f6955))
  (segment (start 153.49 154) (end 152.6 154) (width 0.25) (layer "B.Cu") (net 51) (tstamp 9fa86961-775d-4849-9762-04f99d99afb8))
  (segment (start 157.6 154) (end 157.6 153.2) (width 0.25) (layer "F.Cu") (net 52) (tstamp 7cbd9c65-ec56-4053-8e2a-3015ae2af4ae))
  (segment (start 155.4 154) (end 155.4 153.2) (width 0.25) (layer "F.Cu") (net 52) (tstamp d0bf8cc1-f686-4080-95a5-412e61ac38d9))
  (via (at 157.6 154) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 52) (tstamp 1d87c253-271c-4653-9290-316cbe53b1da))
  (via (at 155.4 154) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 52) (tstamp a91221bc-b028-4c4e-b8ff-6b4bff53e6b5))
  (segment (start 158.49 154) (end 157.6 154) (width 0.25) (layer "B.Cu") (net 52) (tstamp 310bb259-900e-49fe-bc0d-d14c6e845aef))
  (segment (start 154.51 154) (end 155.4 154) (width 0.25) (layer "B.Cu") (net 52) (tstamp 8bdd3771-a40a-4144-bd51-7ce8cf2e274c))
  (segment (start 163.2 154) (end 163.2 153.2) (width 0.25) (layer "F.Cu") (net 53) (tstamp 49611896-e639-4c54-b26a-cadfbe3fd514))
  (segment (start 160.4 154) (end 160.4 153.2) (width 0.25) (layer "F.Cu") (net 53) (tstamp b976dcad-cbb3-4cc6-b361-57ccba9766a2))
  (via (at 160.4 154) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 53) (tstamp 3cee2750-d838-4ade-a039-3b4e0b519a74))
  (via (at 163.2 154) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 53) (tstamp 6668ad79-30ba-4c06-a949-49e1c18f0de5))
  (segment (start 159.51 154) (end 160.4 154) (width 0.25) (layer "B.Cu") (net 53) (tstamp a663bd5a-18ee-4fc5-890a-78a67af31454))
  (segment (start 163.99 154) (end 163.2 154) (width 0.25) (layer "B.Cu") (net 53) (tstamp fbbcc37e-5764-4e93-bac6-dfd57a2c5777))
  (segment (start 165.8 154) (end 165.8 153.2) (width 0.25) (layer "F.Cu") (net 54) (tstamp 0b32eae2-f6f5-49d7-83ad-1aa54d8e9151))
  (segment (start 168.2 154) (end 168.2 153.2) (width 0.25) (layer "F.Cu") (net 54) (tstamp 75b7bcf1-b353-4618-ba04-c1324aae57a7))
  (segment (start 165.7 145.241086) (end 165.7 144.4495) (width 0.25) (layer "F.Cu") (net 54) (tstamp d96fdfdd-1477-4700-8fab-80bef8954b53))
  (via (at 165.8 154) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 54) (tstamp 8c98bcb7-75a4-425f-9da2-9220cb451dde))
  (via (at 168.2 154) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 54) (tstamp faef6073-da73-42d8-ac41-1bd2d495848f))
  (via (at 165.7 144.4495) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 54) (tstamp fe24d64c-304e-43fe-9266-b62c72ad862a))
  (segment (start 168.99 154) (end 168.2 154) (width 0.25) (layer "B.Cu") (net 54) (tstamp 165badd9-090a-4b29-ace8-b0d0a6365d1c))
  (segment (start 155.41381 144.4495) (end 165.7 144.4495) (width 0.25) (layer "B.Cu") (net 54) (tstamp 4b1ba65e-3e44-405f-8aa5-b74f15873643))
  (segment (start 153.775 140.575) (end 153.775 142.81069) (width 0.25) (layer "B.Cu") (net 54) (tstamp 732ca91a-de56-478f-8f36-de58882f9e10))
  (segment (start 165.01 154) (end 165.8 154) (width 0.25) (layer "B.Cu") (net 54) (tstamp a1148f4e-66a4-48d1-a6fa-fedd25c2c000))
  (segment (start 153.775 142.81069) (end 155.41381 144.4495) (width 0.25) (layer "B.Cu") (net 54) (tstamp ae6db93c-fed2-47c7-a6c7-bb259d241310))
  (segment (start 170.8 154) (end 170.8 153.2) (width 0.25) (layer "F.Cu") (net 55) (tstamp f1b367ef-3bc5-4547-998c-1c68e6f97802))
  (segment (start 173.6 154) (end 173.6 153.2) (width 0.25) (layer "F.Cu") (net 55) (tstamp f6fe888d-b5b9-41f3-89d3-e7092e28559a))
  (via (at 173.6 154) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 55) (tstamp c0bae15c-8419-4e99-8719-cedf4f191713))
  (via (at 170.8 154) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 55) (tstamp ca63cae9-2348-4dad-975b-4d8e1c9cfd79))
  (segment (start 174.49 154) (end 173.6 154) (width 0.25) (layer "B.Cu") (net 55) (tstamp 23292669-c11a-4daa-8954-307d1a2a88ed))
  (segment (start 170.01 154) (end 170.8 154) (width 0.25) (layer "B.Cu") (net 55) (tstamp 731cf85d-791e-4898-a59c-96c257d4fc8f))
  (segment (start 176.2 154) (end 176.2 153.2) (width 0.25) (layer "F.Cu") (net 56) (tstamp 8643699e-98d9-45f5-a0f1-d980f8665d0c))
  (segment (start 178.6 154) (end 178.6 153.2) (width 0.25) (layer "F.Cu") (net 56) (tstamp 8f2b1dd4-3e6a-4f95-865a-b588dd9e9bc7))
  (via (at 176.2 154) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 56) (tstamp 87e7eed8-f52d-4e36-a7b0-b24ab3be6f58))
  (via (at 178.6 154) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 56) (tstamp f789e490-d0d3-436b-a41b-b4562f661769))
  (segment (start 175.51 154) (end 176.2 154) (width 0.25) (layer "B.Cu") (net 56) (tstamp 60017f47-db9d-4be7-bc77-555659ef1459))
  (segment (start 179.49 154) (end 178.6 154) (width 0.25) (layer "B.Cu") (net 56) (tstamp 95d22901-bb9e-4830-92fa-433d1c4e2d07))
  (segment (start 181.4 154) (end 181.4 153.2) (width 0.25) (layer "F.Cu") (net 57) (tstamp 0869db35-39c1-4662-a25c-f8d917268e65))
  (segment (start 183.3 145.05) (end 183.3 143.9495) (width 0.25) (layer "F.Cu") (net 57) (tstamp 82d488d8-4af4-4d75-ad69-9e5c399793ea))
  (via (at 181.4 154) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 57) (tstamp 4f45abf7-f66b-48a3-8d7c-4aae91fecf1d))
  (via (at 183.3 143.9495) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 57) (tstamp 6ce47063-3315-45ac-bdb5-7f2740c24603))
  (segment (start 180.51 154) (end 181.4 154) (width 0.25) (layer "B.Cu") (net 57) (tstamp 146a0c83-2d47-42c4-9390-aad4463bc281))
  (segment (start 154.275 140.575) (end 154.275 142.675) (width 0.25) (layer "B.Cu") (net 57) (tstamp 8d35ddb2-628a-4fbd-bef4-f3fae43dd7d7))
  (segment (start 183.2505 143.9) (end 183.3 143.9495) (width 0.25) (layer "B.Cu") (net 57) (tstamp 989e0910-7dd5-4204-a0ee-587973a1212e))
  (segment (start 155.5 143.9) (end 183.2505 143.9) (width 0.25) (layer "B.Cu") (net 57) (tstamp b1a19c37-89d4-4f8e-9c7f-74401c09da3b))
  (segment (start 154.275 142.675) (end 155.5 143.9) (width 0.25) (layer "B.Cu") (net 57) (tstamp bd8c16fb-dd2e-42b5-acbd-bbcc07121ee4))
  (segment (start 153.41 119.9225) (end 152.9375 119.45) (width 0.25) (layer "B.Cu") (net 60) (tstamp 39337374-72fa-4741-b507-34adb989edba))
  (segment (start 153.41 121.8) (end 153.41 119.9225) (width 0.25) (layer "B.Cu") (net 60) (tstamp 7d8e22b6-af9d-4f51-91f0-e18ee9ba6497))
  (segment (start 188.2 153.4) (end 188.2 152.9) (width 0.1524) (layer "F.Cu") (net 61) (tstamp 18131db8-1425-4439-b1b9-afaa168f8794))
  (segment (start 192.29 153.9) (end 188.7 153.9) (width 0.1524) (layer "F.Cu") (net 61) (tstamp 61610ca3-dee2-4c8f-92fb-d5675352c98e))
  (segment (start 192.89 153.3) (end 192.29 153.9) (width 0.1524) (layer "F.Cu") (net 61) (tstamp 91064d20-1555-4caa-bd34-df070b90e191))
  (segment (start 188.7 153.9) (end 188.2 153.4) (width 0.1524) (layer "F.Cu") (net 61) (tstamp 9de97d8d-bc7f-43b8-96bc-0f9bbd3fc049))
  (via (at 188.2 152.9) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 61) (tstamp 5c9ee0c5-ebac-4a77-b150-40103931e46a))
  (segment (start 189.18 152.9) (end 189.23 152.95) (width 0.1524) (layer "B.Cu") (net 61) (tstamp 3717c85b-33a0-416a-adfe-1ae2eccf8b0e))
  (segment (start 188.2 152.9) (end 189.18 152.9) (width 0.1524) (layer "B.Cu") (net 61) (tstamp a411fce5-88e0-4937-8ce7-5c47cb76bc83))
  (segment (start 188.7 154.3) (end 188.2 154.8) (width 0.1524) (layer "F.Cu") (net 62) (tstamp 1ec5fafa-b8be-428a-a427-8f94eb0faf5c))
  (segment (start 192.89 154.3) (end 188.7 154.3) (width 0.1524) (layer "F.Cu") (net 62) (tstamp 855ae4d7-a881-4c3c-b6b7-d70a9b8ee7c8))
  (segment (start 188.2 154.8) (end 188.2 156) (width 0.1524) (layer "F.Cu") (net 62) (tstamp fdbf8ff0-3ca5-4437-8169-bcefe23cce88))
  (via (at 188.2 156) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 62) (tstamp dbc00b04-7038-433a-8a88-4885b4fbbf07))
  (segment (start 188.2 156) (end 189.18 156) (width 0.1524) (layer "B.Cu") (net 62) (tstamp 4c654fed-281a-429e-9308-afb0d9d65c30))
  (segment (start 189.18 156) (end 189.23 155.95) (width 0.1524) (layer "B.Cu") (net 62) (tstamp e994029b-3c10-46fa-ac7c-0acb341d6783))
  (segment (start 187.375 143.575) (end 187.375 149.125) (width 0.25) (layer "B.Cu") (net 63) (tstamp 24c172d0-90ce-4259-8bde-fd00fdf8b7d1))
  (segment (start 155.775 140.575) (end 155.775 141.695) (width 0.25) (layer "B.Cu") (net 63) (tstamp 3109e668-1b38-4852-86af-4359594f72b2))
  (segment (start 155.275 141.187391) (end 155.88 141.792391) (width 0.25) (layer "B.Cu") (net 63) (tstamp 4fd01562-6c49-485e-9f49-f2f26745ceee))
  (segment (start 155.88 141.792391) (end 155.88 141.8) (width 0.25) (layer "B.Cu") (net 63) (tstamp 6fad7c17-6415-4096-8893-23f4f9e2de43))
  (segment (start 155.88 142.88) (end 156.4 143.4) (width 0.25) (layer "B.Cu") (net 63) (tstamp 73c75322-ab98-44f4-9d54-4865eae8fe2a))
  (segment (start 155.775 141.695) (end 155.88 141.8) (width 0.25) (layer "B.Cu") (net 63) (tstamp 86f30085-b785-4f85-9cb4-88229e929ece))
  (segment (start 156.4 143.4) (end 187.2 143.4) (width 0.25) (layer "B.Cu") (net 63) (tstamp a7eb37e7-192d-4d75-a5fe-a9084153739e))
  (segment (start 155.88 141.8) (end 155.88 142.88) (width 0.25) (layer "B.Cu") (net 63) (tstamp aafa3fcc-4324-41f4-bd8c-f728e94e2ef9))
  (segment (start 155.275 140.575) (end 155.275 141.187391) (width 0.25) (layer "B.Cu") (net 63) (tstamp b8e257de-cc10-4d02-ab40-051bf10ff1c5))
  (segment (start 187.2 143.4) (end 187.375 143.575) (width 0.25) (layer "B.Cu") (net 63) (tstamp eab5987e-dbd7-4d07-a240-8cc92b7c4a38))
  (via (at 150.583828 139.194609) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 65) (tstamp 21fe88a6-78ab-48d7-921a-6f224f57cced))
  (segment (start 150.903437 138.875) (end 150.583828 139.194609) (width 0.1524) (layer "B.Cu") (net 65) (tstamp 7979e354-586b-4aba-960f-360728508350))
  (segment (start 152.075 138.875) (end 150.903437 138.875) (width 0.1524) (layer "B.Cu") (net 65) (tstamp b13aad87-fe4f-41b8-a484-ab291d5e0002))
  (via (at 151.2 139.4) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 66) (tstamp a6430115-2401-425d-ad25-3a6540b0fef1))
  (segment (start 152.075 139.375) (end 151.225 139.375) (width 0.1524) (layer "B.Cu") (net 66) (tstamp 43a60f36-f75e-4394-8509-d5f505ef46b2))
  (segment (start 151.225 139.375) (end 151.2 139.4) (width 0.1524) (layer "B.Cu") (net 66) (tstamp cc53731f-57c3-4028-8ee7-8b36398372c6))
  (segment (start 157.0096 136.3404) (end 157.0096 130.612862) (width 0.1524) (layer "B.Cu") (net 69) (tstamp 2efe0f7d-e113-40a4-90e9-dee07d63e526))
  (segment (start 156.975 136.375) (end 157.0096 136.3404) (width 0.1524) (layer "B.Cu") (net 69) (tstamp 6444d2bb-c157-457a-bc49-39491b62a001))
  (segment (start 157.0096 130.612862) (end 156.498368 130.101631) (width 0.1524) (layer "B.Cu") (net 69) (tstamp 8d26fd45-7299-402a-a168-dd724f94f7cb))
  (segment (start 175.8 108.6) (end 175.8 128.2) (width 0.1524) (layer "F.Cu") (net 70) (tstamp 03ac2e22-dd9c-4e97-a74e-1ba9b82d2a2f))
  (segment (start 175.8 128.2) (end 172.6 131.4) (width 0.1524) (layer "F.Cu") (net 70) (tstamp 62f75139-e1cf-4866-9e50-b339a7ef0d29))
  (segment (start 172.6 131.4) (end 158.1007 131.4) (width 0.1524) (layer "F.Cu") (net 70) (tstamp d982b930-ae39-4d36-81d7-10a77cf6437e))
  (via (at 158.1007 131.4) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 70) (tstamp e3b0f608-3bdc-402d-90bc-7c9b108abcb0))
  (segment (start 158.2435 133.504704) (end 157.9464 133.207604) (width 0.1524) (layer "B.Cu") (net 70) (tstamp 1d3bba95-2c1a-41b5-858a-55069da69b46))
  (segment (start 157.9464 131.5543) (end 158.1007 131.4) (width 0.1524) (layer "B.Cu") (net 70) (tstamp 7550b8c8-e112-49bc-b13e-ecf3a6db61db))
  (segment (start 157.525 136.875) (end 158.2435 136.1565) (width 0.1524) (layer "B.Cu") (net 70) (tstamp 90ba4180-379f-41f3-9ec2-c401bd5319cf))
  (segment (start 156.975 136.875) (end 157.525 136.875) (width 0.1524) (layer "B.Cu") (net 70) (tstamp b5bf9372-08b2-42ac-a2cd-b98efe5b9e43))
  (segment (start 158.2435 136.1565) (end 158.2435 133.504704) (width 0.1524) (layer "B.Cu") (net 70) (tstamp c2ca81dc-e667-4142-bd92-e00ec42daff7))
  (segment (start 157.9464 133.207604) (end 157.9464 131.5543) (width 0.1524) (layer "B.Cu") (net 70) (tstamp c8d23eb5-f788-4402-953f-e9c854af2922))
  (segment (start 160 139.2) (end 159.325 139.875) (width 0.1524) (layer "B.Cu") (net 72) (tstamp 09b3ea9d-26df-450f-a333-291f4211d5ec))
  (segment (start 159.325 139.875) (end 156.975 139.875) (width 0.1524) (layer "B.Cu") (net 72) (tstamp 219c9231-1083-44bb-ac08-e1e7806524f7))
  (segment (start 162.4875 135.875) (end 161.325 135.875) (width 0.1524) (layer "B.Cu") (net 72) (tstamp 257ccea6-e310-4aa0-a5b6-bfc3e11f57be))
  (segment (start 160 138.995328) (end 160 139.2) (width 0.1524) (layer "B.Cu") (net 72) (tstamp 2e422d67-1e4b-41ca-a471-5503463368a5))
  (segment (start 160.004503 138.990825) (end 160 138.995328) (width 0.1524) (layer "B.Cu") (net 72) (tstamp 4bfe6678-4050-46f7-8701-8b2cf7563d67))
  (segment (start 160.004502 137.195498) (end 160.004503 138.990825) (width 0.1524) (layer "B.Cu") (net 72) (tstamp 63b3d8b3-f672-4d89-be23-2186cce1d538))
  (segment (start 161.325 135.875) (end 160.004502 137.195498) (width 0.1524) (layer "B.Cu") (net 72) (tstamp eca8786c-3ebb-4e61-a047-db6e1d7f1819))
  (segment (start 156.275 141.075) (end 156.275 140.575) (width 0.1524) (layer "B.Cu") (net 73) (tstamp 1cf743d2-ba57-469b-aa67-c1e949baa28c))
  (segment (start 163.928101 140.578926) (end 163.107027 141.4) (width 0.1524) (layer "B.Cu") (net 73) (tstamp 2b9bdabd-2216-4bc6-b542-22165c29c1cb))
  (segment (start 163.928101 136.871899) (end 163.928101 140.578926) (width 0.1524) (layer "B.Cu") (net 73) (tstamp 5b4e17fc-c390-4df9-a007-f30e67c2912b))
  (segment (start 156.6 141.4) (end 156.275 141.075) (width 0.1524) (layer "B.Cu") (net 73) (tstamp 9426e2f6-f157-4b18-9138-a1f960ba2454))
  (segment (start 163.107027 141.4) (end 156.6 141.4) (width 0.1524) (layer "B.Cu") (net 73) (tstamp a46adbc4-ebed-41a0-ab18-deb937b93c10))
  (segment (start 166.7125 136.525) (end 164.275 136.525) (width 0.1524) (layer "B.Cu") (net 73) (tstamp b03cc1b2-70ee-4cb4-9512-cae482ffe258))
  (segment (start 164.275 136.525) (end 163.928101 136.871899) (width 0.1524) (layer "B.Cu") (net 73) (tstamp e8a690c1-c213-4d12-9f38-987f603933ea))
  (segment (start 154.775 140.575) (end 154.775 141.655) (width 0.25) (layer "B.Cu") (net 74) (tstamp 80bfadaf-9bd4-468e-913f-779f16c5ca21))
  (segment (start 154.775 141.655) (end 154.92 141.8) (width 0.25) (layer "B.Cu") (net 74) (tstamp e8a1882d-2648-408c-be6c-b06ff8cd3bae))
  (via (at 151.5 119.5) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 75) (tstamp 6d214271-713f-40af-9b92-61eff9e023f9))
  (via (at 150.874259 137.757569) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 75) (tstamp 840c0305-1fb0-4ebd-a4ff-3600626e493a))
  (segment (start 150.99169 137.875) (end 150.874259 137.757569) (width 0.1524) (layer "B.Cu") (net 75) (tstamp 2f5f4f5d-2785-4916-9973-e7a8d2c9a4b5))
  (segment (start 152.075 137.875) (end 150.99169 137.875) (width 0.1524) (layer "B.Cu") (net 75) (tstamp b424f89e-672b-4636-be07-253791ce7cdc))
  (segment (start 183.8 140.6) (end 182.8476 141.5524) (width 0.1524) (layer "F.Cu") (net 76) (tstamp 07d93507-6475-4e05-83e4-9d1dcded9050))
  (segment (start 160.302131 138.000499) (end 157.701632 135.4) (width 0.1524) (layer "F.Cu") (net 76) (tstamp 4cb504e1-59b4-42a0-94ad-1b372feb4e8a))
  (segment (start 183 137.8) (end 183.8 138.6) (width 0.1524) (layer "F.Cu") (net 76) (tstamp 4fdd3522-13bd-4e1a-9ef5-c2c3537b9665))
  (segment (start 169.702131 138.000499) (end 160.302131 138.000499) (width 0.1524) (layer "F.Cu") (net 76) (tstamp 660728e9-c914-475e-a2f9-921e1b26524b))
  (segment (start 152 135.4) (end 151.4 136) (width 0.1524) (layer "F.Cu") (net 76) (tstamp 696375f4-22f8-4cb2-9b00-93be109405e7))
  (segment (start 157.701632 135.4) (end 152 135.4) (width 0.1524) (layer "F.Cu") (net 76) (tstamp 958a6845-b745-4a5b-a491-c229996206c8))
  (segment (start 182.8476 141.5524) (end 173.254032 141.5524) (width 0.1524) (layer "F.Cu") (net 76) (tstamp d97ee328-eb4f-4d96-ab7b-2be919c79ff9))
  (segment (start 173.254032 141.5524) (end 169.702131 138.000499) (width 0.1524) (layer "F.Cu") (net 76) (tstamp e30ef125-ec30-4323-9767-27430c349013))
  (segment (start 183.8 138.6) (end 183.8 140.6) (width 0.1524) (layer "F.Cu") (net 76) (tstamp f5001dbc-68aa-4f33-9ac0-554bc5165cbd))
  (via (at 151.4 136) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 76) (tstamp 405f4ccb-6007-481d-a6e3-078a33425b6c))
  (via (at 183 137.8) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 76) (tstamp 447aa751-4187-4aae-8658-2a7de6a5a6cc))
  (segment (start 181.38 137.665) (end 182.865 137.665) (width 0.1524) (layer "B.Cu") (net 76) (tstamp 2a097dca-501e-4585-adf0-92eab695af41))
  (segment (start 182.865 137.665) (end 183 137.8) (width 0.1524) (layer "B.Cu") (net 76) (tstamp 73951cf4-9274-4424-8553-8db429c0d0a9))
  (segment (start 152.075 136.375) (end 151.775 136.375) (width 0.1524) (layer "B.Cu") (net 76) (tstamp 9685c82d-0909-4d8a-9873-51582b510292))
  (segment (start 151.775 136.375) (end 151.4 136) (width 0.1524) (layer "B.Cu") (net 76) (tstamp ee799e16-035a-4be7-9ad9-c4bb24fb91de))
  (segment (start 183.4 139.2) (end 183.2 139) (width 0.1524) (layer "F.Cu") (net 77) (tstamp 11216c37-bba9-466a-893f-7f199ff99298))
  (segment (start 182.702336 141.2) (end 183.4 140.502336) (width 0.1524) (layer "F.Cu") (net 77) (tstamp 1894f8c1-ce1e-4598-ae8e-fddea6265b34))
  (segment (start 157.6 134.8) (end 160.448099 137.648099) (width 0.1524) (layer "F.Cu") (net 77) (tstamp 318ed33e-278b-4188-8b2c-0a926d6fa26c))
  (segment (start 160.448099 137.648099) (end 169.848099 137.648099) (width 0.1524) (layer "F.Cu") (net 77) (tstamp 43a55b80-b56a-4e53-8eb2-9635b5219622))
  (segment (start 153.2 134.8) (end 157.6 134.8) (width 0.1524) (layer "F.Cu") (net 77) (tstamp a87214da-da36-4e4d-bbef-b51e480dd14a))
  (segment (start 169.848099 137.648099) (end 173.4 141.2) (width 0.1524) (layer "F.Cu") (net 77) (tstamp a904b9a0-102a-40c7-bd01-bf5a52abd0aa))
  (segment (start 173.4 141.2) (end 182.702336 141.2) (width 0.1524) (layer "F.Cu") (net 77) (tstamp bd2917d5-57ec-4390-ae65-5367b9d18ff3))
  (segment (start 183.4 140.502336) (end 183.4 139.2) (width 0.1524) (layer "F.Cu") (net 77) (tstamp ed3fbc85-0b5a-4f69-8672-a6fe065a7b1b))
  (via (at 153.2 134.8) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 77) (tstamp 8241c044-f30e-4211-abe6-94958c202bae))
  (via (at 183.2 139) (size 0.45) (drill 0.2) (layers "F.Cu" "B.Cu") (net 77) (tstamp af3b1d89-3476-435e-9ec4-4b382e141e17))
  (segment (start 183.2 139) (end 183.135 138.935) (width 0.1524) (layer "B.Cu") (net 77) (tstamp 713a1e0b-89fe-480c-b5a4-b2754d2de32d))
  (segment (start 153.275 134.875) (end 153.2 134.8) (width 0.1524) (layer "B.Cu") (net 77) (tstamp 7a1bcecd-d45f-4c3a-bb98-209b801cb30a))
  (segment (start 153.275 135.675) (end 153.275 134.875) (width 0.1524) (layer "B.Cu") (net 77) (tstamp 89ac7737-8c49-4d8b-9953-b4c18ad0bf69))
  (segment (start 183.135 138.935) (end 181.38 138.935) (width 0.1524) (layer "B.Cu") (net 77) (tstamp cc58a6d5-1d23-4c29-8c5c-03d950df306d))
  (segment (start 154.775 135.025) (end 155.6 134.2) (width 0.1524) (layer "B.Cu") (net 78) (tstamp 3b4612fd-ed06-45d9-ac26-a19a9fdfb415))
  (segment (start 155.6 134.2) (end 155.6 131.4) (width 0.1524) (layer "B.Cu") (net 78) (tstamp 3c0a68f2-e19f-4003-a903-8d5fb7262284))
  (segment (start 154.775 135.675) (end 154.775 135.025) (width 0.1524) (layer "B.Cu") (net 78) (tstamp 764e01fd-c7ba-430f-8283-0b55170ac641))
  (segment (start 155.6 131.4) (end 155.4 131.2) (width 0.1524) (layer "B.Cu") (net 78) (tstamp f9f82af5-f25b-4f3b-8d7a-d7217a4bb692))
  (segment (start 156 130.701632) (end 156 130.6) (width 0.1524) (layer "B.Cu") (net 79) (tstamp 03418dc3-b18b-4ee9-8fe4-4b5e49f3a7dd))
  (segment (start 156.3048 131.006432) (end 156 130.701632) (width 0.1524) (layer "B.Cu") (net 79) (tstamp 93a87c51-8d86-41d7-976a-b01f9d671d22))
  (segment (start 156.3048 134.491937) (end 156.3048 131.006432) (width 0.1524) (layer "B.Cu") (net 79) (tstamp 9d23d927-eb65-4bf0-97d0-4f205b011aad))
  (segment (start 155.775 135.021736) (end 156.3048 134.491937) (width 0.1524) (layer "B.Cu") (net 79) (tstamp c21c6d23-cdcb-4daa-b886-28319ea17822))
  (segment (start 155.775 135.675) (end 155.775 135.021736) (width 0.1524) (layer "B.Cu") (net 79) (tstamp d862be8b-169c-4828-8964-032eb82aa324))
  (segment (start 168.4 135.4) (end 167.925 135.875) (width 0.25) (layer "B.Cu") (net 80) (tstamp 37746acc-6320-4854-b1f1-0b0190bce913))
  (segment (start 167.925 135.875) (end 166.7125 135.875) (width 0.25) (layer "B.Cu") (net 80) (tstamp da8bdc04-bb6c-40d3-834d-a64872ac4e11))
  (segment (start 190.3 154.1) (end 189.9 154.5) (width 0.1524) (layer "B.Cu") (net 83) (tstamp 01c5357f-2503-4a79-908a-b7fa2721f7fa))
  (segment (start 192.0988 148.861301) (end 192.063699 148.8262) (width 0.1524) (layer "B.Cu") (net 83) (tstamp 078fda1e-c069-4ae0-9620-9e384e35f7a6))
  (segment (start 190.3 153.7426) (end 190.3 154.1) (width 0.1524) (layer "B.Cu") (net 83) (tstamp 0f492e30-5771-4d36-bb3a-8e6301dcba88))
  (segment (start 192.063699 148.8262) (end 191.8262 148.8262) (width 0.1524) (layer "B.Cu") (net 83) (tstamp 0f7a6434-b7da-4aac-8174-d49bf50f9f8d))
  (segment (start 189.23 153.45) (end 190.0074 153.45) (width 0.1524) (layer "B.Cu") (net 83) (tstamp 12b8d896-fc45-4b5c-b32b-b3e3c92221ea))
  (segment (start 189.2788 154.4988) (end 191.71666 154.4988) (width 0.1524) (layer "B.Cu") (net 83) (tstamp 1bf10b7a-958f-4270-8bbb-9f2a33d4bbe3))
  (segment (start 190.0074 153.45) (end 190.3 153.7426) (width 0.1524) (layer "B.Cu") (net 83) (tstamp 1d36bec6-dd2b-496d-a74b-ffa59866d24d))
  (segment (start 191.7625 148.7625) (end 191.7625 148.15) (width 0.1524) (layer "B.Cu") (net 83) (tstamp 1fbebdab-6261-41c5-ba71-b044b90aaf1f))
  (segment (start 192.0988 154.11666) (end 192.0988 148.861301) (width 0.1524) (layer "B.Cu") (net 83) (tstamp 53bccb2c-6a45-465c-a319-b2c410cfa7ae))
  (segment (start 189.28 154.5) (end 189.23 154.45) (width 0.1524) (layer "B.Cu") (net 83) (tstamp 9dc980d5-366d-486c-9a61-ec6b7df0c710))
  (segment (start 191.7625 146.45) (end 191.7625 148.15) (width 0.1524) (layer "B.Cu") (net 83) (tstamp bfc93f38-a748-4ac3-8a6c-9380b3e07b92))
  (segment (start 189.9 154.5) (end 189.28 154.5) (width 0.1524) (layer "B.Cu") (net 83) (tstamp c91e8299-1849-47dd-ab1b-02ecb44b7bd8))
  (segment (start 191.8262 148.8262) (end 191.7625 148.7625) (width 0.1524) (layer "B.Cu") (net 83) (tstamp d2d48e9c-3e70-45a9-b536-735b2884a0af))
  (segment (start 191.71666 154.4988) (end 192.0988 154.11666) (width 0.1524) (layer "B.Cu") (net 83) (tstamp e2dd61b8-3213-4b29-9dbc-2d277a48ffe4))
  (segment (start 189.23 154.45) (end 189.2788 154.4988) (width 0.1524) (layer "B.Cu") (net 83) (tstamp f3de301b-42d3-418a-ac38-ca443d159c48))
  (segment (start 189.8 154.9) (end 189.8012 154.9012) (width 0.1524) (layer "B.Cu") (net 84) (tstamp 0c428a70-f504-479b-9955-3720020997d3))
  (segment (start 188.4526 153.95) (end 188.3 154.1026) (width 0.1524) (layer "B.Cu") (net 84) (tstamp 17f857a9-a280-45b9-8f52-8364a6540919))
  (segment (start 192.7262 148.8262) (end 192.8 148.7524) (width 0.1524) (layer "B.Cu") (net 84) (tstamp 3e5fb135-7d57-4840-82b0-9f5dff4264a5))
  (segment (start 188.3 154.8) (end 188.45 154.95) (width 0.1524) (layer "B.Cu") (net 84) (tstamp 424eeb7b-df53-4951-b3cc-41d80e1bcde4))
  (segment (start 188.3 154.1026) (end 188.3 154.8) (width 0.1524) (layer "B.Cu") (net 84) (tstamp 4c53d69a-01b4-4195-94d1-a8fbb0a01ed5))
  (segment (start 189.8012 154.9012) (end 191.88334 154.9012) (width 0.1524) (layer "B.Cu") (net 84) (tstamp 7b91e503-1c9d-4c7a-8e7b-269f05fcd755))
  (segment (start 191.88334 154.9012) (end 192.5012 154.28334) (width 0.1524) (layer "B.Cu") (net 84) (tstamp 81e79fb6-8cb7-4292-afb6-86f4fbdbb69d))
  (segment (start 192.536301 148.8262) (end 192.7262 148.8262) (width 0.1524) (layer "B.Cu") (net 84) (tstamp 8dfaf06a-8c29-486e-9892-73fadd95aa9f))
  (segment (start 192.5012 154.28334) (end 192.5012 148.861301) (width 0.1524) (layer "B.Cu") (net 84) (tstamp ad461f2f-a2cb-4925-a6a8-0a0383cfd1af))
  (segment (start 188.45 154.95) (end 189.23 154.95) (width 0.1524) (layer "B.Cu") (net 84) (tstamp b53c887f-0362-417d-9d40-889abade704b))
  (segment (start 189.23 154.95) (end 189.75 154.95) (width 0.1524) (layer "B.Cu") (net 84) (tstamp b7421721-8ad5-44f6-9363-d1a9c7d09d66))
  (segment (start 192.5012 148.861301) (end 192.536301 148.8262) (width 0.1524) (layer "B.Cu") (net 84) (tstamp be7d1c0d-2f26-444c-b5e8-f9d0a44725a4))
  (segment (start 192.8375 148.15) (end 192.8375 146.45) (width 0.1524) (layer "B.Cu") (net 84) (tstamp c7ad2cf6-5acd-49db-a03e-149a506bd040))
  (segment (start 192.8 148.1875) (end 192.8375 148.15) (width 0.1524) (layer "B.Cu") (net 84) (tstamp dbbb38fd-0b03-4360-aba1-905dabdee9ad))
  (segment (start 189.75 154.95) (end 189.8 154.9) (width 0.1524) (layer "B.Cu") (net 84) (tstamp deb17124-ef87-4bf0-a432-1759c8491aec))
  (segment (start 189.23 153.95) (end 188.4526 153.95) (width 0.1524) (layer "B.Cu") (net 84) (tstamp f39480e2-cfa1-46e9-95e0-eedfc7164619))
  (segment (start 192.8 148.7524) (end 192.8 148.1875) (width 0.1524) (layer "B.Cu") (net 84) (tstamp fabad8fe-45e7-4e01-b911-54d435023e55))

  (group "" (id 45616dea-dbb5-48f3-9189-429ad38655fd)
    (members
      01065175-7c01-4368-8779-bb35965f6cb4
      059ba0e7-f558-47c3-bb2e-0e1423cb7741
      0bc9bc17-3416-4939-901f-7f358270b581
      1110c232-f341-48cc-b84d-ba90ca04337b
      1200001b-7938-4ba4-942e-434c7ab17c31
      2b259426-6943-4fac-a589-7602907648a5
      2e68f97d-0bb4-491f-b3cd-5bea688cdb47
      389bf5a5-a942-4c7c-9e24-cf86e886d331
      39337374-72fa-4741-b507-34adb989edba
      4668c841-f35f-41a7-b0b8-e2c693772000
      49b88b1c-5693-4acb-be36-44710154839a
      4ca10ff1-f91a-4098-893a-211fdfacb763
      560b91d7-8fff-4c42-b53d-2a72347b4061
      57ba07f7-23d5-44c4-89f1-03be3d7fffbf
      6d214271-713f-40af-9b92-61eff9e023f9
      7d1fc2c2-7dac-402b-add3-fcd0eb27863a
      7d8e22b6-af9d-4f51-91f0-e18ee9ba6497
      aa78f927-42d8-4ba7-b3ae-f1bcdf880f70
      adbaacb2-b567-44d5-acff-6ec885896993
      b0453f78-a608-49a3-b8b3-288a0dfc0552
      cc0cb76a-7a54-4836-bcc4-75c47c58b45d
      e49bb379-7a56-4797-b30b-8b170deba133
      ec092202-beea-46c9-800c-b66ce60e1791
      ee444db6-8ea7-406d-9333-affcc0134eb8
    )
  )
  (group "" (id 9982561e-8cf4-4ee2-a4d2-2352baeb0216)
    (members
      034f9683-0fc4-4a40-b806-ad28dfb318ea
      0636146e-9994-41c5-917b-a153fb5c4a01
      295ae101-8923-44f1-8ff8-97406ff9c246
      37746acc-6320-4854-b1f1-0b0190bce913
      7ed8f25f-18b0-48c8-8f56-7eb23011c3eb
      852a552d-6836-49d0-ba8a-9a5804bcdbc5
      8695ce4d-e917-4d02-9ba3-58156db32e65
      b7b48860-6d23-4c59-b333-a7116ba32f95
      bc04bda0-beeb-4a95-ab89-10189cc0f580
      c42b5006-f4b0-409d-a515-1873d308e6ee
      da8bdc04-bb6c-40d3-834d-a64872ac4e11
      dc393316-1a95-4e33-9d2c-f1c2f3509df9
    )
  )
)
