(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "LPC804M101JHI33" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -31.75 21.59 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "LPC804M101JHI33" (id 1) (at 24.13 21.59 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DFN_QFN:VQFN-32-1EP_5x5mm_P0.5mm_EP3.5x3.5mm_ThermalVias" (id 2) (at 0 -26.67 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.nxp.com/docs/en/nxp/data-sheets/LPC804_DS.pdf" (id 3) (at 0 -24.13 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Low-Cost Microcontrollers (MCUs) based on Arm® Cortex®-M0+ Core" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LPC804M101JHI33_0_0"
      (pin tri_state line (at 35.56 15.24 180) (length 2.54)
        (name "PIO0_17/ADC_9" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 35.56 5.08 180) (length 2.54)
        (name "PIO0_21/ACMP_I5" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 35.56 -17.78 180) (length 2.54)
        (name "PIO0_29" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 35.56 -15.24 180) (length 2.54)
        (name "PIO0_28" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 35.56 -12.7 180) (length 2.54)
        (name "PIO0_27" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 35.56 -10.16 180) (length 2.54)
        (name "PIO0_26" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 35.56 7.62 180) (length 2.54)
        (name "PIO0_20" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -35.56 17.78 0) (length 2.54)
        (name "PIO0_15/ADC_8" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -35.56 -17.78 0) (length 2.54)
        (name "PIO0_1/ADC_0/ACMP_I2/TDI/CLKIN" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -35.56 2.54 0) (length 2.54)
        (name "PIO0_9/ADC_4" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -35.56 0 0) (length 2.54)
        (name "PIO0_8/ADC_5" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -35.56 12.7 0) (length 2.54)
        (name "PIO0_13/ADC_10" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -1.27 22.86 270) (length 2.54)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 35.56 -20.32 180) (length 2.54)
        (name "PIO0_30" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -35.56 -5.08 0) (length 2.54)
        (name "PIO0_7/ADC_1/ACMPVREF" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 22.86 270) (length 2.54)
        (name "VREFP" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -35.56 -20.32 0) (length 2.54)
        (name "PIO0_0/ACMP_I1/TDO" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -35.56 15.24 0) (length 2.54)
        (name "PIO0_14/ADC_2/ACMP_I3" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 35.56 10.16 180) (length 2.54)
        (name "PIO0_19/DACOUT" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 35.56 -7.62 180) (length 2.54)
        (name "PIO0_25" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 35.56 -5.08 180) (length 2.54)
        (name "PIO0_24" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 35.56 0 180) (length 2.54)
        (name "PIO0_23" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -35.56 10.16 0) (length 2.54)
        (name "PIO0_12" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 35.56 2.54 180) (length 2.54)
        (name "PIO0_22" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 35.56 12.7 180) (length 2.54)
        (name "PIO0_18" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 35.56 17.78 180) (length 2.54)
        (name "PIO0_16/ADC_3/ACMP_I4" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -25.4 90) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -35.56 -7.62 0) (length 2.54)
        (name "~{RESET}/PIO0_5" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -35.56 -10.16 0) (length 2.54)
        (name "PIO0_4/ADC_11/TRSTN" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -35.56 -12.7 0) (length 2.54)
        (name "SWCLK/PIO0_3/TCK" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -35.56 -15.24 0) (length 2.54)
        (name "SWDIO/PIO0_2/TMS" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -35.56 7.62 0) (length 2.54)
        (name "PIO0_11/ADC_6/WKTCLKIN" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -35.56 5.08 0) (length 2.54)
        (name "PIO0_10/ADC_7" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "LPC804M101JHI33_0_1"
      (rectangle (start -33.02 20.32) (end 33.02 -22.86)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
  )
)
