(footprint "CapTouch_Mutual_5X_Slider" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr smd)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b46b4ee0-5b58-4222-89c0-97eca790d463)
  )
  (fp_text value "CapTouch_Mutual_5X_Slider" (at 0 1 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2d7ff3ea-719d-418f-9ecb-9501cb40fe06)
  )
  (fp_text user "${REF}" (at 0 2.5 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ac03b83d-d5ac-449e-9772-4ea6ce3f94e3)
  )
  (fp_line (start -36.5 -9.75) (end -8.75 -9.75) (layer "Dwgs.User") (width 0.1) (tstamp fecaa04e-ebb1-478f-8c2a-7aad3f284602))
  (pad "1" smd custom (at -36.5 -5.75) (size 0 0) (layers "F.Cu")
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
          (xy 0 4)
          (xy 0 -4)
          (xy 7 -4)
          (xy 1.4 -2)
          (xy 12.6 2)
          (xy 7 4)
        ) (width 0.1) (fill yes))
    ) (tstamp dfdef2c6-6745-4d2f-aa9a-38d76a3dcc9a))
  (pad "2" smd custom (at -28.5 -5.75) (size 0 0) (layers "F.Cu")
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
          (xy 0 4)
          (xy 5.6 2)
          (xy -5.6 -2)
          (xy 0 -4)
          (xy 4.2 -4)
          (xy -1.4 -2)
          (xy 9.8 2)
          (xy 4.2 4)
        ) (width 0.1) (fill yes))
    ) (tstamp c1b58782-641e-423a-9e18-8e70d9392ed4))
  (pad "3" smd custom (at -23.25 -5.75) (size 0 0) (layers "F.Cu")
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
          (xy 0 4)
          (xy 5.6 2)
          (xy -5.6 -2)
          (xy 0 -4)
          (xy 4.2 -4)
          (xy -1.4 -2)
          (xy 9.8 2)
          (xy 4.2 4)
        ) (width 0.1) (fill yes))
    ) (tstamp 861250a0-8eb3-402d-8c29-b788f8b81437))
  (pad "4" smd custom (at -18 -5.75) (size 0 0) (layers "F.Cu")
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
          (xy 0 4)
          (xy 5.6 2)
          (xy -5.6 -2)
          (xy 0 -4)
          (xy 4.2 -4)
          (xy -1.4 -2)
          (xy 9.8 2)
          (xy 4.2 4)
        ) (width 0.1) (fill yes))
    ) (tstamp 5915d36e-03b6-4e39-a571-7b0468e82e55))
  (pad "5" smd custom (at -12.75 -5.75) (size 0 0) (layers "F.Cu")
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
          (xy 0 4)
          (xy 5.6 2)
          (xy -5.6 -2)
          (xy 0 -4)
          (xy 4.2 -4)
          (xy -1.4 -2)
          (xy 9.8 2)
          (xy 4.2 4)
        ) (width 0.1) (fill yes))
    ) (tstamp d295d2ac-a606-4fbc-950e-5ab6358a9402))
  (pad "6" smd custom (at -7.5 -5.75) (size 0 0) (layers "F.Cu")
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
          (xy 0 4)
          (xy 5.6 2)
          (xy -5.6 -2)
          (xy 0 -4)
          (xy 4.2 -4)
          (xy -1.4 -2)
          (xy 9.8 2)
          (xy 4.2 4)
        ) (width 0.1) (fill yes))
    ) (tstamp f93fd3d6-ae7d-409b-a8c6-300fbf640b3e))
  (pad "7" smd custom (at -2.25 -5.75) (size 0 0) (layers "F.Cu")
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
          (xy 0 4)
          (xy 5.6 2)
          (xy -5.6 -2)
          (xy 0 -4)
          (xy 4.2 -4)
          (xy -1.4 -2)
          (xy 9.8 2)
          (xy 4.2 4)
        ) (width 0.1) (fill yes))
    ) (tstamp 3a53101b-5aab-4de7-ad66-01d03cade217))
  (pad "8" smd custom (at 3 -5.75) (size 0 0) (layers "F.Cu")
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
          (xy 0 4)
          (xy 5.6 2)
          (xy -5.6 -2)
          (xy 0 -4)
          (xy 4.2 -4)
          (xy -1.4 -2)
          (xy 9.8 2)
          (xy 4.2 4)
        ) (width 0.1) (fill yes))
    ) (tstamp 95f06b8b-8455-4695-8fa4-f7ca7a2e4fc1))
  (pad "9" smd custom (at 8.25 -5.75) (size 0 0) (layers "F.Cu")
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
          (xy 0 4)
          (xy 5.6 2)
          (xy -5.6 -2)
          (xy 0 -4)
          (xy 4.2 -4)
          (xy -1.4 -2)
          (xy 9.8 2)
          (xy 4.2 4)
        ) (width 0.1) (fill yes))
    ) (tstamp 4727e83d-6548-438e-8031-d85ec334c93f))
  (pad "10" smd custom (at 13.5 -5.75) (size 0 0) (layers "F.Cu")
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
          (xy 0 4)
          (xy 5.6 2)
          (xy -5.6 -2)
          (xy 0 -4)
          (xy 4.2 -4)
          (xy -1.4 -2)
          (xy 9.8 2)
          (xy 4.2 4)
        ) (width 0.1) (fill yes))
    ) (tstamp 01559fff-f374-49df-abb8-df5c798aceab))
  (pad "11" smd custom (at 18.75 -5.75) (size 0 0) (layers "F.Cu")
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
          (xy 0 4)
          (xy 5.6 2)
          (xy -5.6 -2)
          (xy 0 -4)
          (xy 4.2 -4)
          (xy -1.4 -2)
          (xy 9.8 2)
          (xy 4.2 4)
        ) (width 0.1) (fill yes))
    ) (tstamp 03a98535-40c3-4499-af1f-3bd1eb16ece8))
  (pad "12" smd custom (at 24 -5.75) (size 0 0) (layers "F.Cu")
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
          (xy 0 4)
          (xy 5.6 2)
          (xy -5.6 -2)
          (xy 0 -4)
          (xy 4.2 -4)
          (xy -1.4 -2)
          (xy 9.8 2)
          (xy 4.2 4)
        ) (width 0.1) (fill yes))
    ) (tstamp a3c4b868-774e-4e1f-8cda-7369a7be87fb))
  (pad "13" smd custom (at 36.25 -5.75 180) (size 0 0) (layers "F.Cu")
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
          (xy 0 4)
          (xy 0 -4)
          (xy 7 -4)
          (xy 1.4 -2)
          (xy 12.6 2)
          (xy 7 4)
        ) (width 0.1) (fill yes))
    ) (tstamp c930b846-2beb-4d19-9b0f-1b8c0bdfc1e1))
  (pad "14" smd custom (at -36.5 -5.75 180) (size 0 0) (layers "B.Cu")
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_line (start 0 -4) (end 0 4) (width 0.45))
      (gr_line (start 0 4) (end -72 4) (width 0.45))
      (gr_line (start 0 -4) (end -72 -4) (width 0.45))
      (gr_line (start 0 0) (end -72 0) (width 0.45))
    ) (tstamp d77a641b-f5be-4038-b933-6e16ea82b832))
  (zone (net 0) (net_name "") (layers *.Cu) (tstamp c892d7bf-2193-41c5-a171-3c3a2345df78) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 36.5 -1.5)
        (xy -36.75 -1.5)
        (xy -36.75 -10)
        (xy 36.5 -10)
      )
    )
  )
)
