(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 4.69)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" signal)
    (2 "In2.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 2" (type "prepreg") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 3" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints yes)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "VDDF")
  (net 2 "GND")
  (net 3 "/Sensor_Controller/LPC_~{RST}")
  (net 4 "Net-(C10-Pad1)")
  (net 5 "Net-(C11-Pad2)")
  (net 6 "VCC")
  (net 7 "/Power_Management/PS_SWITCH")
  (net 8 "/Power_Management/LED_A")
  (net 9 "VDD")
  (net 10 "Net-(C20-Pad1)")
  (net 11 "Net-(C22-Pad1)")
  (net 12 "Net-(C22-Pad2)")
  (net 13 "Net-(C23-Pad2)")
  (net 14 "Net-(C24-Pad2)")
  (net 15 "/WiFi_Display/PREVGH")
  (net 16 "/WiFi_Display/PREVGL")
  (net 17 "Net-(C27-Pad2)")
  (net 18 "Net-(C29-Pad2)")
  (net 19 "Net-(C30-Pad2)")
  (net 20 "Net-(C31-Pad2)")
  (net 21 "Net-(C32-Pad2)")
  (net 22 "Net-(D1-Pad2)")
  (net 23 "Net-(D1-Pad3)")
  (net 24 "Net-(D1-Pad4)")
  (net 25 "VBUS")
  (net 26 "unconnected-(J3-Pad3)")
  (net 27 "unconnected-(J3-Pad4)")
  (net 28 "/Power_Management/LED_K")
  (net 29 "unconnected-(J4-Pad1)")
  (net 30 "/WiFi_Display/GDR")
  (net 31 "/WiFi_Display/RESE")
  (net 32 "unconnected-(J4-Pad6)")
  (net 33 "unconnected-(J4-Pad7)")
  (net 34 "/WiFi_Display/EPD_BUSY")
  (net 35 "/WiFi_Display/EPD_~{RES}")
  (net 36 "/WiFi_Display/EPD_D{slash}~{C}")
  (net 37 "/WiFi_Display/EPD_CS")
  (net 38 "/WiFi_Display/EPD_SCLK")
  (net 39 "/WiFi_Display/EPD_SDI")
  (net 40 "/Sensor_Controller/LPC_~{ISP}")
  (net 41 "/Sensor_Controller/I2C_SDA")
  (net 42 "/Sensor_Controller/I2C_SCL")
  (net 43 "/Sensor_Controller/LED_R")
  (net 44 "/Sensor_Controller/LED_G")
  (net 45 "/Sensor_Controller/LED_B")
  (net 46 "/Sensor_Controller/LPC_SWDIO")
  (net 47 "/Sensor_Controller/LPC_SWCLK")
  (net 48 "/Sensor_Controller/CAPT_X0")
  (net 49 "Net-(R10-Pad2)")
  (net 50 "Net-(R11-Pad1)")
  (net 51 "/Sensor_Controller/CAPT_X1")
  (net 52 "Net-(R13-Pad2)")
  (net 53 "Net-(R14-Pad2)")
  (net 54 "/Sensor_Controller/CAPT_X2")
  (net 55 "Net-(R16-Pad2)")
  (net 56 "Net-(R17-Pad2)")
  (net 57 "/Sensor_Controller/CAPT_X3")
  (net 58 "Net-(R19-Pad2)")
  (net 59 "Net-(R20-Pad2)")
  (net 60 "/Sensor_Controller/CAPT_X4")
  (net 61 "Net-(R22-Pad1)")
  (net 62 "/Power_Management/ADC_BAT")
  (net 63 "Net-(R27-Pad2)")
  (net 64 "Net-(J2-PadA5)")
  (net 65 "Net-(J2-PadB5)")
  (net 66 "/Sensor_Controller/CAPT_YH")
  (net 67 "/Sensor_Controller/LSM_A0")
  (net 68 "/Sensor_Controller/LSM_INT1")
  (net 69 "/Sensor_Controller/LSM_INT2")
  (net 70 "unconnected-(U1-Pad10)")
  (net 71 "unconnected-(U1-Pad11)")
  (net 72 "/Sensor_Controller/SPI_CS")
  (net 73 "/Power_Management/LED_PWM")
  (net 74 "/Sensor_Controller/ALS_INT")
  (net 75 "/Sensor_Controller/RTC_CLKO")
  (net 76 "/Sensor_Controller/RTC_INT")
  (net 77 "/Sensor_Controller/CAPT_YL")
  (net 78 "/Power_Management/DCDC_EN")
  (net 79 "/Power_Management/CHG_~{STBY}")
  (net 80 "/Power_Management/CHG_~{ACT}")
  (net 81 "/Sensor_Controller/SPI_~{INT}")
  (net 82 "/Sensor_Controller/SPI_MISO")
  (net 83 "Net-(U6-Pad2)")
  (net 84 "Net-(L1-Pad1)")
  (net 85 "Net-(L2-Pad1)")
  (net 86 "/WiFi_Display/USB_D+")
  (net 87 "/WiFi_Display/USB_D-")
  (net 88 "unconnected-(U12-Pad4)")
  (net 89 "unconnected-(U12-Pad7)")
  (net 90 "unconnected-(U12-Pad9)")
  (net 91 "unconnected-(U12-Pad10)")
  (net 92 "unconnected-(U12-Pad12)")
  (net 93 "unconnected-(U12-Pad15)")
  (net 94 "unconnected-(U12-Pad17)")
  (net 95 "Net-(SW3-Pad2)")
  (net 96 "unconnected-(U12-Pad24)")
  (net 97 "unconnected-(U12-Pad25)")
  (net 98 "unconnected-(U12-Pad28)")
  (net 99 "unconnected-(U12-Pad29)")
  (net 100 "/WiFi_Display/UART_RX")
  (net 101 "/WiFi_Display/UART_TX")
  (net 102 "unconnected-(U12-Pad32)")
  (net 103 "unconnected-(U12-Pad33)")
  (net 104 "unconnected-(U12-Pad34)")
  (net 105 "unconnected-(U12-Pad35)")
  (net 106 "Net-(BT1-Pad1)")
  (net 107 "unconnected-(J1-Pad6)")
  (net 108 "unconnected-(J1-Pad7)")
  (net 109 "unconnected-(J1-Pad8)")
  (net 110 "unconnected-(U4-Pad2)")

  (footprint "Touch_Sensor:CapTouch_Mutual_5X_Slider" (layer "F.Cu")
    (tedit 0) (tstamp 14df72c9-e155-4a3d-8347-b6e900e6bc7f)
    (at 151.125 154.875)
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/7fcaff45-24f7-4019-910f-2a69e797182e")
    (attr smd)
    (fp_text reference "T1" (at 0 -0.5 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0600c853-70d3-4588-8a1d-64b942976d9f)
    )
    (fp_text value "Cap_Touch_Slider_5P" (at 0.1 1.35 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e453b54c-6b9d-46c8-bb8d-2fb526a9432e)
    )
    (fp_text user "${REF}" (at 0 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cb8a236c-dbfb-4e28-beb9-df1c062d10b7)
    )
    (fp_line (start -36.5 -9.75) (end -8.75 -9.75) (layer "Dwgs.User") (width 0.1) (tstamp 3d076d1d-a196-40fd-b544-cfc34cdf16f8))
    (pad "1" smd custom (at -36.5 -5.75) (size 0 0) (layers "F.Cu")
      (net 48 "/Sensor_Controller/CAPT_X0") (pinfunction "X0") (pintype "passive")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0 4)
            (xy 0 -4)
            (xy 7 -4)
            (xy 1.4 -2)
            (xy 12.6 2)
            (xy 7 4)
          ) (width 0.1) (fill yes))
      ) (tstamp 36376fa9-0108-4f3a-b7c8-fe9bc5150cf8))
    (pad "2" smd custom (at -28.5 -5.75) (size 0 0) (layers "F.Cu")
      (net 49 "Net-(R10-Pad2)") (pinfunction "X01A") (pintype "passive")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0 4)
            (xy 5.6 2)
            (xy -5.6 -2)
            (xy 0 -4)
            (xy 4.2 -4)
            (xy -1.4 -2)
            (xy 9.8 2)
            (xy 4.2 4)
          ) (width 0.1) (fill yes))
      ) (tstamp da832fc5-3b2b-4586-9345-616d8775a408))
    (pad "3" smd custom (at -23.25 -5.75) (size 0 0) (layers "F.Cu")
      (net 50 "Net-(R11-Pad1)") (pinfunction "X01B") (pintype "passive")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0 4)
            (xy 5.6 2)
            (xy -5.6 -2)
            (xy 0 -4)
            (xy 4.2 -4)
            (xy -1.4 -2)
            (xy 9.8 2)
            (xy 4.2 4)
          ) (width 0.1) (fill yes))
      ) (tstamp 765f1393-1682-4232-a9e9-4ba5fca8d904))
    (pad "4" smd custom (at -18 -5.75) (size 0 0) (layers "F.Cu")
      (net 51 "/Sensor_Controller/CAPT_X1") (pinfunction "X1") (pintype "passive")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0 4)
            (xy 5.6 2)
            (xy -5.6 -2)
            (xy 0 -4)
            (xy 4.2 -4)
            (xy -1.4 -2)
            (xy 9.8 2)
            (xy 4.2 4)
          ) (width 0.1) (fill yes))
      ) (tstamp d205c6d7-ccaf-4d05-9c38-00644fef0f29))
    (pad "5" smd custom (at -12.75 -5.75) (size 0 0) (layers "F.Cu")
      (net 52 "Net-(R13-Pad2)") (pinfunction "X12A") (pintype "passive")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0 4)
            (xy 5.6 2)
            (xy -5.6 -2)
            (xy 0 -4)
            (xy 4.2 -4)
            (xy -1.4 -2)
            (xy 9.8 2)
            (xy 4.2 4)
          ) (width 0.1) (fill yes))
      ) (tstamp 2a850f62-ff0a-458b-bd60-50e4a3abfc3b))
    (pad "6" smd custom (at -7.5 -5.75) (size 0 0) (layers "F.Cu")
      (net 53 "Net-(R14-Pad2)") (pinfunction "X12B") (pintype "passive")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0 4)
            (xy 5.6 2)
            (xy -5.6 -2)
            (xy 0 -4)
            (xy 4.2 -4)
            (xy -1.4 -2)
            (xy 9.8 2)
            (xy 4.2 4)
          ) (width 0.1) (fill yes))
      ) (tstamp 3afd4624-08d5-4816-b124-511701b9d2c8))
    (pad "7" smd custom (at -2.25 -5.75) (size 0 0) (layers "F.Cu")
      (net 54 "/Sensor_Controller/CAPT_X2") (pinfunction "X2") (pintype "passive")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0 4)
            (xy 5.6 2)
            (xy -5.6 -2)
            (xy 0 -4)
            (xy 4.2 -4)
            (xy -1.4 -2)
            (xy 9.8 2)
            (xy 4.2 4)
          ) (width 0.1) (fill yes))
      ) (tstamp 54d7cd0c-8805-4ca6-9f53-dc21ad74e272))
    (pad "8" smd custom (at 3 -5.75) (size 0 0) (layers "F.Cu")
      (net 55 "Net-(R16-Pad2)") (pinfunction "X23A") (pintype "passive")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0 4)
            (xy 5.6 2)
            (xy -5.6 -2)
            (xy 0 -4)
            (xy 4.2 -4)
            (xy -1.4 -2)
            (xy 9.8 2)
            (xy 4.2 4)
          ) (width 0.1) (fill yes))
      ) (tstamp e89afc33-2bfd-4ea5-88e9-c7dfbfcea3dc))
    (pad "9" smd custom (at 8.25 -5.75) (size 0 0) (layers "F.Cu")
      (net 56 "Net-(R17-Pad2)") (pinfunction "X23B") (pintype "passive")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0 4)
            (xy 5.6 2)
            (xy -5.6 -2)
            (xy 0 -4)
            (xy 4.2 -4)
            (xy -1.4 -2)
            (xy 9.8 2)
            (xy 4.2 4)
          ) (width 0.1) (fill yes))
      ) (tstamp e991009e-85a9-4671-9fe7-ac956b1d8c9c))
    (pad "10" smd custom (at 13.5 -5.75) (size 0 0) (layers "F.Cu")
      (net 57 "/Sensor_Controller/CAPT_X3") (pinfunction "X3") (pintype "passive")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0 4)
            (xy 5.6 2)
            (xy -5.6 -2)
            (xy 0 -4)
            (xy 4.2 -4)
            (xy -1.4 -2)
            (xy 9.8 2)
            (xy 4.2 4)
          ) (width 0.1) (fill yes))
      ) (tstamp f263906c-92d9-4c2a-a74a-a3fc5db8dc48))
    (pad "11" smd custom (at 18.75 -5.75) (size 0 0) (layers "F.Cu")
      (net 58 "Net-(R19-Pad2)") (pinfunction "X34A") (pintype "passive")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0 4)
            (xy 5.6 2)
            (xy -5.6 -2)
            (xy 0 -4)
            (xy 4.2 -4)
            (xy -1.4 -2)
            (xy 9.8 2)
            (xy 4.2 4)
          ) (width 0.1) (fill yes))
      ) (tstamp 4f51fa88-4b3b-476c-8ab5-ae305810d76a))
    (pad "12" smd custom (at 24 -5.75) (size 0 0) (layers "F.Cu")
      (net 59 "Net-(R20-Pad2)") (pinfunction "X34B") (pintype "passive")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0 4)
            (xy 5.6 2)
            (xy -5.6 -2)
            (xy 0 -4)
            (xy 4.2 -4)
            (xy -1.4 -2)
            (xy 9.8 2)
            (xy 4.2 4)
          ) (width 0.1) (fill yes))
      ) (tstamp e87cd9ea-ee96-4a52-a198-ecaab58101ba))
    (pad "13" smd custom (at 36.25 -5.75 180) (size 0 0) (layers "F.Cu")
      (net 60 "/Sensor_Controller/CAPT_X4") (pinfunction "X4") (pintype "passive")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0 4)
            (xy 0 -4)
            (xy 7 -4)
            (xy 1.4 -2)
            (xy 12.6 2)
            (xy 7 4)
          ) (width 0.1) (fill yes))
      ) (tstamp 8c3f4bd0-cef1-4660-b4a3-91260bc620a7))
    (pad "14" smd custom (at -36.5 -5.75 180) (size 0 0) (layers "B.Cu")
      (net 66 "/Sensor_Controller/CAPT_YH") (pinfunction "YH") (pintype "passive")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 0 -4) (end 0 4) (width 0.45))
        (gr_line (start 0 4) (end -72 4) (width 0.45))
        (gr_line (start 0 -4) (end -72 -4) (width 0.45))
        (gr_line (start 0 0) (end -72 0) (width 0.45))
      ) (tstamp 33dc8e40-e891-4f10-978c-83cb3e08403d))
    (zone (net 0) (net_name "") (layers *.Cu) (tstamp 44cd0096-dabe-46fd-8d28-8a22c910a61b) (hatch edge 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254)
      (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 187.625 153.375)
          (xy 114.375 153.375)
          (xy 114.375 144.875)
          (xy 187.625 144.875)
        )
      )
    )
  )

  (footprint "LED_SMD:LED_Lumex_SML-LX0404SIUPGUSB" (layer "F.Cu")
    (tedit 5DDA4ABB) (tstamp 227d7d66-a27f-4daf-8f25-b3a33d60e86e)
    (at 83.3 119.5)
    (descr "Lumex RGB LED, clear, SMD, https://www.lumex.com/spec/SML-LX0404SIUPGUSB.pdf")
    (tags "LED RGB")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/b9b42071-a3cd-4576-9a71-5529d1a4b62d")
    (attr smd)
    (fp_text reference "D1" (at 0 -1.75) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d11255dc-72d0-4047-ae66-f096b8272334)
    )
    (fp_text value "FC-B1010RGBT-HG" (at 0 1.75) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1335ac4d-8eb2-410f-8026-d1a518e8be60)
    )
    (fp_text user "${REFERENCE}" (at 0 -1) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.1)))
      (tstamp 0b0d7583-29e0-4fc5-bdca-2702083504ef)
    )
    (fp_line (start -0.825 -0.825) (end -0.825 -0.25) (layer "F.SilkS") (width 0.1) (tstamp 54503d77-32e9-4efe-a95b-4fb4ad74efde))
    (fp_line (start -0.25 -0.825) (end -0.825 -0.825) (layer "F.SilkS") (width 0.1) (tstamp 5ddbd7ce-0731-4610-8519-caec22b01dc1))
    (fp_line (start 0.9 0.9) (end 0.9 -0.9) (layer "F.CrtYd") (width 0.05) (tstamp 44c37f3c-0075-40f7-8b23-6493941b7392))
    (fp_line (start -0.9 0.9) (end 0.9 0.9) (layer "F.CrtYd") (width 0.05) (tstamp 66544ef9-8bc2-40c4-a338-a1836641f0ca))
    (fp_line (start -0.9 -0.9) (end -0.9 0.9) (layer "F.CrtYd") (width 0.05) (tstamp 66618269-42ce-4ec2-b4af-a2b93d31703a))
    (fp_line (start 0.9 -0.9) (end -0.9 -0.9) (layer "F.CrtYd") (width 0.05) (tstamp 6bb06277-2884-46e3-a443-37bc1e518134))
    (fp_line (start 0.5 0.5) (end 0.5 -0.5) (layer "F.Fab") (width 0.1) (tstamp 53f54166-47e0-4ca1-aac6-da2217742358))
    (fp_line (start 0.5 -0.5) (end -0.25 -0.5) (layer "F.Fab") (width 0.1) (tstamp 67b1b279-e142-4020-9046-55d2843446c1))
    (fp_line (start -0.25 -0.5) (end -0.5 -0.25) (layer "F.Fab") (width 0.1) (tstamp c157df10-5482-4496-88b2-f6db41cee92b))
    (fp_line (start -0.5 -0.25) (end -0.5 0.5) (layer "F.Fab") (width 0.1) (tstamp efe69f82-2599-4af7-a698-7ba32b71683c))
    (fp_line (start -0.5 0.5) (end 0.5 0.5) (layer "F.Fab") (width 0.1) (tstamp f634123a-43a1-4757-9fb6-aa283060443d))
    (pad "1" smd roundrect (at -0.425 -0.425) (size 0.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pinfunction "A") (pintype "passive") (tstamp 098c9f7e-d0a1-4423-9452-6eb3b6c6ba89))
    (pad "2" smd roundrect (at 0.425 -0.425) (size 0.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(D1-Pad2)") (pinfunction "RK") (pintype "passive") (tstamp f440d6e5-291a-4ab2-8a6a-6be070c8146d))
    (pad "3" smd roundrect (at 0.425 0.425) (size 0.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(D1-Pad3)") (pinfunction "GK") (pintype "passive") (tstamp 5112af12-dcdd-4bb9-a9dc-1755363bf833))
    (pad "4" smd roundrect (at -0.425 0.425) (size 0.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(D1-Pad4)") (pinfunction "BK") (pintype "passive") (tstamp 0f043b1b-2189-44d9-8231-3e70097a7545))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_Lumex_SML-LX0404SIUPGUSB.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_SO:MSOP-8_3x3mm_P0.65mm" (layer "B.Cu")
    (tedit 5E509FDD) (tstamp 034f9683-0fc4-4a40-b806-ad28dfb318ea)
    (at 117.4 138.6 180)
    (descr "MSOP, 8 Pin (https://www.jedec.org/system/files/docs/mo-187F.pdf variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "MSOP SO")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/f34a969a-2b53-42a3-8a58-dcfec9de65d9")
    (attr smd)
    (fp_text reference "U6" (at 0 2.45) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 3d239003-a982-42b2-96f2-cc87a2df6b86)
    )
    (fp_text value "PCF8563TS" (at 0 -2.45) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7f584bf8-05a6-47ae-9727-599edcb214da)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.75 0.75) (thickness 0.11)) (justify mirror))
      (tstamp 1e9047c5-4abd-4738-b89d-ac697fb155b6)
    )
    (fp_line (start 0 1.61) (end 1.5 1.61) (layer "B.SilkS") (width 0.12) (tstamp 70c66147-3203-4a50-a1c4-7e1ef7972096))
    (fp_line (start 0 -1.61) (end 1.5 -1.61) (layer "B.SilkS") (width 0.12) (tstamp 99ecfcdf-ccd1-432b-be17-8e1fc8c1ae74))
    (fp_line (start 0 1.61) (end -2.925 1.61) (layer "B.SilkS") (width 0.12) (tstamp e19e0098-16c6-4d7a-a489-33e040b0a0ea))
    (fp_line (start 0 -1.61) (end -1.5 -1.61) (layer "B.SilkS") (width 0.12) (tstamp e4aa84d1-c696-474d-937b-31469018d42f))
    (fp_line (start 3.18 1.75) (end -3.18 1.75) (layer "B.CrtYd") (width 0.05) (tstamp 3eacd064-0daf-48b2-ac37-2b03bb622197))
    (fp_line (start -3.18 1.75) (end -3.18 -1.75) (layer "B.CrtYd") (width 0.05) (tstamp 4a67c36a-f9e3-44ae-8ced-6a64e98c8259))
    (fp_line (start -3.18 -1.75) (end 3.18 -1.75) (layer "B.CrtYd") (width 0.05) (tstamp 54cdfb53-4090-4a09-b3fe-b47ef69b33bf))
    (fp_line (start 3.18 -1.75) (end 3.18 1.75) (layer "B.CrtYd") (width 0.05) (tstamp ff8cc47a-6056-42c0-a36b-78ac820375e8))
    (fp_line (start -0.75 1.5) (end 1.5 1.5) (layer "B.Fab") (width 0.1) (tstamp 087c3d89-10ef-43af-b16b-4ca34978f689))
    (fp_line (start 1.5 -1.5) (end -1.5 -1.5) (layer "B.Fab") (width 0.1) (tstamp 5b34678f-a230-4b26-92bf-36962adeee1c))
    (fp_line (start 1.5 1.5) (end 1.5 -1.5) (layer "B.Fab") (width 0.1) (tstamp b1fc3668-a718-44ef-98af-38f7653da7f1))
    (fp_line (start -1.5 0.75) (end -0.75 1.5) (layer "B.Fab") (width 0.1) (tstamp c8be6b47-48a4-4615-aaa6-b280a99459e5))
    (fp_line (start -1.5 -1.5) (end -1.5 0.75) (layer "B.Fab") (width 0.1) (tstamp f2b8d59c-82da-47a7-ab02-dcbb808d8bbc))
    (pad "1" smd roundrect (at -2.1125 0.975 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C11-Pad2)") (pinfunction "OSCI") (pintype "input") (tstamp 1b028326-3b4b-427d-aa8a-634f2aa774cb))
    (pad "2" smd roundrect (at -2.1125 0.325 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 83 "Net-(U6-Pad2)") (pinfunction "OSCO") (pintype "output") (tstamp 2300159b-b078-4250-b47c-762f2eeedeb3))
    (pad "3" smd roundrect (at -2.1125 -0.325 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "/Sensor_Controller/RTC_INT") (pinfunction "~{INT}") (pintype "output") (tstamp 11d99526-4c54-410a-adb9-4941099e35a9))
    (pad "4" smd roundrect (at -2.1125 -0.975 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp fcf2ab7a-ab02-4c90-8a5a-073a64893796))
    (pad "5" smd roundrect (at 2.1125 -0.975 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 41 "/Sensor_Controller/I2C_SDA") (pinfunction "SDA") (pintype "bidirectional") (tstamp d67b858f-a429-46be-a47e-3089844f9a73))
    (pad "6" smd roundrect (at 2.1125 -0.325 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 42 "/Sensor_Controller/I2C_SCL") (pinfunction "SCL") (pintype "input") (tstamp 17c297bc-e69d-4c7a-a626-06b5946cc20c))
    (pad "7" smd roundrect (at 2.1125 0.325 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 75 "/Sensor_Controller/RTC_CLKO") (pinfunction "CLKO") (pintype "output") (tstamp 84d6a252-792d-4756-8d90-5bc49be5c649))
    (pad "8" smd roundrect (at 2.1125 0.975 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pinfunction "VDD") (pintype "power_in") (tstamp 39cd3654-bd60-47d1-b8ec-fc743ff8a937))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/MSOP-8_3x3mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 0636146e-9994-41c5-917b-a153fb5c4a01)
    (at 57.058334 120.93 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/96e0fa9f-4507-4a4a-9ffb-5ab0c8bcb735")
    (attr smd)
    (fp_text reference "C11" (at 0 1.16) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp b42b7e53-8a93-4621-a1ee-d66a7f63b7ae)
    )
    (fp_text value "12pF" (at 0 -1.16) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 13155ded-fcfe-404e-9e67-5e03948ccb85)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
      (tstamp 7ca6a0ee-aa22-4a1b-9665-d9e2af80d75e)
    )
    (fp_line (start -0.107836 0.36) (end 0.107836 0.36) (layer "B.SilkS") (width 0.12) (tstamp 4af68891-d2f8-4ae0-a32e-ae9397bea0de))
    (fp_line (start -0.107836 -0.36) (end 0.107836 -0.36) (layer "B.SilkS") (width 0.12) (tstamp e3d66935-5a40-4671-98d1-42115a97498b))
    (fp_line (start -0.91 0.46) (end 0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 1655dc0e-ba48-432b-aac7-2f1979188896))
    (fp_line (start 0.91 0.46) (end 0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 6db2e7ab-c862-41c6-a36b-f006f4b39227))
    (fp_line (start 0.91 -0.46) (end -0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 9ea7b523-0f11-4833-ac5d-e7c07fb0cbe0))
    (fp_line (start -0.91 -0.46) (end -0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp f8966627-b967-4136-b063-bfbb96322ffb))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 106cb87d-df5d-4634-95da-e0f94baf6ba0))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 5d6d7ce9-5521-4d13-b9a4-6757692fdc81))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp d552cd7f-a889-46bc-94eb-b3882fdae4d3))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp ff786075-2d10-489e-9eb5-53ae274c23a6))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 0fa6e7d2-7806-427f-a852-c7ee6f764a8c))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C11-Pad2)") (pintype "passive") (tstamp 0d625222-a631-4b47-bf5e-5c9392850038))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 06379db1-87be-4496-965b-ca45806e0f0e)
    (at 180 154)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/4e156625-9fd4-4d5d-ad39-7ecbeed0c927")
    (attr smd)
    (fp_text reference "R21" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 8b1a72d4-167d-4b93-806a-8192a572b7b7)
    )
    (fp_text value "2.2k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp db4118ec-4a2d-41f8-9c7c-f4ed2ac071af)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp ecb0578b-34e7-4ce1-abfd-00d58ed5dee0)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 1be5c6fc-d915-413d-891a-30b8e50c9be4))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp f93d209e-ea37-4a3d-8f4f-c0d353046cea))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 3004f14d-f4a4-4d22-b55b-29ecf5f5c3f7))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 9617491b-fdc7-4c3f-bd75-defb5998ad2f))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp c404f95d-a41e-475e-8266-bcfab9203f28))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp fc3ed583-9ea3-46e0-b6a1-3801576595cf))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 4a05cffd-e671-4b09-85b7-bb37226e012a))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 4f81e6b7-c3f2-4c21-82d5-1cfe684b6518))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 92adb299-772f-4f05-8ae8-a9ded5622bda))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp dd2c9251-88e5-4c6f-bf09-160becb8edd6))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(R20-Pad2)") (pintype "passive") (tstamp 954575bd-b79d-4cde-b39f-aa8cddf4deff))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 60 "/Sensor_Controller/CAPT_X4") (pintype "passive") (tstamp 43e1f678-1f03-4674-b4c1-ebf99fbc881d))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 071cf0bb-fece-4c5d-b50e-b43ecc787a1a)
    (at 175 154)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/688f1d59-c60e-402d-83ce-d3f5c3a70b2a")
    (attr smd)
    (fp_text reference "R20" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp eba7e27b-fdee-4bb7-8329-f39435bec7e0)
    )
    (fp_text value "2.2k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 808274b0-c550-4631-a879-107223408191)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 8c1c88ff-f711-4d8d-87e3-130916c764cc)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 807c148d-2346-4f3f-bbe6-0b06a57598b5))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp ede66ab1-5f24-4387-ac33-a82f9244eab4))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 0840ab9f-a7c6-479a-ac35-0fccd3a5e62b))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 563efd66-2d08-4f8a-b63e-d97e79d747fa))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 58a65da6-62ef-4fab-93a3-86edec1bab76))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp c915f1f9-3d17-4204-8667-05d6ff67d542))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 6e8cb1f3-c089-4c09-81a8-3253e7cc07c6))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 74a2e861-ff4a-4874-99bf-0e79aa2216d2))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp c6fad81d-5142-4432-a964-41206306f381))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp f55c0b1a-9ab5-4018-a006-1fbd43976982))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(R19-Pad2)") (pintype "passive") (tstamp 42f80f86-ab21-43a2-8c3e-e4aea0ab0645))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(R20-Pad2)") (pintype "passive") (tstamp e85ae928-4688-46cf-9e29-6f941dc78bca))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 09a12715-75af-41d2-9ec8-fe0ad1b18df3)
    (at 77.48 143.42 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/8e358922-00a2-42cd-bd67-5db2e820b238")
    (attr smd)
    (fp_text reference "R35" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 46fba4d7-c53e-4938-a271-1873c5f2358e)
    )
    (fp_text value "10k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e750e191-00cf-42cc-a11f-089c18e29f52)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 1e598cab-89ef-4f29-bd8f-ba04c5798eb5)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 4320378c-5c3a-4941-9119-9ab9c1f4150e))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 7ccd8841-edf6-4c66-8cef-7e3bb10c77dd))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 779e3480-4fe9-4347-86ef-0cf40e9c43a8))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 9009b691-eea3-49c8-a3f2-3cca6b78566b))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp b531843f-5de1-4258-813f-3a0fe3fd696a))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp c271089f-6152-4848-9e08-8e84c7ce3ccc))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 69655ffe-8065-443f-bb9a-694b7b234499))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 71c98dc1-7646-47e7-b324-5cd8237df741))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 8f08e8db-ac93-4e56-aabe-50bdec0fe3a8))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 93af2d7c-0c2c-44af-967c-7345f4635565))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 30 "/WiFi_Display/GDR") (pintype "passive") (tstamp a1b00e48-f621-4bf9-9120-0a7f608a0c3c))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp f00596d9-cc74-4508-a73f-a3525e96bd65))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 0dd8d6eb-738f-4f1f-baf7-7e5a32fe166e)
    (at 42 112 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/385d375a-ca1a-4131-ba57-58095b1d80c5")
    (attr smd)
    (fp_text reference "R9" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 8a634fff-c68f-4053-91d2-8850406e7b45)
    )
    (fp_text value "100k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d5ef7cb5-37ff-4fea-aee3-948ce57b795e)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 16e753c0-0055-4662-82a8-779a0b5fd0df)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 50b983e5-549d-466b-881f-59a5dee158a9))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp e9382b42-60bd-425d-81f0-8e1190dda9f4))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 03c5b918-c4ff-411a-86b6-63372e8e6b5c))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 2240bb6f-e15c-45e5-88e2-c4407cd0fbcc))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 69efbcba-a79f-4ca1-968b-5e47164c8394))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 6dd24d57-fd0d-4f67-b520-9f8fc1436dfa))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 2123a139-da6c-4b72-b613-58220072f56f))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 4f2b2c4e-a302-476e-a6e1-8dbd39c6a4a6))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp e56d8dcf-6f9a-4dfc-bd44-cb020a612ccb))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp e7c23ad0-cc69-470f-af6e-9d00ce3e56da))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp 34c23e1f-f879-48c8-88ec-be92279cee8d))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 47 "/Sensor_Controller/LPC_SWCLK") (pintype "passive") (tstamp 8d9c660c-eebe-4c93-b4b5-28eb34030a55))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.62x3.51mm_ThermalVias" (layer "B.Cu")
    (tedit 5F7512B7) (tstamp 10440c11-568a-4a47-8c71-3eed2018c78f)
    (at 145.2 116.7)
    (descr "SOIC, 8 Pin (https://www.monolithicpower.com/en/documentview/productdocument/index/version/2/document_type/Datasheet/lang/en/sku/MP2303A/document_id/494#page=14), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/387129f7-eb5e-4379-8091-080031f64ead")
    (attr smd)
    (fp_text reference "U8" (at 0 3.4) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 54a899ff-ad4f-4cfe-b25c-0abda6c956b7)
    )
    (fp_text value "TP4056" (at 0 -3.4) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e65666f6-525d-4d0e-bb6b-c6ee4441b00d)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.98 0.98) (thickness 0.15)) (justify mirror))
      (tstamp 6792ce9b-932a-4e43-860b-adc5399d0a95)
    )
    (fp_line (start 0 2.56) (end 1.95 2.56) (layer "B.SilkS") (width 0.12) (tstamp 20391906-002b-4875-a0aa-60eaba8e7b62))
    (fp_line (start 0 -2.56) (end 1.95 -2.56) (layer "B.SilkS") (width 0.12) (tstamp 80df2173-1af2-422a-9488-2b7f7b2c7def))
    (fp_line (start 0 2.56) (end -3.45 2.56) (layer "B.SilkS") (width 0.12) (tstamp b2108ceb-33a9-4b0d-a067-a16bc681b3c8))
    (fp_line (start 0 -2.56) (end -1.95 -2.56) (layer "B.SilkS") (width 0.12) (tstamp b5a5a039-0040-40ee-8da9-b943d65ef2b3))
    (fp_line (start 3.7 -2.7) (end 3.7 2.7) (layer "B.CrtYd") (width 0.05) (tstamp 190ee863-7958-4f9f-a03a-b4a75b7eed28))
    (fp_line (start -3.7 2.7) (end -3.7 -2.7) (layer "B.CrtYd") (width 0.05) (tstamp 310e31e5-6dd2-4617-84c1-322287ff9c3e))
    (fp_line (start 3.7 2.7) (end -3.7 2.7) (layer "B.CrtYd") (width 0.05) (tstamp 9d57f103-95fa-4cb1-9eac-34c7068996de))
    (fp_line (start -3.7 -2.7) (end 3.7 -2.7) (layer "B.CrtYd") (width 0.05) (tstamp dc97a36b-52e8-4c24-b87e-eeb3ca58ed83))
    (fp_line (start -0.975 2.45) (end 1.95 2.45) (layer "B.Fab") (width 0.1) (tstamp 256e036b-061d-4734-82fd-b1d4f2ddb5ff))
    (fp_line (start 1.95 2.45) (end 1.95 -2.45) (layer "B.Fab") (width 0.1) (tstamp 3e78c855-3cdb-41d2-8b07-5d2d0f9e6540))
    (fp_line (start -1.95 -2.45) (end -1.95 1.475) (layer "B.Fab") (width 0.1) (tstamp 5a7ab131-b1d5-4ddb-b804-fe78bcb2de53))
    (fp_line (start -1.95 1.475) (end -0.975 2.45) (layer "B.Fab") (width 0.1) (tstamp 5e85febd-9696-4dc9-b92f-75a7ecda1cca))
    (fp_line (start 1.95 -2.45) (end -1.95 -2.45) (layer "B.Fab") (width 0.1) (tstamp a162bbc6-ff53-4a36-bbc0-8ef43793a5be))
    (pad "" smd roundrect (at -0.655 -0.875) (size 1.1 1.47) (layers "B.Paste") (roundrect_rratio 0.227273) (tstamp 478ecfbf-1fbe-4f3d-854b-e4a930a97d85))
    (pad "" smd roundrect (at 0.655 0.875) (size 1.1 1.47) (layers "B.Paste") (roundrect_rratio 0.227273) (tstamp b1fd67c7-7562-4864-aff5-e59b0780fe94))
    (pad "" smd roundrect (at -0.655 0.875) (size 1.1 1.47) (layers "B.Paste") (roundrect_rratio 0.227273) (tstamp b99aa3f1-6f17-464f-91bc-637ecfb641c1))
    (pad "" smd roundrect (at 0.655 -0.875) (size 1.1 1.47) (layers "B.Paste") (roundrect_rratio 0.227273) (tstamp c9e80e0c-c15a-4a4b-9d5e-2d11d9ad3f93))
    (pad "1" smd roundrect (at -2.48 1.905) (size 1.94 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "TEMP") (pintype "input") (tstamp c2229409-cfcc-4e4b-a52c-4487e48d0db7))
    (pad "2" smd roundrect (at -2.48 0.635) (size 1.94 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(R22-Pad1)") (pinfunction "PROG") (pintype "input") (tstamp 583a9ebe-e062-4005-bb11-e32cc800012c))
    (pad "3" smd roundrect (at -2.48 -0.635) (size 1.94 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp caa47198-c9dc-4ade-8890-4e40a7521549))
    (pad "4" smd roundrect (at -2.48 -1.905) (size 1.94 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "VBUS") (pinfunction "VCC") (pintype "power_in") (tstamp c3262c36-ed5a-4a65-87e9-766cabbe11aa))
    (pad "5" smd roundrect (at 2.48 -1.905) (size 1.94 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "VCC") (pinfunction "BAT") (pintype "power_out") (tstamp 5fbf29d2-98d0-4064-920a-3a3c0e1958de))
    (pad "6" smd roundrect (at 2.48 -0.635) (size 1.94 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 79 "/Power_Management/CHG_~{STBY}") (pinfunction "~{STDBY}") (pintype "open_collector") (tstamp 507b5472-4f49-4970-b0a0-b63c3a3244bb))
    (pad "7" smd roundrect (at 2.48 0.635) (size 1.94 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 80 "/Power_Management/CHG_~{ACT}") (pinfunction "~{CHRG}") (pintype "open_collector") (tstamp 1c2620d3-f95e-4a74-84b1-a3a79fe32254))
    (pad "8" smd roundrect (at 2.48 1.905) (size 1.94 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "VBUS") (pinfunction "CE") (pintype "input") (tstamp d176e24f-d29d-4e12-accc-39aff2519d45))
    (pad "9" smd rect (at 0 0) (size 1.9 2.5) (layers "F.Cu") (tstamp 0990f4a8-e3a1-4dcd-af14-447f19a10c87))
    (pad "9" thru_hole circle (at 0.7 1) (size 0.5 0.5) (drill 0.2) (layers *.Cu) (tstamp 8080f1db-9cde-45b1-86eb-d15ec7d44b75))
    (pad "9" smd rect (at 0 0) (size 2.62 3.51) (layers "B.Cu" "B.Mask") (tstamp 9434fffe-f6cf-4480-a723-ef0809ba5bef))
    (pad "9" thru_hole circle (at -0.7 -1) (size 0.5 0.5) (drill 0.2) (layers *.Cu) (tstamp a62cc872-f880-469f-b855-37b3cd39aaba))
    (pad "9" thru_hole circle (at 0.7 0) (size 0.5 0.5) (drill 0.2) (layers *.Cu) (tstamp ab59fc22-fa73-4c97-b864-7f4810b358c3))
    (pad "9" thru_hole circle (at -0.7 0) (size 0.5 0.5) (drill 0.2) (layers *.Cu) (tstamp b3667535-6582-44d8-bcf0-0987116cabc6))
    (pad "9" thru_hole circle (at -0.7 1) (size 0.5 0.5) (drill 0.2) (layers *.Cu) (tstamp c916b4a8-7588-4385-a524-c45237dcd1d8))
    (pad "9" thru_hole circle (at 0.7 -1) (size 0.5 0.5) (drill 0.2) (layers *.Cu) (tstamp eba00c27-f5df-4524-b44e-7ac90a243755))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.62x3.51mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958) (tstamp 1200001b-7938-4ba4-942e-434c7ab17c31)
    (at 159.6 113 180)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/bc3dd482-6ae8-4f1e-9fb1-4aba830a1ef6")
    (attr smd)
    (fp_text reference "Q1" (at 0 2.4) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7db79227-c6cc-4c38-9f58-2d3f41745a18)
    )
    (fp_text value "CJ3401" (at 0 -2.4) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 80439d74-7503-4d50-b522-97a686469980)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.32 0.32) (thickness 0.05)) (justify mirror))
      (tstamp e72d02f6-258a-4375-96bb-845c4b826956)
    )
    (fp_line (start 0 -1.56) (end -0.65 -1.56) (layer "B.SilkS") (width 0.12) (tstamp 339ccb93-723f-4891-9990-d64340a27477))
    (fp_line (start 0 1.56) (end 0.65 1.56) (layer "B.SilkS") (width 0.12) (tstamp cba17fab-102b-435e-90e7-8424743e195e))
    (fp_line (start 0 -1.56) (end 0.65 -1.56) (layer "B.SilkS") (width 0.12) (tstamp df66f786-4cf9-446c-bae7-d05984dfe223))
    (fp_line (start 0 1.56) (end -1.675 1.56) (layer "B.SilkS") (width 0.12) (tstamp e6f6a59a-5790-4c34-95bf-cb3bc15fb00b))
    (fp_line (start -1.92 1.7) (end -1.92 -1.7) (layer "B.CrtYd") (width 0.05) (tstamp 50b413c7-3fb9-46a2-8195-fa0cab725111))
    (fp_line (start 1.92 -1.7) (end 1.92 1.7) (layer "B.CrtYd") (width 0.05) (tstamp 7e28eddc-bf87-4e5d-9f31-4372cb68fabf))
    (fp_line (start 1.92 1.7) (end -1.92 1.7) (layer "B.CrtYd") (width 0.05) (tstamp f7b0a7aa-8ab0-4514-805e-1eeb80513b83))
    (fp_line (start -1.92 -1.7) (end 1.92 -1.7) (layer "B.CrtYd") (width 0.05) (tstamp f8d874a9-0dc2-475c-b45d-20a3da27240e))
    (fp_line (start -0.65 1.125) (end -0.325 1.45) (layer "B.Fab") (width 0.1) (tstamp 0543d8b7-6612-4c58-8ee3-69fe537e221b))
    (fp_line (start -0.325 1.45) (end 0.65 1.45) (layer "B.Fab") (width 0.1) (tstamp 0cd65df6-1e53-4083-9b3a-876203329400))
    (fp_line (start 0.65 -1.45) (end -0.65 -1.45) (layer "B.Fab") (width 0.1) (tstamp 4e6fa70a-292b-4053-881f-14ae48875bed))
    (fp_line (start -0.65 -1.45) (end -0.65 1.125) (layer "B.Fab") (width 0.1) (tstamp 56fe1c02-6d75-4f8c-a41d-9dc698f76b78))
    (fp_line (start 0.65 1.45) (end 0.65 -1.45) (layer "B.Fab") (width 0.1) (tstamp dbca82ca-8fb1-4103-93cb-d00aa6fa3979))
    (pad "1" smd roundrect (at -0.9375 0.95 180) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "VBUS") (pinfunction "G") (pintype "input") (tstamp 485904a6-19f5-4c0a-b9d9-782a40709cfb))
    (pad "2" smd roundrect (at -0.9375 -0.95 180) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "VCC") (pinfunction "S") (pintype "passive") (tstamp 501a54fe-678e-4abc-bfc4-4eaad23337f0))
    (pad "3" smd roundrect (at 0.9375 0 180) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "/Power_Management/PS_SWITCH") (pinfunction "D") (pintype "passive") (tstamp e9e58dc6-3984-4e30-a7d5-5bbfea5d1ea7))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 1321ba86-318b-4f01-9894-2bbcf57c791d)
    (at 174.9 124.4)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/7ecea5e6-cfca-4dab-b398-b484a5f246fd")
    (attr smd)
    (fp_text reference "C24" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 009f1259-0822-432f-8e12-89573ffcb0e1)
    )
    (fp_text value "1uF/50V" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 08352e74-c7fc-4f1b-96fe-0e1715ab86d0)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 31ff1ea2-2f7a-4c46-aec6-c631fb6927e1)
    )
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp 2dc75118-ec03-4635-9e70-fbf06de2be15))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp afe711da-4a8c-4bad-a474-68bba3075fba))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 1f9c378a-d8be-41eb-b681-07eebe943650))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 64b0ec6e-38bc-4c48-892c-84385b7c3491))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 7ca30736-3013-4b06-95a3-c379d6b3b17d))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 8e709239-d177-48eb-9978-8b63db34c477))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 4a97fd30-fb67-4afb-aa60-ea39d0f7f76f))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 7f73177d-ed87-4e79-81ce-379d48fed7b1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp b594bcc9-4930-429e-b6e0-7b20c6561a3b))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp e7e942dc-3511-4a3c-891d-ef583a3976cd))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp feeca604-5304-4a88-be73-448ae977ab3c))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(C24-Pad2)") (pintype "passive") (tstamp 7272484e-494d-49b3-a0f8-940d7814758b))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 14c67ec2-e7e0-46ef-bf26-7f59d45e273e)
    (at 138 154)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/852f2b59-4349-4ded-9ff8-40f442f4a468")
    (attr smd)
    (fp_text reference "R13" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp c324d956-ad69-4fd0-8ccf-935cf75b869a)
    )
    (fp_text value "2.2k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e8057a74-a353-4516-b452-d45e0aef1105)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 307fcbb5-2cfc-45ef-90a1-c6e4e50615c6)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 09e06a23-b16d-46c6-a340-db94caaef8b0))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 4cf31fa7-0823-4a72-bd69-ab03bcf50e1e))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 30eabeda-5b93-492d-b8de-47e94ba569e5))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 6d313a03-80d0-42d3-be68-d578ce583cc4))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp a6d85825-1790-4c6f-9e46-151bfbb9c889))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp e5264624-8c64-4d77-853d-a22ea99657d4))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 0ceb13ff-4416-4fd2-83bb-2cd26b7c2917))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 1009d022-b3ee-4c86-ba77-dc1d8836405e))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 2071bde3-0159-4622-a3e4-7e2a9c57ac67))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 6a9d4a18-ce9b-48b5-a900-d679ca87a850))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 51 "/Sensor_Controller/CAPT_X1") (pintype "passive") (tstamp e8ccba4c-7854-4a33-a7ab-d0de2c348177))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(R13-Pad2)") (pintype "passive") (tstamp de7aeb98-b2bc-42b8-a75b-4648a77771cf))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 1926dfd2-fa9a-459a-9831-251deda68485)
    (at 47.5 105.5 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/00dacdc9-2378-49a8-b5b4-fb10ee89b4a3")
    (attr smd)
    (fp_text reference "R30" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4c278fa2-e2c7-4088-aad5-34295374b8e1)
    )
    (fp_text value "5k1" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 76b8d1b1-fb34-4a44-a70f-835a8c800651)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 874acfff-5174-4f7d-8e28-1787542b91b5)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 414c03ba-82ad-4be2-99e8-e3e59b10f4e1))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp ea5bc969-f012-40c1-a407-e262633f4e84))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 1029d08e-05b6-4670-a745-8e219be9ce2e))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 8380926f-b40d-4750-8030-17278e9fcffa))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 96a8b84f-53ba-4421-8070-869a580f98b9))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp bab33f0e-b95d-49c9-9950-7069845fefeb))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 292c7d73-8aa4-45c5-876a-c95d0603c9e3))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 9a66b406-c023-4005-8e79-4d7ad7bc268c))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp a344e292-2023-49dc-b9c2-b91cdb1b775b))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp d47709da-cd12-45d8-a54a-9a32aab30ef4))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 65 "Net-(J2-PadB5)") (pintype "passive") (tstamp b94abc15-0c7a-411f-9d01-e1b1f3279c81))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 1715e392-1094-48c5-bdbc-0fd8cc5243fe))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "B.Cu")
    (tedit 5F6F9B37) (tstamp 1e9924e2-d09c-41b6-b226-7c4b181ca046)
    (at 180.8 110.6 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/bc1119e7-c235-4e01-bcba-765c92c9171d")
    (attr smd)
    (fp_text reference "U9" (at 0 2.4 -270) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp decfe496-7ac0-4b52-9180-246d8b56e81e)
    )
    (fp_text value "PAM2804AAB010" (at 0 -2.4 -270) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 97508770-0e85-4e04-8781-80db62f74bd3)
    )
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp d6210ba9-9d0e-4dc1-a492-2a8cc0c649d2)
    )
    (fp_line (start 0 -1.56) (end -0.8 -1.56) (layer "B.SilkS") (width 0.12) (tstamp 28c5635f-bcde-46bf-8eac-111673b8dafc))
    (fp_line (start 0 1.56) (end -1.8 1.56) (layer "B.SilkS") (width 0.12) (tstamp 86fd2747-a482-4616-bc7f-f3d771a7edf9))
    (fp_line (start 0 1.56) (end 0.8 1.56) (layer "B.SilkS") (width 0.12) (tstamp 96b92b64-97bd-4af7-bedc-2cfbf22bbb1f))
    (fp_line (start 0 -1.56) (end 0.8 -1.56) (layer "B.SilkS") (width 0.12) (tstamp 9b108b5c-e631-48fa-b94a-4a189be1ab71))
    (fp_line (start -2.05 1.7) (end -2.05 -1.7) (layer "B.CrtYd") (width 0.05) (tstamp 2f8bf747-b18c-433b-b45a-1a5fe7bb53a8))
    (fp_line (start 2.05 -1.7) (end 2.05 1.7) (layer "B.CrtYd") (width 0.05) (tstamp 59418740-8dc4-45a2-a633-02865c67a53f))
    (fp_line (start -2.05 -1.7) (end 2.05 -1.7) (layer "B.CrtYd") (width 0.05) (tstamp 6f44e423-aa59-46f3-a09b-dcf1b222c3d5))
    (fp_line (start 2.05 1.7) (end -2.05 1.7) (layer "B.CrtYd") (width 0.05) (tstamp 8714d00b-98bc-4c62-ae1d-32281fb60c76))
    (fp_line (start 0.8 1.45) (end 0.8 -1.45) (layer "B.Fab") (width 0.1) (tstamp 0d4e988f-6beb-4920-be2a-e52d78a65fa4))
    (fp_line (start -0.8 -1.45) (end -0.8 1.05) (layer "B.Fab") (width 0.1) (tstamp 6153c9b9-4d7c-41e3-8f6d-13d153bd9877))
    (fp_line (start -0.4 1.45) (end 0.8 1.45) (layer "B.Fab") (width 0.1) (tstamp 6aba3f23-9a72-435a-b52e-f119586bcef4))
    (fp_line (start 0.8 -1.45) (end -0.8 -1.45) (layer "B.Fab") (width 0.1) (tstamp 74700514-f0bf-4f06-98dd-43e82d4a7035))
    (fp_line (start -0.8 1.05) (end -0.4 1.45) (layer "B.Fab") (width 0.1) (tstamp d4f7a701-2433-46e0-80f3-09ccc7ee357c))
    (pad "1" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 73 "/Power_Management/LED_PWM") (pinfunction "EN") (pintype "input") (tstamp 1fbbff41-f3ae-4a63-aafd-aca488af22c3))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 7f2b6590-31ee-4edc-9292-0de077ab8c1e))
    (pad "3" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 84 "Net-(L1-Pad1)") (pinfunction "SW") (pintype "power_out") (tstamp 7b10b0fb-78fa-4f00-9fbe-3282a1b659ca))
    (pad "4" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "/Power_Management/PS_SWITCH") (pinfunction "VIN") (pintype "power_in") (tstamp 1cf5385c-0a9e-4bfb-9af3-8e177327d2de))
    (pad "5" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 28 "/Power_Management/LED_K") (pinfunction "FB") (pintype "input") (tstamp 8b99292e-99a1-44af-a8e9-6f17f8956d51))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 217e1922-6758-4300-9065-183181884750)
    (at 59.48 142.92 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/72db94ec-ec8f-4f52-b14a-cad4ace8165c")
    (attr smd)
    (fp_text reference "R22" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 63919fdf-4f76-4612-a23e-24caf4651692)
    )
    (fp_text value "1.2k/1%" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0dbd98e3-f380-420a-8980-062e99eeb227)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp fa66ce41-81c8-47c6-b260-581b6a50e02b)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 7195475c-46a6-46f9-a8b2-07be11e60ee1))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp ea191c79-ece6-4d65-829e-449535533f01))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 28f282b9-8683-4938-ac30-602cda7276ed))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp b94aa31d-8325-4d0c-86d4-a56c22c14a5a))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp d8999d6b-10e9-4293-a175-53a5d56940d7))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp e4bc7ada-072d-4c8b-a504-36c9c5415360))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 2561e86d-bd9e-49bc-86cf-50fd2bfe9879))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 4c4e906a-a31b-4c8a-b64f-41e629ae2948))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp a9e6caad-f9bf-4d42-a0eb-dbb0d47a89d4))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp ebfad4e6-93e3-420d-963b-06c58cce9c10))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(R22-Pad1)") (pintype "passive") (tstamp 19e863dc-0dce-475a-b6c3-b44c712b8b12))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 9bffa444-d5e8-4460-8a0c-af5acf071641))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 226393cd-22b5-4983-be87-3e20bc5f5e28)
    (at 68.98 137.54 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/45d7985c-1554-4487-86cc-8a66b6c5acbf")
    (attr smd)
    (fp_text reference "C12" (at 0 1.16) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 41840057-a5c6-4d10-8d67-734ffb8f616f)
    )
    (fp_text value "100nF" (at 0 -1.16) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4e6171df-0285-4054-b9ed-521c80c367c1)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
      (tstamp 472de63d-67a4-4f01-b7c9-8a19c3e4c2f6)
    )
    (fp_line (start -0.107836 -0.36) (end 0.107836 -0.36) (layer "B.SilkS") (width 0.12) (tstamp 6619f656-d6db-45b9-b056-dc8fc5bde40d))
    (fp_line (start -0.107836 0.36) (end 0.107836 0.36) (layer "B.SilkS") (width 0.12) (tstamp af6504c7-8ade-4819-acd9-c897b0faa00c))
    (fp_line (start -0.91 0.46) (end 0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 020bb31b-2d28-4f41-b8b0-13fbd99ec555))
    (fp_line (start 0.91 -0.46) (end -0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 300e8828-ea8d-42b1-b729-ababef1a1976))
    (fp_line (start -0.91 -0.46) (end -0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 663926df-5a4d-4a00-8f46-a12bc231da49))
    (fp_line (start 0.91 0.46) (end 0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp c3c96d2a-1999-4f84-b9af-f7dc68b0cfe4))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 2b9d5a16-b9d6-4870-a55a-348b713c794c))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 461cb3b1-fabf-4c9f-9c14-b0f8731efee8))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp adad789a-33f8-4f0d-b121-bd58eab931b5))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp eb2eb7ec-6bac-4f2a-918d-2602a00efcf5))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 66 "/Sensor_Controller/CAPT_YH") (pintype "passive") (tstamp 0959f107-6371-4c78-b9b9-7311cb488452))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "/Sensor_Controller/CAPT_YL") (pintype "passive") (tstamp 2b72268e-c336-4c91-b986-01b20066c08a))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 244bc15e-3ae8-4870-bfa7-c97f8c79c39c)
    (at 47.5 97.54 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/b6fbb578-d9a9-41b6-94c1-87e986c95da5")
    (attr smd)
    (fp_text reference "R32" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 6ef62af6-0b3a-4f43-9b46-0302dc586129)
    )
    (fp_text value "10k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f0712750-74d9-4531-8453-432780b60d5f)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 7eabcb3f-61ef-48fc-b94b-7d08daad20d9)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 1d5de519-5468-486c-ae84-6f53c307fc64))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp d5d1dee7-dd17-489b-88ad-195d9656f347))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 32882d00-0786-40dd-9bf3-e215e00e32dc))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 6b4ecdea-3d21-468e-a254-707b75f31f9b))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 88f64c12-e6a7-4827-bd68-c7d0dd2e7e7b))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp ab7519fb-fa08-4e73-9af8-e224aee27e52))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 39c07f9d-98c0-4981-afa6-2afeab0abc8a))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 5b6c93bf-e610-4321-88c7-13f752b9788e))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 745dc813-72b2-49b5-8ef4-d40529dc0fb6))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 9f2ed64e-6d3b-46bd-9176-3a34622a8de1))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "VDD") (pintype "passive") (tstamp 5abcfa10-5fef-4172-930f-4b1017fc0b5b))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 35 "/WiFi_Display/EPD_~{RES}") (pintype "passive") (tstamp b87a3a50-d423-48ea-8987-f615be48113c))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 26394413-ed32-480a-afcf-831ead25ec12)
    (at 159 154)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/ff08df82-82e0-4f66-81d6-9361e8ff617f")
    (attr smd)
    (fp_text reference "R17" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp da103916-30f6-4d9e-bd80-72d95b00b726)
    )
    (fp_text value "2.2k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 97402c3d-c134-4aab-8950-3eb3030a5ddf)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp c32e4068-0bbb-4cbf-8426-66eb97e40e5c)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 1ae97f36-8b82-4cba-8ea9-f578959766fd))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 9f0857ff-458b-49c4-9e3e-529e1a0c08fa))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 167a9f0d-30b1-4b99-a270-2e64b34e1017))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 221869d1-02f8-4607-8bb7-37c5d7b48861))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 5a81c4f9-d660-493f-bbed-409e0343192b))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 831350e9-07a6-42e6-ada2-8095e0debd17))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 81bd237a-9bde-4705-a7d7-a99b367e10cf))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 9f3b88ac-71ba-445b-a9ed-e7019fc1fc0b))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp bc6ec194-af13-4709-a76f-4b2ecad0f2eb))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp d751e8a6-4117-419e-a949-849d7e17d914))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(R16-Pad2)") (pintype "passive") (tstamp 8de703ce-f09c-4742-9b4e-d5a9ef5b34ad))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(R17-Pad2)") (pintype "passive") (tstamp 1ba300a6-c588-4e7e-af84-16bdabb09857))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 26df824f-ac33-4e74-b441-fb2f5c05fd25)
    (at 122.5 154)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/225641de-f04d-4386-b398-c9e4eea312d2")
    (attr smd)
    (fp_text reference "R10" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 868a406a-0022-46a6-88a9-c65c24185b5a)
    )
    (fp_text value "2.2k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a982f870-0738-4390-a0ac-df25808c04d7)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp b3b71614-d96e-406f-94b3-98c46e7d9f71)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 5576b6fc-7b29-4cef-ba22-228822ea77aa))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 59297b19-632d-44f5-af15-44bc435a1738))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 53d4862b-849b-4a08-815c-b0a179fc03ef))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 67563aaf-d8a3-40f6-8578-af5c9e58def3))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 9d720ea2-baea-4ddd-a3aa-48a8d169a4a1))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp ef059274-f56f-4317-a5c7-bd10d9cfe8ae))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 52b9a64f-37ec-4bdf-a263-08dd68cd867a))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 9e0b8868-5f28-48d1-a9c2-4a10863171a7))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp d17a3e60-41f0-401f-a8c0-97bc5cc3bdee))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp d6d0cade-7956-4794-ae69-f04ac8df62e4))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 48 "/Sensor_Controller/CAPT_X0") (pintype "passive") (tstamp d50d89ac-668e-4078-b987-41243b62c2ee))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(R10-Pad2)") (pintype "passive") (tstamp 42784d53-3bc1-45ed-ba43-0c9006c67ecc))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 279b4d26-74e0-4dd7-8c04-8045465f6bc5)
    (at 174.9 119.9)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/de5e0106-37c5-4989-9533-3c8be3a2ae94")
    (attr smd)
    (fp_text reference "C31" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f7562b17-fce9-4658-ac42-8e9e81658504)
    )
    (fp_text value "1uF/50V" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a47f679b-4aa7-42f5-b4c8-f1b0bac7b24e)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp bf4ca68a-f7fd-46d6-84ff-f09eaae6b91c)
    )
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp 4c96c2bf-be19-4bb5-8c72-a00c594b5fa9))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp 9e37d154-39c3-44a8-8476-e97241b7f32f))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp c8eac3dd-2e98-40a9-961f-020203e74a27))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp c958e914-9300-4007-bedb-ec66e3b39950))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp d22a5050-d3ee-4798-9975-c3b14f9bfd5d))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp f25cb490-2e58-4b4a-a002-7fcf2f2f4806))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 46c0cc17-413c-48aa-9fe0-1b2a692aa79d))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 6cfeaf3c-7a99-4681-a7bc-ddf6e7bd2d5e))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 87cd3a53-c294-42de-a9dd-a44501480e73))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp e606b722-953e-4eca-836d-864344e5f334))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp eed154e5-b8eb-4099-a0bf-5b245276ca03))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(C31-Pad2)") (pintype "passive") (tstamp 3eab41a1-4e00-4bc4-9a80-0cf32609574b))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (tedit 58645DC7) (tstamp 28f8e5f0-7257-44c2-bff6-a4c199377988)
    (at 169 120.8 180)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/a9a8016b-33a5-48af-954e-c479e1f25276")
    (attr smd)
    (fp_text reference "D4" (at 0 2) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp ab6aecf0-5474-4129-b2ff-249f5546d28b)
    )
    (fp_text value "RBR2MM30BTR" (at 0 -2.1) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 9e32adee-c7c6-4c1a-8cbc-143139bf04ba)
    )
    (fp_text user "${REFERENCE}" (at 0 2) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 9949b888-a918-4bd8-a370-334f5137d07c)
    )
    (fp_line (start -2.25 -1) (end 1.65 -1) (layer "B.SilkS") (width 0.12) (tstamp 65afe781-adf2-4144-88b7-117fc3fbbef6))
    (fp_line (start -2.25 1) (end -2.25 -1) (layer "B.SilkS") (width 0.12) (tstamp 737e34c4-9b80-4433-82cf-3940e9cbf3bd))
    (fp_line (start -2.25 1) (end 1.65 1) (layer "B.SilkS") (width 0.12) (tstamp 7b2f9605-b99b-4958-9464-cfd5e6f63e4c))
    (fp_line (start 2.35 1.15) (end 2.35 -1.15) (layer "B.CrtYd") (width 0.05) (tstamp 020e6e92-9ec3-46f4-95d7-f16bf33cf172))
    (fp_line (start -2.35 1.15) (end -2.35 -1.15) (layer "B.CrtYd") (width 0.05) (tstamp 04601928-da12-40e1-a158-b42168895cdd))
    (fp_line (start -2.35 1.15) (end 2.35 1.15) (layer "B.CrtYd") (width 0.05) (tstamp 3217d8f4-18b4-43e6-a000-f3524758ef7c))
    (fp_line (start 2.35 -1.15) (end -2.35 -1.15) (layer "B.CrtYd") (width 0.05) (tstamp 3493d6f3-768a-4fc6-8e15-7189c43cb1bc))
    (fp_line (start -1.4 -0.9) (end -1.4 0.9) (layer "B.Fab") (width 0.1) (tstamp 1eb39a27-b6fc-483f-afb1-7056edae9c75))
    (fp_line (start -1.4 0.9) (end 1.4 0.9) (layer "B.Fab") (width 0.1) (tstamp 2563eb79-bcbc-4435-8a85-452275ae8dd3))
    (fp_line (start -0.35 0) (end 0.25 0.4) (layer "B.Fab") (width 0.1) (tstamp 305c2a43-13af-4d42-9e98-45a7f86411a5))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4) (layer "B.Fab") (width 0.1) (tstamp 510d4455-4831-47f3-a9ae-510c0e077311))
    (fp_line (start 0.25 0) (end 0.75 0) (layer "B.Fab") (width 0.1) (tstamp 7c280c7b-3578-4408-b65b-2a7e5544cab1))
    (fp_line (start 0.25 -0.4) (end -0.35 0) (layer "B.Fab") (width 0.1) (tstamp 82cb542c-cc21-4d4d-a762-99b49416d096))
    (fp_line (start -0.75 0) (end -0.35 0) (layer "B.Fab") (width 0.1) (tstamp 8925b410-6d59-4c9d-9f9f-54581586ac3a))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer "B.Fab") (width 0.1) (tstamp 8957c93a-2fbb-4625-8b62-5ed03bdc663b))
    (fp_line (start 1.4 -0.9) (end -1.4 -0.9) (layer "B.Fab") (width 0.1) (tstamp 9601d96f-62c1-414d-b3d1-8609c10f6a6a))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer "B.Fab") (width 0.1) (tstamp e2432ebf-42d2-4085-825c-96524d254dbf))
    (fp_line (start 1.4 0.9) (end 1.4 -0.9) (layer "B.Fab") (width 0.1) (tstamp f9cae35d-35d1-4bc5-a36e-1f3c0f05324e))
    (pad "1" smd rect (at -1.65 0 180) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "K") (pintype "passive") (tstamp ea9fc206-662a-40e1-a27d-bfe2ebc24049))
    (pad "2" smd rect (at 1.65 0 180) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "Net-(C22-Pad1)") (pinfunction "A") (pintype "passive") (tstamp 06540d6f-ece8-408b-910f-a2aa61e9355d))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 2b259426-6943-4fac-a589-7602907648a5)
    (at 65.48 140.92 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/b0e1f2f9-8869-4117-9f57-9fc491871861")
    (attr smd)
    (fp_text reference "R28" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp fff79040-0349-4f57-9c14-ef3b7e61ff4d)
    )
    (fp_text value "5.1k/1%" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 605d48db-f266-4c76-90a7-ec225c25b0c5)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 4c2232c6-78dd-4cd5-87b2-67c9044a9930)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 3a7c9a3a-46ef-4c3c-b5c7-5dda1b723ba4))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp ca6a0032-eb9b-424c-b374-cb42f2a04e3d))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 5ae8e899-92cc-49ff-a192-205dd1465f54))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 9b625148-3472-4760-aacf-96617bad7980))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp bafbfa75-bda2-4f04-8d3b-e4b444af3acb))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp ea886d58-5152-4ba2-aadf-189c3fdf982b))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 22ba11d8-8a26-4eae-bf47-3e6188bf5852))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp a042d380-fd01-4702-afb3-817497801d4c))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp b20568c6-2d00-49c3-a0a2-7229b29305aa))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp bf5cca0d-1e23-4311-9db9-0cebf9bf8acb))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(R27-Pad2)") (pintype "passive") (tstamp edc7daa6-9cd6-437f-95cc-d86fbd3b3c54))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 1b82510e-67a0-482f-a1c7-16065a1c2e88))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 2e68f97d-0bb4-491f-b3cd-5bea688cdb47)
    (at 183.3 111.2 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/7de2ce23-77a2-4da0-b343-e039cbb2217b")
    (attr smd)
    (fp_text reference "C18" (at 0 1.43 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp b252bcf7-83fa-4590-9671-7ce615bce521)
    )
    (fp_text value "4.7uF" (at 0 -1.43 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f131cc5a-2664-4742-8bac-17248283ba71)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp d61c54c4-c563-479b-9263-152fcfc7c590)
    )
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp 835bf769-a4a8-467e-8c83-9c768500bfe2))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp bb069eb0-fd6c-40a1-b68f-388af3f94d13))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 1c10b31f-b3db-4716-a69d-e9690d59a72e))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 5aaa20e6-1e77-44c4-b6cb-e42fc48a40f5))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 9f05fc03-f27b-438e-b822-452aac7d694b))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp d9b17df6-5ac0-494e-a5f2-bfca8d064f29))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 0254e687-80ef-45d3-beb9-7b7eb6761692))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 744226a9-08f1-4a4d-a55a-dea2dbaaefec))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp a1d482d4-aa48-46e3-ba5c-a9e825a85d46))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp aaaf0153-088b-4ada-92bf-f597b5a15ae6))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "/Power_Management/PS_SWITCH") (pintype "passive") (tstamp c96ddf13-ca31-47db-abad-b2401dbb45f3))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp eb3eac71-0c2f-455b-b3a5-69b08032c6f8))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (layer "B.Cu")
    (tedit 5A64794F) (tstamp 38127ad4-cca1-4c78-aee2-2e28b559f919)
    (at 185.3 135.7 180)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/9ca062cc-08da-433e-bffe-2c55fb0f798f")
    (attr exclude_from_pos_files)
    (fp_text reference "JP1" (at 0 1.8) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0d7664b5-1586-4e8b-b98d-88d1aa73994e)
    )
    (fp_text value "Jumper_2_Open" (at 0 -1.9) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 79cf566d-caed-4559-bf8b-a2ab7cc0cc5c)
    )
    (fp_line (start 1.4 -1) (end -1.4 -1) (layer "B.SilkS") (width 0.12) (tstamp 91a9af8f-3a58-43bd-ae78-a5400c39cd9f))
    (fp_line (start -1.4 -1) (end -1.4 1) (layer "B.SilkS") (width 0.12) (tstamp 964e2994-5538-404d-81cc-5c29debd4395))
    (fp_line (start -1.4 1) (end 1.4 1) (layer "B.SilkS") (width 0.12) (tstamp a4b011e3-b437-4c98-8707-906d2f1932e5))
    (fp_line (start 1.4 1) (end 1.4 -1) (layer "B.SilkS") (width 0.12) (tstamp df33c9e2-0097-4b83-86f1-90c82408441e))
    (fp_line (start -1.65 1.25) (end 1.65 1.25) (layer "B.CrtYd") (width 0.05) (tstamp d76fc4e8-7ba0-42e1-ab4c-e414582be8bb))
    (fp_line (start -1.65 1.25) (end -1.65 -1.25) (layer "B.CrtYd") (width 0.05) (tstamp e694fc6d-6452-44c3-817d-d848973fc169))
    (fp_line (start 1.65 -1.25) (end 1.65 1.25) (layer "B.CrtYd") (width 0.05) (tstamp f1e0bbcd-607c-44fc-8908-f558a33432d3))
    (fp_line (start 1.65 -1.25) (end -1.65 -1.25) (layer "B.CrtYd") (width 0.05) (tstamp fb8d5a2c-afe4-47f5-9e70-1e90c86e21b9))
    (pad "1" smd custom (at -0.725 0 180) (size 0.3 0.3) (layers "B.Cu" "B.Mask")
      (net 106 "Net-(BT1-Pad1)") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1 0)
            (xy 0.5 -0.75)
            (xy -0.5 -0.75)
            (xy -0.5 0.75)
            (xy 0.5 0.75)
          ) (width 0) (fill yes))
      ) (tstamp 83869a2f-1976-4b95-8777-0e71f675e57d))
    (pad "2" smd custom (at 0.725 0 180) (size 0.3 0.3) (layers "B.Cu" "B.Mask")
      (net 6 "VCC") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.5 -0.75)
            (xy -0.65 -0.75)
            (xy -0.15 0)
            (xy -0.65 0.75)
            (xy 0.5 0.75)
          ) (width 0) (fill yes))
      ) (tstamp e484df0b-90ea-4a13-b115-915b9b8f228e))
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 389bf5a5-a942-4c7c-9e24-cf86e886d331)
    (at 163.1 140.6 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/5098fb42-bc7c-42e8-9420-50e3b2cde494")
    (attr smd)
    (fp_text reference "R23" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f31b7269-380f-4ffa-a522-13a349bb99d1)
    )
    (fp_text value "27.4k/1%" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 3ca5c00c-7751-48d9-b285-427e04f40740)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp d80b60cf-4925-4049-bd7c-e876aa70077b)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 98de562d-c708-4f10-8583-5c25bbb50169))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp e3dfa01e-3d6f-46b8-9b9b-d791fbfdeb0c))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 58da578b-95fc-453d-a2c2-61adad486303))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 5fa17f37-bdf9-44ee-8119-107cb867b887))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp c8e0090c-f40a-44a5-b96b-d8310ce9463d))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp d77b4982-23bb-449b-8442-0f585bf961ed))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 208d190b-7b86-4f37-ba8a-96afc27bd5e4))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp ba6ef5fb-63b5-4a89-9528-66b082c78529))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp c21c432c-9c02-4987-af4f-28c9765fdcf7))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp d7da7b58-2eaf-4646-b9cb-4ba565b06ada))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "VCC") (pintype "passive") (tstamp 76e6186d-f265-49e6-9c67-2bd1679127a4))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 62 "/Power_Management/ADC_BAT") (pintype "passive") (tstamp 3ee39d29-10da-4461-934c-8b97c1ba4139))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 3a8b6329-61e9-45be-9849-4b4d0f99dbeb)
    (at 174.9 125.9)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/59ed7485-a176-4f28-a203-6093f26603a7")
    (attr smd)
    (fp_text reference "C29" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4a03865e-4a35-4c58-8391-461821a80a03)
    )
    (fp_text value "1uF/50V" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5091702b-afbd-41d3-a6cb-75ae95bc37d9)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 50edf5b9-d54c-496c-93d0-f30645219324)
    )
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp 67d683cc-ab42-41d3-92fe-4f3d8cc05b03))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp 959ee9b8-bd33-4eb6-ba77-02dd4458c741))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 125f651a-b88c-4126-af4d-15b333ea8127))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 53d51f00-e51e-49d7-b5fb-43b536055a07))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 9e36483c-b79b-4aea-adb0-149aeb2ff12c))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp ccba2986-717c-4d0e-8691-061c9f4fd01d))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 0deee350-3ce8-43de-b2d0-5cd8d40cdcaa))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 39994704-4a55-4993-96e7-ce3ce3e9f098))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 98f87a6a-7cc8-4f89-95ae-31f3a30ea1e6))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp f8ce3691-1e38-41cb-8150-0c07230346a1))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 2800d593-d01c-4ff1-9542-380b8647eaf5))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(C29-Pad2)") (pintype "passive") (tstamp 117f8306-102c-4bcf-8da7-cfeb5751fc9a))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-666" (layer "B.Cu")
    (tedit 5A02FF57) (tstamp 3aff516b-5fe2-4568-b035-6f4a5297999f)
    (at 192.9 147.2 -90)
    (descr "SOT666")
    (tags "SOT-666")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/b277339b-9993-4d9c-83f1-94c3e1969272")
    (attr smd)
    (fp_text reference "U11" (at 0 1.75 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 80c9154b-577d-4d26-abd2-6c2e768bad49)
    )
    (fp_text value "USBLC6-2P6" (at 0 -1.75 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 6a719da2-7d52-483a-9d0c-702376c392f0)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
      (tstamp 9dcf340c-c9e5-4832-b08e-7eb423a0a266)
    )
    (fp_line (start -0.8 -0.9) (end 0.8 -0.9) (layer "B.SilkS") (width 0.12) (tstamp 55c78095-0430-4058-b26a-4f03d7aadf68))
    (fp_line (start 0.8 0.9) (end -1.1 0.9) (layer "B.SilkS") (width 0.12) (tstamp ed625d72-292b-4204-9f50-a0488198d441))
    (fp_line (start -1.5 1.1) (end 1.5 1.1) (layer "B.CrtYd") (width 0.05) (tstamp 79d2bccc-e7b3-4d71-9155-a31a045ddb6a))
    (fp_line (start -1.5 -1.1) (end 1.5 -1.1) (layer "B.CrtYd") (width 0.05) (tstamp 9245cacd-ff6a-45ff-96bc-9853f8a04430))
    (fp_line (start -1.5 1.1) (end -1.5 -1.1) (layer "B.CrtYd") (width 0.05) (tstamp c5c0084d-82f8-40dc-98df-8f34eb71594c))
    (fp_line (start 1.5 -1.1) (end 1.5 1.1) (layer "B.CrtYd") (width 0.05) (tstamp e55f6686-f164-4c9d-b923-2ae183eda345))
    (fp_line (start 0.65 -0.85) (end -0.65 -0.85) (layer "B.Fab") (width 0.1) (tstamp 09ea0d68-2376-4ee5-b15b-e5fa7f7641db))
    (fp_line (start 0.65 0.85) (end -0.33 0.85) (layer "B.Fab") (width 0.1) (tstamp 7f9ea9d4-75ed-457c-8138-56eab532a2c8))
    (fp_line (start -0.65 0.53) (end -0.33 0.85) (layer "B.Fab") (width 0.1) (tstamp e3e8c907-2d96-4c29-ab8b-c7d6b367f76f))
    (fp_line (start -0.65 0.53) (end -0.65 -0.85) (layer "B.Fab") (width 0.1) (tstamp e889f87e-178f-4fdd-bfb4-f22e60cbb081))
    (fp_line (start 0.65 0.85) (end 0.65 -0.85) (layer "B.Fab") (width 0.1) (tstamp fbe6bcae-fd86-4649-b431-d1d8b3dfc067))
    (pad "1" smd rect (at -0.85 0.5375 270) (size 0.5 0.375) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 86 "/WiFi_Display/USB_D+") (pinfunction "I/O1") (pintype "passive") (tstamp ad80fb9b-2940-44a0-b984-5bb2ca7ded04))
    (pad "2" smd rect (at -0.925 0 270) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive") (tstamp a06e0270-f84e-4751-b217-be9cda5b6a8a))
    (pad "3" smd rect (at -0.85 -0.5375 270) (size 0.5 0.375) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 87 "/WiFi_Display/USB_D-") (pinfunction "I/O2") (pintype "passive") (tstamp 6b529606-7e7c-4c37-aa5d-230741ab0aaf))
    (pad "4" smd rect (at 0.85 -0.5375 270) (size 0.5 0.375) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 87 "/WiFi_Display/USB_D-") (pinfunction "I/O2") (pintype "passive") (tstamp 5e5abe92-b1c2-43bd-9010-138e3fbd8fa9))
    (pad "5" smd rect (at 0.925 0 270) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "VBUS") (pinfunction "VBUS") (pintype "passive") (tstamp 296f96c1-2f68-4990-8d78-5133994883ba))
    (pad "6" smd rect (at 0.85 0.5375 270) (size 0.5 0.375) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 86 "/WiFi_Display/USB_D+") (pinfunction "I/O1") (pintype "passive") (tstamp c02dae34-f334-48ec-bc33-4c24d0d98b3f))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-666.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 3c8f0ee5-2905-48f8-980d-16c50caf8473)
    (at 133 154 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/93a9dbdb-d19d-4957-b2bc-942977ecca26")
    (attr smd)
    (fp_text reference "R12" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d9403c5e-b9ef-4f90-916a-9042281fc480)
    )
    (fp_text value "2.2k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a3e21f03-1ee5-4d49-b818-1e22cac4a057)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 96eec8b7-1873-4d43-96d1-8b0cbc8c31ae)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 91ad4c4e-70d4-4f6f-8a6b-468e6043ae37))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp a21d7e60-eb90-426a-8727-b92d9cdfbd71))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 1306c618-e9d6-4f9c-8dad-aec4f3bb87d5))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 5c2e2978-61cb-4d5d-8d5d-b926f277264d))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 756d392d-24f3-44a4-8875-92f6c0d33701))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 9f32b52a-dd73-4334-bd99-4c792116ada8))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 2d51da5b-0ac2-4918-805d-a90d4fe8f82a))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 6da00c72-40c8-47bb-aeed-103373f111d9))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 95894ccb-e575-4bb8-9bfb-38b3b3d81345))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp d0bd9bbc-e966-415d-85bc-66b9fc85361d))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 51 "/Sensor_Controller/CAPT_X1") (pintype "passive") (tstamp b9a7fe8c-f6eb-4a3d-a00a-d08b7acfc10d))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(R11-Pad1)") (pintype "passive") (tstamp fb03efd1-d65c-483a-afe9-87bf80f9617a))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Button_Switch_SMD:Panasonic_EVQPUJ_EVQPUA" (layer "B.Cu")
    (tedit 5A02FC95) (tstamp 3dc2effe-ce89-4859-b08e-4e141203499a)
    (at 158.4 107.4 180)
    (descr "http://industrial.panasonic.com/cdbs/www-data/pdf/ATV0000/ATV0000CE5.pdf")
    (tags "SMD SMT SPST EVQPUJ EVQPUA")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/50c3f9e1-72d8-4c24-85e0-c5f7d5eb3021")
    (attr smd)
    (fp_text reference "SW2" (at 0 4.5) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 85d355f7-a945-4b1e-a077-538eb0c48f8b)
    )
    (fp_text value "EVQPUA02K" (at 0 -3.5) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp c04c1663-475f-416f-8e67-791195f37492)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp cd204456-bcff-435b-ba6f-d2ad378dacc2)
    )
    (fp_line (start 2.35 1.85) (end 1.425 1.85) (layer "B.SilkS") (width 0.12) (tstamp 26a1224a-39f9-4d08-9082-44228cb235dd))
    (fp_line (start -1.425 1.85) (end -2.35 1.85) (layer "B.SilkS") (width 0.12) (tstamp aa852409-314a-43a5-a600-bbb2dfab0329))
    (fp_line (start 2.35 -1.85) (end -2.35 -1.85) (layer "B.SilkS") (width 0.12) (tstamp cc570866-967c-42e8-86fa-8584cabef770))
    (fp_line (start 2.45 -0.275) (end 2.45 0.275) (layer "B.SilkS") (width 0.12) (tstamp cf2c0af0-a2ee-4380-8361-76a2cd2557cb))
    (fp_line (start -2.45 -0.275) (end -2.45 0.275) (layer "B.SilkS") (width 0.12) (tstamp f0ad0976-65df-4f10-9373-49198dff5bcb))
    (fp_line (start -3.9 -2.25) (end -3.9 3.25) (layer "B.CrtYd") (width 0.05) (tstamp 32932905-014a-47d7-9d6e-8a1eae5f5f53))
    (fp_line (start 3.9 3.25) (end -3.9 3.25) (layer "B.CrtYd") (width 0.05) (tstamp 65dedb2b-88b3-4f64-8c77-18fd95549666))
    (fp_line (start 3.9 -2.25) (end -3.9 -2.25) (layer "B.CrtYd") (width 0.05) (tstamp 9f7251d2-b5d5-45c1-8475-8488fa04d943))
    (fp_line (start 3.9 -2.25) (end 3.9 3.25) (layer "B.CrtYd") (width 0.05) (tstamp d17035f7-ddd3-4cf3-b3b7-b6613923c3ed))
    (fp_line (start -2.35 -1.75) (end -2.35 1.75) (layer "B.Fab") (width 0.1) (tstamp 02074905-d2bb-4bb1-b4fb-2711cdcaa242))
    (fp_line (start -1.3 2.75) (end -1.3 1.75) (layer "B.Fab") (width 0.1) (tstamp 08300c1f-07c2-423c-b5d5-acd350ad8cc4))
    (fp_line (start 2.35 -1.75) (end -2.35 -1.75) (layer "B.Fab") (width 0.1) (tstamp 496c153f-cc7d-46cb-9886-6d37579ad345))
    (fp_line (start 1.3 2.75) (end -1.3 2.75) (layer "B.Fab") (width 0.1) (tstamp 828d1081-ff68-401f-8675-b8e6c41b3cbf))
    (fp_line (start 2.35 -1.75) (end 2.35 1.75) (layer "B.Fab") (width 0.1) (tstamp c172ce33-dbec-456e-8241-59be851364c7))
    (fp_line (start 1.3 2.75) (end 1.3 1.75) (layer "B.Fab") (width 0.1) (tstamp c8bead37-9359-43ab-aa40-129ef3102b6d))
    (fp_line (start 2.35 1.75) (end -2.35 1.75) (layer "B.Fab") (width 0.1) (tstamp e459ba3b-1fc9-4a81-b851-2b83e8a92b17))
    (pad "1" smd rect (at 2.625 0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive") (tstamp 0b1b5735-9cc7-4da7-8553-6c7863f044a4))
    (pad "1" smd rect (at -2.625 0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive") (tstamp fa8b2414-74f8-4a58-a79f-bd6912047b6a))
    (pad "2" smd rect (at -2.625 -0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "/Sensor_Controller/LPC_~{RST}") (pinfunction "2") (pintype "passive") (tstamp 2d1710b0-356c-49ae-8f46-927cf3960a5f))
    (pad "2" smd rect (at 2.625 -0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "/Sensor_Controller/LPC_~{RST}") (pinfunction "2") (pintype "passive") (tstamp f087bccb-ba96-484e-a94b-f944740d5db8))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/Panasonic_EVQPUJ_EVQPUA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (tedit 58645DC7) (tstamp 4668c841-f35f-41a7-b0b8-e2c693772000)
    (at 154.4 112 180)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/b5b31630-e16e-4c4b-a1c5-fb069ecbb43b")
    (attr smd)
    (fp_text reference "D2" (at 0 2) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 11e3dd5d-6d6e-4343-b74b-485a73d8cbd4)
    )
    (fp_text value "RBR2MM30BTR" (at 0 -2.1) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2229ca8b-d64e-49db-9bff-2694becb44e7)
    )
    (fp_text user "${REFERENCE}" (at 0 2) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a7d577d5-212c-48e7-aa1d-ccf87cf50704)
    )
    (fp_line (start -2.25 1) (end 1.65 1) (layer "B.SilkS") (width 0.12) (tstamp 1d3a726a-a4ad-449c-829e-1502ee89364d))
    (fp_line (start -2.25 1) (end -2.25 -1) (layer "B.SilkS") (width 0.12) (tstamp 5d5eedf7-c5d8-4e8a-b5e8-ddfa7cd166c9))
    (fp_line (start -2.25 -1) (end 1.65 -1) (layer "B.SilkS") (width 0.12) (tstamp ae125281-bfaf-40c0-ac4c-b32deea32bb8))
    (fp_line (start -2.35 1.15) (end -2.35 -1.15) (layer "B.CrtYd") (width 0.05) (tstamp 17ceaaba-7293-440c-9009-b98478a65106))
    (fp_line (start -2.35 1.15) (end 2.35 1.15) (layer "B.CrtYd") (width 0.05) (tstamp 29fcf295-31d9-42a4-80e4-265d500aea50))
    (fp_line (start 2.35 1.15) (end 2.35 -1.15) (layer "B.CrtYd") (width 0.05) (tstamp 8592dbb1-ff0e-4c75-9c63-6151e3d8747a))
    (fp_line (start 2.35 -1.15) (end -2.35 -1.15) (layer "B.CrtYd") (width 0.05) (tstamp e070a86c-ec43-473e-9414-62b5edb02e7a))
    (fp_line (start -1.4 -0.9) (end -1.4 0.9) (layer "B.Fab") (width 0.1) (tstamp 09c952b1-3558-40de-8887-7000fb598a15))
    (fp_line (start 1.4 -0.9) (end -1.4 -0.9) (layer "B.Fab") (width 0.1) (tstamp 218c9e41-606a-428f-bde7-17489acd9bdb))
    (fp_line (start -0.75 0) (end -0.35 0) (layer "B.Fab") (width 0.1) (tstamp 26bbc775-c329-4cd1-8531-056b4a7cb662))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer "B.Fab") (width 0.1) (tstamp 2e99ed41-787a-4f29-9e23-bf1df12058f8))
    (fp_line (start -0.35 0) (end 0.25 0.4) (layer "B.Fab") (width 0.1) (tstamp 79698fa1-a166-4089-9792-4d1086b7d9b6))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer "B.Fab") (width 0.1) (tstamp 7cacf749-8953-47ef-bf06-dfceeb90138d))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4) (layer "B.Fab") (width 0.1) (tstamp a83f1500-f8b8-4722-bb31-ae31e669c842))
    (fp_line (start 0.25 0) (end 0.75 0) (layer "B.Fab") (width 0.1) (tstamp b468c7fb-d6ca-48d9-94c5-3d4f1bb43ca1))
    (fp_line (start 0.25 -0.4) (end -0.35 0) (layer "B.Fab") (width 0.1) (tstamp b4b28668-08a8-46cb-a192-23847594ff01))
    (fp_line (start 1.4 0.9) (end 1.4 -0.9) (layer "B.Fab") (width 0.1) (tstamp c47249eb-ec06-45ed-8886-301bf6e3d1fa))
    (fp_line (start -1.4 0.9) (end 1.4 0.9) (layer "B.Fab") (width 0.1) (tstamp eab38140-0431-44f0-ab96-785055c12665))
    (pad "1" smd rect (at -1.65 0 180) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "/Power_Management/PS_SWITCH") (pinfunction "K") (pintype "passive") (tstamp 276987a2-7db4-478e-b9fc-234214692ec0))
    (pad "2" smd rect (at 1.65 0 180) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "VBUS") (pinfunction "A") (pintype "passive") (tstamp a4a54b82-2990-413b-ad01-08443415aa35))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 4ca10ff1-f91a-4098-893a-211fdfacb763)
    (at 51.5 105.5 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/2563902e-2890-4913-a645-9f387a8737a7")
    (attr smd)
    (fp_text reference "C13" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 75a27c15-e306-4b35-af97-3e8621eef754)
    )
    (fp_text value "4.7uF" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 462d3d3d-bef3-4a79-81f2-12d19f233a7f)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp d3388eb4-5f64-4abb-8d8a-f1ee9714d83a)
    )
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp 0714c0c7-ac00-43e4-821d-22968f5fe521))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp bd1b0f34-2a0b-44c2-997b-abde9ec47a79))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 395cafc6-4f07-45db-853d-6af7f479eac7))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 6c9ce9c3-fe34-4563-81fe-15e97ba69b49))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp b0920a4a-059e-459e-ab05-12797cd696a7))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp fc713e09-ad5a-4b1b-a343-f9ac2ea14595))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 6b131d07-2e82-4329-9f1b-f715045c092c))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp d437a66c-7b61-4ba0-aaf8-71db44822adc))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp d5850f71-b966-418b-b3a8-9627dbbee18d))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp e7cc3828-f005-4c10-82f6-29fddd8c1855))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "VCC") (pintype "passive") (tstamp ea901b6f-c8bf-473d-b86b-ef25b9397be5))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp d98c1a08-e2ee-45ef-8a67-a1c3f0d821ce))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEF0) (tstamp 4d1ecefd-f385-4125-964f-8286276e15ed)
    (at 45.98 139.92 180)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/100c41f7-cf02-4b78-98a6-db06cc5ba264")
    (attr smd)
    (fp_text reference "FB1" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 994a0b94-e07b-43c2-b6f0-df42832b0306)
    )
    (fp_text value "1k/100MHz, ILBB0603ER102V" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 6e530789-b2b1-440b-80b2-98fd4a2293d3)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 4b5f09be-1b10-4374-b77b-d1d94193fd86)
    )
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer "B.SilkS") (width 0.12) (tstamp 8858c48a-8fbe-4332-a117-3fc927136158))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer "B.SilkS") (width 0.12) (tstamp f5502751-d91f-479b-b255-63e914f1043f))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 1a9a6307-8cb3-429a-bf7b-ef45d39168a4))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 42cda592-f41e-4a53-b7bc-9a1a96352ec4))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp abe903d6-f946-4ca1-8fb4-36df7245ec67))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp b7b99049-5165-401f-a190-d66720fcefc1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 16d567fb-626c-49d5-94e5-28fd162bca88))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp d7ab9f59-1fa2-4e01-9ff4-b7af966724ef))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp e3f3d6d9-4cf1-47be-bbf6-621f9514696a))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp ffb93eb7-2f89-431c-b1dc-62eb71e61617))
    (pad "1" smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp c169c252-4a18-404f-bb85-4e45526b5ebd))
    (pad "2" smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(C10-Pad1)") (pintype "passive") (tstamp fb30f8ba-c4e7-440d-9ba0-ecd7afdaa721))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 4e67c116-c710-44ef-aec1-fac3a78937fd)
    (at 88.96 124.51 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/a7e4c83d-2e2a-4884-9cc9-c0dadff5206a")
    (attr smd)
    (fp_text reference "C1" (at 0 1.16) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2eef7c4b-1d27-4e92-88a2-531e765eb7e0)
    )
    (fp_text value "100nF" (at 0 -1.16) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 46157b9c-be13-47f5-93e8-1cf79c472dbc)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
      (tstamp ee8b635b-6d41-4de1-99df-4ef5db127d52)
    )
    (fp_line (start -0.107836 -0.36) (end 0.107836 -0.36) (layer "B.SilkS") (width 0.12) (tstamp 02dff03a-f7c9-4675-91c1-2e955ec4714a))
    (fp_line (start -0.107836 0.36) (end 0.107836 0.36) (layer "B.SilkS") (width 0.12) (tstamp 983622b1-4773-40e8-ac36-a257cbd67873))
    (fp_line (start 0.91 -0.46) (end -0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 3ad2f333-55a7-4c13-b9cb-73970c108b0f))
    (fp_line (start -0.91 0.46) (end 0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp b9961134-5f10-40cf-9e9b-868e07781625))
    (fp_line (start 0.91 0.46) (end 0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp ccaeeb80-5fd3-4aab-8464-7df7076f30ac))
    (fp_line (start -0.91 -0.46) (end -0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp fa69e575-abfa-43e2-9610-c231da506d22))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 0c858c21-a1c4-41fc-b03e-95a7c4cbfa80))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 0d157f50-fe66-4c72-ac5b-ec5409cd32c2))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 3b90bf3c-2738-41e4-ab74-dd425eaae3ab))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp f5fe65a9-c0ab-4e9d-9f27-eb948c2ae389))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp 3ab2ee24-abd2-435f-b118-6b12bedfdac7))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp c5be0b92-13d7-4882-9edc-6f086268504b))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 560b91d7-8fff-4c42-b53d-2a72347b4061)
    (at 37.48 145.92 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/2147fc42-79ee-4a85-b8a6-66ccb58fff39")
    (attr smd)
    (fp_text reference "C14" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d535d415-79ed-4288-9d84-3f6b4318ac5f)
    )
    (fp_text value "4.7uF" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 6a89deeb-7e10-484b-aa39-e882673e420a)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 61cbb8a1-0760-44dd-9217-8e53291fc157)
    )
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp 21bdd760-9ab4-4017-8c0b-afc91a6d0739))
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp 30e75019-a659-4a7e-875c-e69f4d80f518))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 003d3ecb-6910-49eb-9d60-52090432b203))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 3ed09a44-e7c7-40d4-90bd-8970975856ee))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 7127f945-01fc-4efc-8406-62122ca9a1f1))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp f120e6d1-82c5-4a8a-8ef7-c83fe9a36179))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 0cc5c9e9-770e-40e2-85ce-69ab9e9fedea))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 5f369b18-0ec6-466c-ad97-a47ce15979f8))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 884e2a48-1a60-4500-a4f0-3384bf5803d2))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp e40015f8-5e96-4940-8faf-931cae3c1b2b))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp e722cc4d-8b51-4679-927a-dd66c03f292c))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp ca69d446-e2a9-4d88-8a4d-409ccb109d36))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 5650ddff-c5f0-498f-8aaf-7c8cb67bab37)
    (at 174.9 128.9)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/8ade4f9a-b824-4c00-b090-a166074fdf98")
    (attr smd)
    (fp_text reference "C23" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp fd0e1af4-a735-4a1d-ab69-5269829e1c28)
    )
    (fp_text value "1uF/50V" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp df0a50bb-485a-4c7d-8316-f9469aad0b3f)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp b589158a-d0cd-40de-b311-c481a50048e6)
    )
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp 06f2039c-ff4a-4491-9889-3f314ea69b33))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp 2dae44fd-f9ab-43fe-97f1-560a21ddb070))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 0d77fed2-991d-4696-9ff2-c6c8c4e04154))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 17c6b762-6ff9-4930-9ae6-e309880a3fa2))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 25dc9c04-9e80-42cb-8912-23d2e04a041f))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp a39ec1e1-f288-48da-8ea7-ce9d35766421))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 06c5c09e-4114-41c8-a4f2-634075099364))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 8d048212-d735-46f1-9d8b-5d89c534730f))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp af44dc8a-aecc-4bf8-aa32-f05c27efffa7))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp d0064468-dee3-4a1e-83bf-5c074b9ab9ef))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp ef3ef5bc-ecec-475d-88df-5ac96930f274))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(C23-Pad2)") (pintype "passive") (tstamp 9b56fbb6-f886-47e5-8a18-f0396e5baf5e))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 57ba07f7-23d5-44c4-89f1-03be3d7fffbf)
    (at 72.52 124.66 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/5c56e763-eeb5-455b-8c25-846e8ddcc102")
    (attr smd)
    (fp_text reference "R25" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5f6c1231-c9e7-46cb-b29e-0060e356637a)
    )
    (fp_text value "10k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4bf96d01-75ce-409b-b1cd-297ff35af05d)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 2975b14e-41eb-452f-b2e7-2e65f286456e)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 1b764483-9ae0-46f1-b2e0-cb97482d2f91))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 64d5b7e2-dc41-4ea8-91d3-1c06d3b7eaeb))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 0377f5d3-2d4d-4c01-a126-cd0289a47881))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 3eba88c5-52bf-4c0b-8e3c-8f2c2fcebd21))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 9457f249-306a-4c43-8719-bd6a13f61ea9))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp a2baec2c-d5a9-48ab-aa84-852ce6e24430))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 10e49206-22dd-40b4-a900-b88d107a4138))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 5b446841-7ee8-4f79-9657-10a1e4335eb6))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 8b8425d2-e87b-4929-b8d8-daa1c986f18c))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp b009bb50-d6b0-41cd-b93d-3c9261de2ea8))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "VBUS") (pintype "passive") (tstamp 2268dc69-c8e4-4694-aad0-5fea790ae04e))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp fde958ab-7fcc-47ec-9bad-9059ac694027))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 58b88994-723e-40d2-8fb9-98403b8c0975)
    (at 82.46 139.4 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/35ed39c6-cb9d-4b31-9a1b-4646e6c39a13")
    (attr smd)
    (fp_text reference "C28" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 92085fdd-fea5-4fd6-93e4-af1a67aea759)
    )
    (fp_text value "1uF/50V" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5885999e-87e0-498b-b073-cf90c8e0aeaa)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 378173bf-93e8-46ac-a3fe-7bebd677bd57)
    )
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp 5ef6c2b9-03e5-4637-a8fd-782a5a83a1fa))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp 6ff332bb-9ab0-4ca4-b373-76c39b6c5bb6))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 3ba3f4e5-69d2-43dd-a2f4-faf75243f7f2))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 3f676555-2cf2-4426-a2c3-6c7a0db3a662))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 46e68a54-0094-4c83-b3a8-46b09a544863))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp beed6871-cd7c-4000-a34f-118b2ffa8512))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp a1c742dd-07ad-424d-aae9-3b434c47794a))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp c62fe7f8-bffe-49c8-a56d-84fddcab1c2b))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp ed53de20-2b83-4633-a775-83a71ea4ee0b))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp f34518ae-93cd-4054-a422-e20b64ea7989))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 847ae362-8fb9-411d-9827-f6c59422fb5c))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "VDD") (pintype "passive") (tstamp 46bc8e2f-ac0f-4da1-9183-efb8659c6cb5))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 684fb381-e33c-450b-9a80-3f3f79f82b15)
    (at 62.27 111.3 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/6c6fb0a5-2807-42a3-bfcc-2ef023793f96")
    (attr smd)
    (fp_text reference "C4" (at 0 1.16) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d4e3a54f-0992-472f-8621-92781ce7ed6d)
    )
    (fp_text value "100nF" (at 0 -1.16) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 45f97375-a37e-4e2f-b80b-939efa51a81f)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
      (tstamp b70b2d94-e148-495a-80d9-1c059c36df51)
    )
    (fp_line (start -0.107836 0.36) (end 0.107836 0.36) (layer "B.SilkS") (width 0.12) (tstamp 712e5ace-a30f-487a-a185-0796f364566f))
    (fp_line (start -0.107836 -0.36) (end 0.107836 -0.36) (layer "B.SilkS") (width 0.12) (tstamp a9c26dc7-7ddb-4021-824d-30b18e0f604d))
    (fp_line (start -0.91 0.46) (end 0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 7ffe0ff6-19ce-415c-8d8d-5bb4d27c0961))
    (fp_line (start -0.91 -0.46) (end -0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 9970c24a-134f-48ee-ad8e-84f8fec74ee2))
    (fp_line (start 0.91 -0.46) (end -0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp b8bb9891-eb2d-4043-907c-a61560836213))
    (fp_line (start 0.91 0.46) (end 0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp d810e4dd-2052-4d4a-a828-8a42dff14833))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 15b6af81-8def-42fb-b174-981cba0d4d9a))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 2f8adfb7-2fe5-463c-b217-8c13e9757a86))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 96df8a23-1fe2-48d3-b8b4-f78b9d73b6df))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp af543cdc-a039-4d34-8e80-453d6dfb7626))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp 03c97026-d19a-4b58-8ea5-0b9b70b26339))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 03501c9f-8511-4bd0-bcc9-937842649bec))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-666" (layer "B.Cu")
    (tedit 5A02FF57) (tstamp 712f1fd6-029a-4525-8357-c07359d32f03)
    (at 195.4 147.2 -90)
    (descr "SOT666")
    (tags "SOT-666")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/977bde71-d79a-4262-9cc5-f31fae627590")
    (attr smd)
    (fp_text reference "U13" (at 0 1.75 -270) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 45d99599-3c2d-42a8-b0f8-e37470d726ff)
    )
    (fp_text value "USBLC6-2P6" (at 0 -1.75 -270) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 9a660cd2-2ef2-4a09-85b2-d5ad98c6de4c)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
      (tstamp f4571330-5106-4324-b234-eac6dcc29b72)
    )
    (fp_line (start -0.8 -0.9) (end 0.8 -0.9) (layer "B.SilkS") (width 0.12) (tstamp 39c1c1f5-71df-43bf-8c0b-1627587bb198))
    (fp_line (start 0.8 0.9) (end -1.1 0.9) (layer "B.SilkS") (width 0.12) (tstamp 46bdcdb3-2688-4f58-83f4-5e85992b6107))
    (fp_line (start -1.5 1.1) (end 1.5 1.1) (layer "B.CrtYd") (width 0.05) (tstamp 1677d044-bd63-48ff-b63b-b3feb2cebdc5))
    (fp_line (start -1.5 1.1) (end -1.5 -1.1) (layer "B.CrtYd") (width 0.05) (tstamp 427d398f-cb7f-437b-8c5e-2c8b667e8b8c))
    (fp_line (start 1.5 -1.1) (end 1.5 1.1) (layer "B.CrtYd") (width 0.05) (tstamp e34e48a9-d43e-4152-84f3-639fdb2a0569))
    (fp_line (start -1.5 -1.1) (end 1.5 -1.1) (layer "B.CrtYd") (width 0.05) (tstamp f3bc6ec1-440f-4235-ac85-9527c4d7b8fe))
    (fp_line (start 0.65 0.85) (end 0.65 -0.85) (layer "B.Fab") (width 0.1) (tstamp 202947b9-829e-4e83-8e97-6f7f967efc32))
    (fp_line (start 0.65 -0.85) (end -0.65 -0.85) (layer "B.Fab") (width 0.1) (tstamp 4914f67e-14f5-4bcf-9fc0-3a7fc5df2d1c))
    (fp_line (start -0.65 0.53) (end -0.33 0.85) (layer "B.Fab") (width 0.1) (tstamp bbc15ba6-9526-4c9e-886c-0b496b226dfd))
    (fp_line (start 0.65 0.85) (end -0.33 0.85) (layer "B.Fab") (width 0.1) (tstamp bced1dbc-0a69-4de6-85a1-1a4535d0c3e6))
    (fp_line (start -0.65 0.53) (end -0.65 -0.85) (layer "B.Fab") (width 0.1) (tstamp fab26335-5d26-4b23-836d-9f9f40818b33))
    (pad "1" smd rect (at -0.85 0.5375 270) (size 0.5 0.375) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 101 "/WiFi_Display/UART_TX") (pinfunction "I/O1") (pintype "passive") (tstamp a552f05e-f4fa-4331-8d0d-752b917d1742))
    (pad "2" smd rect (at -0.925 0 270) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive") (tstamp 8ef8d120-5af9-4314-ae99-6b1f7c0533e6))
    (pad "3" smd rect (at -0.85 -0.5375 270) (size 0.5 0.375) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 100 "/WiFi_Display/UART_RX") (pinfunction "I/O2") (pintype "passive") (tstamp 0ae43ca7-29d0-4e83-8e4e-9270453940fc))
    (pad "4" smd rect (at 0.85 -0.5375 270) (size 0.5 0.375) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 100 "/WiFi_Display/UART_RX") (pinfunction "I/O2") (pintype "passive") (tstamp 62101fdc-bd38-4430-8ede-f73287f451c5))
    (pad "5" smd rect (at 0.925 0 270) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "VBUS") (pinfunction "VBUS") (pintype "passive") (tstamp 56f08d1e-5db4-4282-b3c2-bb350253fde1))
    (pad "6" smd rect (at 0.85 0.5375 270) (size 0.5 0.375) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 101 "/WiFi_Display/UART_TX") (pinfunction "I/O1") (pintype "passive") (tstamp d668ab34-3c8e-4eb7-a5e7-d316c144ce7b))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-666.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 71ca6e8d-c1c6-4908-8bcc-cc05d65c76e7)
    (at 62.27 110.25 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/08a6c28a-e899-4622-bc28-0af06dccdee9")
    (attr smd)
    (fp_text reference "C7" (at 0 1.16) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 25360ba5-e32b-4cdb-933d-04e21f4bb1d9)
    )
    (fp_text value "10nF" (at 0 -1.16) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5851c52a-fba0-4500-9148-3ce5c2a4aef3)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
      (tstamp f85836b6-4782-42ec-8ad3-b52a43f8cc41)
    )
    (fp_line (start -0.107836 0.36) (end 0.107836 0.36) (layer "B.SilkS") (width 0.12) (tstamp 839abacf-dea3-494b-8026-3d2df30972a7))
    (fp_line (start -0.107836 -0.36) (end 0.107836 -0.36) (layer "B.SilkS") (width 0.12) (tstamp 896f9ccb-629a-4826-9943-0fd704921dd0))
    (fp_line (start 0.91 -0.46) (end -0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 02264127-ba56-421a-8871-e00b85c5e3cf))
    (fp_line (start -0.91 -0.46) (end -0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 5448c6a6-97a9-413c-b798-214141277b61))
    (fp_line (start -0.91 0.46) (end 0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 89e7f6f7-4f75-47ad-bf49-9da0f7692005))
    (fp_line (start 0.91 0.46) (end 0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp ef9f324c-70ff-4ec8-a527-760737a913b9))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 521e85da-da8f-4eb1-aff6-83ad369730af))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 7499d1d2-cc24-4f3c-8179-93710c423154))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 90240f78-9ae0-4f53-9a60-2074e695091c))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 971b9fba-4a75-405b-9b76-0b6f9a863bac))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp 84cf1403-408c-495e-9630-578f526ca15c))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp dc3168fd-3060-47ee-9c43-2c892df4bd4a))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 79eb008b-eb5c-4e26-93a2-6f5e1f9eb4fc)
    (at 174.9 118.4)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/b4770654-29c0-4fc2-8a72-b7b5e1e4d05a")
    (attr smd)
    (fp_text reference "C26" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0f2e3d82-7aa2-46df-8abc-7fa3ea4b9372)
    )
    (fp_text value "1uF/50V" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 926ebdce-e76c-4f7f-8a54-b345f5ff3927)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp a066fbb9-2e83-4439-8bc1-dc24f76b1294)
    )
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp d322dcb0-4b42-4fd1-86be-2478d332c9e1))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp ef8353fd-ef2e-4228-904c-d933425604dd))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 1efcbc3f-07ed-4ced-b535-cb78a798b5a9))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 80bbe12f-3695-4687-8ca2-94963df54481))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp cbbe1107-f3f7-45e7-a117-a707e40795ae))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp dcfd65f2-1ff8-45ec-bd9f-d3fa941f9e1b))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 25eb3656-9c65-4c12-bdab-4dfd45dee27f))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 4a75e7fb-5af5-429e-adf6-adf7c0aae4a8))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 9521df45-5bee-4b09-a2e3-5e9ea57fc33a))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp db0350ba-2e64-46cd-aeb6-50d299b4e91b))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 0aa95f6d-69d6-4c3d-9463-24537e3d1dd4))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 16 "/WiFi_Display/PREVGL") (pintype "passive") (tstamp c074c292-82f1-434d-92d7-99f37469dee0))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Button_Switch_SMD:Panasonic_EVQPUJ_EVQPUA" (layer "B.Cu")
    (tedit 5A02FC95) (tstamp 7c2a174f-35b6-4466-9b6a-e5a41813c832)
    (at 150.4 107.4 180)
    (descr "http://industrial.panasonic.com/cdbs/www-data/pdf/ATV0000/ATV0000CE5.pdf")
    (tags "SMD SMT SPST EVQPUJ EVQPUA")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/ad0ceda8-36a4-411d-8eb9-98e6845a3a17")
    (attr smd)
    (fp_text reference "SW1" (at 0 4.5) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp ab5c0926-48d9-4028-a4dc-6678d08e75af)
    )
    (fp_text value "EVQPUA02K" (at 0 -3.5) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4f0b6af4-b46e-4538-93d0-b7c5bb246083)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 8f717386-801b-48dc-82cd-f01b16584350)
    )
    (fp_line (start -2.45 -0.275) (end -2.45 0.275) (layer "B.SilkS") (width 0.12) (tstamp 03901ba5-96c2-4b22-ac48-ffa7763a5c94))
    (fp_line (start 2.45 -0.275) (end 2.45 0.275) (layer "B.SilkS") (width 0.12) (tstamp 2edb4960-2349-4b3d-bf55-2525f126a3f0))
    (fp_line (start 2.35 1.85) (end 1.425 1.85) (layer "B.SilkS") (width 0.12) (tstamp 3360c184-96a5-42a5-ba35-06618b3183e9))
    (fp_line (start 2.35 -1.85) (end -2.35 -1.85) (layer "B.SilkS") (width 0.12) (tstamp 4b60a8c8-b675-4d1d-bba3-92e0c459d8db))
    (fp_line (start -1.425 1.85) (end -2.35 1.85) (layer "B.SilkS") (width 0.12) (tstamp fc50ec4b-1f70-4d26-a8fd-2c58fbaba624))
    (fp_line (start 3.9 -2.25) (end -3.9 -2.25) (layer "B.CrtYd") (width 0.05) (tstamp 496c7c28-d9b7-43a2-9ab9-36dc0fdd7e00))
    (fp_line (start 3.9 -2.25) (end 3.9 3.25) (layer "B.CrtYd") (width 0.05) (tstamp 78a09d7d-7649-4d53-b555-f983a9a04f26))
    (fp_line (start -3.9 -2.25) (end -3.9 3.25) (layer "B.CrtYd") (width 0.05) (tstamp a9e45979-9029-41e0-b160-b709cad16e12))
    (fp_line (start 3.9 3.25) (end -3.9 3.25) (layer "B.CrtYd") (width 0.05) (tstamp f9af92dc-4bb1-47ae-a043-9d475a55ad5c))
    (fp_line (start 1.3 2.75) (end 1.3 1.75) (layer "B.Fab") (width 0.1) (tstamp 28d3166b-77b9-4ed3-8c67-e00b3e944b58))
    (fp_line (start 2.35 1.75) (end -2.35 1.75) (layer "B.Fab") (width 0.1) (tstamp 49aadf9a-fd81-4ab8-ace2-5ffb9da1ff01))
    (fp_line (start 1.3 2.75) (end -1.3 2.75) (layer "B.Fab") (width 0.1) (tstamp 5679d703-bf0d-4861-9fe9-28e2f857f62b))
    (fp_line (start 2.35 -1.75) (end 2.35 1.75) (layer "B.Fab") (width 0.1) (tstamp a70fafd5-3b5f-40be-a312-4e83d56d88bf))
    (fp_line (start 2.35 -1.75) (end -2.35 -1.75) (layer "B.Fab") (width 0.1) (tstamp b6105d0d-98d6-4b97-a2c8-d41e79693943))
    (fp_line (start -2.35 -1.75) (end -2.35 1.75) (layer "B.Fab") (width 0.1) (tstamp f7db98b9-1847-4d73-a874-96785b53cc78))
    (fp_line (start -1.3 2.75) (end -1.3 1.75) (layer "B.Fab") (width 0.1) (tstamp faf30b43-b2c3-4368-b67f-185783587590))
    (pad "1" smd rect (at 2.625 0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive") (tstamp b0939504-a2db-435a-bcc8-d6290025c73f))
    (pad "1" smd rect (at -2.625 0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive") (tstamp eda9caa4-66ac-4d86-a8a6-dcbfc9fe5903))
    (pad "2" smd rect (at 2.625 -0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "/Sensor_Controller/LPC_~{ISP}") (pinfunction "2") (pintype "passive") (tstamp 289727e8-1973-4f9c-9913-e8f2b620742c))
    (pad "2" smd rect (at -2.625 -0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "/Sensor_Controller/LPC_~{ISP}") (pinfunction "2") (pintype "passive") (tstamp 8314b4f5-250f-49e2-8a13-33d624c278c0))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/Panasonic_EVQPUJ_EVQPUA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Inductor_SMD:L_1210_3225Metric" (layer "B.Cu")
    (tedit 5F68FEF0) (tstamp 7d1fc2c2-7dac-402b-add3-fcd0eb27863a)
    (at 153.3 119.4 180)
    (descr "Inductor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/7a1f2c6b-9ca1-4af3-bf3c-5c9c2c2e3f32")
    (attr smd)
    (fp_text reference "L2" (at 0 2.28) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f96a6449-1179-4aab-bbd1-d29f43b19c20)
    )
    (fp_text value "2.2uH/1.5A, BRL3225T2R2M" (at 0 -2.28) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 169d5d1f-bb77-43e9-a4f7-7917ae665f8e)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.8 0.8) (thickness 0.12)) (justify mirror))
      (tstamp 77a7a142-bcdf-474d-b0a5-acc637b6f07a)
    )
    (fp_line (start -0.602064 1.36) (end 0.602064 1.36) (layer "B.SilkS") (width 0.12) (tstamp 06f35939-7af4-4739-9b87-69128d88932a))
    (fp_line (start -0.602064 -1.36) (end 0.602064 -1.36) (layer "B.SilkS") (width 0.12) (tstamp 418bb36c-4f60-4a3d-945a-e88bdbf30f81))
    (fp_line (start -2.28 1.58) (end 2.28 1.58) (layer "B.CrtYd") (width 0.05) (tstamp 3089e5ea-f3aa-4061-b626-7e16d2662243))
    (fp_line (start -2.28 -1.58) (end -2.28 1.58) (layer "B.CrtYd") (width 0.05) (tstamp 57551be9-437f-452c-9777-686b1051752d))
    (fp_line (start 2.28 1.58) (end 2.28 -1.58) (layer "B.CrtYd") (width 0.05) (tstamp 623cab55-76dd-41eb-8054-d9fb7c9b477d))
    (fp_line (start 2.28 -1.58) (end -2.28 -1.58) (layer "B.CrtYd") (width 0.05) (tstamp e50c6ed6-22ab-47b0-8848-9f971b8a41b4))
    (fp_line (start 1.6 -1.25) (end -1.6 -1.25) (layer "B.Fab") (width 0.1) (tstamp 4e495535-73a5-4f8b-b361-23597d9a85db))
    (fp_line (start -1.6 -1.25) (end -1.6 1.25) (layer "B.Fab") (width 0.1) (tstamp 50b92fcd-0a06-48c1-b706-197e62dc24a5))
    (fp_line (start 1.6 1.25) (end 1.6 -1.25) (layer "B.Fab") (width 0.1) (tstamp 565170d4-e506-4550-a149-0bdbcc9dc88a))
    (fp_line (start -1.6 1.25) (end 1.6 1.25) (layer "B.Fab") (width 0.1) (tstamp 8f719a75-21cd-4f20-8236-1fa4c5e41f81))
    (pad "1" smd roundrect (at -1.4 0 180) (size 1.25 2.65) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 85 "Net-(L2-Pad1)") (pinfunction "1") (pintype "passive") (tstamp 7b578300-4474-46d2-b8de-88f7e4013340))
    (pad "2" smd roundrect (at 1.4 0 180) (size 1.25 2.65) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 9 "VDD") (pinfunction "2") (pintype "passive") (tstamp bc359569-2635-4498-a0e3-6d841f11b36e))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 7d68677c-5326-4665-a3c5-ae55f8c3bb66)
    (at 91.85 124.52 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/61e7f132-cec4-465b-aa57-86a109c5fe88")
    (attr smd)
    (fp_text reference "R3" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp bb350d53-f544-4f52-8e80-331a4d5f04aa)
    )
    (fp_text value "4k7" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 104b597b-4c43-4d47-8047-8a9b894da72e)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 754de932-970d-4847-ac83-f53dcf776cd2)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 33b43a2a-a5b2-4373-a0d6-19c05353209b))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 8e1dab39-df24-4681-890a-90a07f64259b))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 30a20e78-660d-4d6c-940c-9a783bd93c14))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 5de11ea8-2c1c-45f8-a53f-6f3feb433c0a))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 6791244d-40dc-4651-8880-8434053d17ba))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp f7a86f33-ee9e-48c0-a13c-0247dda4b98a))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 40ab2bf6-e76b-4f72-8007-cfb0eb36074f))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 7e30cfef-c526-46f8-9e80-1504afec1279))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp a37f1a71-d18d-443e-ba6a-278f2a4d1d6c))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp b7ad052e-9347-4728-8118-26d475bac57f))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp eaeda4e1-1b24-43c1-84b5-c312f9145342))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 42 "/Sensor_Controller/I2C_SCL") (pintype "passive") (tstamp 2c8a36e7-ca8b-45df-b76d-59de0b4e92da))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 7f9e53a4-b637-4449-8e34-b620debdb296)
    (at 86.09 124.51 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/d8468354-a2cc-4351-aa35-2e7bdee71071")
    (attr smd)
    (fp_text reference "C2" (at 0 1.16) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 04a1d56f-f939-4adb-ad80-d98fe6818e0c)
    )
    (fp_text value "100nF" (at 0 -1.16) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 92d4e39a-9db1-43b8-bdba-bdddc46963a5)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
      (tstamp 5001a481-bc3a-413f-acb7-9066a37098a9)
    )
    (fp_line (start -0.107836 -0.36) (end 0.107836 -0.36) (layer "B.SilkS") (width 0.12) (tstamp 93ae75bc-4328-4262-92e1-b5f6f1d4d255))
    (fp_line (start -0.107836 0.36) (end 0.107836 0.36) (layer "B.SilkS") (width 0.12) (tstamp ef0013d5-019e-4994-997d-469e8d298944))
    (fp_line (start 0.91 0.46) (end 0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 0ab0584a-1e00-417a-b0de-ae29f77273fd))
    (fp_line (start -0.91 0.46) (end 0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 197eb725-36cf-4295-b288-5d3d3e7ce5c8))
    (fp_line (start -0.91 -0.46) (end -0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 5848a774-adae-4bea-86a8-725647c734e8))
    (fp_line (start 0.91 -0.46) (end -0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp d0eb86b9-8c95-46cd-899e-69af84c7f11e))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 514ed829-4035-4325-8137-4ec90c9dd886))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 6b1a05b3-9634-4da3-8f94-365e2da6e703))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 7eef0b40-0096-4af8-886c-bd74ff80b00b))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp a9791ffc-8b0a-494f-9ef2-a1971fd8041b))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp 957f9e53-5ec3-459f-a470-3f0806b58ee8))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp ae342d38-bb03-4ffe-9632-3fecd496522e))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958) (tstamp 830f235c-cfb1-48de-9ca8-e2c2d9955dd9)
    (at 169.4 126.2 180)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/f27783ed-9efe-4703-8c28-0816eaad2c35")
    (attr smd)
    (fp_text reference "Q2" (at 0 2.4) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e42fe7d2-af11-4777-ad13-86bbab1ae9d9)
    )
    (fp_text value "SI1308EDL" (at 0 -2.4) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5421654f-13fd-4b21-a4fe-82869dc9ae54)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.32 0.32) (thickness 0.05)) (justify mirror))
      (tstamp 90771145-6a42-46db-9d25-7b17c27f80dd)
    )
    (fp_line (start 0 -1.56) (end -0.65 -1.56) (layer "B.SilkS") (width 0.12) (tstamp 4c610214-837a-417f-bb83-d760295b6f63))
    (fp_line (start 0 1.56) (end -1.675 1.56) (layer "B.SilkS") (width 0.12) (tstamp 4e189d1c-afb9-453c-976d-15248061a901))
    (fp_line (start 0 -1.56) (end 0.65 -1.56) (layer "B.SilkS") (width 0.12) (tstamp 50202cff-99ad-4375-b0d6-483aa7cee68b))
    (fp_line (start 0 1.56) (end 0.65 1.56) (layer "B.SilkS") (width 0.12) (tstamp 9d537d4c-a0c9-48ae-a8e5-f5ad53d64d86))
    (fp_line (start -1.92 1.7) (end -1.92 -1.7) (layer "B.CrtYd") (width 0.05) (tstamp 28da967a-58a0-442b-84c5-0c6bfe34dadf))
    (fp_line (start 1.92 1.7) (end -1.92 1.7) (layer "B.CrtYd") (width 0.05) (tstamp 64d09917-0a09-4334-8b14-0dcee4e3ac5e))
    (fp_line (start -1.92 -1.7) (end 1.92 -1.7) (layer "B.CrtYd") (width 0.05) (tstamp b6943e55-e8ed-41ca-948c-e9a4e160e91c))
    (fp_line (start 1.92 -1.7) (end 1.92 1.7) (layer "B.CrtYd") (width 0.05) (tstamp f7061b02-7da1-43e2-9593-b59a02f500a8))
    (fp_line (start 0.65 -1.45) (end -0.65 -1.45) (layer "B.Fab") (width 0.1) (tstamp 29fc5c75-e0f8-4d66-8b30-f1c5ebc0b2ec))
    (fp_line (start -0.325 1.45) (end 0.65 1.45) (layer "B.Fab") (width 0.1) (tstamp 6fa88215-bc1e-4d23-81c4-513e10d5aff5))
    (fp_line (start -0.65 -1.45) (end -0.65 1.125) (layer "B.Fab") (width 0.1) (tstamp a09326a6-f91e-4ff5-a7d5-fd6fd37ba303))
    (fp_line (start 0.65 1.45) (end 0.65 -1.45) (layer "B.Fab") (width 0.1) (tstamp d61e88ee-d8cd-4834-88f9-4274b691c3b5))
    (fp_line (start -0.65 1.125) (end -0.325 1.45) (layer "B.Fab") (width 0.1) (tstamp fe297dd7-73d4-401e-9102-3ef3240fb7da))
    (pad "1" smd roundrect (at -0.9375 0.95 180) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 30 "/WiFi_Display/GDR") (pinfunction "G") (pintype "input") (tstamp 13e13a6f-8ea6-47eb-8887-a32e627143fe))
    (pad "2" smd roundrect (at -0.9375 -0.95 180) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "/WiFi_Display/RESE") (pinfunction "S") (pintype "passive") (tstamp 0428e785-a8cc-4d06-9956-bcbeae17a743))
    (pad "3" smd roundrect (at 0.9375 0 180) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(C22-Pad2)") (pinfunction "D") (pintype "passive") (tstamp 0f481208-5023-4d75-b0f6-4619745df4aa))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 85db620f-0936-4015-b90f-7d195f73fece)
    (at 174.9 122.9)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/e62f2693-a028-431a-b2ab-4c5c401d17d0")
    (attr smd)
    (fp_text reference "C30" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4792c1ca-0755-4b46-82ac-8d2ce775705e)
    )
    (fp_text value "1uF/50V" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 653f71b2-30db-4798-a6a5-045ec65e1df5)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 534952b5-7fe3-4f62-bbea-5f9fd03a667c)
    )
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp 0952cd5d-15ac-4949-bf38-1e696debfa44))
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp 1d8db80b-b6ce-4eba-9498-dea9fe1fbf70))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 3d69bc7f-ae72-4fe9-94d7-d899f178bbfe))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 40c2d070-79bc-4fb9-9279-17c2f680f04e))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp bb6f2087-e894-4513-ad02-35ed08998bbc))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp c950d5d2-5e3c-4ab8-a4f4-56f6551c9558))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 90ba32c5-6410-4512-93ae-38b161bf6d3f))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp b1556e2c-c69e-49d6-8987-f213324313a2))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp ca30d885-c63d-44d5-8ad7-69844ae0dad8))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp e7ea066d-360d-483d-b7a8-9925a9671d45))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp d71eaf8d-17ed-4706-8f9c-eabb30363291))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(C30-Pad2)") (pintype "passive") (tstamp 3a55e3ee-ef19-45c7-81c3-0881f5d8530f))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "ESP32_Module:ESP32-C3-MINI-1" (layer "B.Cu")
    (tedit 0) (tstamp 87501285-62ab-4d19-824d-19f4277b0e70)
    (at 123.35 112.75 -90)
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/e999ee1a-2a83-42f5-928b-d28b8b805ac0")
    (attr smd)
    (fp_text reference "U12" (at -0.6 -7.1 -270 unlocked) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f06d5c4b-6886-4b63-b297-12250c38456e)
    )
    (fp_text value "ESP32-C3-Mini-1" (at 0 -1 -270 unlocked) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp bfde603e-e316-4731-93ed-07571bfb220c)
    )
    (fp_text user "${REF}" (at 0 -2.5 -270 unlocked) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e0b82b99-49b4-4f92-be3e-83d42cafb0d3)
    )
    (fp_line (start -6.6 5.6) (end -6.6 11) (layer "Dwgs.User") (width 0.1) (tstamp 42f7b6c7-b235-4337-af7c-74a950153d03))
    (fp_line (start -6.6 5.6) (end -6.6 -5.6) (layer "Dwgs.User") (width 0.1) (tstamp 53fd91bd-c64d-4af5-8350-fd0232b9315f))
    (fp_line (start 6.6 -5.6) (end 6.6 5.6) (layer "Dwgs.User") (width 0.1) (tstamp 7104a1ed-94c3-4cd8-a7bf-228f031c1d2d))
    (fp_line (start -6.6 -5.6) (end 6.6 -5.6) (layer "Dwgs.User") (width 0.1) (tstamp 715d3dbc-acd2-4756-85b0-44e1979db720))
    (fp_line (start 6.6 5.6) (end 6.6 11) (layer "Dwgs.User") (width 0.1) (tstamp 89e358c3-65bf-4f17-9044-becd3e4200e0))
    (fp_line (start 6.6 11) (end -6.6 11) (layer "Dwgs.User") (width 0.1) (tstamp a1c3590e-f145-4e7d-a255-70826f537ba1))
    (fp_line (start 6.6 5.6) (end -6.6 5.6) (layer "Dwgs.User") (width 0.1) (tstamp b797daa2-1186-4972-a823-94bc01d0ed38))
    (fp_line (start 6.6 11) (end -6.6 5.6) (layer "Dwgs.User") (width 0.1) (tstamp eb8730c1-84b9-4db0-abd4-ff9192c86b40))
    (pad "1" smd rect (at -5.9 4 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp cff1aad7-9b56-41b4-a3d5-13bbdf87b093))
    (pad "2" smd rect (at -5.9 3.2 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp fd516020-4377-4ff7-8c31-cb221bf5be6e))
    (pad "3" smd rect (at -5.9 2.4 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "VDD") (pinfunction "3V3") (pintype "power_in") (tstamp 96710aae-5380-4c5e-806e-f6019b40f3ee))
    (pad "4" smd rect (at -5.9 1.6 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 88 "unconnected-(U12-Pad4)") (pinfunction "NC") (pintype "no_connect") (tstamp 508710d6-b6f2-4918-bf27-5ccc2137b129))
    (pad "5" smd rect (at -5.9 0.8 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "/WiFi_Display/EPD_~{RES}") (pinfunction "IO2") (pintype "tri_state") (tstamp e3e034b3-276e-4c5e-b331-101621d904ee))
    (pad "6" smd rect (at -5.9 0 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 34 "/WiFi_Display/EPD_BUSY") (pinfunction "IO3") (pintype "tri_state") (tstamp 48eedbce-e092-4fa6-8c3c-8f6659b97f7d))
    (pad "7" smd rect (at -5.9 -0.8 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 89 "unconnected-(U12-Pad7)") (pinfunction "NC") (pintype "no_connect") (tstamp d393fe7b-421c-4973-952b-3e70a10d8aef))
    (pad "8" smd rect (at -5.9 -1.6 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 10 "Net-(C20-Pad1)") (pinfunction "EN") (pintype "input") (tstamp 764e8695-9cc5-495f-a278-c2225ea409f9))
    (pad "9" smd rect (at -5.9 -2.4 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 90 "unconnected-(U12-Pad9)") (pinfunction "NC") (pintype "no_connect") (tstamp 27beecaf-994e-49e0-8ff5-0797cd15bd39))
    (pad "10" smd rect (at -5.9 -3.2 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 91 "unconnected-(U12-Pad10)") (pinfunction "NC") (pintype "no_connect") (tstamp 94d9d8b4-042c-4ec1-a1ed-03e7eac8aa86))
    (pad "11" smd rect (at -5.9 -4 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp cb787e48-f293-4926-8cae-1d82f20e2004))
    (pad "12" smd rect (at -4.8 -4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 92 "unconnected-(U12-Pad12)") (pinfunction "IO0") (pintype "tri_state+no_connect") (tstamp 5d312589-0b24-41d1-afd5-af4498214dfd))
    (pad "13" smd rect (at -4 -4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 81 "/Sensor_Controller/SPI_~{INT}") (pinfunction "IO1") (pintype "tri_state") (tstamp 7aa827bf-0c69-45f9-86a0-c35929d3c6e1))
    (pad "14" smd rect (at -3.2 -4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp cea6f4eb-9ef5-451b-9c34-3b486f663a40))
    (pad "15" smd rect (at -2.4 -4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 93 "unconnected-(U12-Pad15)") (pinfunction "NC") (pintype "no_connect") (tstamp fbc434da-e162-4193-866e-adb61a0152f7))
    (pad "16" smd rect (at -1.6 -4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "/WiFi_Display/EPD_CS") (pinfunction "IO10") (pintype "tri_state") (tstamp 98ff7360-2f4d-41c4-b31d-fd299a99a037))
    (pad "17" smd rect (at -0.8 -4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 94 "unconnected-(U12-Pad17)") (pinfunction "NC") (pintype "no_connect") (tstamp f862175f-c138-49a5-a077-434074a19537))
    (pad "18" smd rect (at 0 -4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 38 "/WiFi_Display/EPD_SCLK") (pinfunction "IO4") (pintype "tri_state") (tstamp 02aef84a-a630-45d5-ac32-46c2d8753034))
    (pad "19" smd rect (at 0.8 -4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "/WiFi_Display/EPD_SDI") (pinfunction "IO5") (pintype "tri_state") (tstamp f6d6fde4-2ff3-423c-9880-d66b104212d5))
    (pad "20" smd rect (at 1.6 -4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 82 "/Sensor_Controller/SPI_MISO") (pinfunction "IO6") (pintype "tri_state") (tstamp f7a1d5fe-496c-4090-b078-b43b41e23dd0))
    (pad "21" smd rect (at 2.4 -4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 72 "/Sensor_Controller/SPI_CS") (pinfunction "IO7") (pintype "tri_state") (tstamp 8dd047ad-0c2c-4787-8f00-93f8e4a7591a))
    (pad "22" smd rect (at 3.2 -4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "/WiFi_Display/EPD_D{slash}~{C}") (pinfunction "IO8") (pintype "tri_state") (tstamp 513dec86-c952-4f8c-9e27-134ee70d3650))
    (pad "23" smd rect (at 4 -4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 95 "Net-(SW3-Pad2)") (pinfunction "IO9") (pintype "tri_state") (tstamp 4d8a535c-260c-4b8c-ac66-a8d204437ce1))
    (pad "24" smd rect (at 4.8 -4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 96 "unconnected-(U12-Pad24)") (pinfunction "NC") (pintype "no_connect") (tstamp 59a69132-8d5f-493e-9b7c-7d0b26c4d017))
    (pad "25" smd rect (at 5.9 -4 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 97 "unconnected-(U12-Pad25)") (pinfunction "NC") (pintype "no_connect") (tstamp 1dbc434a-9b34-4dab-bab5-3d1156eb2ae7))
    (pad "26" smd rect (at 5.9 -3.2 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 87 "/WiFi_Display/USB_D-") (pinfunction "IO18") (pintype "tri_state") (tstamp 3d2ddbd6-4364-4a4c-9060-079e7dc84a2d))
    (pad "27" smd rect (at 5.9 -2.4 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 86 "/WiFi_Display/USB_D+") (pinfunction "IO19") (pintype "tri_state") (tstamp ea17eaf1-4c6e-40c4-aac7-2dedd1365fca))
    (pad "28" smd rect (at 5.9 -1.6 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 98 "unconnected-(U12-Pad28)") (pinfunction "NC") (pintype "no_connect") (tstamp bbb1703b-483e-4697-b0dd-3bbab52b9173))
    (pad "29" smd rect (at 5.9 -0.8 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 99 "unconnected-(U12-Pad29)") (pinfunction "NC") (pintype "no_connect") (tstamp cd8d9d25-4747-47c1-83dc-ecf2558614d8))
    (pad "30" smd rect (at 5.9 0 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 100 "/WiFi_Display/UART_RX") (pinfunction "RXD0") (pintype "tri_state") (tstamp f4be51d4-436f-49ed-9b4f-eb06a1daec0a))
    (pad "31" smd rect (at 5.9 0.8 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 101 "/WiFi_Display/UART_TX") (pinfunction "TXD0") (pintype "tri_state") (tstamp 5dd662d0-c581-44d0-b1c3-3ae5f9d21dde))
    (pad "32" smd rect (at 5.9 1.6 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 102 "unconnected-(U12-Pad32)") (pinfunction "NC") (pintype "no_connect") (tstamp 8e0eab20-0b37-44db-97b4-4d7bc90b1317))
    (pad "33" smd rect (at 5.9 2.4 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 103 "unconnected-(U12-Pad33)") (pinfunction "NC") (pintype "no_connect") (tstamp 2adac89d-cb68-4fb8-bb8b-33707b4bf7df))
    (pad "34" smd rect (at 5.9 3.2 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 104 "unconnected-(U12-Pad34)") (pinfunction "NC") (pintype "no_connect") (tstamp d5ba88f5-7f66-4943-a441-270774ad8ea9))
    (pad "35" smd rect (at 5.9 4 270) (size 0.8 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 105 "unconnected-(U12-Pad35)") (pinfunction "NC") (pintype "no_connect") (tstamp 4b940b5f-7b55-4c3f-bb48-e667b9cf8167))
    (pad "36" smd rect (at 4.8 4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp de973b81-adc5-4b39-a916-24f1b29bce2a))
    (pad "37" smd rect (at 4 4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 0cd886c8-2e62-41ec-b5f3-578e4fd5ffa7))
    (pad "38" smd rect (at 3.2 4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 87d21be9-e7b0-4bf9-a1b5-908eaf5777e0))
    (pad "39" smd rect (at 2.4 4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 03ed6c31-0861-46fd-90a2-705234bbf253))
    (pad "40" smd rect (at 1.6 4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp e2b605ab-2011-4f89-8272-e6d305b0ec53))
    (pad "41" smd rect (at 0.8 4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 4c924c44-3d4b-47a5-980a-7ab67b98dbc0))
    (pad "42" smd rect (at 0 4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 4c324237-9628-4b30-813f-9cb4039ada68))
    (pad "43" smd rect (at -0.8 4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 4d0743d9-e7b7-4d2d-9177-c39dd3566d11))
    (pad "44" smd rect (at -1.6 4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp d750b942-fee5-4f56-95e1-467c5ceab102))
    (pad "45" smd rect (at -2.4 4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp acaefc5e-cb01-424f-b6a2-416fadcbd8fd))
    (pad "46" smd rect (at -3.2 4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp d1c38329-8ca7-4745-b868-2402d8c46714))
    (pad "47" smd rect (at -4 4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 3f367c8b-e437-4a39-9372-8fad6af54d41))
    (pad "48" smd rect (at -4.8 4.9 270) (size 0.4 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp a83b5140-b738-49cc-bed4-d31417856f01))
    (pad "49" smd rect (at 0 1.975 270) (size 1.45 1.45) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 03911903-1c44-453e-83c1-3a8035c53a9b))
    (pad "49" smd rect (at 0 0 270) (size 1.45 1.45) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 26ad627a-4bb6-4def-857e-4b27333165a5))
    (pad "49" smd rect (at 1.975 1.975 180) (size 1.45 1.45) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 60ded7ac-3b08-4300-9936-2226080e45d9))
    (pad "49" smd rect (at 1.975 0 270) (size 1.45 1.45) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 7ea3d4c3-02a3-4f07-a556-c56a2615ef6e))
    (pad "49" smd rect (at -1.975 0 270) (size 1.45 1.45) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp aa1be952-04dd-447c-964c-b473bf3b5624))
    (pad "49" smd rect (at 1.975 -1.975 270) (size 1.45 1.45) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp b30fa555-136e-491c-bb09-810eb99acab6))
    (pad "49" smd rect (at -1.975 -1.975 270) (size 1.45 1.45) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp d5ea7269-4356-4671-994f-e2088f3ba2d8))
    (pad "49" smd roundrect (at -1.975 1.975 270) (size 1.45 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0)
      (chamfer_ratio 0.414) (chamfer bottom_left)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp d72e4bda-11c3-4e24-874c-0753a1fbb00e))
    (pad "49" smd rect (at 0 -1.975 270) (size 1.45 1.45) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp ddcde53d-9e57-49be-b17b-486eb68b5c8c))
    (pad "50" smd rect (at 5.95 4.95 270) (size 0.7 0.7) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 758f0efc-f8e3-4260-95ae-7a4c698684be))
    (pad "51" smd rect (at 5.95 -4.95 270) (size 0.7 0.7) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 5c34a94c-95f9-4f34-8896-9eefe7fb8c63))
    (pad "52" smd rect (at -5.95 -4.95 270) (size 0.7 0.7) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 1ed5f7e4-5c01-4e23-8be1-eaf328a84f94))
    (pad "53" smd rect (at -5.95 4.95 270) (size 0.7 0.7) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp f24c1f0d-0d72-4597-b045-71b218b3580c))
    (zone (net 0) (net_name "") (layers *.Cu "Dwgs.User") (tstamp dacb4ece-0a8f-4336-921c-254aaafb81ff) (hatch edge 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 117.75 119.35)
          (xy 117.75 106.15)
          (xy 112.35 106.15)
          (xy 112.35 119.35)
        )
      )
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 875f318c-ca2b-41d9-8455-86aa24bccdd8)
    (at 42.705 145.92 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/07ce96f0-ebcf-4468-9381-7d40b1b2a8d8")
    (attr smd)
    (fp_text reference "C15" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 59b87915-8700-4b78-82bb-93aa220310a0)
    )
    (fp_text value "4.7uF" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 830822dc-6c19-4aee-bbed-b42bd882f9df)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 60cc7178-87b8-4b14-ac75-02656e898c92)
    )
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp 345e650e-cab7-4f7c-8e23-a05d24685517))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp e790bb4f-9dff-4404-b663-07e29edeaeed))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 704c6497-67dc-4a16-9bcf-2962ec77d988))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp b76e5a12-e08f-4e98-8857-f987e760b41f))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp cef9d15e-689d-43e1-93d6-5b82b944a2c8))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp e04b0306-e349-4290-a4f4-969de632f7a7))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 9644d594-a1ff-48ac-8e51-3a42885e90ca))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp aa26397f-2c61-4c36-b526-44883c3a246c))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp cfb41a97-08cc-4b99-8529-6dc1b8d2d38e))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp ed0ba555-e6e4-43f1-8a65-2507c46d0243))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "VCC") (pintype "passive") (tstamp e8f2a94c-6ae6-48b5-84e1-f3f736a72d58))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 7a46462b-3f17-4fbd-a4b7-2b7ff0c165f3))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Inductor_SMD:L_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEF0) (tstamp 8ac28aef-b21c-4cbf-9b32-e308d2b47121)
    (at 166.5 126.2 90)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/d75d19d3-5b46-4b22-ae5d-4fe9be559e81")
    (attr smd)
    (fp_text reference "L3" (at 0 1.55 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 1a01a243-0538-4f32-bc4f-6e6d3a2b29b9)
    )
    (fp_text value "10uH, MLZ2012M100WTD25" (at 0 -1.55 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 38f6482f-0aaf-45ed-bc0f-e38c1774af8a)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp a3eecc3b-9693-4fba-9c8d-88827e35f56f)
    )
    (fp_line (start -0.399622 -0.56) (end 0.399622 -0.56) (layer "B.SilkS") (width 0.12) (tstamp 416cae2b-8f64-4020-a72c-29a7c6c6528f))
    (fp_line (start -0.399622 0.56) (end 0.399622 0.56) (layer "B.SilkS") (width 0.12) (tstamp c0583c07-405c-4673-b60d-8bafe03ee917))
    (fp_line (start 1.75 0.85) (end 1.75 -0.85) (layer "B.CrtYd") (width 0.05) (tstamp 234e5200-8ac4-4b3d-8553-93e8ec0a472b))
    (fp_line (start -1.75 0.85) (end 1.75 0.85) (layer "B.CrtYd") (width 0.05) (tstamp 84d568ff-21bb-4778-9ad5-ae603a21efca))
    (fp_line (start 1.75 -0.85) (end -1.75 -0.85) (layer "B.CrtYd") (width 0.05) (tstamp d6487cd5-1215-4561-a252-63a73f4469be))
    (fp_line (start -1.75 -0.85) (end -1.75 0.85) (layer "B.CrtYd") (width 0.05) (tstamp ffb3fcb7-37e2-46e1-bc6d-7fc06cf10451))
    (fp_line (start 1 0.45) (end 1 -0.45) (layer "B.Fab") (width 0.1) (tstamp 09222965-8dc7-4477-a769-e10b1a478704))
    (fp_line (start 1 -0.45) (end -1 -0.45) (layer "B.Fab") (width 0.1) (tstamp 0e2f7410-b777-4e95-bcc1-acb2df40bd76))
    (fp_line (start -1 0.45) (end 1 0.45) (layer "B.Fab") (width 0.1) (tstamp aa5166b2-88d1-4b0e-ad7d-f929d9e5acd3))
    (fp_line (start -1 -0.45) (end -1 0.45) (layer "B.Fab") (width 0.1) (tstamp c1e4c5ac-392a-4b2d-abac-8233bd6a10d0))
    (pad "1" smd roundrect (at -1.0625 0 90) (size 0.875 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "VDD") (pinfunction "1") (pintype "passive") (tstamp 41bfc507-4059-4be2-b39d-db68af57f2a9))
    (pad "2" smd roundrect (at 1.0625 0 90) (size 0.875 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(C22-Pad2)") (pinfunction "2") (pintype "passive") (tstamp 43b6599b-674e-4d0e-a909-f946dcb4e152))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_DFN_QFN:VQFN-32-1EP_5x5mm_P0.5mm_EP3.5x3.5mm_ThermalVias" (layer "B.Cu")
    (tedit 5DC5F6A8) (tstamp 8d4e399c-f677-4283-8935-ce15932c7076)
    (at 154.525 138.125 180)
    (descr "VQFN, 32 Pin (https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT4222H.pdf#page=40), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "VQFN NoLead")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/b5f834de-c7bf-4a4a-886f-7479a73ef33d")
    (attr smd)
    (fp_text reference "U5" (at 0 3.8) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 81b58340-3615-446f-bd2d-e2c9fb45f689)
    )
    (fp_text value "LPC804M101JHI33" (at 0 -3.8) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 1ea0601f-2b25-4c9c-9727-a0536b027d3c)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d78289a0-123a-4021-b5d0-b19f9bd4ec89)
    )
    (fp_line (start 2.61 -2.61) (end 2.61 -2.135) (layer "B.SilkS") (width 0.12) (tstamp 0a86c5b4-cab0-4951-9a04-8b3644547237))
    (fp_line (start 2.135 2.61) (end 2.61 2.61) (layer "B.SilkS") (width 0.12) (tstamp 36b371dc-6f64-47c0-bcd0-ba4657bcf187))
    (fp_line (start -2.61 -2.61) (end -2.61 -2.135) (layer "B.SilkS") (width 0.12) (tstamp 4034aff1-5049-48ca-b36a-e7cb54d38628))
    (fp_line (start 2.61 2.61) (end 2.61 2.135) (layer "B.SilkS") (width 0.12) (tstamp 9562f308-7d98-4081-b2e9-7acd2e53edcd))
    (fp_line (start 2.135 -2.61) (end 2.61 -2.61) (layer "B.SilkS") (width 0.12) (tstamp 97a665d9-00ae-43eb-8df6-4358ffa0d9aa))
    (fp_line (start -2.135 -2.61) (end -2.61 -2.61) (layer "B.SilkS") (width 0.12) (tstamp cd191336-45b2-4507-a30d-15f715df2f00))
    (fp_line (start -2.135 2.61) (end -2.61 2.61) (layer "B.SilkS") (width 0.12) (tstamp f910f391-c593-4e00-b6af-f1a415db2252))
    (fp_line (start 3.1 -3.1) (end 3.1 3.1) (layer "B.CrtYd") (width 0.05) (tstamp 4bc718e3-0dda-4cd7-9758-383baad8d602))
    (fp_line (start -3.1 3.1) (end -3.1 -3.1) (layer "B.CrtYd") (width 0.05) (tstamp 77443a9c-0d00-4bc2-a011-044a70edf3bb))
    (fp_line (start 3.1 3.1) (end -3.1 3.1) (layer "B.CrtYd") (width 0.05) (tstamp 7eb498f8-3ea7-4de6-9294-6c95d16d6b05))
    (fp_line (start -3.1 -3.1) (end 3.1 -3.1) (layer "B.CrtYd") (width 0.05) (tstamp ab80ae95-becf-4df3-b500-e9eb27ee5a69))
    (fp_line (start 2.5 -2.5) (end -2.5 -2.5) (layer "B.Fab") (width 0.1) (tstamp 0718ae16-c052-4435-8986-04c79eff36ff))
    (fp_line (start -1.5 2.5) (end 2.5 2.5) (layer "B.Fab") (width 0.1) (tstamp 1b24b644-34fd-49a9-b59c-abe20300f0b4))
    (fp_line (start 2.5 2.5) (end 2.5 -2.5) (layer "B.Fab") (width 0.1) (tstamp 2008c2c7-e713-48af-b3f9-4185630b35bf))
    (fp_line (start -2.5 -2.5) (end -2.5 1.5) (layer "B.Fab") (width 0.1) (tstamp 60d21545-7f8a-42ab-8eb3-ae6b05bdc437))
    (fp_line (start -2.5 1.5) (end -1.5 2.5) (layer "B.Fab") (width 0.1) (tstamp a60e2f43-13b8-45bb-953d-5feafe2717d1))
    (pad "" smd roundrect (at 0.875 -0.875 180) (size 1.46 1.46) (layers "B.Paste") (roundrect_rratio 0.171233) (tstamp 0867358d-8e73-414e-983f-1bd765f23dd0))
    (pad "" smd roundrect (at -0.875 -0.875 180) (size 1.46 1.46) (layers "B.Paste") (roundrect_rratio 0.171233) (tstamp 64df99fb-1e45-44f8-ab6b-8f66ba435516))
    (pad "" smd roundrect (at 0.875 0.875 180) (size 1.46 1.46) (layers "B.Paste") (roundrect_rratio 0.171233) (tstamp 861fbf20-22a7-4d6c-b256-ee2969680dd1))
    (pad "" smd roundrect (at -0.875 0.875 180) (size 1.46 1.46) (layers "B.Paste") (roundrect_rratio 0.171233) (tstamp c28d6b33-5ebc-4726-954c-d28f1747730f))
    (pad "1" smd roundrect (at -2.45 1.75 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 72 "/Sensor_Controller/SPI_CS") (pinfunction "PIO0_17/ADC_9") (pintype "tri_state") (tstamp 22251edf-dc68-4b2f-895d-e60c35544813))
    (pad "2" smd roundrect (at -2.45 1.25 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 73 "/Power_Management/LED_PWM") (pinfunction "PIO0_13/ADC_10") (pintype "tri_state") (tstamp 9a394f02-f4c9-4e9e-a35b-25d8d348013c))
    (pad "3" smd roundrect (at -2.45 0.75 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 40 "/Sensor_Controller/LPC_~{ISP}") (pinfunction "PIO0_12") (pintype "tri_state") (tstamp 583ea787-682f-4c0e-960b-39187d520ef5))
    (pad "4" smd roundrect (at -2.45 0.25 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/Sensor_Controller/LPC_~{RST}") (pinfunction "~{RESET}/PIO0_5") (pintype "tri_state") (tstamp fec7b2e2-1865-427f-bb89-da2b4032b804))
    (pad "5" smd roundrect (at -2.45 -0.25 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 74 "/Sensor_Controller/ALS_INT") (pinfunction "PIO0_4/ADC_11/TRSTN") (pintype "tri_state") (tstamp da047157-a0fe-4c80-8269-a34593421eec))
    (pad "6" smd roundrect (at -2.45 -0.75 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 47 "/Sensor_Controller/LPC_SWCLK") (pinfunction "SWCLK/PIO0_3/TCK") (pintype "tri_state") (tstamp 184ddae0-b65e-45be-9afd-e5be77bd26ab))
    (pad "7" smd roundrect (at -2.45 -1.25 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 46 "/Sensor_Controller/LPC_SWDIO") (pinfunction "SWDIO/PIO0_2/TMS") (pintype "tri_state") (tstamp 1bd692a3-1ee2-45ab-868b-df34ac55930b))
    (pad "8" smd roundrect (at -2.45 -1.75 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 75 "/Sensor_Controller/RTC_CLKO") (pinfunction "PIO0_11/ADC_6/WKTCLKIN") (pintype "tri_state") (tstamp a8b141cb-5408-4b57-8861-2f86502c64e9))
    (pad "9" smd roundrect (at -1.75 -2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "/Sensor_Controller/RTC_INT") (pinfunction "PIO0_10/ADC_7") (pintype "tri_state") (tstamp 718fa5f6-68ec-4871-b5fb-3d878002568e))
    (pad "10" smd roundrect (at -1.25 -2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 66 "/Sensor_Controller/CAPT_YH") (pinfunction "PIO0_21/ACMP_I5") (pintype "tri_state") (tstamp c77dca70-51fe-4501-8a1b-d52e7a0f4494))
    (pad "11" smd roundrect (at -0.75 -2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 66 "/Sensor_Controller/CAPT_YH") (pinfunction "PIO0_29") (pintype "tri_state") (tstamp 17bc7786-adb4-4c8f-a72f-3b2580483235))
    (pad "12" smd roundrect (at -0.25 -2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "/Sensor_Controller/CAPT_YL") (pinfunction "PIO0_28") (pintype "tri_state") (tstamp ea8cc298-006a-4cce-a6db-da84a05c12c9))
    (pad "13" smd roundrect (at 0.25 -2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 48 "/Sensor_Controller/CAPT_X0") (pinfunction "PIO0_27") (pintype "tri_state") (tstamp edae1377-8be7-43ca-b978-0191d68d7646))
    (pad "14" smd roundrect (at 0.75 -2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 51 "/Sensor_Controller/CAPT_X1") (pinfunction "PIO0_26") (pintype "tri_state") (tstamp 58809354-3508-40ed-a59e-3d84eaadc50e))
    (pad "15" smd roundrect (at 1.25 -2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 54 "/Sensor_Controller/CAPT_X2") (pinfunction "PIO0_20") (pintype "tri_state") (tstamp 66aea0da-01bd-4c71-843a-efab9ffc2410))
    (pad "16" smd roundrect (at 1.75 -2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 57 "/Sensor_Controller/CAPT_X3") (pinfunction "PIO0_15/ADC_8") (pintype "tri_state") (tstamp 27bc1461-5044-4d22-bc07-9b28fd61c7d0))
    (pad "17" smd roundrect (at 2.45 -1.75 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 60 "/Sensor_Controller/CAPT_X4") (pinfunction "PIO0_1/ADC_0/ACMP_I2/TDI/CLKIN") (pintype "tri_state") (tstamp cd6b32e8-4005-4172-affa-bded613733b9))
    (pad "18" smd roundrect (at 2.45 -1.25 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 69 "/Sensor_Controller/LSM_INT2") (pinfunction "PIO0_9/ADC_4") (pintype "tri_state") (tstamp 4819db47-20fc-400d-ad88-2414d80ecaf8))
    (pad "19" smd roundrect (at 2.45 -0.75 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 68 "/Sensor_Controller/LSM_INT1") (pinfunction "PIO0_8/ADC_5") (pintype "tri_state") (tstamp 4eeb82c6-cf0e-4e50-887c-feb1b9da3349))
    (pad "20" smd roundrect (at 2.45 -0.25 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pinfunction "VDD") (pintype "power_in") (tstamp a6e50901-1d09-433f-a9ad-9187b741384a))
    (pad "21" smd roundrect (at 2.45 0.25 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 78 "/Power_Management/DCDC_EN") (pinfunction "PIO0_30") (pintype "tri_state") (tstamp a4b30c23-38df-41b0-9740-0be1a1fc9ee9))
    (pad "22" smd roundrect (at 2.45 0.75 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(C10-Pad1)") (pinfunction "PIO0_7/ADC_1/ACMPVREF") (pintype "tri_state") (tstamp 60c7a89f-cf38-4767-93ca-13362366ed3a))
    (pad "23" smd roundrect (at 2.45 1.25 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(C10-Pad1)") (pinfunction "VREFP") (pintype "power_in") (tstamp 86651daa-9530-4f84-8536-fcd5cdf84a1a))
    (pad "24" smd roundrect (at 2.45 1.75 180) (size 0.8 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 79 "/Power_Management/CHG_~{STBY}") (pinfunction "PIO0_0/ACMP_I1/TDO") (pintype "tri_state") (tstamp c50decdc-0569-428e-a532-0a06e3edd122))
    (pad "25" smd roundrect (at 1.75 2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 62 "/Power_Management/ADC_BAT") (pinfunction "PIO0_14/ADC_2/ACMP_I3") (pintype "tri_state") (tstamp 43f3ddd7-77ae-4ec0-ab1b-4b7e7aa8d056))
    (pad "26" smd roundrect (at 1.25 2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 80 "/Power_Management/CHG_~{ACT}") (pinfunction "PIO0_19/DACOUT") (pintype "tri_state") (tstamp a85f74c0-f145-4bdf-9318-01572a9240b3))
    (pad "27" smd roundrect (at 0.75 2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 42 "/Sensor_Controller/I2C_SCL") (pinfunction "PIO0_25") (pintype "tri_state") (tstamp 0b863510-fed8-4696-94d5-d6bedbbeae7f))
    (pad "28" smd roundrect (at 0.25 2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 41 "/Sensor_Controller/I2C_SDA") (pinfunction "PIO0_24") (pintype "tri_state") (tstamp 6b776a7f-fddb-4482-9082-d5c542156fcd))
    (pad "29" smd roundrect (at -0.25 2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 81 "/Sensor_Controller/SPI_~{INT}") (pinfunction "PIO0_23") (pintype "tri_state") (tstamp 725bae75-512b-4205-8aba-a3c823ba4659))
    (pad "30" smd roundrect (at -0.75 2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 38 "/WiFi_Display/EPD_SCLK") (pinfunction "PIO0_22") (pintype "tri_state") (tstamp 72e58744-fb03-4138-9888-78c8d3cc9b81))
    (pad "31" smd roundrect (at -1.25 2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 82 "/Sensor_Controller/SPI_MISO") (pinfunction "PIO0_18") (pintype "tri_state") (tstamp 4a33fbae-d00e-4009-b2a2-49ae2db7e6f1))
    (pad "32" smd roundrect (at -1.75 2.45 180) (size 0.25 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 39 "/WiFi_Display/EPD_SDI") (pinfunction "PIO0_16/ADC_3/ACMP_I4") (pintype "tri_state") (tstamp 9e70ee1d-70a7-4a49-b89e-4a504423242a))
    (pad "33" thru_hole circle (at -1.45 0 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp 27c498d3-09f5-48f9-aa73-eca266251f87))
    (pad "33" smd rect (at 0 0 180) (size 3.5 3.5) (layers "B.Cu" "B.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp 28942866-840e-4447-a963-f9e1c307fbdf))
    (pad "33" thru_hole circle (at 0 -1.45 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp 2e575a2c-e28a-49ad-b2bf-6a96341b4ed1))
    (pad "33" thru_hole circle (at 0 1.45 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp 56c97341-29cc-4f56-9f57-422930246679))
    (pad "33" thru_hole circle (at 1.45 1.45 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp 5da56b94-3ac9-45a4-a7b4-d2be9a1d223b))
    (pad "33" thru_hole circle (at 1.45 0 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp c7823fe5-4edd-426e-b800-bdd338366f6b))
    (pad "33" thru_hole circle (at 0 0 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp cb4c0074-52e4-4a3c-9ec3-922e622a6c2f))
    (pad "33" thru_hole circle (at 1.45 -1.45 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp e026c0d4-6b22-427c-96dc-93f8cc050d35))
    (pad "33" smd rect (at 0 0 180) (size 3.5 3.5) (layers "F.Cu")
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp e2e76162-0f63-4528-bfa2-706ecb55eb99))
    (pad "33" thru_hole circle (at -1.45 1.45 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp e2f297ce-9ff5-4269-ae98-d9c591935d44))
    (pad "33" thru_hole circle (at -1.45 -1.45 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp ee19ae5b-4deb-4e6c-81fb-516765cef346))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/VQFN-32-1EP_5x5mm_P0.5mm_EP3.5x3.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 8ef911c1-1720-4804-8f8e-c0032d72a0d7)
    (at 169.5 154)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/4cdd1cf5-2bc6-4e6b-9649-5f3bff87da65")
    (attr smd)
    (fp_text reference "R19" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a90f10c4-07e5-40ee-b1de-881f775eabc0)
    )
    (fp_text value "2.2k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a357ae2b-9549-447d-9118-b80e31c33e94)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp cc66ca54-6cd2-4e82-b2c9-2547963aa97d)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 0e0324c4-9bb1-422a-95ad-5c3d31056f25))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 45ed7c4e-17fd-4568-83a0-55fe5d72907d))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 36434f13-46ef-4352-83a2-b52ebed7c1b3))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 53b63f0b-f6c4-47ba-af74-cfd4fcb4078b))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp d4a4300c-f188-47e1-9eb5-2fa413ab5622))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp dbcd69a0-abca-4178-900f-bdc15a8d94a1))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 5718dccd-2ed9-431a-aa44-42c071741664))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 82b96e40-67f7-483f-b8a4-7c075346ffc0))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp f698c811-94fb-461c-8f24-4dcf481c755b))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp fb80273d-7bda-4964-b81f-f7b9663c3c6e))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 57 "/Sensor_Controller/CAPT_X3") (pintype "passive") (tstamp 75a9da9e-0e56-4cfb-ae0e-bbe4eda743eb))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(R19-Pad2)") (pintype "passive") (tstamp bb3f4d73-2e8f-4038-a821-4a21959c4c6d))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_JST:JST_PH_B2B-PH-SM4-TB_1x02-1MP_P2.00mm_Vertical" (layer "B.Cu")
    (tedit 5B78AD87) (tstamp 930fcce0-6fc7-4bf8-a6f1-facc121e11cd)
    (at 193.2 138.6 -90)
    (descr "JST PH series connector, B2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH side entry")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/5065d46b-5f7e-440b-b3b9-6db133d83adc")
    (attr smd)
    (fp_text reference "BT1" (at 0 5.45 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4557fea1-fd2e-4aad-a7b8-267bd7c89807)
    )
    (fp_text value "Li-Po 1000-2000mAh" (at 0 -4.45 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 71d75b93-64d5-4253-b6b8-2a1496b5d333)
    )
    (fp_text user "${REFERENCE}" (at 0 1 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0112e727-824f-49e0-9a40-e702d6de2702)
    )
    (fp_line (start -4.085 -0.01) (end -4.085 -0.86) (layer "B.SilkS") (width 0.12) (tstamp 08f8ba10-d63f-468f-b8e1-cb14a0252f5e))
    (fp_line (start -4.085 4.36) (end 4.085 4.36) (layer "B.SilkS") (width 0.12) (tstamp 22191cb3-b2e0-4c39-9bdb-61eafbca46c7))
    (fp_line (start -4.085 -0.86) (end -1.76 -0.86) (layer "B.SilkS") (width 0.12) (tstamp 222e4d92-dc30-4f90-8a22-05f95edb1705))
    (fp_line (start 4.085 -0.01) (end 4.085 -0.86) (layer "B.SilkS") (width 0.12) (tstamp 29cd335a-6498-4b47-9f15-418b3ec2b96a))
    (fp_line (start 4.085 -0.86) (end 1.76 -0.86) (layer "B.SilkS") (width 0.12) (tstamp 2d6741bb-9af6-4c69-9e33-e533b4bb840e))
    (fp_line (start -4.085 3.51) (end -4.085 4.36) (layer "B.SilkS") (width 0.12) (tstamp 74682856-e109-4255-9b5f-957def300e18))
    (fp_line (start -1.76 -0.86) (end -1.76 -3.25) (layer "B.SilkS") (width 0.12) (tstamp 92be2371-21e6-4c97-8d62-fba82729df07))
    (fp_line (start 4.085 4.36) (end 4.085 3.51) (layer "B.SilkS") (width 0.12) (tstamp c6d6cf19-49d2-4c73-ba8b-833e4153581a))
    (fp_line (start -4.7 4.75) (end -4.7 -3.75) (layer "B.CrtYd") (width 0.05) (tstamp 0d0429e1-7734-426e-9078-4fa78512a0e7))
    (fp_line (start 4.7 4.75) (end -4.7 4.75) (layer "B.CrtYd") (width 0.05) (tstamp 35929fdb-cb3b-465e-93b5-f51df2dab10a))
    (fp_line (start 4.7 -3.75) (end 4.7 4.75) (layer "B.CrtYd") (width 0.05) (tstamp 5c24bbf4-6a9a-4b3f-ae0b-be7b6b99c1fb))
    (fp_line (start -4.7 -3.75) (end 4.7 -3.75) (layer "B.CrtYd") (width 0.05) (tstamp 8bff54a6-e951-4823-888c-8ff6dc803c5a))
    (fp_line (start -3.975 -0.75) (end -3.975 4.25) (layer "B.Fab") (width 0.1) (tstamp 15d776e6-0f79-4e3d-a1fc-1dd65697d6fa))
    (fp_line (start 0.75 2.75) (end 0.75 2.25) (layer "B.Fab") (width 0.1) (tstamp 1a25c20c-753f-472b-baff-d0729e88958f))
    (fp_line (start -3.975 -0.75) (end 3.975 -0.75) (layer "B.Fab") (width 0.1) (tstamp 1c5ed236-9011-4611-8680-0c3053caf3f6))
    (fp_line (start 1.25 2.25) (end 1.25 2.75) (layer "B.Fab") (width 0.1) (tstamp 25265eb2-9016-4950-a98f-4f7ffc33b7e0))
    (fp_line (start 3.975 -0.75) (end 3.975 4.25) (layer "B.Fab") (width 0.1) (tstamp 29c99fb1-f1a1-4ffc-99b1-e358a7d0a022))
    (fp_line (start -3.975 4.25) (end 3.975 4.25) (layer "B.Fab") (width 0.1) (tstamp 329cad0e-d28d-48c8-b974-78afbee64345))
    (fp_line (start -0.75 2.25) (end -0.75 2.75) (layer "B.Fab") (width 0.1) (tstamp 41851ac6-9e89-49c7-8276-842f9887a962))
    (fp_line (start -1.25 2.25) (end -0.75 2.25) (layer "B.Fab") (width 0.1) (tstamp 5ebe6b9f-8a90-4ccb-9577-e2812079b31c))
    (fp_line (start -0.75 2.75) (end -1.25 2.75) (layer "B.Fab") (width 0.1) (tstamp 6e53eed8-ab8a-4d38-a25a-f5d45c1b8afe))
    (fp_line (start 1.25 2.75) (end 0.75 2.75) (layer "B.Fab") (width 0.1) (tstamp 807c9bfa-f5c6-44f2-9fd3-13c350559ed2))
    (fp_line (start 0.75 2.25) (end 1.25 2.25) (layer "B.Fab") (width 0.1) (tstamp 811fc315-1729-455d-a206-8970e026fc4f))
    (fp_line (start -1 -0.042893) (end -0.5 -0.75) (layer "B.Fab") (width 0.1) (tstamp 82790e35-40a0-4535-9c90-301047013a68))
    (fp_line (start -1.25 2.75) (end -1.25 2.25) (layer "B.Fab") (width 0.1) (tstamp a9ecc861-373a-45c3-b907-2a56133fc9b3))
    (fp_line (start -1.5 -0.75) (end -1 -0.042893) (layer "B.Fab") (width 0.1) (tstamp cccea3e8-ab49-4b6d-b090-0022fc55c2af))
    (pad "1" smd roundrect (at -1 -0.5 270) (size 1 5.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 106 "Net-(BT1-Pad1)") (pinfunction "+") (pintype "passive") (tstamp 9e91f664-7223-4008-9717-4e3689f95dfc))
    (pad "2" smd roundrect (at 1 -0.5 270) (size 1 5.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "-") (pintype "passive") (tstamp cc6be4bc-28c0-4417-8da5-f265464b4484))
    (pad "MP" smd roundrect (at -3.4 1.75 270) (size 1.6 3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.15625) (tstamp 1133215f-620e-4913-95aa-e2529f5aa6b7))
    (pad "MP" smd roundrect (at 3.4 1.75 270) (size 1.6 3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.15625) (tstamp afbfa340-b350-4156-a9c7-08e55a3aa2fb))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_B2B-PH-SM4-TB_1x02-1MP_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 9b6cc922-a122-4c01-9443-bbdb32494d75)
    (at 127.5 154 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/77551999-4e6f-40be-807f-b54e7caa6297")
    (attr smd)
    (fp_text reference "R11" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 30141ae9-9c00-4fb9-b8d2-564d06112160)
    )
    (fp_text value "2.2k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 070b98c6-e821-49b7-ad2f-3a80e510a5f4)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp ecb3987a-4598-4873-aadd-ffcccac3f6d6)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 4b677dd3-1f4f-45f7-b3ba-30614b34fc1a))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp a3b59683-6558-4b2a-b676-96c90134ced4))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 1639d553-01fd-44d6-986c-ae8cbad1c6fb))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 4db1f014-8fce-4776-bb8f-29942e802774))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 7255e838-4065-475b-a781-bed8a0a56479))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 927bbdc9-2e59-4b10-9d50-6f4a18c9ba43))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp d1ec9174-1047-4198-bd53-d700926641a8))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp e08c4572-558f-4a24-b09a-857d914da1b2))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp e52aecdb-9f80-4d60-932b-23e752714d73))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp e65e1c99-cc43-4268-87fe-d67051a0fd2b))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(R11-Pad1)") (pintype "passive") (tstamp d632f4ff-b47f-43d3-9359-ad6bf91be9cd))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(R10-Pad2)") (pintype "passive") (tstamp 4f7ed4af-60d4-4a30-8226-a2362e4048bd))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 9becb878-ef3d-4619-9b23-f622900f60fe)
    (at 174.9 127.4)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/c7529554-fb1b-436d-8376-0e1625341df0")
    (attr smd)
    (fp_text reference "C27" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 20d6da1d-577e-436d-a368-d51b990ccd1b)
    )
    (fp_text value "1uF/50V" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 23550477-115c-4637-a099-11311bfa30f9)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 3f131a9c-e592-49c4-88a8-3485f89e087e)
    )
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp 8617bc90-d39e-48cf-b7f3-54edf5c42dce))
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp a25620d1-8b35-4eb3-b2e7-65a938da6398))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 03a72157-a183-4a09-b582-1f3ff0110a96))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 2dd0df51-04af-4a8f-a20c-e0b96f6b822e))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp b0d5aecc-9dce-45b9-8a47-283124bcb7a3))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp dc77433c-904b-4874-89fd-74097aceb019))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 6e3a9079-b001-41a0-98b2-9b13d8b4c969))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 71d405ce-9c8a-4930-987b-f5151bc045d6))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 8719e39d-50bb-4d36-b596-ffd771f68842))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 8733df1d-4dfc-4dfe-9745-aa73cfd503ee))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 5f19aa1d-4005-4978-8b13-75236fdaa706))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(C27-Pad2)") (pintype "passive") (tstamp fd878961-2968-4646-adbe-0428c970fcfd))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 9fc61cda-71fb-47cf-bc26-abdb8ef0df6b)
    (at 81.36 111 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/137e690e-b61b-45c0-892e-e0c090818fe7")
    (attr smd)
    (fp_text reference "R2" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 338edc16-2ec8-4d79-9e78-eabd22957b10)
    )
    (fp_text value "4k7" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 6e0e8737-a373-4be2-828f-1ab0c8f0d0f6)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 7dc055c1-ace0-4333-8fd7-f2a1d47ddf2d)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 052ca3e4-eae4-4fe6-9b53-f14d3283a085))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp e2f661d3-be51-4a35-ac6f-350d09fc0632))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 14abcc7d-f443-462d-8b98-463a28674fbf))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 2ffd4aaa-809c-48d6-a9cc-46e32c856318))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 3a18cc49-3d53-4786-bddf-cefee90b1b3c))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 68d19009-93e4-40e6-8f82-bbed402c3f24))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 4aabc145-70b2-452e-b551-64526e47fc8d))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 4c848b74-6f4a-4077-88fc-7fa36810aa3d))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp c812c830-0235-476d-bcb8-f4befa86a26a))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp e073dd7f-c811-478e-934d-75059605b0ba))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp a92192dd-b6a0-4632-8d84-e079276d1d31))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 41 "/Sensor_Controller/I2C_SDA") (pintype "passive") (tstamp 8106362f-b6a2-44f6-95c0-801e9ea94a6b))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_LGA:Bosch_LGA-8_2.5x2.5mm_P0.65mm_ClockwisePinNumbering" (layer "B.Cu")
    (tedit 5A0FA816) (tstamp 9fdfe07f-e16c-4e3e-bade-7f7e07316c4f)
    (at 127.9 139.8 180)
    (descr "LGA-8")
    (tags "lga land grid array")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/e686e57b-c43c-476c-b407-df572672ff85")
    (attr smd)
    (fp_text reference "U2" (at 0.015 2.465) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 1735f0dc-8fbb-45b6-83fa-c61e50b8f9a6)
    )
    (fp_text value "BME280" (at 0.015 -2.535) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 3031a0f7-e197-4fc6-bff1-5f0e2e0fe5db)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
      (tstamp 70cfbc53-845b-4e66-8b72-ecfab87e62b5)
    )
    (fp_line (start 1.35 -1.35) (end 1.35 -1.2) (layer "B.SilkS") (width 0.1) (tstamp 023db6ba-a1c3-49a5-8ac8-1460c670a066))
    (fp_line (start -1.35 -1.36) (end -1.2 -1.36) (layer "B.SilkS") (width 0.1) (tstamp 4dbbed8f-686a-4913-95d6-65280cded19a))
    (fp_line (start 1.35 -1.35) (end 1.2 -1.35) (layer "B.SilkS") (width 0.1) (tstamp 633df951-8c96-46f8-8f2d-42d58fda6ad5))
    (fp_line (start -1.35 -1.35) (end -1.35 -1.2) (layer "B.SilkS") (width 0.1) (tstamp 90f012bf-c1e7-4c83-af4a-6e77d0860faf))
    (fp_line (start 1.35 1.35) (end 1.35 1.2) (layer "B.SilkS") (width 0.1) (tstamp 929102ee-ecc3-4f5c-9d0b-435055047197))
    (fp_line (start 1.2 1.35) (end 1.35 1.35) (layer "B.SilkS") (width 0.1) (tstamp b78f4b2a-e94b-4200-8f5e-9fcc887a219d))
    (fp_line (start -1.35 1.2) (end -1.35 1.45) (layer "B.SilkS") (width 0.1) (tstamp c9b986ad-00c7-4718-b31d-8c003b17428f))
    (fp_line (start 1.41 -1.54) (end -1.41 -1.54) (layer "B.CrtYd") (width 0.05) (tstamp 107e39cb-16e0-4954-bcd3-8df3250ea398))
    (fp_line (start -1.41 -1.54) (end -1.41 1.54) (layer "B.CrtYd") (width 0.05) (tstamp 3b3f988a-6e80-4650-bac3-5bd97bfc41bd))
    (fp_line (start -1.41 1.54) (end 1.41 1.54) (layer "B.CrtYd") (width 0.05) (tstamp 4a71624e-cb7d-4123-ac22-6eb65fbcc371))
    (fp_line (start 1.41 1.54) (end 1.41 -1.54) (layer "B.CrtYd") (width 0.05) (tstamp 6941e982-ba9f-4892-b9d9-70f802acf8bf))
    (fp_line (start -1.25 0.5) (end -0.5 1.25) (layer "B.Fab") (width 0.1) (tstamp 01ccdcfb-4524-4845-9cfc-271852b93dfd))
    (fp_line (start 1.25 -1.25) (end -1.25 -1.25) (layer "B.Fab") (width 0.1) (tstamp 0ebfbe5e-bbec-4c7e-9fad-b578931fc372))
    (fp_line (start -1.25 -1.25) (end -1.25 0.5) (layer "B.Fab") (width 0.1) (tstamp 157167a0-592d-4872-b915-a643151b29ed))
    (fp_line (start -0.5 1.25) (end 1.25 1.25) (layer "B.Fab") (width 0.1) (tstamp dba90a98-b79c-43f9-a5c7-aa9f81e8729b))
    (fp_line (start 1.25 1.25) (end 1.25 -1.25) (layer "B.Fab") (width 0.1) (tstamp df17960c-3eae-4594-9c53-cc593181af82))
    (pad "1" smd rect (at -0.975 1.025 90) (size 0.5 0.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 16ac23ed-6ef2-41cc-953d-db115806a0e6))
    (pad "2" smd rect (at -0.325 1.025 90) (size 0.5 0.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "VDDF") (pinfunction "CSB") (pintype "input") (tstamp 27766c82-d132-4fec-a370-69da8457535a))
    (pad "3" smd rect (at 0.325 1.025 90) (size 0.5 0.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 41 "/Sensor_Controller/I2C_SDA") (pinfunction "SDI") (pintype "bidirectional") (tstamp 719c6679-3f8e-4db3-9ff2-270e3727f3c5))
    (pad "4" smd rect (at 0.975 1.025 90) (size 0.5 0.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 42 "/Sensor_Controller/I2C_SCL") (pinfunction "SCK") (pintype "input") (tstamp da848b1a-0e2d-4d5e-bade-3f5a03aa8d0f))
    (pad "5" smd rect (at 0.975 -1.025 90) (size 0.5 0.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "SDO") (pintype "bidirectional") (tstamp 36893633-982e-4401-ac2d-d6de11b53ec9))
    (pad "6" smd rect (at 0.325 -1.025 90) (size 0.5 0.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "VDDF") (pinfunction "VDDIO") (pintype "power_in") (tstamp 74901deb-88dc-45ad-8810-f5c6c327a334))
    (pad "7" smd rect (at -0.325 -1.025 90) (size 0.5 0.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 7b5fd1b1-844a-4e03-9554-cefb5f2c3782))
    (pad "8" smd rect (at -0.975 -1.025 90) (size 0.5 0.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "VDDF") (pinfunction "VDD") (pintype "power_in") (tstamp 9aca941e-8122-431e-ae0c-2425446d4ff3))
    (model "${KICAD6_3DMODEL_DIR}/Package_LGA.3dshapes/Bosch_LGA-8_2.5x2.5mm_P0.65mm_ClockwisePinNumbering.wrl"
      (offset (xyz 0.01500000025 -0.03500000059 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical_SMD" (layer "B.Cu")
    (tedit 59FED6E3) (tstamp a1bb3317-b16d-495e-91c3-219519108e5e)
    (at 116.9 125.1)
    (descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x05 1.27mm double row")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/d5ff02e9-b34c-4646-bb15-bf1695940209")
    (attr smd)
    (fp_text reference "J1" (at 0 4.235) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 256da29a-83e1-4192-8627-7b15c8bdc30c)
    )
    (fp_text value "Conn_02x05_Odd_Even" (at 0 -4.235) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 6d64b09d-0dfd-4a35-8b7e-3a5672be487b)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 9a5d72d3-41af-4cd7-897d-5d21e0585242)
    )
    (fp_line (start -1.765 -3.235) (end 1.765 -3.235) (layer "B.SilkS") (width 0.12) (tstamp 241fc6cd-adf3-4ef3-955f-65f983f27c81))
    (fp_line (start -1.765 3.235) (end -1.765 3.17) (layer "B.SilkS") (width 0.12) (tstamp 6e456bde-52d5-4145-a936-eb6fc0c9ea46))
    (fp_line (start -1.765 3.235) (end 1.765 3.235) (layer "B.SilkS") (width 0.12) (tstamp 8515203a-c19b-47d3-8197-0f24a236b636))
    (fp_line (start -3.09 3.17) (end -1.765 3.17) (layer "B.SilkS") (width 0.12) (tstamp a5d3355e-0247-4c34-a686-4c2ca8db2292))
    (fp_line (start -1.765 -3.17) (end -1.765 -3.235) (layer "B.SilkS") (width 0.12) (tstamp c7594c9d-4fbf-46c0-97b5-506ed456a419))
    (fp_line (start 1.765 -3.17) (end 1.765 -3.235) (layer "B.SilkS") (width 0.12) (tstamp da747909-ce6d-4ae0-80fa-724f0e494e72))
    (fp_line (start 1.765 3.235) (end 1.765 3.17) (layer "B.SilkS") (width 0.12) (tstamp f1e6a886-7b32-481a-bbfc-f668916f264c))
    (fp_line (start 4.3 3.7) (end -4.3 3.7) (layer "B.CrtYd") (width 0.05) (tstamp 31ddf1c5-8bd5-4213-b7c9-438dcf803146))
    (fp_line (start -4.3 -3.7) (end 4.3 -3.7) (layer "B.CrtYd") (width 0.05) (tstamp 4890fbba-5bd1-469a-90ea-a2b004b2be78))
    (fp_line (start 4.3 -3.7) (end 4.3 3.7) (layer "B.CrtYd") (width 0.05) (tstamp 8062717d-7552-4634-aaa1-f303f085c257))
    (fp_line (start -4.3 3.7) (end -4.3 -3.7) (layer "B.CrtYd") (width 0.05) (tstamp db5fae20-df74-4e62-b61a-98f365c2e7fe))
    (fp_line (start 1.705 -3.175) (end -1.705 -3.175) (layer "B.Fab") (width 0.1) (tstamp 06eb3590-5fa1-486b-8a49-0bad7e726cdd))
    (fp_line (start -2.75 0.2) (end -2.75 -0.2) (layer "B.Fab") (width 0.1) (tstamp 234df8d9-2ed5-4c60-9752-b7276ce9678d))
    (fp_line (start -1.705 1.47) (end -2.75 1.47) (layer "B.Fab") (width 0.1) (tstamp 309903aa-4411-4ca4-b9f5-75fbe3d0cd71))
    (fp_line (start 1.705 -2.34) (end 2.75 -2.34) (layer "B.Fab") (width 0.1) (tstamp 356aa333-3067-4f82-a36f-144123ef5833))
    (fp_line (start -2.75 2.74) (end -2.75 2.34) (layer "B.Fab") (width 0.1) (tstamp 40d3b5b1-0d9d-4290-af84-d7378f30b220))
    (fp_line (start -2.75 -0.2) (end -1.705 -0.2) (layer "B.Fab") (width 0.1) (tstamp 52c39cf7-9421-4b49-b359-dc5e409624cd))
    (fp_line (start 2.75 1.07) (end 1.705 1.07) (layer "B.Fab") (width 0.1) (tstamp 5d46253b-0b50-4329-9abf-132692c6cf0f))
    (fp_line (start -2.75 -1.47) (end -1.705 -1.47) (layer "B.Fab") (width 0.1) (tstamp 5f92b6ae-11fc-4b6a-8645-74415f553b4c))
    (fp_line (start 1.705 0.2) (end 2.75 0.2) (layer "B.Fab") (width 0.1) (tstamp 61b3f364-0bca-4c53-9945-2792515a445e))
    (fp_line (start -2.75 1.07) (end -1.705 1.07) (layer "B.Fab") (width 0.1) (tstamp 66e1b670-432a-4975-8302-aee6a9e44bf9))
    (fp_line (start 1.705 3.175) (end 1.705 -3.175) (layer "B.Fab") (width 0.1) (tstamp 6c71a5df-b30a-4824-8006-e81e5e97b857))
    (fp_line (start -1.27 3.175) (end 1.705 3.175) (layer "B.Fab") (width 0.1) (tstamp 70ed67df-9eda-4d18-a231-e4aa81a665c1))
    (fp_line (start 2.75 -0.2) (end 1.705 -0.2) (layer "B.Fab") (width 0.1) (tstamp 74493079-1000-4bf7-a893-9301fd73c9d9))
    (fp_line (start 2.75 -1.47) (end 1.705 -1.47) (layer "B.Fab") (width 0.1) (tstamp 776917fe-62a0-484d-b928-4055ced2ac90))
    (fp_line (start 2.75 -2.74) (end 1.705 -2.74) (layer "B.Fab") (width 0.1) (tstamp 79a96bd2-adba-40b8-bd4f-100a61f1f50e))
    (fp_line (start 1.705 1.47) (end 2.75 1.47) (layer "B.Fab") (width 0.1) (tstamp 7bd310c5-b6ed-4ad1-bd5b-b475825a4947))
    (fp_line (start -1.705 2.74) (end -1.27 3.175) (layer "B.Fab") (width 0.1) (tstamp 8145c8bb-ea6f-408a-89ef-da8a99e84090))
    (fp_line (start -1.705 -2.34) (end -2.75 -2.34) (layer "B.Fab") (width 0.1) (tstamp 91b384dd-5f28-464e-b640-37097fad3d4f))
    (fp_line (start 2.75 -1.07) (end 2.75 -1.47) (layer "B.Fab") (width 0.1) (tstamp 92d17004-8f0f-4437-959e-aea791efa5d5))
    (fp_line (start 2.75 -2.34) (end 2.75 -2.74) (layer "B.Fab") (width 0.1) (tstamp 97023a0d-6da9-431a-a4de-08f59e0646e1))
    (fp_line (start -1.705 -3.175) (end -1.705 2.74) (layer "B.Fab") (width 0.1) (tstamp 9ec8979b-383e-4012-b0a8-a197d46dba71))
    (fp_line (start 1.705 -1.07) (end 2.75 -1.07) (layer "B.Fab") (width 0.1) (tstamp aa88c50b-9bf0-4d9e-a265-8a4daabd70aa))
    (fp_line (start 2.75 2.74) (end 2.75 2.34) (layer "B.Fab") (width 0.1) (tstamp ae637d19-ae9c-486c-be46-9762a736e77e))
    (fp_line (start -2.75 2.34) (end -1.705 2.34) (layer "B.Fab") (width 0.1) (tstamp b15287f7-ce5f-42ce-9495-2b51379f2698))
    (fp_line (start -2.75 1.47) (end -2.75 1.07) (layer "B.Fab") (width 0.1) (tstamp ba44e59f-fee4-4cd7-aae3-ee2237360d10))
    (fp_line (start -1.705 -1.07) (end -2.75 -1.07) (layer "B.Fab") (width 0.1) (tstamp bcb6aea3-dc8c-447b-8874-dc05037dedba))
    (fp_line (start 2.75 1.47) (end 2.75 1.07) (layer "B.Fab") (width 0.1) (tstamp c28d2a67-906d-466c-962a-ae27f3f5269d))
    (fp_line (start 2.75 0.2) (end 2.75 -0.2) (layer "B.Fab") (width 0.1) (tstamp d53f060a-61a9-4462-a1a2-6bdc06bfec00))
    (fp_line (start -1.705 0.2) (end -2.75 0.2) (layer "B.Fab") (width 0.1) (tstamp ef90ccd3-c683-4981-97be-fce66c169c45))
    (fp_line (start -1.705 2.74) (end -2.75 2.74) (layer "B.Fab") (width 0.1) (tstamp f316167a-74ae-414e-8058-816ced75cf20))
    (fp_line (start 2.75 2.34) (end 1.705 2.34) (layer "B.Fab") (width 0.1) (tstamp f32efb9a-0057-4100-8b1b-7d0a211e2fa2))
    (fp_line (start -2.75 -2.74) (end -1.705 -2.74) (layer "B.Fab") (width 0.1) (tstamp f3337f69-290b-4abe-acec-b255ec312c2c))
    (fp_line (start 1.705 2.74) (end 2.75 2.74) (layer "B.Fab") (width 0.1) (tstamp f434dad9-059c-4e8b-ab00-1fea3512e9b5))
    (fp_line (start -2.75 -2.34) (end -2.75 -2.74) (layer "B.Fab") (width 0.1) (tstamp f61b25bf-560f-4fc3-97fc-370fec898f5a))
    (fp_line (start -2.75 -1.07) (end -2.75 -1.47) (layer "B.Fab") (width 0.1) (tstamp fa3b63e3-3bb6-441d-9e65-7c92584435d7))
    (pad "1" smd rect (at -1.95 2.54) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "VDDF") (pinfunction "Pin_1") (pintype "passive") (tstamp 39321b80-f8d2-4fc2-9206-0b8cfe47530a))
    (pad "2" smd rect (at 1.95 2.54) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 46 "/Sensor_Controller/LPC_SWDIO") (pinfunction "Pin_2") (pintype "passive") (tstamp 47022f3b-bc70-46f5-8e63-23533616b3e4))
    (pad "3" smd rect (at -1.95 1.27) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive") (tstamp 762037a1-880e-4f8d-95ef-bf65edab381a))
    (pad "4" smd rect (at 1.95 1.27) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 47 "/Sensor_Controller/LPC_SWCLK") (pinfunction "Pin_4") (pintype "passive") (tstamp 18d28863-9273-4508-81a8-5aefbf9962d0))
    (pad "5" smd rect (at -1.95 0) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Pin_5") (pintype "passive") (tstamp 4cb6b8d3-02f3-46c9-9aa8-74327bddd986))
    (pad "6" smd rect (at 1.95 0) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 107 "unconnected-(J1-Pad6)") (pinfunction "Pin_6") (pintype "passive+no_connect") (tstamp 979512d8-cd76-4c28-add8-42cd3094bb70))
    (pad "7" smd rect (at -1.95 -1.27) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 108 "unconnected-(J1-Pad7)") (pinfunction "Pin_7") (pintype "passive+no_connect") (tstamp 85193aea-ae77-45f0-92e7-ac2eff0eeb7d))
    (pad "8" smd rect (at 1.95 -1.27) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 109 "unconnected-(J1-Pad8)") (pinfunction "Pin_8") (pintype "passive+no_connect") (tstamp 6371f893-89cf-4e7a-913b-3dc95b6ad9a9))
    (pad "9" smd rect (at -1.95 -2.54) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Pin_9") (pintype "passive") (tstamp bfa4e90a-6fcf-4d7e-acbe-87c5273076f9))
    (pad "10" smd rect (at 1.95 -2.54) (size 2.4 0.74) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "/Sensor_Controller/LPC_~{RST}") (pinfunction "Pin_10") (pintype "passive") (tstamp a738a243-6f85-4732-bc0c-761a0f7794bb))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical_SMD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "KiCAD_Mods:Connector_FPC_FFC_JS_AFC07-S24ECA-00" (layer "B.Cu")
    (tedit 60028AE1) (tstamp a7809bd2-2991-4911-98e9-a5d4b79b7761)
    (at 178.425 124.65 -90)
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/3a1a01f4-238a-4b56-a295-7725401edea8")
    (attr smd)
    (fp_text reference "J4" (at 0 -1.8 -270) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f74f86b1-b7c5-4d6e-b63f-f2c1aa50eb19)
    )
    (fp_text value "AFC07-S24ECA-00" (at 0 -4.9 -270) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5356db46-9624-4ffc-a0ab-b525257511e2)
    )
    (fp_text user "1" (at 7.5 0.15 -270) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f2e0ee48-89ba-41d6-aaff-fe246dd6fba9)
    )
    (fp_line (start -6 0.83) (end 6 0.83) (layer "B.SilkS") (width 0.12) (tstamp 025cb963-110b-42a9-bf59-81b0d381a587))
    (fp_line (start -8.76 -3.97) (end -8.76 -0.61) (layer "B.SilkS") (width 0.12) (tstamp 032fcc36-4046-4e0c-b48e-41ca81fff7b0))
    (fp_line (start -6 -0.83) (end -6 -3.97) (layer "B.SilkS") (width 0.12) (tstamp 0c3d915e-2d65-4232-9fc5-d6654103c05f))
    (fp_line (start 6 -0.61) (end 6 0.83) (layer "B.SilkS") (width 0.12) (tstamp 3c5eb6e0-e290-4d64-bafe-0b25f3ec8eaa))
    (fp_line (start 8.76 -3.97) (end 8.76 -0.61) (layer "B.SilkS") (width 0.12) (tstamp 50610d67-636c-442a-bbd0-d92b0be12b60))
    (fp_line (start -8.76 -0.61) (end -6 -0.61) (layer "B.SilkS") (width 0.12) (tstamp 67f66976-b98a-45f6-bede-42f032a54862))
    (fp_line (start -6 -3.97) (end -8.76 -3.97) (layer "B.SilkS") (width 0.12) (tstamp 7190449d-e958-40d1-af0b-9e4d50e3db42))
    (fp_line (start 6 -3.97) (end 8.76 -3.97) (layer "B.SilkS") (width 0.12) (tstamp a79e90f6-7851-4ac0-80d8-160004bcc08e))
    (fp_line (start -6 -0.83) (end 6 -0.83) (layer "B.SilkS") (width 0.12) (tstamp b9ef4c0e-99f9-4688-bba4-0630e7171bec))
    (fp_line (start -6 -0.61) (end -6 0.83) (layer "B.SilkS") (width 0.12) (tstamp c6d36843-190c-4170-9d7d-a000ff22db8f))
    (fp_line (start 6 -0.83) (end 6 -3.97) (layer "B.SilkS") (width 0.12) (tstamp cb7f21a9-7edc-419d-a575-716d31a2076e))
    (fp_line (start 8.76 -0.61) (end 6 -0.61) (layer "B.SilkS") (width 0.12) (tstamp fd9c701c-1915-4e5e-b8a0-7ee8d4480d01))
    (fp_poly (pts
        (xy 6.6 -0.6)
        (xy 6 -0.6)
        (xy 6 0)
      ) (layer "B.SilkS") (width 0.1) (fill solid) (tstamp e9b5d04e-4223-4b25-868d-e10038e00748))
    (fp_line (start 9 1.05) (end 9 -4.2) (layer "B.CrtYd") (width 0.05) (tstamp 64d7488c-adc3-4c77-a4da-ce84cbf14188))
    (fp_line (start -9 -4.2) (end 9 -4.2) (layer "B.CrtYd") (width 0.05) (tstamp 808f0c2a-1abd-462a-8a95-d01a31c44532))
    (fp_line (start -9 1.05) (end 9 1.05) (layer "B.CrtYd") (width 0.05) (tstamp 8867963c-2e90-42e2-bc5f-f4076d85b975))
    (fp_line (start -9 1.05) (end -9 -4.2) (layer "B.CrtYd") (width 0.05) (tstamp ae770fd8-be83-47eb-ac60-0c0e3e9a23aa))
    (pad "1" smd rect (at 5.75 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "unconnected-(J4-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect") (tstamp bdf9ebea-bbb7-4637-955f-dd15c4b20e8d))
    (pad "2" smd rect (at 5.25 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 30 "/WiFi_Display/GDR") (pinfunction "Pin_2") (pintype "passive") (tstamp 237d3841-5d1f-465d-97c8-57de4d21ad20))
    (pad "3" smd rect (at 4.75 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 31 "/WiFi_Display/RESE") (pinfunction "Pin_3") (pintype "passive") (tstamp f18622d4-98c4-475e-8ec7-40e52c4b178a))
    (pad "4" smd rect (at 4.25 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "Net-(C23-Pad2)") (pinfunction "Pin_4") (pintype "passive") (tstamp cf3cf7d4-071e-4621-8f34-dc3e515688b7))
    (pad "5" smd rect (at 3.75 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "Net-(C27-Pad2)") (pinfunction "Pin_5") (pintype "passive") (tstamp f70b5b4b-1f8c-4c6f-9538-574ab420dba6))
    (pad "6" smd rect (at 3.25 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 32 "unconnected-(J4-Pad6)") (pinfunction "Pin_6") (pintype "passive+no_connect") (tstamp 278f916e-4447-44d1-b865-885e99cf15d0))
    (pad "7" smd rect (at 2.75 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "unconnected-(J4-Pad7)") (pinfunction "Pin_7") (pintype "passive+no_connect") (tstamp 8e5c3ace-092b-42e5-9047-8eed0daec53f))
    (pad "8" smd rect (at 2.25 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Pin_8") (pintype "passive") (tstamp d8d7f49b-1b23-437e-8249-f58773828103))
    (pad "9" smd rect (at 1.75 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 34 "/WiFi_Display/EPD_BUSY") (pinfunction "Pin_9") (pintype "passive") (tstamp 700055f7-359e-46f8-a89b-f3896e2b5dbc))
    (pad "10" smd rect (at 1.25 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "/WiFi_Display/EPD_~{RES}") (pinfunction "Pin_10") (pintype "passive") (tstamp 0e152cf3-24c0-466e-b9db-95d4426e6de7))
    (pad "11" smd rect (at 0.75 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "/WiFi_Display/EPD_D{slash}~{C}") (pinfunction "Pin_11") (pintype "passive") (tstamp 45adee83-97bc-4e26-ac68-86b31b4c7466))
    (pad "12" smd rect (at 0.25 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "/WiFi_Display/EPD_CS") (pinfunction "Pin_12") (pintype "passive") (tstamp 928ee37c-0cb6-413d-9f51-629f33a6ba0b))
    (pad "13" smd rect (at -0.25 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 38 "/WiFi_Display/EPD_SCLK") (pinfunction "Pin_13") (pintype "passive") (tstamp a39ecece-979f-4f5c-aff3-83e5c4280482))
    (pad "14" smd rect (at -0.75 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "/WiFi_Display/EPD_SDI") (pinfunction "Pin_14") (pintype "passive") (tstamp a0ae1e37-0c56-454d-9d9d-ef5045a97ce8))
    (pad "15" smd rect (at -1.25 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "VDD") (pinfunction "Pin_15") (pintype "passive") (tstamp 38b1daaf-8dd8-45a8-b42b-0b38a8893fed))
    (pad "16" smd rect (at -1.75 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "VDD") (pinfunction "Pin_16") (pintype "passive") (tstamp e102e0ed-c731-4751-a432-c3583b7c9a1f))
    (pad "17" smd rect (at -2.25 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Pin_17") (pintype "passive") (tstamp e021bed0-e5ac-4cf4-9b2e-a0e07aafd52d))
    (pad "18" smd rect (at -2.75 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "Net-(C29-Pad2)") (pinfunction "Pin_18") (pintype "passive") (tstamp a6f4f86a-5b80-4e6f-bdbf-36599fb28daf))
    (pad "19" smd rect (at -3.25 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "Net-(C24-Pad2)") (pinfunction "Pin_19") (pintype "passive") (tstamp 15b815b0-6456-4221-be25-0e020c8ddd67))
    (pad "20" smd rect (at -3.75 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "Net-(C30-Pad2)") (pinfunction "Pin_20") (pintype "passive") (tstamp 453a2347-3353-4215-9c4d-46177ae3dc2c))
    (pad "21" smd rect (at -4.25 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "/WiFi_Display/PREVGH") (pinfunction "Pin_21") (pintype "passive") (tstamp 832608e3-3c1e-4061-9c00-b068f3eb3d62))
    (pad "22" smd rect (at -4.75 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "Net-(C31-Pad2)") (pinfunction "Pin_22") (pintype "passive") (tstamp 4d547913-abc4-4606-90a7-2eed61bbb55e))
    (pad "23" smd rect (at -5.25 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "/WiFi_Display/PREVGL") (pinfunction "Pin_23") (pintype "passive") (tstamp 17c715c4-c689-4e34-a12f-08cb598fc967))
    (pad "24" smd rect (at -5.75 0 90) (size 0.3 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "Net-(C32-Pad2)") (pinfunction "Pin_24") (pintype "passive") (tstamp 8d48f40c-8178-498b-8803-b1b6e7434f9a))
    (pad "MP" smd rect (at -7.4 -2.35 270) (size 2 3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "MountPin") (pintype "passive") (tstamp 495827f0-5b44-4444-a781-edc2547faaee))
    (pad "MP" smd rect (at 7.4 -2.35 270) (size 2 3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "MountPin") (pintype "passive") (tstamp 6232f840-56ce-4f2a-9ed5-eb5bbe05647d))
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp a97790f4-8eb7-4798-9001-bf7b8ccaa31b)
    (at 80.09 114.98 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/52292911-df09-41d8-8302-b073853448b2")
    (attr smd)
    (fp_text reference "R6" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 04ab4e42-ed35-49d8-aa83-8ca1715cf2ed)
    )
    (fp_text value "350R" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 804a9ab9-6b40-4b2c-a5dc-f7adead5d6d0)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp e7352185-251b-4c3e-b407-9cdd96c382d0)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp ad4867ff-605a-4b7e-8e52-8c3bf4a003af))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp cb5e63d7-8f1b-4f05-a20d-9b46f9c56684))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 09267bb6-7088-4265-9359-862b0c4df6fa))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 50fa5d55-7085-44cf-a391-18454e5531ed))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp aa333ef5-bfa0-49c0-8a82-650e75856c55))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp dd0982c8-4c71-4f8f-9c2f-2bc76efe93c2))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 5da14cf2-201c-4a6f-ab97-1f5c2e4cfa5f))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 93e1dd29-1d20-4129-aada-f2ab00ec5485))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 9cb07d34-0cd8-4543-b7da-5dc9896cb79e))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp b9666282-1e05-4f76-b531-5120baef8f70))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(D1-Pad3)") (pintype "passive") (tstamp 8be1b51e-7666-403b-9ae3-f35f40c03e66))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 44 "/Sensor_Controller/LED_G") (pintype "passive") (tstamp c398c749-b1cd-45e3-bb82-b498eb606dde))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp a98105ab-00fb-497a-b386-34dd4b968be3)
    (at 46.98 136.92 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/7d8b0c60-4781-4aae-a53d-c586cbf927ed")
    (attr smd)
    (fp_text reference "C20" (at 0 1.16) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp ce171eab-a480-4ce9-969e-540871619188)
    )
    (fp_text value "100nF" (at 0 -1.16) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 997c2b86-e823-445e-9560-ab4d47aa2c19)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
      (tstamp 8a9e0411-442c-4a5e-a3ea-38c656c77b22)
    )
    (fp_line (start -0.107836 0.36) (end 0.107836 0.36) (layer "B.SilkS") (width 0.12) (tstamp 5a6a08ce-d607-46ba-9076-0b266002b2ec))
    (fp_line (start -0.107836 -0.36) (end 0.107836 -0.36) (layer "B.SilkS") (width 0.12) (tstamp a749317a-6047-4d75-92cf-45ed130d88c9))
    (fp_line (start -0.91 -0.46) (end -0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 7880aeac-7156-4df1-87d5-21b0aee450fe))
    (fp_line (start 0.91 -0.46) (end -0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp d98db492-254c-468d-ab85-f09e70938da9))
    (fp_line (start 0.91 0.46) (end 0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp ddf15e8d-3103-4c27-ba61-27ff64d5bb66))
    (fp_line (start -0.91 0.46) (end 0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp fae61bc3-41da-45d5-a79e-fe85b507ebf6))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 1dfc0f58-20bc-484b-af3a-b109a9c844ee))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 4c4e6c83-2bbe-4579-af24-b59d284256a9))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 6338ebc0-33fd-4463-afb0-3cba177a64c0))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 9afae567-0717-4ae1-98b7-b3ce4e60e6a0))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(C20-Pad1)") (pintype "passive") (tstamp 65d7769a-f785-44e4-9069-f47a76d16a33))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp c68639ab-ac48-4c2c-b10a-fbe7b2c7a174))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp a9cd9147-a9b6-41cd-81b9-a24e33a9227d)
    (at 178.3 111.1 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/2615342f-3cc9-47ef-8bcb-532586fcdd97")
    (attr smd)
    (fp_text reference "R26" (at 0 1.43 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e7709e1e-d553-4f25-9c48-3d38e60ca0d8)
    )
    (fp_text value "2R/0.5%" (at 0 -1.43 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e5d003f7-8e88-4216-95e1-4ce79308ddcf)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp ae7b7483-33ce-4b51-a09f-5cf1847ca0dd)
    )
    (fp_line (start -0.237258 -0.5225) (end 0.237258 -0.5225) (layer "B.SilkS") (width 0.12) (tstamp 5af1ba78-751b-45a4-b81f-2acc639b6451))
    (fp_line (start -0.237258 0.5225) (end 0.237258 0.5225) (layer "B.SilkS") (width 0.12) (tstamp a0d01b50-4bd3-45ba-b2d8-6b6ca69916f0))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 3c80a748-6a0c-4510-85f1-455029d19a86))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 781cd9cb-a5f4-4d74-8d28-6f3c9b19b1b3))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 7a3c6bb1-e643-4ae8-b7bb-2cd8786467b6))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 8fe31c17-4ffb-4a9a-b5c2-abc618648b08))
    (fp_line (start 0.8 0.4125) (end 0.8 -0.4125) (layer "B.Fab") (width 0.1) (tstamp 514ebca3-be25-4279-902b-9fbddc053051))
    (fp_line (start 0.8 -0.4125) (end -0.8 -0.4125) (layer "B.Fab") (width 0.1) (tstamp 5d225da1-77f1-4c3c-8fe3-b050ed0f29a0))
    (fp_line (start -0.8 -0.4125) (end -0.8 0.4125) (layer "B.Fab") (width 0.1) (tstamp 5fe89951-89c4-4325-970a-50525f0a0e8f))
    (fp_line (start -0.8 0.4125) (end 0.8 0.4125) (layer "B.Fab") (width 0.1) (tstamp 6e354681-82bd-40fc-87d6-f32aa59933da))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 28 "/Power_Management/LED_K") (pintype "passive") (tstamp e4be497d-ecea-4503-be1f-d889729ebb75))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 78f98a21-5734-4d4b-98bb-8a740223bce3))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp aa78f927-42d8-4ba7-b3ae-f1bcdf880f70)
    (at 75.98 124.92 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/6c84cf61-52c7-4b7a-9c9e-ec40be31c6d8")
    (attr smd)
    (fp_text reference "C19" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 07f03192-3ebb-4e88-a680-1a00758dbfda)
    )
    (fp_text value "10uF" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 9ac2d23a-cedf-42e1-a18a-b3ac5218f97a)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 1739d637-947d-4642-aff2-fe8088ebadef)
    )
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp 7d02a602-fa8d-4815-a50b-194d18067601))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp 9ec8b252-ceb0-452d-9593-36c933a32592))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 055c38a3-3c92-476f-af5e-7a4de2926680))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 4826952e-9a7c-469e-a126-4250d3de3a4a))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 64fdb7fe-1fbd-4c9e-b07b-20c53d43468f))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp e7a98667-41e4-4dbd-8606-5398de23bf4f))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp b4b7038c-5265-46ab-ad83-aadc2d9e5e8a))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp ea0fffa4-b48b-4624-908d-d36cfb3d1ec6))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp fe08190e-8cd1-4535-80e3-b3a8b22efde0))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp fee7ada3-70b7-4a0f-818e-b4db437411e2))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "VDD") (pintype "passive") (tstamp c475a6fb-1936-4569-a182-ca9a79efae63))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 6b247820-a2e0-4240-ad14-c6a7ee767403))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp abc34439-9b02-4022-a81e-62a8cd8854da)
    (at 78.45 112.99 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/5bb8fc73-3b84-4fec-a5b9-236b7a12debc")
    (attr smd)
    (fp_text reference "R4" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 3e026644-7cd5-4619-871f-c201838e1d58)
    )
    (fp_text value "100k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 253d4a1b-4d38-401d-8530-f379c84e1ac6)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp fc0b3927-d4fe-4397-aef5-2d521568c534)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 6f2943e6-f5a8-4522-9c81-5250a5cca95b))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp ed7115b3-29a6-4eac-9244-b2c273a72de7))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 0199e30d-eb6f-4e4f-8aac-41d14eb6770f))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 1a834adc-0fd8-4ed9-8089-5d245415ae13))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp d727613f-be10-405d-bd08-19267bede21b))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp dba114bf-98e9-4f5b-a9dc-02193cc39000))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 4372a5e2-085e-4816-a52a-36848a533cff))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 712b8bd1-a02e-4272-b3f2-f2be0b71d11f))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp c414cc05-0852-4dec-821d-2c79c61fed3c))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp e4620475-5ddc-4219-977b-796ed2eed581))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp 12dd37ba-4fb9-4cf9-bb3b-c5e34558af6d))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/Sensor_Controller/LPC_~{RST}") (pintype "passive") (tstamp 616010f7-b11e-4a11-b933-942f4e186999))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp b0453f78-a608-49a3-b8b3-288a0dfc0552)
    (at 69.56 124.14 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/bb143e55-5b21-48df-8ac4-9dd5a084e89f")
    (attr smd)
    (fp_text reference "R27" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 575bd10e-6bc2-4b0f-aca9-9c3f2d87fcdd)
    )
    (fp_text value "22.8k/1%" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 876c22fe-2498-44d7-98f2-d9aff4eabb0c)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp a5d08036-df94-457d-a2d1-78d7f017d5b3)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 339d8b78-c73a-409d-a04b-42e84cfb1eb9))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp ad47806f-7d4d-49f2-b32a-e5aaca29e374))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 251ee8ea-d8e2-437b-889a-b17bbf8d0cf2))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 35aba278-1584-4fa5-b0de-d9d13621c627))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp c6bbe283-68b2-4dcf-a953-ee33c6ef2331))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp eb6236b9-4f1f-415b-b261-b822f433a05d))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 5dc2f7b8-a63b-41c0-9cd6-5bc7b0edc6c9))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 938e3f21-dbc5-4e6f-a01e-076aab60d9b4))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp cd0b3cdc-99c0-4430-a1a0-2f450fba1953))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp fb37a393-c5ef-4707-a19d-417c0818921d))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "VDD") (pintype "passive") (tstamp 27d37ada-0f4c-4967-a2b8-23829ff4d071))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(R27-Pad2)") (pintype "passive") (tstamp d402f73e-9894-4c4b-a929-a1c5d12b078b))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp b4715512-396c-483a-86ad-71688915c951)
    (at 35.75 119.39 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/c423217a-4e4a-4996-b7c2-cac25b2f8b20")
    (attr smd)
    (fp_text reference "R5" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 38e7b483-06c8-46b6-a2c9-42ec3561c1a6)
    )
    (fp_text value "260R" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7c914bc7-f25a-45cb-af8d-5093a637a37b)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp ece799b2-9bce-4c84-8154-0a622516a37d)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 4d6e1fa8-354f-4fb1-ada1-f57eea551837))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp e909e3e7-fbc0-40a4-b542-58feeef9e0df))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 502bc288-cece-491b-9934-11f6e5b0cda5))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp c199d2ff-bc10-4eb0-9883-0b902d221f8c))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp e273a2e8-4d30-4795-99d7-88f9b7c66d92))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp f5244595-5b58-4db3-a3ac-1620ed028c5c))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 122ec572-9553-42b0-9234-f185a938219d))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 51bf06b6-f86a-44e8-bc01-720c8a33464f))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp e8e3f326-5ecb-4fb7-90f9-8ea48f477d7f))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp ebac0124-5821-4cdc-af8b-10bdbad850df))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(D1-Pad2)") (pintype "passive") (tstamp 4dc8104c-8ef7-49e8-8a43-857fbe6152a9))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 43 "/Sensor_Controller/LED_R") (pintype "passive") (tstamp 73263f08-97d1-482d-92f9-920b2442fc26))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp b59d7c25-3678-43d4-8a78-9fb304e6c001)
    (at 34.48 123.37 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/f7622d79-b5a7-44a2-937d-b5c487b37ebf")
    (attr smd)
    (fp_text reference "R8" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 726ea5ff-c760-4444-a2ad-2b4f51b697ea)
    )
    (fp_text value "100k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 409a88b2-b7e7-483c-8337-a0b3101146fd)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 7850b36e-9f11-48fc-be5a-466fc700edd5)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 24bbe7b3-2794-400a-adc4-226cde27db2d))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp a4e348c2-8730-4d2a-b857-790d252e414f))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 2dad0fa6-bffb-4f7d-a4b8-2ba94d358685))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 443b6076-53d6-41f7-9647-4652df201587))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 91a026ae-7f2f-4fd9-8819-f2a059abf8f0))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp e0440ffa-460d-4d10-8f86-243d346eba59))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 07affaa3-1124-46a9-aeb2-ba645cf02e42))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 1831d5d9-90b5-4f4f-8363-81cf0508da46))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 354528e9-5e4e-45eb-b00d-12c6fc0f3eb3))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp b91d9cc8-6c02-4975-98c6-328a1d85ed41))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp b4b0f20a-6548-41d6-bccc-9ed9bc0c8b92))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 46 "/Sensor_Controller/LPC_SWDIO") (pintype "passive") (tstamp 25e4deaf-7a4d-4afe-aace-591f6b9d57b3))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_USB:USB_C_Receptacle_XKB_U262-16XN-4BVC11" (layer "B.Cu")
    (tedit 5E1305FC) (tstamp b7f70fd6-816a-4b8b-b891-5d04a3af75d5)
    (at 192.9 154.2 -90)
    (descr "USB Type C, right-angle, SMT, https://datasheet.lcsc.com/szlcsc/1811141824_XKB-Enterprise-U262-161N-4BVC11_C319148.pdf")
    (tags "USB C Type-C Receptacle SMD")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/42c410e1-c833-4f75-9dc0-4b6bca6833e1")
    (attr smd)
    (fp_text reference "J2" (at 0 5.715 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5c4dbd5a-14bc-4f3b-bc0f-d83b7b081c93)
    )
    (fp_text value "XKB-U262-161N-4BS165" (at 0 -4.935 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp aa1554d4-4f73-4f1c-8bc6-54506943dc8f)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 99393fdd-d9e9-45ed-8f76-b7e0c80f8d9d)
    )
    (fp_line (start 4.58 -3.785) (end -4.58 -3.785) (layer "B.SilkS") (width 0.12) (tstamp 375b2832-e9b5-43d4-9a34-673e25b14962))
    (fp_line (start 4.58 -2.08) (end 4.58 -3.785) (layer "B.SilkS") (width 0.12) (tstamp 74c81772-684b-4abf-bde0-12994031e7f6))
    (fp_line (start 4.58 -0.07) (end 4.58 1.85) (layer "B.SilkS") (width 0.12) (tstamp b0a6865c-d709-4d1c-83a1-ad74081e3062))
    (fp_line (start -4.58 1.85) (end -4.58 -0.07) (layer "B.SilkS") (width 0.12) (tstamp df3916ea-4b4f-4a3d-a393-37a053aea798))
    (fp_line (start -4.58 -3.785) (end -4.58 -2.08) (layer "B.SilkS") (width 0.12) (tstamp ecddc703-16b3-43fd-97bb-af4b6db2c3a8))
    (fp_line (start -5.32 -4.18) (end -5.32 4.75) (layer "B.CrtYd") (width 0.05) (tstamp 2f909e82-e446-4d1a-bbb5-d35f65bb1fb7))
    (fp_line (start 5.32 -4.18) (end -5.32 -4.18) (layer "B.CrtYd") (width 0.05) (tstamp 38bbcad3-1ee2-444f-89bd-b15e087075e6))
    (fp_line (start -5.32 4.75) (end 5.32 4.75) (layer "B.CrtYd") (width 0.05) (tstamp 68cedb9a-8f82-4d47-b55f-99e44b9ca86d))
    (fp_line (start 5.32 4.75) (end 5.32 -4.18) (layer "B.CrtYd") (width 0.05) (tstamp d747c55e-b310-40ac-b572-02fb97a04fd6))
    (fp_line (start 4.47 -3.675) (end 4.47 3.675) (layer "B.Fab") (width 0.1) (tstamp 35efb65d-9b6b-4c63-bdd4-a8d6a1d5f041))
    (fp_line (start -4.47 3.675) (end -4.47 -3.675) (layer "B.Fab") (width 0.1) (tstamp b7b8ba21-fe4f-4afb-b9cb-713eeb02910f))
    (fp_line (start -4.47 3.675) (end 4.47 3.675) (layer "B.Fab") (width 0.1) (tstamp d8770668-a851-40d2-bf03-7056e4c36bd1))
    (fp_line (start -4.47 -3.675) (end 4.47 -3.675) (layer "B.Fab") (width 0.1) (tstamp ee6cbbd4-e29e-4d6b-8ed5-1ccd7b42a8d0))
    (pad "" np_thru_hole circle (at 2.89 2.605 270) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask) (tstamp 9368da43-3947-4055-9870-ec822283eff6))
    (pad "" np_thru_hole circle (at -2.89 2.605 270) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask) (tstamp f967adad-9500-405b-ac60-ecb143e524fd))
    (pad "A1" smd rect (at -3.35 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive") (tstamp 08d82666-e741-4e31-a0fb-9e5a2bca0769))
    (pad "A4" smd rect (at -2.55 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "VBUS") (pinfunction "VBUS") (pintype "passive") (tstamp c05a0ec3-fbf8-41ac-aa18-480168705788))
    (pad "A5" smd rect (at -1.25 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 64 "Net-(J2-PadA5)") (pinfunction "CC1") (pintype "bidirectional") (tstamp acbf36aa-611d-4f06-a181-d8d43dd89c22))
    (pad "A6" smd rect (at -0.25 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 86 "/WiFi_Display/USB_D+") (pinfunction "D+") (pintype "bidirectional") (tstamp c74b463c-d943-4ce5-85ab-0a86a5370994))
    (pad "A7" smd rect (at 0.25 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 87 "/WiFi_Display/USB_D-") (pinfunction "D-") (pintype "bidirectional") (tstamp 9c33fbec-276d-4929-af11-b9bbd4453b76))
    (pad "A8" smd rect (at 1.25 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 100 "/WiFi_Display/UART_RX") (pinfunction "SBU1") (pintype "bidirectional") (tstamp a4e663d1-908e-40a8-b408-28ee0f79a882))
    (pad "A9" smd rect (at 2.55 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "VBUS") (pinfunction "VBUS") (pintype "passive") (tstamp e3b7a090-8536-4322-9158-0c23192e8bd6))
    (pad "A12" smd rect (at 3.35 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive") (tstamp 347092df-520a-4304-bce1-0b546f56ceaf))
    (pad "B1" smd rect (at 3.05 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive") (tstamp ca89f65e-e30f-49f2-8616-15c5ddb4bfbc))
    (pad "B4" smd rect (at 2.25 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "VBUS") (pinfunction "VBUS") (pintype "passive") (tstamp 919aa72a-5cdd-4e47-8834-99557c6742a4))
    (pad "B5" smd rect (at 1.75 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 65 "Net-(J2-PadB5)") (pinfunction "CC2") (pintype "bidirectional") (tstamp 45f54814-05ec-4929-bb16-c4fd314dd07c))
    (pad "B6" smd rect (at 0.75 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 86 "/WiFi_Display/USB_D+") (pinfunction "D+") (pintype "bidirectional") (tstamp 606ff535-0c7c-41f0-b6dd-4bc7d807146b))
    (pad "B7" smd rect (at -0.75 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 87 "/WiFi_Display/USB_D-") (pinfunction "D-") (pintype "bidirectional") (tstamp 78b2b580-612b-4e2f-8fdc-f04e6080572a))
    (pad "B8" smd rect (at -1.75 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 101 "/WiFi_Display/UART_TX") (pinfunction "SBU2") (pintype "bidirectional") (tstamp 8e3267b9-f86b-4212-9570-237be7cdc9f7))
    (pad "B9" smd rect (at -2.25 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "VBUS") (pinfunction "VBUS") (pintype "passive") (tstamp 9fd37cf2-0e7b-4c81-8b12-88fc1bd4abdd))
    (pad "B12" smd rect (at -3.05 3.67 270) (size 0.3 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive") (tstamp 237108a2-a73b-4e83-8ad0-871ad2a9d59e))
    (pad "S1" thru_hole oval (at 4.32 -1.075 270) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive") (tstamp 0c5cdebb-154c-4f4a-8ce7-a029b1f7db98))
    (pad "S1" thru_hole oval (at 4.32 3.105 270) (size 1 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive") (tstamp 2b5339b6-5264-4f38-b713-c1872113fa99))
    (pad "S1" thru_hole oval (at -4.32 3.105 270) (size 1 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive") (tstamp adbb9b3b-cc5b-4215-9bee-0e03177f3698))
    (pad "S1" thru_hole oval (at -4.32 -1.075 270) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive") (tstamp b0ca2fa4-f91d-4492-b244-c92b3f1ad2ec))
    (model "${KICAD6_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_XKB_U262-16XN-4BVC11.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_SO:MSOP-8_3x3mm_P0.65mm" (layer "B.Cu")
    (tedit 5E509FDD) (tstamp bc04bda0-beeb-4a95-ab89-10189cc0f580)
    (at 117.4 134.7 180)
    (descr "MSOP, 8 Pin (https://www.jedec.org/system/files/docs/mo-187F.pdf variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "MSOP SO")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/5e31b07e-6edf-49dd-8861-29f3783f96cd")
    (attr smd)
    (fp_text reference "U3" (at 0 2.45) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 455e28d1-4e8d-4772-8f23-fea0d6086aa6)
    )
    (fp_text value "BL24C256A-SFRC" (at 0 -2.45) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f2e1a211-0a00-4015-aad3-e01187629cbb)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.75 0.75) (thickness 0.11)) (justify mirror))
      (tstamp c0ec6b07-f6a0-45db-8719-f14db3ebd5d5)
    )
    (fp_line (start 0 1.61) (end 1.5 1.61) (layer "B.SilkS") (width 0.12) (tstamp 97b6051f-adaa-4771-85a7-f92a46668f23))
    (fp_line (start 0 -1.61) (end -1.5 -1.61) (layer "B.SilkS") (width 0.12) (tstamp aeb293c5-8472-4d12-b4a4-40674335df21))
    (fp_line (start 0 1.61) (end -2.925 1.61) (layer "B.SilkS") (width 0.12) (tstamp d349f801-6410-4b6f-9bfd-d178b825c942))
    (fp_line (start 0 -1.61) (end 1.5 -1.61) (layer "B.SilkS") (width 0.12) (tstamp ed7f323a-9a83-4f55-bc0e-ed9216e11cb1))
    (fp_line (start -3.18 1.75) (end -3.18 -1.75) (layer "B.CrtYd") (width 0.05) (tstamp 272f8220-b7bc-49b2-a347-8fa9938bec47))
    (fp_line (start 3.18 1.75) (end -3.18 1.75) (layer "B.CrtYd") (width 0.05) (tstamp 30ad2469-2625-4b2b-a99a-b796d50866de))
    (fp_line (start -3.18 -1.75) (end 3.18 -1.75) (layer "B.CrtYd") (width 0.05) (tstamp a1424326-750b-4088-9fe5-7fa64ce71460))
    (fp_line (start 3.18 -1.75) (end 3.18 1.75) (layer "B.CrtYd") (width 0.05) (tstamp c89eeb5a-d0b8-4936-b71d-a40c8bbf13d7))
    (fp_line (start -0.75 1.5) (end 1.5 1.5) (layer "B.Fab") (width 0.1) (tstamp 4ccd8e5d-acb3-4bc8-aa0f-08b449537fa2))
    (fp_line (start -1.5 -1.5) (end -1.5 0.75) (layer "B.Fab") (width 0.1) (tstamp 5338764b-7f7a-4f22-8037-4cdaf8f59161))
    (fp_line (start 1.5 1.5) (end 1.5 -1.5) (layer "B.Fab") (width 0.1) (tstamp 550f4f34-b804-42da-a740-0e221644f4cd))
    (fp_line (start -1.5 0.75) (end -0.75 1.5) (layer "B.Fab") (width 0.1) (tstamp c6727eb7-7f49-4efa-9e85-2bd615951340))
    (fp_line (start 1.5 -1.5) (end -1.5 -1.5) (layer "B.Fab") (width 0.1) (tstamp e206a525-d827-4059-8706-1551a778b857))
    (pad "1" smd roundrect (at -2.1125 0.975 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "A0") (pintype "input") (tstamp c71f0662-f7ee-4c2e-a23e-8f8bf8836425))
    (pad "2" smd roundrect (at -2.1125 0.325 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "A1") (pintype "input") (tstamp 4ec37775-b337-4eb3-95f4-b43bbc03f14c))
    (pad "3" smd roundrect (at -2.1125 -0.325 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "A2") (pintype "input") (tstamp 731ce20a-5584-4181-b2df-933b2be41657))
    (pad "4" smd roundrect (at -2.1125 -0.975 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 454cf39f-5076-489c-b17c-93499213524e))
    (pad "5" smd roundrect (at 2.1125 -0.975 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 41 "/Sensor_Controller/I2C_SDA") (pinfunction "SDA") (pintype "bidirectional") (tstamp 2336c947-65cf-409b-86b1-e13b16834329))
    (pad "6" smd roundrect (at 2.1125 -0.325 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 42 "/Sensor_Controller/I2C_SCL") (pinfunction "SCL") (pintype "input") (tstamp 95971152-5d60-4f70-81e1-016073990cd5))
    (pad "7" smd roundrect (at 2.1125 0.325 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "WP") (pintype "input") (tstamp fe3f84ae-b0d3-4c07-9af6-ab27ca704eba))
    (pad "8" smd roundrect (at 2.1125 0.975 180) (size 1.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pinfunction "VCC") (pintype "power_in") (tstamp ecdbe1ee-e4aa-49c9-8aa8-3daf8b3a620c))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/MSOP-8_3x3mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp bc7df6c8-11c9-4287-8edb-a0a9670ba4dd)
    (at 176.1 107.5 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/9c3337a3-b1d9-42c7-b871-ae280cc7c859")
    (attr smd)
    (fp_text reference "C17" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e5d20853-ef6e-4ff6-84df-4840c254d4c6)
    )
    (fp_text value "10uF" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 15d19ea4-2ed4-4099-969c-8367dc310697)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp a0b414ac-f98d-4991-ac82-f86e0c53a215)
    )
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp 0fd825f9-b38e-45a6-a176-4dd8b159ebc2))
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp 866d035a-16af-48f8-8a39-63218a4a8cae))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 9f244187-5856-4e32-bd71-b2acb861d950))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp be42f4cb-53be-44f9-8ad7-b8b9c564666b))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp bfb18f7d-01c8-4f78-bdb8-2f8904e462e6))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp ede81694-6810-4c22-9f13-19703ec80b12))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 21a29a99-46e4-4295-b8c0-acef8865107c))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 5510f931-ba0c-47c4-a00c-9ad1c5b3979c))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 8d197a8c-1ed9-4a72-96cd-6968203b4d19))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp afc50c62-6dce-4002-a19d-cca66d2277a9))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/Power_Management/LED_A") (pintype "passive") (tstamp 681eb4eb-f03c-4174-b8ed-3f71bd63a62c))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 8780721f-f8db-4b65-9b1a-947e65eb9436))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp be58c61b-9ebb-4fd7-9c53-227358ce1677)
    (at 90.64 128.47 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/568992a3-2d20-4370-8147-67be49b51947")
    (attr smd)
    (fp_text reference "C3" (at 0 1.16) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp b8bb1f14-d2e5-404e-81c7-12d70e5a7fb2)
    )
    (fp_text value "100nF" (at 0 -1.16) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a97e9da6-2ed8-4f5d-9c32-78d88cf03d94)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
      (tstamp 5078d587-0602-483e-bb0c-cdf618404d19)
    )
    (fp_line (start -0.107836 -0.36) (end 0.107836 -0.36) (layer "B.SilkS") (width 0.12) (tstamp 26159000-0b5c-4630-b159-6b032ca54cb5))
    (fp_line (start -0.107836 0.36) (end 0.107836 0.36) (layer "B.SilkS") (width 0.12) (tstamp 754ff76f-39f4-4f3b-86e3-eb1699bb5b73))
    (fp_line (start 0.91 -0.46) (end -0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 14700925-69e9-410f-94ef-0ffcebcf535f))
    (fp_line (start -0.91 -0.46) (end -0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 31a73d5f-3b51-4d23-80bc-eceb1f4be525))
    (fp_line (start -0.91 0.46) (end 0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 58c35daf-6b69-4560-89a2-fa494b78862d))
    (fp_line (start 0.91 0.46) (end 0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 9cacdd15-1e28-4310-9f56-548afa63c61d))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 893d6e3f-84c4-4a3f-8138-5bee4b6a0b33))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 94de779f-e6f7-4cde-a971-37d0c61150a3))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp aa18482a-1c96-4fc9-948c-4696fcafdf50))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp c98c3e74-722a-44b4-a012-1ac944523d3c))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp 6ab25c23-43df-4d21-b98b-af7ad986d0fd))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 6a1e4fa7-6a6d-4658-a371-e823c77ec520))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_LGA:LGA-14_3x2.5mm_P0.5mm_LayoutBorder3x4y" (layer "B.Cu")
    (tedit 5D9F7937) (tstamp bedb2d63-7071-4452-9cee-8fa66de5b0f1)
    (at 136.2 129.6 180)
    (descr "LGA, 14 Pin (http://www.st.com/resource/en/datasheet/lsm6ds3.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "LGA NoLead")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/06e56a77-f6fa-4386-b7c1-79cf55ed810a")
    (attr smd)
    (fp_text reference "U1" (at 0 2.2) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp b6a76da6-b7b9-46e1-9b5e-860c2d2f07b1)
    )
    (fp_text value "LSM6DS3" (at 0 -2.2) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f9c7ece3-c077-4b01-b5a0-8ce8ab1cb937)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.75 0.75) (thickness 0.11)) (justify mirror))
      (tstamp 183a4388-85a1-45b6-b94c-ae2299be7ce1)
    )
    (fp_line (start -0.96 -1.36) (end -1.61 -1.36) (layer "B.SilkS") (width 0.12) (tstamp 23297984-5a74-4021-a865-1dea68fea909))
    (fp_line (start 0.96 -1.36) (end 1.61 -1.36) (layer "B.SilkS") (width 0.12) (tstamp 8851f350-c031-42d4-b5cb-a80ea78d2a4a))
    (fp_line (start -0.96 1.36) (end -1.61 1.36) (layer "B.SilkS") (width 0.12) (tstamp 8ef68c83-cde6-4d1f-8c90-1f0347409c3c))
    (fp_line (start -1.61 -1.36) (end -1.61 -1.21) (layer "B.SilkS") (width 0.12) (tstamp 98971603-1f92-4710-83e0-efd3d91c36e1))
    (fp_line (start 1.61 1.36) (end 1.61 1.21) (layer "B.SilkS") (width 0.12) (tstamp 9e52bf7f-8541-4eea-8cac-7f043ef74d4d))
    (fp_line (start 1.61 -1.36) (end 1.61 -1.21) (layer "B.SilkS") (width 0.12) (tstamp ab4898f6-ec0a-4974-9cfb-bd6a0357bfdf))
    (fp_line (start 0.96 1.36) (end 1.61 1.36) (layer "B.SilkS") (width 0.12) (tstamp fb75f1f3-6ed6-4808-9dbe-bc66a95a093e))
    (fp_line (start -1.75 -1.5) (end 1.75 -1.5) (layer "B.CrtYd") (width 0.05) (tstamp 34130493-82ca-4e99-a5ac-cb51224ad304))
    (fp_line (start 1.75 -1.5) (end 1.75 1.5) (layer "B.CrtYd") (width 0.05) (tstamp 6e02743f-ff1d-4d30-9a24-5823fa3ae574))
    (fp_line (start 1.75 1.5) (end -1.75 1.5) (layer "B.CrtYd") (width 0.05) (tstamp 856f1b3a-d2c9-4de4-8113-81a128eed687))
    (fp_line (start -1.75 1.5) (end -1.75 -1.5) (layer "B.CrtYd") (width 0.05) (tstamp d80d5d83-348e-444e-b669-de0293714ca3))
    (fp_line (start -1.5 -1.25) (end -1.5 0.625) (layer "B.Fab") (width 0.1) (tstamp 322e78d1-e3ce-4886-97b7-2b737a1e22cc))
    (fp_line (start 1.5 1.25) (end 1.5 -1.25) (layer "B.Fab") (width 0.1) (tstamp 4660cd09-2f17-46c2-aaf8-a2a8cc253eb4))
    (fp_line (start -1.5 0.625) (end -0.875 1.25) (layer "B.Fab") (width 0.1) (tstamp 8d182b79-1a63-453f-817c-37863dc281cb))
    (fp_line (start 1.5 -1.25) (end -1.5 -1.25) (layer "B.Fab") (width 0.1) (tstamp a7611074-070b-4af3-9627-e74c77580f76))
    (fp_line (start -0.875 1.25) (end 1.5 1.25) (layer "B.Fab") (width 0.1) (tstamp dcb0b219-61c7-49e0-9069-3a695bc6af58))
    (pad "1" smd custom (at -1.1625 0.75 180) (size 0.223223 0.223223) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 67 "/Sensor_Controller/LSM_A0") (pinfunction "SDO/SA0") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.2375 -0.081066)
            (xy 0.2375 -0.125)
            (xy -0.2375 -0.125)
            (xy -0.2375 0.125)
            (xy 0.031434 0.125)
          ) (width 0.15) (fill yes))
      ) (tstamp 994f531d-d3e5-40db-92b6-cd52c7bf32c7))
    (pad "2" smd roundrect (at -1.1625 0.25 180) (size 0.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "SDX") (pintype "bidirectional") (tstamp 301e9ba3-d757-4d65-8442-c56aef0d5d9d))
    (pad "3" smd roundrect (at -1.1625 -0.25 180) (size 0.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "SCX") (pintype "input") (tstamp 81c88955-83cc-4e3d-b1df-9bf574602497))
    (pad "4" smd custom (at -1.1625 -0.75 180) (size 0.223223 0.223223) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 68 "/Sensor_Controller/LSM_INT1") (pinfunction "INT1") (pintype "output")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.2375 0.081066)
            (xy 0.031434 -0.125)
            (xy -0.2375 -0.125)
            (xy -0.2375 0.125)
            (xy 0.2375 0.125)
          ) (width 0.15) (fill yes))
      ) (tstamp 07eab6db-6493-4ba2-99f6-f9759ab1b8c0))
    (pad "5" smd custom (at -0.5 -0.9125 180) (size 0.223223 0.223223) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "VDDF") (pinfunction "VDDIO") (pintype "power_in")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.125 -0.2375)
            (xy -0.125 -0.2375)
            (xy -0.125 0.031434)
            (xy 0.081066 0.2375)
            (xy 0.125 0.2375)
          ) (width 0.15) (fill yes))
      ) (tstamp 6b4a3c60-cf1a-4507-834d-8587eeda1bb0))
    (pad "6" smd roundrect (at 0 -0.9125 180) (size 0.4 0.625) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 37169c03-3ee2-443d-8f34-7b8ee69867f8))
    (pad "7" smd custom (at 0.5 -0.9125 180) (size 0.223223 0.223223) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.125 0.031434)
            (xy 0.125 -0.2375)
            (xy -0.125 -0.2375)
            (xy -0.125 0.2375)
            (xy -0.081066 0.2375)
          ) (width 0.15) (fill yes))
      ) (tstamp 4dc9509d-45f1-4148-9426-81720d1301c7))
    (pad "8" smd custom (at 1.1625 -0.75 180) (size 0.223223 0.223223) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "VDDF") (pinfunction "VDD") (pintype "power_in")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.2375 -0.125)
            (xy -0.031434 -0.125)
            (xy -0.2375 0.081066)
            (xy -0.2375 0.125)
            (xy 0.2375 0.125)
          ) (width 0.15) (fill yes))
      ) (tstamp 3d64f3ed-5957-4107-a249-b281801ed4ae))
    (pad "9" smd roundrect (at 1.1625 -0.25 180) (size 0.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 69 "/Sensor_Controller/LSM_INT2") (pinfunction "INT2") (pintype "output") (tstamp f37710d1-3c6d-49db-a557-89f92f9c6633))
    (pad "10" smd roundrect (at 1.1625 0.25 180) (size 0.625 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 70 "unconnected-(U1-Pad10)") (pinfunction "NC") (pintype "no_connect") (tstamp 2210e876-16ba-43a5-a245-979513e1c7aa))
    (pad "11" smd custom (at 1.1625 0.75 180) (size 0.223223 0.223223) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 71 "unconnected-(U1-Pad11)") (pinfunction "NC") (pintype "no_connect")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.2375 -0.125)
            (xy -0.2375 -0.125)
            (xy -0.2375 -0.081066)
            (xy -0.031434 0.125)
            (xy 0.2375 0.125)
          ) (width 0.15) (fill yes))
      ) (tstamp 80cfcaf7-0915-4f80-bfab-9c8365808da4))
    (pad "12" smd custom (at 0.5 0.9125 180) (size 0.223223 0.223223) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "VDDF") (pinfunction "CS") (pintype "input")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.125 -0.031434)
            (xy -0.081066 -0.2375)
            (xy -0.125 -0.2375)
            (xy -0.125 0.2375)
            (xy 0.125 0.2375)
          ) (width 0.15) (fill yes))
      ) (tstamp c5fef5b8-569a-4bab-a419-ac0b4062a936))
    (pad "13" smd roundrect (at 0 0.9125 180) (size 0.4 0.625) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 42 "/Sensor_Controller/I2C_SCL") (pinfunction "SCL") (pintype "input") (tstamp a5e34a11-ccd5-4bff-9ab3-aa46eb01f715))
    (pad "14" smd custom (at -0.5 0.9125 180) (size 0.223223 0.223223) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 41 "/Sensor_Controller/I2C_SDA") (pinfunction "SDA") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.125 -0.2375)
            (xy 0.081066 -0.2375)
            (xy -0.125 -0.031434)
            (xy -0.125 0.2375)
            (xy 0.125 0.2375)
          ) (width 0.15) (fill yes))
      ) (tstamp 339b5a7b-145b-4619-87d5-9920c0ca7dfd))
    (model "${KICAD6_3DMODEL_DIR}/Package_LGA.3dshapes/LGA-14_3x2.5mm_P0.5mm_LayoutBorder3x4y.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp c18d8f0d-9434-4bfc-bce5-9a4623ea1a5b)
    (at 154 154)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/6e1caec3-a6d0-4a90-9938-6cdd78bb7478")
    (attr smd)
    (fp_text reference "R16" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 83eccd2c-7eca-4030-b440-86dbb3c124c4)
    )
    (fp_text value "2.2k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0345edad-18ee-4c71-bc5d-bb13e9ef823e)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp e8412301-7691-4904-bd9b-8a0fe7b98b4f)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 3c7ac3a4-3b70-4458-b1db-6904a1fadc07))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 84638afd-94ec-4c2a-a87b-c394319e87c3))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 2aed225d-6d7c-4abd-9715-f66423df9118))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 3e1bd748-7cf3-4faf-ad0c-74dc6a9e4eb5))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 5a5523fd-be7e-4e81-a706-2721e820b560))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 7e462183-f4bc-44c5-a69d-f57eca835bd3))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 03781969-6d2e-46ac-88e1-e6cab9bae4be))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 1145946f-b9ce-463a-9fe2-d568af4360be))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 427575de-17d3-4f65-b48a-ecb3d1a28788))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp df4049e8-e0ca-404a-8dc0-bb6845153bd3))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 54 "/Sensor_Controller/CAPT_X2") (pintype "passive") (tstamp f586b135-26dd-4e27-8219-c0bf441648a9))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(R16-Pad2)") (pintype "passive") (tstamp 2c87135e-8ae7-4048-ba8d-f5f66ad911d8))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp c1e82e01-95b3-4e5c-969d-4587a2c9043f)
    (at 143 154)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/c7843172-09e9-4c84-8d8b-9e36fed5d8f0")
    (attr smd)
    (fp_text reference "R14" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp eadea057-473d-4e37-8985-65cdacde671d)
    )
    (fp_text value "2.2k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp ea663bf3-e968-4c88-b337-83185d522047)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 1d3504e6-02f4-407c-b644-8efdec39ba86)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 8806d6ae-19e3-4465-bf3b-a891d10384a6))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 94de928d-f43a-4cc4-bdc3-3168b525cfd7))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 1def6cf0-628c-48e2-abd4-7a201774f452))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 8e1873ce-ccb4-421e-a2a8-783371ca06f1))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 9f128694-0ceb-4581-80d7-81d95cb6f4b5))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp cf748d95-1c1b-4de5-8bc5-8df4c53a2a56))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 360777eb-2a87-4139-b94a-4f0fc45ef2c7))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 491dee5f-f83e-4d78-baac-750faabd4c4c))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 5de8362f-ae7c-4017-ade5-1b7775a84cec))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp a8623c18-8e18-4f84-bcbf-600cb0aed4e8))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(R13-Pad2)") (pintype "passive") (tstamp 07f662b5-c20f-4a5d-8cd9-77f31c4a447d))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(R14-Pad2)") (pintype "passive") (tstamp d9a27493-8ac5-4645-84bb-9e6847f47e4b))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Crystal:Crystal_SMD_MicroCrystal_CM9V-T1A-2Pin_1.6x1.0mm" (layer "B.Cu")
    (tedit 5D24C13B) (tstamp c42b5006-f4b0-409d-a515-1873d308e6ee)
    (at 121.7 138.1 90)
    (descr "SMD Crystal MicroCrystal CM9V-T1A series https://www.microcrystal.com/fileadmin/Media/Products/32kHz/Datasheet/CM9V-T1A.pdf, 1.6x1.0mm^2 package")
    (tags "SMD SMT crystal")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/3188079d-fd99-4090-8af4-8f4aa53c565d")
    (attr smd)
    (fp_text reference "Y1" (at 0 1.7 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 1837caf3-7fe3-483e-a7a9-2ea5ee517e80)
    )
    (fp_text value "32768Hz" (at 0 -1.7 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 1f247c34-0a27-44b5-aa54-7a3039ed43bd)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
      (tstamp 1b9cd306-1bd3-4644-ac3d-7b40cdd0974f)
    )
    (fp_line (start -0.1 -0.7) (end 0.1 -0.7) (layer "B.SilkS") (width 0.12) (tstamp 76bea174-0ea1-455a-b021-16c7cf6e3bc2))
    (fp_line (start -1.1 0.6) (end -1.1 -0.6) (layer "B.SilkS") (width 0.12) (tstamp 81464acb-805b-48c5-9131-2ab11c5c292a))
    (fp_line (start -0.1 0.7) (end 0.1 0.7) (layer "B.SilkS") (width 0.12) (tstamp ae2f132c-21fc-4cfe-8fba-deb49d04c627))
    (fp_line (start 1.2 -0.9) (end 1.2 0.9) (layer "B.CrtYd") (width 0.05) (tstamp 4896135f-9a21-4f0e-99a0-9a09d992db8e))
    (fp_line (start -1.2 0.9) (end -1.2 -0.9) (layer "B.CrtYd") (width 0.05) (tstamp 54a2fa9f-8b45-4429-9d76-23e167da01bc))
    (fp_line (start 1.2 0.9) (end -1.2 0.9) (layer "B.CrtYd") (width 0.05) (tstamp 853cc42e-4723-4367-a57e-f72273ac6389))
    (fp_line (start -1.2 -0.9) (end 1.2 -0.9) (layer "B.CrtYd") (width 0.05) (tstamp ae37a442-db3a-4a90-985a-05feac7170e8))
    (fp_line (start 0.8 -0.5) (end 0.8 0.5) (layer "B.Fab") (width 0.1) (tstamp 18d89673-0571-4f04-89b6-d7ed63ec8164))
    (fp_line (start -0.8 -0.5) (end 0.8 -0.5) (layer "B.Fab") (width 0.1) (tstamp 6158f42f-3f5b-4820-a484-a5bc69e61e4b))
    (fp_line (start 0.8 0.5) (end -0.8 0.5) (layer "B.Fab") (width 0.1) (tstamp 8c7ebcd7-e2bb-4cca-a405-6c030c5d891e))
    (fp_line (start -0.8 0.5) (end -0.8 -0.5) (layer "B.Fab") (width 0.1) (tstamp 94b1d9af-e849-4f22-ad49-e9f2163877cf))
    (fp_line (start -0.8 0) (end -0.3 -0.5) (layer "B.Fab") (width 0.1) (tstamp ecbe5f54-693f-4ab5-b548-c2f66f8d341a))
    (pad "1" smd rect (at -0.6 0 90) (size 0.6 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 83 "Net-(U6-Pad2)") (pinfunction "1") (pintype "passive") (tstamp 43dcb3e3-c7e3-402d-9650-d76d5cd4637f))
    (pad "2" smd rect (at 0.6 0 90) (size 0.6 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "Net-(C11-Pad2)") (pinfunction "2") (pintype "passive") (tstamp 0781190d-9e86-4489-bf64-a4508c48e1a4))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_MicroCrystal_CM9V-T1A-2Pin_1.6x1.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp c5e08c7e-db3c-4398-bb52-ecff9aea122e)
    (at 91.87 126.5 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/aabae4df-ada0-49e1-88d2-524812bcc349")
    (attr smd)
    (fp_text reference "C10" (at 0 1.16) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 04226619-25f5-4888-ad27-e1ebd9da7260)
    )
    (fp_text value "100nF" (at 0 -1.16) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d083ab07-0b7a-4d2d-9631-f25534bebe9e)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
      (tstamp 485114c1-473b-44c4-b2c7-1b46300051b6)
    )
    (fp_line (start -0.107836 -0.36) (end 0.107836 -0.36) (layer "B.SilkS") (width 0.12) (tstamp 2bef97ab-35cf-4bab-8774-fc1dcdf02834))
    (fp_line (start -0.107836 0.36) (end 0.107836 0.36) (layer "B.SilkS") (width 0.12) (tstamp 4b185791-e04f-4147-b794-5389e8cab64c))
    (fp_line (start -0.91 -0.46) (end -0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 09696426-25b8-45d9-a69c-d73c34f7e8ba))
    (fp_line (start 0.91 0.46) (end 0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 715e7338-ee11-482b-8bbe-7a1c583ac087))
    (fp_line (start 0.91 -0.46) (end -0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp ae0a5aac-80d1-434a-b9a2-e0d87beb49dd))
    (fp_line (start -0.91 0.46) (end 0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp ff967518-0d0f-40b5-85e0-af862e63a8f0))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 31d3294e-f4ae-43cf-aa10-681044030ef3))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 352dc4da-0e58-47e3-b153-c8b56067ffd2))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 60fc4256-83b7-4913-8120-741d1d08a0d5))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 8c1546ff-b5ee-439e-b839-0bd6a7697aa5))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(C10-Pad1)") (pintype "passive") (tstamp 1a64fe25-350c-4fbb-a989-e104f0d518f7))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 611414ed-8ef1-44b2-b12c-f94b55c49730))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (tedit 58645DC7) (tstamp c75ce1de-807a-44c9-add0-7205ae600acb)
    (at 169 123.2 180)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/88ac2693-582e-4101-9907-13f627fe32f7")
    (attr smd)
    (fp_text reference "D5" (at 0 2) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7412f750-3d49-4737-ae2a-dae74cc1fde4)
    )
    (fp_text value "RBR2MM30BTR" (at 0 -2.1) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e7d40930-f99e-46a7-915f-6ae6f35b2eb3)
    )
    (fp_text user "${REFERENCE}" (at 0 2) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2ddf2e49-d6e6-4406-b45d-dc3efd97a102)
    )
    (fp_line (start -2.25 1) (end 1.65 1) (layer "B.SilkS") (width 0.12) (tstamp 1c5e42be-34db-45a1-9748-c7f7944bea97))
    (fp_line (start -2.25 -1) (end 1.65 -1) (layer "B.SilkS") (width 0.12) (tstamp 1d717c38-c9c8-4f04-bd0d-8538b865d85a))
    (fp_line (start -2.25 1) (end -2.25 -1) (layer "B.SilkS") (width 0.12) (tstamp 5b50c1cd-8e32-4f17-94a9-fc98ee0f2a17))
    (fp_line (start -2.35 1.15) (end -2.35 -1.15) (layer "B.CrtYd") (width 0.05) (tstamp 2bbcee5a-a3cb-48b8-b971-055d0fbc7081))
    (fp_line (start 2.35 -1.15) (end -2.35 -1.15) (layer "B.CrtYd") (width 0.05) (tstamp 8c0a52d0-5d42-48eb-a8b2-f041ab492944))
    (fp_line (start -2.35 1.15) (end 2.35 1.15) (layer "B.CrtYd") (width 0.05) (tstamp b344164d-174c-4758-9a87-4f78e2b0bb7b))
    (fp_line (start 2.35 1.15) (end 2.35 -1.15) (layer "B.CrtYd") (width 0.05) (tstamp bd31f8c3-1cf5-4d35-a4ed-c60d2400f006))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4) (layer "B.Fab") (width 0.1) (tstamp 006c1a0a-6d96-449f-aca8-a7e2526f70e5))
    (fp_line (start 1.4 -0.9) (end -1.4 -0.9) (layer "B.Fab") (width 0.1) (tstamp 1268c09a-b5f5-4801-95ea-be5482da7274))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer "B.Fab") (width 0.1) (tstamp 1ffebe54-5632-47f3-85de-665491e33338))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer "B.Fab") (width 0.1) (tstamp 40f67971-dc80-4dc6-921c-ac4074511bae))
    (fp_line (start -0.35 0) (end 0.25 0.4) (layer "B.Fab") (width 0.1) (tstamp 5695161b-5f5b-48d1-b529-defa0d0623ae))
    (fp_line (start 0.25 0) (end 0.75 0) (layer "B.Fab") (width 0.1) (tstamp 600e5226-9f72-46c4-9a9d-1d4e2f2db054))
    (fp_line (start -1.4 -0.9) (end -1.4 0.9) (layer "B.Fab") (width 0.1) (tstamp 699f3ad0-b286-4f56-ad18-4aebda3518a3))
    (fp_line (start -1.4 0.9) (end 1.4 0.9) (layer "B.Fab") (width 0.1) (tstamp 9665d5ce-4f48-4042-9653-f3b3bed29351))
    (fp_line (start -0.75 0) (end -0.35 0) (layer "B.Fab") (width 0.1) (tstamp a813361c-d52a-4e2f-84a3-bf1b7719099d))
    (fp_line (start 0.25 -0.4) (end -0.35 0) (layer "B.Fab") (width 0.1) (tstamp ae79e0af-e3bd-4feb-82b5-ab99d3ab4c99))
    (fp_line (start 1.4 0.9) (end 1.4 -0.9) (layer "B.Fab") (width 0.1) (tstamp c0c3716f-78e8-4f8b-b67c-d926f80f3bf7))
    (pad "1" smd rect (at -1.65 0 180) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "/WiFi_Display/PREVGH") (pinfunction "K") (pintype "passive") (tstamp 71607f2e-2e25-4173-9e4e-9f171084a245))
    (pad "2" smd rect (at 1.65 0 180) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "Net-(C22-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 01338a16-3eb3-4d7a-b3a2-e8ec3c9e669c))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958) (tstamp cc0cb76a-7a54-4836-bcc4-75c47c58b45d)
    (at 158.4 117.3 180)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/eeea116b-6c1f-4db6-8810-b1e60195ce6b")
    (attr smd)
    (fp_text reference "U7" (at 0 2.4) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp fd6a64fc-725b-45dc-b039-b5d77f88d379)
    )
    (fp_text value "AP2138N-3.3" (at 0 -2.4) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 3c2ed0de-9147-4227-af97-946ece1c5fc8)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.32 0.32) (thickness 0.05)) (justify mirror))
      (tstamp 67d8dd9c-3958-4867-b14d-9b577f0bd180)
    )
    (fp_line (start 0 -1.56) (end 0.65 -1.56) (layer "B.SilkS") (width 0.12) (tstamp 06e4180b-088b-4718-82eb-ce07a002ac15))
    (fp_line (start 0 1.56) (end 0.65 1.56) (layer "B.SilkS") (width 0.12) (tstamp 0ede8e28-6ea3-42ae-a4f7-bbf4d3023452))
    (fp_line (start 0 -1.56) (end -0.65 -1.56) (layer "B.SilkS") (width 0.12) (tstamp b604785c-0f88-488a-be35-b335f9e37e7d))
    (fp_line (start 0 1.56) (end -1.675 1.56) (layer "B.SilkS") (width 0.12) (tstamp f7158098-7385-4521-a8aa-1256ec2df9eb))
    (fp_line (start 1.92 1.7) (end -1.92 1.7) (layer "B.CrtYd") (width 0.05) (tstamp 17712ddd-9c13-4f33-a7be-a2a6ec6b3f95))
    (fp_line (start -1.92 1.7) (end -1.92 -1.7) (layer "B.CrtYd") (width 0.05) (tstamp 5135e8df-7e74-46a8-a777-167dccb5d542))
    (fp_line (start -1.92 -1.7) (end 1.92 -1.7) (layer "B.CrtYd") (width 0.05) (tstamp d590fe94-46f0-42cd-ae08-feeb91d4fcda))
    (fp_line (start 1.92 -1.7) (end 1.92 1.7) (layer "B.CrtYd") (width 0.05) (tstamp e50f7fc6-6235-4df8-a06d-4588fd9842c0))
    (fp_line (start -0.65 -1.45) (end -0.65 1.125) (layer "B.Fab") (width 0.1) (tstamp 1cb99dfe-879c-4279-b59d-81ee3ebcd546))
    (fp_line (start -0.325 1.45) (end 0.65 1.45) (layer "B.Fab") (width 0.1) (tstamp 29e23020-4261-4dff-9564-ee74ffecedd2))
    (fp_line (start 0.65 1.45) (end 0.65 -1.45) (layer "B.Fab") (width 0.1) (tstamp 869c96a1-994b-4d7e-b943-4a145aa54793))
    (fp_line (start -0.65 1.125) (end -0.325 1.45) (layer "B.Fab") (width 0.1) (tstamp 88451ac7-ac41-458b-8c5e-66275395cb88))
    (fp_line (start 0.65 -1.45) (end -0.65 -1.45) (layer "B.Fab") (width 0.1) (tstamp d9ab9d33-f471-414f-aab8-462fe935985c))
    (pad "1" smd roundrect (at -0.9375 0.95 180) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp ea49a98d-c682-40c1-9215-465120995447))
    (pad "2" smd roundrect (at -0.9375 -0.95 180) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pinfunction "VO") (pintype "power_out") (tstamp 581b4931-b434-45d1-bde8-5177d004138c))
    (pad "3" smd roundrect (at 0.9375 0 180) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "VCC") (pinfunction "VI") (pintype "power_in") (tstamp cd8be2eb-2a57-448a-83c3-8ad6ec8f7570))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0201_0603Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp d0779e40-520e-471b-89ac-ea7040f7e1f6)
    (at 84.5 113 180)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/ebb9c173-6f5b-447b-9537-a03e95b5677a")
    (attr smd)
    (fp_text reference "C9" (at 0 1.05) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f5761054-c60b-4816-abc6-2ac92a31541f)
    )
    (fp_text value "10uF" (at 0 -1.05) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp c96d61eb-077b-4904-afad-a0bbf8c62b77)
    )
    (fp_text user "${REFERENCE}" (at 0 0.68) (layer "B.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
      (tstamp 97a67cf6-4afe-44e8-a8f1-0cbcb941a97b)
    )
    (fp_line (start 0.7 -0.35) (end -0.7 -0.35) (layer "B.CrtYd") (width 0.05) (tstamp 70d79353-ece7-4291-b0a8-3fb47bf4397e))
    (fp_line (start -0.7 -0.35) (end -0.7 0.35) (layer "B.CrtYd") (width 0.05) (tstamp 87cfa05a-cdf6-4c8e-9416-da1a8a3605e2))
    (fp_line (start 0.7 0.35) (end 0.7 -0.35) (layer "B.CrtYd") (width 0.05) (tstamp 95401e36-0486-4590-b0c0-6fce141ad381))
    (fp_line (start -0.7 0.35) (end 0.7 0.35) (layer "B.CrtYd") (width 0.05) (tstamp b290007b-dd05-4c00-a436-2eeaf446d404))
    (fp_line (start 0.3 -0.15) (end -0.3 -0.15) (layer "B.Fab") (width 0.1) (tstamp 12449aea-172e-4805-b573-5fc0821655cf))
    (fp_line (start -0.3 0.15) (end 0.3 0.15) (layer "B.Fab") (width 0.1) (tstamp 5cf250fe-befa-485b-94d0-0c14496e5db5))
    (fp_line (start 0.3 0.15) (end 0.3 -0.15) (layer "B.Fab") (width 0.1) (tstamp 8f743f1e-72ed-4bd8-afe9-44fe26ec2123))
    (fp_line (start -0.3 -0.15) (end -0.3 0.15) (layer "B.Fab") (width 0.1) (tstamp e9269a72-9391-4856-8b02-f91a2ded81d0))
    (pad "" smd roundrect (at 0.345 0 180) (size 0.318 0.36) (layers "B.Paste") (roundrect_rratio 0.25) (tstamp 7e10a53a-fb9c-4338-b6a1-a476d9fd325b))
    (pad "" smd roundrect (at -0.345 0 180) (size 0.318 0.36) (layers "B.Paste") (roundrect_rratio 0.25) (tstamp f1e716ae-3596-4481-8722-2d7714503032))
    (pad "1" smd roundrect (at -0.32 0 180) (size 0.46 0.4) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(C10-Pad1)") (pintype "passive") (tstamp 7a368f77-7dbd-45d4-bb13-3a309155a652))
    (pad "2" smd roundrect (at 0.32 0 180) (size 0.46 0.4) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp af875af4-3b2e-4df8-9896-9039123f31d1))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp d1d46201-6542-4bb3-a935-ea07874f4acb)
    (at 73.02 119.9 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/15b9af59-26c6-4279-a932-10b52b9e4eb4")
    (attr smd)
    (fp_text reference "C16" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d70b983b-fe61-46ff-9258-5f01b1bfce01)
    )
    (fp_text value "10uF" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 76f95e66-2ea2-4a9f-b41a-9257f6564053)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 5e01e43c-22fa-4067-aef5-9b242a08ae00)
    )
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp 254cb0c1-7628-4809-8254-8de90637ac9d))
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp e6ea6861-273e-424d-8094-6e3dd7db728e))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 419d302c-1e81-498d-a4f8-af5b8b59e608))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 57306889-91e8-485d-b426-eed7c5dbeac7))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp c95a8a1f-7d66-46f1-9963-e9557edc6d98))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp e51c4103-4a88-41a2-9da7-b6a7dbce4efb))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 49620c81-8b74-41c2-9d73-8306fb818b6b))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 53d2145d-8f41-431d-93ff-d610536b2ae8))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 8700df72-060a-4218-ac1b-a077b6586b1b))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp fc812942-17d7-48dc-bd0a-61cfe4f36591))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "/Power_Management/PS_SWITCH") (pintype "passive") (tstamp 79d816c2-bbf5-4dc8-9aeb-a81ae29f8762))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 007c816b-5017-488f-bb66-0810c1b00510))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "OptoDevice:Lite-On_LTR-303ALS-01" (layer "B.Cu")
    (tedit 5B870A3B) (tstamp d92555c6-6ec1-43cc-a6f9-7f05df037f76)
    (at 146 140.1)
    (descr "ambient light sensor, i2c interface, 6-pin chipled package, http://optoelectronics.liteon.com/upload/download/DS86-2013-0004/LTR-303ALS-01_DS_V1.pdf")
    (tags "ambient light sensor chipled")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/2794166c-ea3e-4417-9ece-5f24c5d9bfc2")
    (attr smd)
    (fp_text reference "U4" (at 0 2.025) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 3e47b3b8-8822-4ee9-b73e-cce87ac4c009)
    )
    (fp_text value "LTR-303ALS-01" (at 0 -2.025) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2d93b6bf-c885-477b-b193-1bd3cc24142d)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 2c598f4c-b0e8-409f-be3f-dc73c089fb73)
    )
    (fp_line (start -1.2 1.1) (end 1 1.1) (layer "B.SilkS") (width 0.12) (tstamp 59a6a3bd-1fb7-407e-b593-866a86265055))
    (fp_line (start -0.98 -1.1) (end 0.99 -1.1) (layer "B.SilkS") (width 0.12) (tstamp c7bebe46-a021-415d-8fb9-06b9206f747a))
    (fp_line (start -1.48 -1.25) (end 1.48 -1.25) (layer "B.CrtYd") (width 0.05) (tstamp 011d08ed-b717-4d5d-874c-5d976b6b0ee9))
    (fp_line (start -1.48 1.25) (end -1.48 -1.25) (layer "B.CrtYd") (width 0.05) (tstamp 6f6d251d-d120-4eff-9fae-23747d5a5353))
    (fp_line (start 1.48 1.25) (end -1.48 1.25) (layer "B.CrtYd") (width 0.05) (tstamp 8dafb58f-473e-4973-9048-c82590b8ca04))
    (fp_line (start 1.48 -1.25) (end 1.48 1.25) (layer "B.CrtYd") (width 0.05) (tstamp bd7aeb04-726e-4c38-9fa8-137ad93094a2))
    (fp_line (start -1 0.5) (end -0.5 1) (layer "B.Fab") (width 0.1) (tstamp 737a4484-60ea-4c83-9301-e4790c8b687b))
    (fp_line (start -0.5 1) (end 1 1) (layer "B.Fab") (width 0.1) (tstamp 8a7df68a-5011-43d3-a205-2b5fc1c9d3d0))
    (fp_line (start 1 -1) (end -1 -1) (layer "B.Fab") (width 0.1) (tstamp 99981404-ba5a-4953-84c8-f98edaa0002c))
    (fp_line (start -1 -1) (end -1 0.5) (layer "B.Fab") (width 0.1) (tstamp dc09973f-454c-4bf8-8be9-ddbcb601c462))
    (fp_line (start 1 1) (end 1 -1) (layer "B.Fab") (width 0.1) (tstamp de7d253c-b7e9-4cb2-adc1-891f593a32ac))
    (pad "1" smd roundrect (at -0.9 0.65) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pinfunction "VDD") (pintype "power_in") (tstamp af9a8237-0ee1-4977-864e-dc474f959004))
    (pad "2" smd roundrect (at -0.9 0) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 110 "unconnected-(U4-Pad2)") (pinfunction "NC") (pintype "no_connect") (tstamp 05881c8c-4a37-4b18-8f37-a81ebb0d0a32))
    (pad "3" smd roundrect (at -0.9 -0.65) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 76dbeade-c98c-47c1-984c-3b33096292e7))
    (pad "4" smd roundrect (at 0.9 -0.65) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 42 "/Sensor_Controller/I2C_SCL") (pinfunction "SCL") (pintype "input") (tstamp 843cd14d-b528-4fb5-ab9a-69203f7a8a29))
    (pad "5" smd roundrect (at 0.9 0) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 74 "/Sensor_Controller/ALS_INT") (pinfunction "INT") (pintype "open_collector") (tstamp 60975524-5518-4d46-bf75-20cc6f4bf38b))
    (pad "6" smd roundrect (at 0.9 0.65) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 41 "/Sensor_Controller/I2C_SDA") (pinfunction "SDA") (pintype "bidirectional") (tstamp 3dd0f7fe-153c-43f9-a771-dbc2c1a86da7))
    (model "${KICAD6_3DMODEL_DIR}/OptoDevice.3dshapes/Lite-On_LTR-303ALS-01.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp db0cad29-d5b4-4042-923f-90eb33243281)
    (at 59.968334 122.92 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/4587f5f5-a764-48df-9175-19439dd1a2f8")
    (attr smd)
    (fp_text reference "C8" (at 0 1.16) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 105b8712-cfab-4472-80f6-459c303252c1)
    )
    (fp_text value "100nF" (at 0 -1.16) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 93e163fb-67b5-424a-a27b-a1f598441601)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
      (tstamp 6f66347e-c936-47e1-9ed0-a7df9871bfc8)
    )
    (fp_line (start -0.107836 -0.36) (end 0.107836 -0.36) (layer "B.SilkS") (width 0.12) (tstamp cf0ae319-a225-4172-9f72-ae0344622c78))
    (fp_line (start -0.107836 0.36) (end 0.107836 0.36) (layer "B.SilkS") (width 0.12) (tstamp dd64d6cd-8a39-427d-b861-81a487d95394))
    (fp_line (start 0.91 0.46) (end 0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 2ef3d7b8-7f1e-40d4-9c64-fee4bf73042a))
    (fp_line (start 0.91 -0.46) (end -0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 4834122e-48f3-4be3-90ec-5d1e539ff2dd))
    (fp_line (start -0.91 0.46) (end 0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 74bff41b-4382-4d73-a6cf-dcff051783dc))
    (fp_line (start -0.91 -0.46) (end -0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp f46cd10b-5e28-4d28-b932-c32e08c63720))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 07dad92f-d0dd-4932-9d92-95fae53cb41a))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 4789d63c-ad71-4bbf-92e0-2202cc4c3ed7))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 4aa58b94-1219-4578-bda1-6477cea774aa))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp c5563eac-9a46-4da5-a1ff-e4b5398c34f3))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp cd37aaf7-ead1-4f22-b9dc-cc73bf95816a))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 95da2d17-9cf9-4e8a-8324-2fcb5e131bc0))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp dbd9500c-3387-426f-8a3e-f88ba54b2224)
    (at 50.48 136.42 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/8ae4a0ac-8d10-4bb4-a45e-465633fe5f14")
    (attr smd)
    (fp_text reference "R33" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f6445a46-cbbd-4944-ace4-a17dd0475aec)
    )
    (fp_text value "10k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 225a58dd-172c-4fe1-a01a-ec8834ec00f0)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 42225565-0bfa-442f-a4c3-d64d32d3a082)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 113a24ff-1cfa-4394-8b37-8bc4f9f9cc45))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp d3c4b7cc-5681-4ce3-aa61-8971052412d5))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 1792e912-a152-47e1-90bd-37c9599c96e6))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 20beee87-1207-4f3c-a036-92e7b4f4e154))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 4b1e0c77-14f6-4012-82db-919482bf2b13))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 8b9270d9-f54a-4c3f-a57a-1781c65bda88))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 4f3ffe5a-2bcd-49dd-a3cf-e46ccce1d7e9))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 7705c5c7-26ca-478e-8861-26e123043306))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp c14b0969-c100-40d4-ac02-407ec9867b7c))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp f5101fb9-f8b3-4a9c-b89c-d6d8b3578a24))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "VDD") (pintype "passive") (tstamp dfe05bf8-d140-4c15-aadb-5cb8176a244c))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(C20-Pad1)") (pintype "passive") (tstamp 3cb7e6f3-fcfa-472d-a245-cb7d2568c70e))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp dc48003d-04ce-4b15-9fdb-e4e9d720db75)
    (at 50.48 122.42 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/b08657b1-8687-4bb6-a8ff-1c55f5e08bd1")
    (attr smd)
    (fp_text reference "C5" (at 0 1.16) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f5478b06-d44e-422c-9c4b-89061deb1e93)
    )
    (fp_text value "100nF" (at -0.1 -1.7) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7364e5e5-fdb5-488d-9ead-a9c83b1e6a31)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.04)))
      (tstamp dfec3404-1d8e-426d-9ffb-4206644d9c41)
    )
    (fp_line (start -0.107836 0.36) (end 0.107836 0.36) (layer "B.SilkS") (width 0.12) (tstamp 636051ce-38ed-49b1-9883-6f874a85c68a))
    (fp_line (start -0.107836 -0.36) (end 0.107836 -0.36) (layer "B.SilkS") (width 0.12) (tstamp cfce1db3-bca9-4728-8f4f-38d502f6ae88))
    (fp_line (start 0.91 -0.46) (end -0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 0d8c772e-a203-48c5-82e1-d6d79a17c36b))
    (fp_line (start 0.91 0.46) (end 0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 35102d9f-338a-4d5b-8d08-f29263f73e95))
    (fp_line (start -0.91 -0.46) (end -0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 817e0100-922b-48d4-8370-42f0a140842b))
    (fp_line (start -0.91 0.46) (end 0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp cdc5493e-d7fc-4a95-8fd1-fa52d9d20c87))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 21102843-5fec-49d8-97c0-f3b1d0191941))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 3fcb6bb1-8d0c-4b8b-bd6a-3a62aef4be56))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 6a964822-311f-4986-8c1b-90e9f956ae6f))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 9458a226-eab3-4562-935c-18b82fbea34c))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/Sensor_Controller/LPC_~{RST}") (pintype "passive") (tstamp ea9aa488-a527-4455-a981-f359550b1e1e))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp a98fd498-72ac-4c65-b5d0-62aefab99587))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp de29cb86-9ec3-47d2-84f9-ba1975e2c788)
    (at 148.5 154)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/835995d5-bcf4-4fa4-aa55-eb4b8b467ea5")
    (attr smd)
    (fp_text reference "R15" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 237b1e1d-800f-47e4-b02d-a342d4463833)
    )
    (fp_text value "2.2k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 079a7835-1b5d-4d2f-8184-31c5030c4f00)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 54163ee5-172c-4924-a381-5503bb612140)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 2d13ece1-6bc8-45e9-8c2c-aff107caec15))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 4f2eebc9-3f64-4151-a32e-e77a983875e7))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 4833f014-e8bc-411b-9735-cc15eadac5ba))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 71d89df0-b80a-4225-9d48-96eb71055456))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp a76aeba2-e9da-4392-97fe-e42d4c901582))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp ac24a6d4-c63b-451b-917e-8fdcd8b0ffbe))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 3393f562-549c-4e8a-b48a-f0054a9f6f63))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 798ea727-f919-4a63-af49-99dd7560d47e))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 8aec5469-eca5-4f03-b735-ba228cc2567f))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp fc6fa1f6-a65c-43ed-aecf-0e80f0996805))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(R14-Pad2)") (pintype "passive") (tstamp 80fe6ff0-fb09-4fb5-b386-dbddefde99cf))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 54 "/Sensor_Controller/CAPT_X2") (pintype "passive") (tstamp ee796564-42f2-4766-a508-475bc6da402c))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp df91479e-4e3f-4f38-bc03-f13c316483d8)
    (at 174.9 121.4)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/4fe6e85d-d828-45ba-aa29-de22abbbb051")
    (attr smd)
    (fp_text reference "C25" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 615335ff-6dbf-4cbc-863b-f85fe38fc0b6)
    )
    (fp_text value "1uF/50V" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7558174c-9e6a-4309-9eb2-2e147989eb76)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 76c49579-17c4-4617-8117-7d8981ea4281)
    )
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp 573e52aa-45ce-4870-b566-61e59995b965))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp 9fe72bb8-d82d-4f9a-9c5e-caada695b36f))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 3bf00323-9d51-415b-9f41-7305e307ec56))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 4595c635-c085-4465-81f5-59224451cfd7))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 89866b86-9ebf-4c11-993d-58acea924933))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp dd9f5f84-18b0-461c-90d1-a9f154c4cefd))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 05ef6d66-f7d6-486c-8be8-87e79a36479c))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 634081fa-dcd1-41e7-8ab4-1a6738a8a264))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 959ff910-dd52-4d4e-b87a-d074bff99352))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp ccf2b39e-41e4-4dbd-9233-411fb27459a7))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp c66dd5f4-171e-4a35-afd5-bd69b4401e61))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 15 "/WiFi_Display/PREVGH") (pintype "passive") (tstamp 0f46cb1b-0601-4d84-9a9b-bc9616b2f62f))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (tedit 58645DC7) (tstamp e3d497ac-5ccc-4dfb-ac5d-446d2c8ecdc0)
    (at 169 118.4)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/803517bf-0db0-45b4-8f88-724fa4a8ce2c")
    (attr smd)
    (fp_text reference "D3" (at 0 2) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp dd178ae8-35fe-46c3-9c19-73f010517636)
    )
    (fp_text value "RBR2MM30BTR" (at 0 -2.1) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp eee3e58d-2199-4ece-a41a-5e2e9f19677a)
    )
    (fp_text user "${REFERENCE}" (at 0 2) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 92725e63-c029-4318-94a9-6b6fa365334e)
    )
    (fp_line (start -2.25 1) (end -2.25 -1) (layer "B.SilkS") (width 0.12) (tstamp 44730429-ec5f-416f-b29c-ffc21bb20ae3))
    (fp_line (start -2.25 1) (end 1.65 1) (layer "B.SilkS") (width 0.12) (tstamp 6e84eb4c-3f7e-4120-b8a6-a476e065ece7))
    (fp_line (start -2.25 -1) (end 1.65 -1) (layer "B.SilkS") (width 0.12) (tstamp c9e9ed2a-4bcb-46d1-9f26-b0d1c271bd0a))
    (fp_line (start 2.35 1.15) (end 2.35 -1.15) (layer "B.CrtYd") (width 0.05) (tstamp 2f9632a5-2ee0-46fc-8c8b-f6798022cf03))
    (fp_line (start -2.35 1.15) (end -2.35 -1.15) (layer "B.CrtYd") (width 0.05) (tstamp 5a9fcad6-3bc1-4fdd-b744-9589f3304922))
    (fp_line (start -2.35 1.15) (end 2.35 1.15) (layer "B.CrtYd") (width 0.05) (tstamp 9e1c60e4-2d91-42cd-8243-cb7a543ec049))
    (fp_line (start 2.35 -1.15) (end -2.35 -1.15) (layer "B.CrtYd") (width 0.05) (tstamp ef2d9b3b-9c3a-4cbc-8fda-0529dabc4622))
    (fp_line (start -0.35 0) (end 0.25 0.4) (layer "B.Fab") (width 0.1) (tstamp 0ef09064-c5a3-4ad1-a766-68544e4876d0))
    (fp_line (start 1.4 0.9) (end 1.4 -0.9) (layer "B.Fab") (width 0.1) (tstamp 17dba404-b339-4694-a399-d16f126e4711))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4) (layer "B.Fab") (width 0.1) (tstamp 21d0f766-77fc-475f-be80-91803ce874b8))
    (fp_line (start 1.4 -0.9) (end -1.4 -0.9) (layer "B.Fab") (width 0.1) (tstamp 21fb1250-dfa4-4016-8f6a-2f5507e99478))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer "B.Fab") (width 0.1) (tstamp 3df36ddf-35f5-45c0-b9b1-9d8de0bbd39a))
    (fp_line (start -1.4 -0.9) (end -1.4 0.9) (layer "B.Fab") (width 0.1) (tstamp 5d2feb08-36eb-4fb3-bbf3-b990b000c871))
    (fp_line (start 0.25 0) (end 0.75 0) (layer "B.Fab") (width 0.1) (tstamp 65aacbd9-45c7-470f-9c5b-d1da638d9b27))
    (fp_line (start -0.75 0) (end -0.35 0) (layer "B.Fab") (width 0.1) (tstamp 6f7f023b-ae5b-4cc2-b52f-d53115880909))
    (fp_line (start 0.25 -0.4) (end -0.35 0) (layer "B.Fab") (width 0.1) (tstamp 72428f87-4d65-4a2c-a9ac-2b0f9a5b9bcc))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer "B.Fab") (width 0.1) (tstamp c12f57c0-16e0-4778-b255-dd9c227bf43c))
    (fp_line (start -1.4 0.9) (end 1.4 0.9) (layer "B.Fab") (width 0.1) (tstamp eaad3188-ac86-426a-a6f1-4ef6f8f61924))
    (pad "1" smd rect (at -1.65 0) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "Net-(C22-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 5af199ff-0acb-46e0-8827-2362706c5b63))
    (pad "2" smd rect (at 1.65 0) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "/WiFi_Display/PREVGL") (pinfunction "A") (pintype "passive") (tstamp c0e5446b-fe43-4faf-b34d-ff77a8c740c2))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp e49bb379-7a56-4797-b30b-8b170deba133)
    (at 69.56 122.15 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/85017d16-d3bb-44bf-aadb-a6eda059e74e")
    (attr smd)
    (fp_text reference "R24" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp eb431cdf-d560-4bad-b676-37ca4bf27eab)
    )
    (fp_text value "100k/1%" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e8f0f4d7-7b6b-435e-b4d2-414f7adb3b81)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp acc3db9c-55fe-4748-a33c-248ec85d059c)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp aa3a7e91-f166-4fb4-bbf8-3a831f57e355))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp edab3239-79f2-4f60-872b-7b97dc512b2c))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 0f1a85f6-1a5f-46ea-8d0e-0665cf7e429e))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 7aecbfaa-345f-4b06-88aa-e1026e14f953))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp af2e2197-9b5b-4988-8f99-a5f54b292204))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp fc818b09-5cf6-44b3-b29e-180e1008d870))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 17794b82-7fdd-47b2-b3c7-e248cf949241))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 7afb269d-e672-43b5-87d0-a4dac4788177))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 803a35aa-4565-451a-97cb-c90792002c3d))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp ef89a8de-a294-42bb-a5ea-78fd00ed3860))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 62 "/Power_Management/ADC_BAT") (pintype "passive") (tstamp 3efc3c21-4727-494e-a82d-02c17e8cdc9b))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 02a7582e-565b-41fa-98a7-4f51033fd776))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp e5f9678e-717c-40e3-ad3a-730d36c2169e)
    (at 174.9 116.9)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/5a64bddd-8972-49cf-93e2-52fb528d00cd")
    (attr smd)
    (fp_text reference "C32" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7f05cb7d-9b3c-4a20-9aef-9e06f672fb00)
    )
    (fp_text value "1uF/50V" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp c453cb26-d4a1-4172-a7e0-9171a28f3191)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp b2b5cebf-6b5d-4ee4-9d99-5eda6fae18d4)
    )
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp 130ab62f-6513-4e4b-97ed-77ceacd5341c))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp f205fc23-e243-43e4-8bba-8a3bed145bc8))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 0f7932f8-4229-4827-b836-13689fd08d9d))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 8a42ec5d-36a4-41b1-ac2b-b6825ea68cdb))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp de4cd396-6459-42cf-8968-f2c3d97e239b))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp ffb433d3-768a-439f-88c6-ce530b8c354e))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 0cae9b3c-c631-4af1-9a77-44a92170611c))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 3e07c77e-a28c-4fcb-a6c6-5e604eed3be5))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp df7c98df-1594-400a-9c3c-4b16c630ccb3))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp e2f166fd-6468-43d6-8b3e-2157a088b59f))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp f0b71bc9-bf8e-4e6e-b6b9-67a2fa4187a1))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(C32-Pad2)") (pintype "passive") (tstamp d9bd8f67-b983-47e6-84ef-7c72a882a883))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp e7357d35-7fcf-49cb-8a5f-057ca79309e6)
    (at 86.7 133.9 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/7f9dfaad-2be6-41c1-a167-4ccb4287e8d1")
    (attr smd)
    (fp_text reference "C21" (at 0 1.43) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 04cc55be-ab45-4b31-9e10-41456aac48e3)
    )
    (fp_text value "4.7uF" (at 0 -1.43) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a16cd7f7-8f55-4f19-b8c3-49e5c217510c)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp aad3eaf6-5324-4782-868e-17f9ab91e63a)
    )
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp 274fa3eb-85d7-4199-b2b0-fe2457891cf0))
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp d91812d1-f8ee-40e0-baa4-a7e45f4ed8b2))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 7b9bb1e8-87bf-4fb4-a604-5d4f2d8c859e))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 8e1bf26b-f3cf-4f87-805e-98a2abf976e3))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp b883cb68-98c1-4d09-85a2-783c7c50cc39))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp e2140fcd-b0ec-4724-830b-6988c9eae874))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 6b49e2c3-c7cf-48fa-b15a-0024c51fb02e))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp a2934e60-f7f2-4afa-8648-b887bffc8556))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp bcb2b53a-b6cc-40e8-bf3a-7676efb243a4))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp dc2ddfbd-54b4-4b74-ae4e-ea5d769aa23b))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "VDD") (pintype "passive") (tstamp efc1a00e-835b-4294-96b1-74b95182f22d))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 7c6a9e2b-7dc4-43e1-9215-ac630e359a1d))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp e756e0cf-4238-49c5-b423-21d39e083c5e)
    (at 40.3 123.44 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/6e82ae84-3c6a-475e-843f-c55bed17d209")
    (attr smd)
    (fp_text reference "R7" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2d075739-c2e1-4a9c-b89e-9bd7fda245d3)
    )
    (fp_text value "300R" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 49db530c-251d-45de-9296-84408777afdd)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp d73f040d-dd3b-4450-9cc5-5eb58c0a7b98)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 794f99b8-d985-45a9-afa7-42dbf2f41879))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 9639aa0c-a74a-478f-bbe1-fe363bd2fd65))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 1f8f38a2-9389-4bd5-afdc-8f119411a49e))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 573a146b-8045-4baa-ad46-225ce3aea83f))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 7ed3873b-4e47-43bb-b2ef-fffa2c87c1ce))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp f805081c-437a-4f7c-8b61-9b72938a73c8))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 1c2c9aac-92fa-48f0-9c99-aef2de4e1eb7))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 2bb5d944-956b-4419-998c-97fc69e63020))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 89a5539d-774d-40ac-8781-5ed54f599556))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp c7228dd3-a7da-4610-a84a-e9e4d58eb263))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(D1-Pad4)") (pintype "passive") (tstamp 6ef80bfd-7359-4348-a2b8-2073ef01edb4))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "/Sensor_Controller/LED_B") (pintype "passive") (tstamp 44c56047-db0a-4954-8f21-959441bfaaaa))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp e8d95a4b-4e79-4665-9cd0-526fa97605fe)
    (at 165.8 122.9 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/349bfb54-48d8-41e2-b24c-d550bd415c38")
    (attr smd)
    (fp_text reference "C22" (at 0 1.43 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d62ef6e7-2947-42de-92e0-07d662b95ece)
    )
    (fp_text value "4.7uF/50V" (at 0 -1.43 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7e37d067-abad-4c7f-a073-e6038a14f7f2)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp afd29a84-a551-4a13-85bf-b0a0df79c45b)
    )
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer "B.SilkS") (width 0.12) (tstamp 0c4a3a74-710d-49bc-83db-ea1e9e14b1aa))
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer "B.SilkS") (width 0.12) (tstamp ea9c60b1-04fd-4bcb-bc53-87e42bf89dd8))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp 15ecc3e0-f2d9-4b23-92f8-7542608740e6))
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp 7f494ad1-052a-4629-9a38-e059f1b86cf0))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer "B.CrtYd") (width 0.05) (tstamp ae7bae80-ca24-4255-9efd-49e58cf75470))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer "B.CrtYd") (width 0.05) (tstamp ef725b0d-6086-4969-be0c-9f96b1136583))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp 1c3c37df-b2af-424e-b329-2311b9f6ceb3))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp 6a2ae24b-989a-478a-a7af-fca8cdd572d2))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer "B.Fab") (width 0.1) (tstamp a1296481-78c3-4459-9b1a-79eb4c946d28))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer "B.Fab") (width 0.1) (tstamp d4b40bc3-cbb2-451a-b8b5-590a1865577d))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(C22-Pad1)") (pintype "passive") (tstamp c6c40cbf-24f1-4e78-9a8a-5696843a00c8))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(C22-Pad2)") (pintype "passive") (tstamp 7e2a1501-856e-476f-baa3-ff983bd28457))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp ebf8f570-88fc-4fd3-a501-cf28d4c817f3)
    (at 47.5 99.53 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/b86b9743-ef60-4657-98d6-63d95505d5e0")
    (attr smd)
    (fp_text reference "R31" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 96e848eb-cbb2-4e80-96aa-35920b23b692)
    )
    (fp_text value "10k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 1d4aa064-1faa-4873-a896-12f258279489)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 679e3123-f95e-476d-bed6-7a0a1c134dcf)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 2a1d940d-5d66-4861-a624-7f78bfc642a7))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp b29caf03-1a0f-4fb9-b116-0e6e41e05789))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 2c55f1e5-a766-4fbc-9e90-94d73ace501c))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 8a48a987-eccb-43b9-abc2-acdc30b7657b))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp d7521d5d-b3bb-4219-b362-e2f941108ad3))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp eac61aa0-c45d-44f4-94dd-7f58476b69ab))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 160d9f9f-bb8d-4313-b3c4-5712bb774fb8))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp b6113dd7-922a-4996-ae0c-775cbebc95a1))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp b87b3739-db9b-4692-9412-e5536f3eaaae))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp efa35552-45f4-4371-85c6-f1db360f7ab4))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "VDD") (pintype "passive") (tstamp 68aff084-5e59-4fd7-a170-f6995ef3e057))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "/WiFi_Display/EPD_D{slash}~{C}") (pintype "passive") (tstamp e9e4a1f1-1b6e-4f9c-bda1-7517144f2086))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp ebfb83f2-7f6a-48c0-aa12-324afcc3906a)
    (at 32.84 121.38 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/d520198b-2a40-455f-b648-af30bd40d0f3")
    (attr smd)
    (fp_text reference "R1" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5585e71f-19d2-41aa-b745-9015f24da9f1)
    )
    (fp_text value "100k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp b3f3204d-9da3-45f8-96ce-aba013599c74)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 58ec57e6-30f3-4898-9c94-a25039367e20)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 6a51d1cb-fe05-40b3-909d-40ef54b3a2ff))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 9f4861ba-74d9-400e-b7b0-093976c80ffd))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 08341754-4e3b-47a1-bee9-33ed00e29609))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 5b9a2ad0-27f4-4aba-9005-bc9d50b1903d))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp b857ba1e-2b45-4ab0-a721-ef9e56debfb5))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp f55662c9-ee3c-4471-ba9d-3c288d24f8ef))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 656533d3-9085-4585-92ff-aea2556ed9f5))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 8b911e8b-b489-41ed-8b13-f8ec364984ba))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 9d67ca75-27e4-46e6-b240-3423a91212c5))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp c89cd3c9-aee1-49d1-9483-7d6bc600aff3))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp 1cf79173-a21a-4ac5-94c6-e6b42bad8105))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 40 "/Sensor_Controller/LPC_~{ISP}") (pintype "passive") (tstamp 0c8ddc40-9c23-4bbb-be73-53f68312212f))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "B.Cu")
    (tedit 5F6F9B37) (tstamp ec092202-beea-46c9-800c-b66ce60e1791)
    (at 153.3 116 180)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/c8699d74-e891-4979-9162-ae2cd3da4c96")
    (attr smd)
    (fp_text reference "U10" (at 0 2.4) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp cb115414-1d88-46d3-9cc0-79b493a94487)
    )
    (fp_text value "TLV62568DBV" (at 0 -2.4) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7ae9ecc6-e30b-4e0a-a592-54b15cd9a9ec)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
      (tstamp 78a41668-797b-4bc5-8ab3-c859b354fc63)
    )
    (fp_line (start 0 1.56) (end 0.8 1.56) (layer "B.SilkS") (width 0.12) (tstamp 11b9a787-fa42-477f-ab08-82e42f31c5a1))
    (fp_line (start 0 -1.56) (end -0.8 -1.56) (layer "B.SilkS") (width 0.12) (tstamp 613fde20-4257-4023-8467-093f42ed08de))
    (fp_line (start 0 -1.56) (end 0.8 -1.56) (layer "B.SilkS") (width 0.12) (tstamp ab73cb86-4065-4324-a54e-f95cf7c4bcc9))
    (fp_line (start 0 1.56) (end -1.8 1.56) (layer "B.SilkS") (width 0.12) (tstamp e6d9a129-40b7-4668-9a0a-b97394c23b61))
    (fp_line (start 2.05 -1.7) (end 2.05 1.7) (layer "B.CrtYd") (width 0.05) (tstamp 1e322f88-8d85-4bf0-9ce9-53d9a259c804))
    (fp_line (start 2.05 1.7) (end -2.05 1.7) (layer "B.CrtYd") (width 0.05) (tstamp 3aed1516-e9bd-4433-b979-d7f5857dc1da))
    (fp_line (start -2.05 -1.7) (end 2.05 -1.7) (layer "B.CrtYd") (width 0.05) (tstamp 5716862c-f02b-4b9b-ae46-feeaf91cd555))
    (fp_line (start -2.05 1.7) (end -2.05 -1.7) (layer "B.CrtYd") (width 0.05) (tstamp 80f6533a-62a4-4221-a03c-3ae80458636c))
    (fp_line (start -0.4 1.45) (end 0.8 1.45) (layer "B.Fab") (width 0.1) (tstamp 0937f0fa-9288-4efa-b18c-6b669dea8e7e))
    (fp_line (start 0.8 -1.45) (end -0.8 -1.45) (layer "B.Fab") (width 0.1) (tstamp 1ef20350-baca-4310-86ac-a0fc06dddc61))
    (fp_line (start 0.8 1.45) (end 0.8 -1.45) (layer "B.Fab") (width 0.1) (tstamp 87517563-5c5f-4d97-a050-41cdfaff7901))
    (fp_line (start -0.8 1.05) (end -0.4 1.45) (layer "B.Fab") (width 0.1) (tstamp bf11e403-5e7a-457a-bb5c-1ead516bfdc3))
    (fp_line (start -0.8 -1.45) (end -0.8 1.05) (layer "B.Fab") (width 0.1) (tstamp d10b8a2b-09df-4362-99de-7de739c35570))
    (pad "1" smd roundrect (at -1.1375 0.95 180) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 78 "/Power_Management/DCDC_EN") (pinfunction "EN") (pintype "input") (tstamp 3af36875-e1eb-437c-92f4-43adcad9be09))
    (pad "2" smd roundrect (at -1.1375 0 180) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp c2fc7f49-f56c-4e2f-a7f1-5f631b469775))
    (pad "3" smd roundrect (at -1.1375 -0.95 180) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 85 "Net-(L2-Pad1)") (pinfunction "SW") (pintype "power_out") (tstamp 59a02827-d8b5-47d4-85d2-dc9f101a4d04))
    (pad "4" smd roundrect (at 1.1375 -0.95 180) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "/Power_Management/PS_SWITCH") (pinfunction "VIN") (pintype "power_in") (tstamp 5ce56aa5-cc59-4c39-b7c0-abc5838aab3b))
    (pad "5" smd roundrect (at 1.1375 0.95 180) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(R27-Pad2)") (pinfunction "FB") (pintype "input") (tstamp bac226e1-e794-4824-8e4e-426fcf793a71))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp ec2e5c35-338b-4597-90f7-ca2929cbada6)
    (at 89 126.5 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/2e594ab1-4a99-4203-a5cc-e5c18959b1aa")
    (attr smd)
    (fp_text reference "C6" (at 0 1.16) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp fad4eecb-dc34-4615-999e-982028b89509)
    )
    (fp_text value "100nF" (at 0 -1.16) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f6da8172-f49e-4776-b23e-6436ed66f1c2)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
      (tstamp 9c3a1f32-ffe3-4744-bc4e-181903d775b7)
    )
    (fp_line (start -0.107836 0.36) (end 0.107836 0.36) (layer "B.SilkS") (width 0.12) (tstamp 09e20f31-1ca4-4e74-8acd-3e8e06c64a0b))
    (fp_line (start -0.107836 -0.36) (end 0.107836 -0.36) (layer "B.SilkS") (width 0.12) (tstamp 98d46e2c-1df6-4d63-a728-d33ab5e4047e))
    (fp_line (start 0.91 0.46) (end 0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 1f46248a-9695-4a68-93db-8e6169a1afdb))
    (fp_line (start 0.91 -0.46) (end -0.91 -0.46) (layer "B.CrtYd") (width 0.05) (tstamp 46729c0a-dc6e-495d-9b5e-5d10cf19a0f7))
    (fp_line (start -0.91 0.46) (end 0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp 952e7e7d-0ed6-4db3-96c2-972b248d94b6))
    (fp_line (start -0.91 -0.46) (end -0.91 0.46) (layer "B.CrtYd") (width 0.05) (tstamp b04c81d3-f33b-4b11-ad93-ead91a3394fb))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 0ab5a12c-73a4-4481-bd69-27a0234781ff))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp 112e69c5-e151-4b3e-b4f6-4290e8e0331a))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer "B.Fab") (width 0.1) (tstamp 13203af3-54b0-46aa-a995-7bf4ecaf7717))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer "B.Fab") (width 0.1) (tstamp ec67697d-a698-44d2-8d0d-3fbd690e281c))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VDDF") (pintype "passive") (tstamp 18137bf6-21e8-4eab-9c78-0b597edf0c9a))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 85520cf8-1112-41ef-92a9-80dc38e3bdd1))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp f43b9359-857e-4768-aefb-fbc77e8c5bce)
    (at 164.5 154)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sensor_controller.kicad_sch")
    (property "Sheetname" "Sensor_Controller")
    (path "/7e8977c0-0289-43b8-80db-6fcde42fe486/154b2b1b-f7bb-4fa8-8160-bc69fc4cb438")
    (attr smd)
    (fp_text reference "R18" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0b7fb85b-a072-4fcd-befd-3ea532afdf9b)
    )
    (fp_text value "2.2k" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5961691b-180e-47bf-8a4e-e9657e479f34)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp a1d1dfb9-51b3-481c-a88e-41c49dc0bf2c)
    )
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp 311f6c4a-294a-441b-a560-ac3491c7cb1e))
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 8ffb7691-4dc2-4737-8f97-60f7cbc405d9))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 2b42e69f-f89a-42cf-a55c-0769c8c07b29))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 2e018315-787f-4a80-9c3b-e34d9840b6d3))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 4f4fc170-56c3-4e85-8dc0-d2038f232da3))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp cd28e71e-c994-43a1-b1e3-2c15cdb96716))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 5ffdfc1c-88f0-4f40-898d-52e01ec09286))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp d307b2a8-1e32-4572-8ed5-506b1d8615cc))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp db380dc8-f8b8-48c9-82cc-eef66980a9ec))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp df790381-cca8-4fe4-9ae5-2069aa52e7e1))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(R17-Pad2)") (pintype "passive") (tstamp f4c198df-bbd2-4bb1-b71c-1a5e4eddd0ff))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 57 "/Sensor_Controller/CAPT_X3") (pintype "passive") (tstamp 705ccafc-8293-418b-b385-f80269af9823))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp f53ef5e2-00a3-48ce-9544-8754764f1379)
    (at 170.4 128.5 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/e5fa1235-e15c-437f-b421-f08c168cc4c8")
    (attr smd)
    (fp_text reference "R34" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e81271ea-8563-481e-896c-8668080e77da)
    )
    (fp_text value "2R2" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp cc1741a3-5bc8-4fc1-b725-b7332e241cd5)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp 9efe1901-2b5b-4c95-b9ae-273fda0dcc56)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp e6cf4ff7-6502-4449-97ea-963ad9494e4b))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp e8fb340f-be19-4de1-8b9c-a40986fee97c))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 04636ec1-1951-47d8-bcd2-f0b05f1d5b91))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp 13e54bc4-4061-422a-a82a-d97d5746d058))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp cd474a7e-8a8f-4461-90ed-f9f5760c3768))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp ebd8b1c8-28c8-4f36-a21a-4190a3a3acb9))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 46409daa-1802-4f79-8233-36629136b911))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 9b0be282-2f14-4006-990c-b8afc9debbfe))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 9d779d83-361b-4eb5-98cd-0f94f207aa1f))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp f42c8f76-027b-4d93-b4e7-741e764a4325))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "/WiFi_Display/RESE") (pintype "passive") (tstamp 67065ca4-ad04-45fc-9671-12948c7d5861))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 65bdce80-000c-444d-86dc-50d9a69900cc))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp f6c499bf-713a-4eae-8077-768814858d90)
    (at 47.5 101.52 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/601ad21f-7a43-42d7-951b-ab43a9658bba")
    (attr smd)
    (fp_text reference "R29" (at 0 1.17) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 438b9b1b-5d6d-4ee9-8935-0391245734ae)
    )
    (fp_text value "5k1" (at 0 -1.17) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a9fd1f24-7775-4107-a609-ce2e0d4e5739)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.26 0.26) (thickness 0.04)) (justify mirror))
      (tstamp f6321d6f-b783-475a-83a2-955ed39a82ef)
    )
    (fp_line (start -0.153641 -0.38) (end 0.153641 -0.38) (layer "B.SilkS") (width 0.12) (tstamp 94e6b51c-0d6b-4337-93ac-10c2c7caebfe))
    (fp_line (start -0.153641 0.38) (end 0.153641 0.38) (layer "B.SilkS") (width 0.12) (tstamp ed702624-fc1e-4d8c-ac42-bbb6f4e312d3))
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp 59d2da2d-d564-41e2-a204-e51505f3be8d))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp a864e3c7-c74a-4222-8c6f-acab6778da44))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer "B.CrtYd") (width 0.05) (tstamp d504e502-d729-4a95-b5b5-ab5c5d33e344))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer "B.CrtYd") (width 0.05) (tstamp fd6f898a-3479-4e50-9bce-87fc2ad1c8e4))
    (fp_line (start 0.525 -0.27) (end -0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 055cbd53-fc55-453f-8612-add19b54906e))
    (fp_line (start 0.525 0.27) (end 0.525 -0.27) (layer "B.Fab") (width 0.1) (tstamp 0eca223e-fbce-437c-9375-ef149ba2d576))
    (fp_line (start -0.525 0.27) (end 0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 6d02d587-9303-4705-8868-de01a16d2afc))
    (fp_line (start -0.525 -0.27) (end -0.525 0.27) (layer "B.Fab") (width 0.1) (tstamp 9edbbd5f-057f-49bc-a2e4-a5b73351b3fc))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(J2-PadA5)") (pintype "passive") (tstamp 8465d87c-ccc1-4934-9008-a1f9727ef81c))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 2339b9d6-2414-4225-a6b9-f49dc110a56b))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Button_Switch_SMD:Panasonic_EVQPUJ_EVQPUA" (layer "B.Cu")
    (tedit 5A02FC95) (tstamp f87f1538-9f33-494f-b7b3-fd491638b700)
    (at 142.4 107.4 180)
    (descr "http://industrial.panasonic.com/cdbs/www-data/pdf/ATV0000/ATV0000CE5.pdf")
    (tags "SMD SMT SPST EVQPUJ EVQPUA")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/a50f8db5-02b5-4d54-8a5b-d177fb2e3369")
    (attr smd)
    (fp_text reference "SW3" (at 0 4.5) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 8e5bf5b6-ab0d-4c10-99a6-66a869ef4ddb)
    )
    (fp_text value "EVQPUA02K" (at 0 -3.5) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 67bd2d66-095c-4208-a5da-6514a13def95)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp ee693f9a-2358-451f-ae36-8d5a7d561e97)
    )
    (fp_line (start -1.425 1.85) (end -2.35 1.85) (layer "B.SilkS") (width 0.12) (tstamp 037b5100-d0ab-4175-89a7-de47eb19572a))
    (fp_line (start 2.35 -1.85) (end -2.35 -1.85) (layer "B.SilkS") (width 0.12) (tstamp 04d67115-8487-4533-931a-8c62b677703f))
    (fp_line (start 2.35 1.85) (end 1.425 1.85) (layer "B.SilkS") (width 0.12) (tstamp 7454b6a8-b36e-437b-85db-9d9105d67284))
    (fp_line (start 2.45 -0.275) (end 2.45 0.275) (layer "B.SilkS") (width 0.12) (tstamp c04c2d5f-1f8d-4b25-9371-60485cd21fb5))
    (fp_line (start -2.45 -0.275) (end -2.45 0.275) (layer "B.SilkS") (width 0.12) (tstamp ebbc8062-991d-41c3-918c-79bbc961da3d))
    (fp_line (start 3.9 3.25) (end -3.9 3.25) (layer "B.CrtYd") (width 0.05) (tstamp 6d1507b2-e297-43a1-bc95-746fdb0b7a81))
    (fp_line (start 3.9 -2.25) (end -3.9 -2.25) (layer "B.CrtYd") (width 0.05) (tstamp 9bdfae59-deda-4d9d-ae1d-7822becf4854))
    (fp_line (start -3.9 -2.25) (end -3.9 3.25) (layer "B.CrtYd") (width 0.05) (tstamp a2bdec57-7a71-4a9b-ad3a-0cbb0e029415))
    (fp_line (start 3.9 -2.25) (end 3.9 3.25) (layer "B.CrtYd") (width 0.05) (tstamp d84c25aa-914a-4f96-93f2-3538a9645b51))
    (fp_line (start -1.3 2.75) (end -1.3 1.75) (layer "B.Fab") (width 0.1) (tstamp 03304a63-91a4-4b8d-bc74-206813b90c0a))
    (fp_line (start 2.35 1.75) (end -2.35 1.75) (layer "B.Fab") (width 0.1) (tstamp 07e249bf-f3bb-4438-a179-4da2fc4962eb))
    (fp_line (start 2.35 -1.75) (end -2.35 -1.75) (layer "B.Fab") (width 0.1) (tstamp 3b993a29-53b3-47d8-a7d2-97fafac0b1ef))
    (fp_line (start -2.35 -1.75) (end -2.35 1.75) (layer "B.Fab") (width 0.1) (tstamp 5b8dd6b4-bbb5-42a1-8062-6d5f367aae4f))
    (fp_line (start 1.3 2.75) (end 1.3 1.75) (layer "B.Fab") (width 0.1) (tstamp 91f8cd54-9ecb-494b-bf61-49d5041dcb54))
    (fp_line (start 1.3 2.75) (end -1.3 2.75) (layer "B.Fab") (width 0.1) (tstamp c289c873-3c00-47c4-8967-822d88216321))
    (fp_line (start 2.35 -1.75) (end 2.35 1.75) (layer "B.Fab") (width 0.1) (tstamp fd39594d-c8a6-461a-a3b4-228e9a0e2719))
    (pad "1" smd rect (at 2.625 0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive") (tstamp ed8ae13c-e62b-432c-b712-08ade7e209c4))
    (pad "1" smd rect (at -2.625 0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive") (tstamp f5eae70a-f52c-4328-9214-c3554ff628c3))
    (pad "2" smd rect (at -2.625 -0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 95 "Net-(SW3-Pad2)") (pinfunction "2") (pintype "passive") (tstamp 4267da53-13d8-47c0-960f-7b4459b0589b))
    (pad "2" smd rect (at 2.625 -0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 95 "Net-(SW3-Pad2)") (pinfunction "2") (pintype "passive") (tstamp a5fc1014-3082-465a-9f5b-283849b985f1))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/Panasonic_EVQPUJ_EVQPUA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Button_Switch_SMD:Panasonic_EVQPUJ_EVQPUA" (layer "B.Cu")
    (tedit 5A02FC95) (tstamp f9007fab-2e08-4532-9f22-40a0d60ceb70)
    (at 134.4 107.4 180)
    (descr "http://industrial.panasonic.com/cdbs/www-data/pdf/ATV0000/ATV0000CE5.pdf")
    (tags "SMD SMT SPST EVQPUJ EVQPUA")
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/d89521b4-2b5f-4235-a4df-eae3d9fa2f04")
    (attr smd)
    (fp_text reference "SW4" (at 0 4.5) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp fab67ee8-a980-4270-a2c1-e911a56e453e)
    )
    (fp_text value "EVQPUA02K" (at 0 -3.5) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 55b1d32c-eccf-49f4-a90c-b398c03d8bac)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 833a34f8-b4db-45d9-9cbf-61d0f533f7cc)
    )
    (fp_line (start 2.45 -0.275) (end 2.45 0.275) (layer "B.SilkS") (width 0.12) (tstamp 23778edf-794c-4ff8-98d5-053d18fa5fd6))
    (fp_line (start -1.425 1.85) (end -2.35 1.85) (layer "B.SilkS") (width 0.12) (tstamp 2c1872ae-c97a-4951-9bfd-516fedc3d25c))
    (fp_line (start 2.35 1.85) (end 1.425 1.85) (layer "B.SilkS") (width 0.12) (tstamp 46c7a4b1-451e-40da-b6ec-1a119e375ddc))
    (fp_line (start 2.35 -1.85) (end -2.35 -1.85) (layer "B.SilkS") (width 0.12) (tstamp 56864517-629b-48de-9331-a01814d41fd9))
    (fp_line (start -2.45 -0.275) (end -2.45 0.275) (layer "B.SilkS") (width 0.12) (tstamp 70dc2e91-d9a9-4f37-94bb-26180ae68ce7))
    (fp_line (start 3.9 3.25) (end -3.9 3.25) (layer "B.CrtYd") (width 0.05) (tstamp 8b282d21-7c9a-4416-bec1-156c96375126))
    (fp_line (start 3.9 -2.25) (end 3.9 3.25) (layer "B.CrtYd") (width 0.05) (tstamp 9a0dda58-c117-49cc-b60c-ce510450d8c3))
    (fp_line (start 3.9 -2.25) (end -3.9 -2.25) (layer "B.CrtYd") (width 0.05) (tstamp dc2ccffc-45e8-4ed5-ae8d-655de2cfbd0a))
    (fp_line (start -3.9 -2.25) (end -3.9 3.25) (layer "B.CrtYd") (width 0.05) (tstamp ff1e80aa-5240-47a2-b700-e665f5f65b33))
    (fp_line (start 1.3 2.75) (end -1.3 2.75) (layer "B.Fab") (width 0.1) (tstamp 0da8d618-1786-47d0-8962-ca473cfa683c))
    (fp_line (start 2.35 -1.75) (end 2.35 1.75) (layer "B.Fab") (width 0.1) (tstamp 13a5edc3-9ba7-4935-8b00-b14ca8c9aafe))
    (fp_line (start 2.35 -1.75) (end -2.35 -1.75) (layer "B.Fab") (width 0.1) (tstamp 27e90440-f79d-4ae8-a709-3436349c4b97))
    (fp_line (start -2.35 -1.75) (end -2.35 1.75) (layer "B.Fab") (width 0.1) (tstamp 3bb9c5ab-0788-4979-9582-6f25a31909e8))
    (fp_line (start -1.3 2.75) (end -1.3 1.75) (layer "B.Fab") (width 0.1) (tstamp 708f28dd-1380-4191-b8c2-c33049c5b933))
    (fp_line (start 2.35 1.75) (end -2.35 1.75) (layer "B.Fab") (width 0.1) (tstamp 9436e234-4a73-4f25-8aa2-c383381e1bf9))
    (fp_line (start 1.3 2.75) (end 1.3 1.75) (layer "B.Fab") (width 0.1) (tstamp db43c00c-23d1-4dc2-8267-d16ee24c989a))
    (pad "1" smd rect (at 2.625 0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive") (tstamp 0ca9703b-4035-4655-8a27-cd9af7ec606d))
    (pad "1" smd rect (at -2.625 0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive") (tstamp 59f73f8e-fbd6-40d2-8786-3054233a8c57))
    (pad "2" smd rect (at -2.625 -0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 10 "Net-(C20-Pad1)") (pinfunction "2") (pintype "passive") (tstamp 83f0fbbb-e940-495d-8031-32c0e51ee852))
    (pad "2" smd rect (at 2.625 -0.85) (size 1.55 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 10 "Net-(C20-Pad1)") (pinfunction "2") (pintype "passive") (tstamp d13be004-795b-45f9-a9be-28410246a219))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/Panasonic_EVQPUJ_EVQPUA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Inductor_SMD:L_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEF0) (tstamp f92bf2e3-54c1-4ee4-8754-6ecb60d99de8)
    (at 180.9 107.6 180)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Sheetfile" "power_management.kicad_sch")
    (property "Sheetname" "Power_Management")
    (path "/d0438112-8947-4af3-8b61-fc1421d15cf5/ed113c5b-a828-44f6-9de0-3b3524d9275b")
    (attr smd)
    (fp_text reference "L1" (at 0 1.55) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp eba3525c-37e9-4ac4-af86-6fa63049cf98)
    )
    (fp_text value "10uH/350mA, MLZ2012M100WTD25" (at 0 -1.55) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp bffbeeb7-c21d-471b-9054-e91d1a0e6bc9)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)) (justify mirror))
      (tstamp 18300a02-4268-4041-b7ae-afea6ed878ab)
    )
    (fp_line (start -0.399622 0.56) (end 0.399622 0.56) (layer "B.SilkS") (width 0.12) (tstamp 57084240-42b8-4bb3-9caf-7abf068fd7a7))
    (fp_line (start -0.399622 -0.56) (end 0.399622 -0.56) (layer "B.SilkS") (width 0.12) (tstamp 890cecdb-5856-4d31-856a-51d80cfc3558))
    (fp_line (start 1.75 -0.85) (end -1.75 -0.85) (layer "B.CrtYd") (width 0.05) (tstamp 54ef8946-52ed-4d16-bd90-c5040c126bf8))
    (fp_line (start -1.75 0.85) (end 1.75 0.85) (layer "B.CrtYd") (width 0.05) (tstamp 74530a27-2fb0-428a-8469-ecccf5090423))
    (fp_line (start 1.75 0.85) (end 1.75 -0.85) (layer "B.CrtYd") (width 0.05) (tstamp c81fe176-32a5-41ba-b76e-040bbd6749ce))
    (fp_line (start -1.75 -0.85) (end -1.75 0.85) (layer "B.CrtYd") (width 0.05) (tstamp dfa11587-5d4f-458f-ba0e-88db0dfa6d07))
    (fp_line (start 1 0.45) (end 1 -0.45) (layer "B.Fab") (width 0.1) (tstamp 0a578e3f-dde5-4919-9d3d-3b4880f1cc17))
    (fp_line (start 1 -0.45) (end -1 -0.45) (layer "B.Fab") (width 0.1) (tstamp a1408923-877f-47da-b45f-9f240c77b0b1))
    (fp_line (start -1 -0.45) (end -1 0.45) (layer "B.Fab") (width 0.1) (tstamp b4ab520b-baa6-4cb7-9970-9eedfd1b537c))
    (fp_line (start -1 0.45) (end 1 0.45) (layer "B.Fab") (width 0.1) (tstamp dc0129be-a6bc-4c2a-937a-9000638f2fd3))
    (pad "1" smd roundrect (at -1.0625 0 180) (size 0.875 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 84 "Net-(L1-Pad1)") (pinfunction "1") (pintype "passive") (tstamp 82f3619a-5174-430c-9ab4-fcb24b9aad0c))
    (pad "2" smd roundrect (at 1.0625 0 180) (size 0.875 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/Power_Management/LED_A") (pinfunction "2") (pintype "passive") (tstamp 13d648bd-d67d-4b9b-bad8-99dd05e606b5))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_HDGC:0.5K-1.5-6PWB" (layer "B.Cu")
    (tedit 0) (tstamp fe2fb94b-8a50-4f8e-b213-7ce150b35a2a)
    (at 165.425 110.05 -90)
    (property "Sheetfile" "WiFi_Display.kicad_sch")
    (property "Sheetname" "WiFi_Display")
    (path "/8489549c-388c-492a-9035-104204196f60/44a9183e-289d-4f05-a8c0-8458fc7f1cd8")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.05 -270) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2579ac89-0f84-4d09-859b-c3e2ad95bc7e)
    )
    (fp_text value "0.5K-1.5-6PWB" (at 0 -3.2 -270) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7526d798-b7e6-4c94-8281-8961c889a56e)
    )
    (fp_line (start -1.75 0) (end -1.75 0.75) (layer "B.SilkS") (width 0.12) (tstamp 40cfb16b-41db-4f2f-afe5-4a090b3769c8))
    (fp_line (start -1.75 0) (end -4.25 0) (layer "B.SilkS") (width 0.12) (tstamp ce63eb8f-38e0-4f81-848d-e737592353a3))
    (fp_line (start -4.55 -4.55) (end 4.55 -4.55) (layer "B.CrtYd") (width 0.05) (tstamp 6e35aa7d-765e-46f0-9707-f40191181384))
    (fp_line (start 4.55 1.3) (end 4.55 -4.55) (layer "B.CrtYd") (width 0.05) (tstamp 88c20351-cfc9-4706-a398-84544aff0f33))
    (fp_line (start -4.55 1.3) (end -4.55 -4.55) (layer "B.CrtYd") (width 0.05) (tstamp c9bffa16-3766-4929-87bc-1ecae6aa93f1))
    (fp_line (start -4.55 1.3) (end 4.55 1.3) (layer "B.CrtYd") (width 0.05) (tstamp f0c12028-a0f1-427b-a86d-ed9a05639cce))
    (pad "1" smd rect (at -1.25 0 270) (size 0.3 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 28 "/Power_Management/LED_K") (pinfunction "Pin_1") (pintype "passive") (tstamp e1a9d088-e77e-4872-aeb8-fabb23a7b225))
    (pad "2" smd rect (at -0.75 0 270) (size 0.3 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 28 "/Power_Management/LED_K") (pinfunction "Pin_2") (pintype "passive") (tstamp e6754f11-8753-47ce-a8ac-2019a2d38416))
    (pad "3" smd rect (at -0.25 0 270) (size 0.3 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 26 "unconnected-(J3-Pad3)") (pinfunction "Pin_3") (pintype "passive+no_connect") (tstamp 23d5cb36-b1da-4db7-b8cb-344522731d53))
    (pad "4" smd rect (at 0.25 0 270) (size 0.3 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 27 "unconnected-(J3-Pad4)") (pinfunction "Pin_4") (pintype "passive+no_connect") (tstamp eb3decee-0b88-40c0-907c-749ae4e8f2dd))
    (pad "5" smd rect (at 0.75 0 270) (size 0.3 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "/Power_Management/LED_A") (pinfunction "Pin_5") (pintype "passive") (tstamp 27c5163e-fb99-4bdf-b265-52fe7dee0afc))
    (pad "6" smd rect (at 1.25 0 270) (size 0.3 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "/Power_Management/LED_A") (pinfunction "Pin_6") (pintype "passive") (tstamp 22470dd4-d9f6-4921-96f0-5f282763d2c2))
    (pad "MP" smd rect (at -3.4 -3.15 270) (size 1.1 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "MountPin") (pintype "passive") (tstamp 47980a62-849d-4634-b212-2f8c247b21aa))
    (pad "MP" smd rect (at 3.4 -3.15 270) (size 1.1 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "MountPin") (pintype "passive") (tstamp bcc062d7-12a9-4df5-9293-dbdcf0446704))
  )

  (gr_rect locked (start 112.5 106.3) (end 191.5 143) (layer "Dwgs.User") (width 0.15) (fill none) (tstamp 3a959ea3-664f-4552-8653-c6e4dcdb715d))
  (gr_line (start 112.5 124.65) (end 191.5 124.65) (layer "Dwgs.User") (width 0.15) (tstamp 88d4e556-1df4-4ec6-8ebf-f46650e267f2))
  (gr_line (start 168.1 111.8) (end 191.5 111.8) (layer "Dwgs.User") (width 0.15) (tstamp b7337c66-9018-416f-ba81-c31151777b59))
  (gr_line (start 168.1 108.3) (end 168.1 111.8) (layer "Dwgs.User") (width 0.15) (tstamp d70287ac-f4b0-4f3f-aecd-335f31ed676c))
  (gr_line (start 191.5 108.3) (end 168.1 108.3) (layer "Dwgs.User") (width 0.15) (tstamp ed19b09f-82d9-4562-b578-d2198bc4f8d5))
  (gr_line (start 112 159.4) (end 197 159.4) (layer "Edge.Cuts") (width 0.1) (tstamp 0c9ca2e1-32e2-4bef-a1a4-7e3dd0070393))
  (gr_arc (start 192 111.4) (mid 191 112.4) (end 190 111.4) (layer "Edge.Cuts") (width 0.1) (tstamp 39b2434a-4f98-45b5-b3aa-9979da5b3973))
  (gr_line (start 192 132) (end 192 117) (layer "Edge.Cuts") (width 0.1) (tstamp 7bac970f-c349-4622-87c8-62f913c75d16))
  (gr_line (start 112 105.4) (end 112 159.4) (layer "Edge.Cuts") (width 0.1) (tstamp 7f546b4f-3242-4f45-bfc3-d7b15c1923be))
  (gr_arc (start 190 117) (mid 191 116) (end 192 117) (layer "Edge.Cuts") (width 0.1) (tstamp 8f07758b-1c3d-4dc7-b517-d263d15ea273))
  (gr_line (start 190 117) (end 190 132) (layer "Edge.Cuts") (width 0.1) (tstamp b4509015-f66f-4ee7-816a-4afd8a7704f1))
  (gr_line (start 197 159.4) (end 197 105.4) (layer "Edge.Cuts") (width 0.1) (tstamp ba32ba7f-8217-4b48-b727-569440c3f6e5))
  (gr_line (start 197 105.4) (end 112 105.4) (layer "Edge.Cuts") (width 0.1) (tstamp bfd41b31-5bd3-4d0a-ae20-1e1fed6828c8))
  (gr_arc (start 192 132) (mid 191 133) (end 190 132) (layer "Edge.Cuts") (width 0.1) (tstamp d2b4f581-9b50-4e03-a29b-793980edda7e))
  (gr_line (start 190 108.6) (end 190 111.4) (layer "Edge.Cuts") (width 0.1) (tstamp ddcf24c1-57c5-45c0-8415-c9c0f89fcfa0))
  (gr_line (start 192 108.6) (end 192 111.4) (layer "Edge.Cuts") (width 0.1) (tstamp df501692-480b-49d2-bf80-6b4ff0bff4be))
  (gr_arc (start 190 108.6) (mid 191 107.6) (end 192 108.6) (layer "Edge.Cuts") (width 0.1) (tstamp f836eaa5-c33a-4040-8328-3e57efb08912))
  (dimension (type aligned) (layer "Dwgs.User") (tstamp 038d57ef-ffab-4d2e-8f36-264c7d3688cd)
    (pts (xy 168.1 108.3) (xy 191.5 108.3))
    (height -3.6)
    (gr_text "23.4000 mm" (at 179.8 103.55) (layer "Dwgs.User") (tstamp 038d57ef-ffab-4d2e-8f36-264c7d3688cd)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp 0d48a53d-1f92-479a-ac00-6cb633e66acb)
    (pts (xy 112.5 106.3) (xy 112.5 143))
    (height 3.5)
    (gr_text "36.7000 mm" (at 107.85 124.65 90) (layer "Dwgs.User") (tstamp 0d48a53d-1f92-479a-ac00-6cb633e66acb)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp 2cd37e26-39f9-4e64-9daf-7287929a872a)
    (pts (xy 191.5 106.3) (xy 191.5 108.3))
    (height -8)
    (gr_text "2.0000 mm" (at 198.35 107.3 90) (layer "Dwgs.User") (tstamp 2cd37e26-39f9-4e64-9daf-7287929a872a)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp 3af81ae6-5c97-4c41-94c3-443993ba5f0b)
    (pts (xy 180.8 133.65) (xy 191.5 133.65))
    (height 11.6)
    (gr_text "10.7000 mm" (at 186.15 144.1) (layer "Dwgs.User") (tstamp 3af81ae6-5c97-4c41-94c3-443993ba5f0b)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp 836dc643-f787-436e-988d-4283e65f8fa8)
    (pts (xy 112.5 106.3) (xy 191.5 106.3))
    (height -3.799993)
    (gr_text "79.0000 mm" (at 152 101.350007) (layer "Dwgs.User") (tstamp 836dc643-f787-436e-988d-4283e65f8fa8)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp d8d81214-7453-47b8-822e-91257695a217)
    (pts (xy 191.5 108.3) (xy 191.5 111.8))
    (height -10.3)
    (gr_text "3.5000 mm" (at 200.65 110.05 90) (layer "Dwgs.User") (tstamp d8d81214-7453-47b8-822e-91257695a217)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp e2a9f3de-2a71-4e63-a781-c051be424d3b)
    (pts (xy 112.5 106.3) (xy 112.5 124.65))
    (height 1.55)
    (gr_text "18.3500 mm" (at 109.8 115.475 90) (layer "Dwgs.User") (tstamp e2a9f3de-2a71-4e63-a781-c051be424d3b)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )

)
