<?xml version="1.0" encoding= "UTF-8" ?>
<configuration name="MIMXRT1052xxxxB" xsi:schemaLocation="http://mcuxpresso.nxp.com/XSD/mex_configuration_1.9 http://mcuxpresso.nxp.com/XSD/mex_configuration_1.9.xsd" uuid="e2d9ad14-bec2-4bd5-9ab7-3ad49c3b682c" version="1.9" xmlns="http://mcuxpresso.nxp.com/XSD/mex_configuration_1.9" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">
   <common>
      <processor>MIMXRT1052xxxxB</processor>
      <package>MIMXRT1052DVL6B</package>
      <board>IMXRT1050-EVKB</board>
      <mcu_data>ksdk2_0</mcu_data>
      <cores selected="core0">
         <core name="Cortex-M7F" id="core0" description="M7 core"/>
      </cores>
      <description>Configuration imported from /home/imi415/Documents/Hardwares/Kinetis_Projects/rt1050_freertos_hello</description>
   </common>
   <preferences>
      <validate_boot_init_only>true</validate_boot_init_only>
      <generate_extended_information>false</generate_extended_information>
      <generate_code_modified_registers_only>false</generate_code_modified_registers_only>
   </preferences>
   <tools>
      <pins name="Pins" version="9.0" enabled="true" update_project_code="true">
         <generated_project_files>
            <file path="board/pin_mux.c" update_enabled="true"/>
            <file path="board/pin_mux.h" update_enabled="true"/>
         </generated_project_files>
         <pins_profile>
            <processor_version>9.0.1</processor_version>
            <power_domains>
               <power_domain name="NVCC_GPIO" value="3.3"/>
               <power_domain name="NVCC_SD0" value="3.3"/>
            </power_domains>
            <pin_labels>
               <pin_label pin_num="M11" pin_signal="GPIO_AD_B0_02" label="LCDIF_RESET" identifier="LCDIF_RESEt;LCDIF_RESET"/>
               <pin_label pin_num="G11" pin_signal="GPIO_AD_B0_03" label="USB_OTG1_OC/J24[1]" identifier="SD1_CD"/>
               <pin_label pin_num="G13" pin_signal="GPIO_AD_B0_10" label="LED_BLUE" identifier="INT1_COMBO;LED_BLUE"/>
               <pin_label pin_num="L10" pin_signal="GPIO_AD_B0_15" label="LCDIF_BL" identifier="CAN2_RX;LCDIF_BL"/>
            </pin_labels>
         </pins_profile>
         <functions_list>
            <function name="BOARD_InitPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>true</callFromInitBoot>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="LPUART1" description="Peripheral LPUART1 is not initialized" problem_level="1" source="Pins:BOARD_InitPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="Peripheral" resourceId="SEMC" description="Peripheral SEMC is not initialized" problem_level="1" source="Pins:BOARD_InitPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="Peripheral" resourceId="LCDIF" description="Peripheral LCDIF is not initialized" problem_level="1" source="Pins:BOARD_InitPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="Peripheral" resourceId="ENET" description="Peripheral ENET is not initialized" problem_level="1" source="Pins:BOARD_InitPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="Peripheral" resourceId="USDHC1" description="Peripheral USDHC1 is not initialized" problem_level="1" source="Pins:BOARD_InitPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="Peripheral" resourceId="GPIO1" description="Peripheral GPIO1 is not initialized" problem_level="1" source="Pins:BOARD_InitPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Pins initialization requires the IOMUXC Driver in the project." problem_level="2" source="Pins:BOARD_InitPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.igpio" description="Pins initialization requires the IGPIO Driver in the project." problem_level="2" source="Pins:BOARD_InitPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="LPUART1" signal="RX" pin_num="L14" pin_signal="GPIO_AD_B0_13">
                     <pin_features>
                        <pin_feature name="software_input_on" value="Disable"/>
                        <pin_feature name="hysteresis_enable" value="Disable"/>
                        <pin_feature name="pull_up_down_config" value="Pull_Down_100K_Ohm"/>
                        <pin_feature name="pull_keeper_select" value="Keeper"/>
                        <pin_feature name="pull_keeper_enable" value="Enable"/>
                        <pin_feature name="open_drain" value="Disable"/>
                        <pin_feature name="speed" value="MHZ_100"/>
                        <pin_feature name="drive_strength" value="R0_6"/>
                        <pin_feature name="slew_rate" value="Slow"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="LPUART1" signal="TX" pin_num="K14" pin_signal="GPIO_AD_B0_12">
                     <pin_features>
                        <pin_feature name="software_input_on" value="Disable"/>
                        <pin_feature name="hysteresis_enable" value="Disable"/>
                        <pin_feature name="pull_up_down_config" value="Pull_Down_100K_Ohm"/>
                        <pin_feature name="pull_keeper_select" value="Keeper"/>
                        <pin_feature name="pull_keeper_enable" value="Enable"/>
                        <pin_feature name="open_drain" value="Disable"/>
                        <pin_feature name="speed" value="MHZ_100"/>
                        <pin_feature name="drive_strength" value="R0_6"/>
                        <pin_feature name="slew_rate" value="Slow"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="SEMC" signal="ADDR, 00" pin_num="C2" pin_signal="GPIO_EMC_09"/>
                  <pin peripheral="SEMC" signal="ADDR, 01" pin_num="G1" pin_signal="GPIO_EMC_10"/>
                  <pin peripheral="SEMC" signal="ADDR, 02" pin_num="G3" pin_signal="GPIO_EMC_11"/>
                  <pin peripheral="SEMC" signal="ADDR, 03" pin_num="H1" pin_signal="GPIO_EMC_12"/>
                  <pin peripheral="SEMC" signal="ADDR, 04" pin_num="A6" pin_signal="GPIO_EMC_13"/>
                  <pin peripheral="SEMC" signal="ADDR, 05" pin_num="B6" pin_signal="GPIO_EMC_14"/>
                  <pin peripheral="SEMC" signal="ADDR, 06" pin_num="B1" pin_signal="GPIO_EMC_15"/>
                  <pin peripheral="SEMC" signal="ADDR, 07" pin_num="A5" pin_signal="GPIO_EMC_16"/>
                  <pin peripheral="SEMC" signal="ADDR, 08" pin_num="A4" pin_signal="GPIO_EMC_17"/>
                  <pin peripheral="SEMC" signal="ADDR, 09" pin_num="B2" pin_signal="GPIO_EMC_18"/>
                  <pin peripheral="SEMC" signal="ADDR, 10" pin_num="G2" pin_signal="GPIO_EMC_23"/>
                  <pin peripheral="SEMC" signal="ADDR, 11" pin_num="B4" pin_signal="GPIO_EMC_19"/>
                  <pin peripheral="SEMC" signal="ADDR, 12" pin_num="A3" pin_signal="GPIO_EMC_20"/>
                  <pin peripheral="SEMC" signal="BA, 0" pin_num="C1" pin_signal="GPIO_EMC_21"/>
                  <pin peripheral="SEMC" signal="BA, 1" pin_num="F1" pin_signal="GPIO_EMC_22"/>
                  <pin peripheral="SEMC" signal="semc_cas" pin_num="D3" pin_signal="GPIO_EMC_24"/>
                  <pin peripheral="SEMC" signal="semc_cke" pin_num="A2" pin_signal="GPIO_EMC_27"/>
                  <pin peripheral="SEMC" signal="semc_clk" pin_num="B3" pin_signal="GPIO_EMC_26"/>
                  <pin peripheral="SEMC" signal="CSX, 0" pin_num="C7" pin_signal="GPIO_EMC_41"/>
                  <pin peripheral="SEMC" signal="CS, 0" pin_num="E1" pin_signal="GPIO_EMC_29"/>
                  <pin peripheral="SEMC" signal="DATA, 00" pin_num="E3" pin_signal="GPIO_EMC_00"/>
                  <pin peripheral="SEMC" signal="DATA, 01" pin_num="F3" pin_signal="GPIO_EMC_01"/>
                  <pin peripheral="SEMC" signal="DATA, 02" pin_num="F4" pin_signal="GPIO_EMC_02"/>
                  <pin peripheral="SEMC" signal="DATA, 03" pin_num="G4" pin_signal="GPIO_EMC_03"/>
                  <pin peripheral="SEMC" signal="DATA, 04" pin_num="F2" pin_signal="GPIO_EMC_04"/>
                  <pin peripheral="SEMC" signal="DATA, 05" pin_num="G5" pin_signal="GPIO_EMC_05"/>
                  <pin peripheral="SEMC" signal="DATA, 06" pin_num="H5" pin_signal="GPIO_EMC_06"/>
                  <pin peripheral="SEMC" signal="DATA, 07" pin_num="H4" pin_signal="GPIO_EMC_07"/>
                  <pin peripheral="SEMC" signal="DATA, 08" pin_num="C6" pin_signal="GPIO_EMC_30"/>
                  <pin peripheral="SEMC" signal="DATA, 09" pin_num="C5" pin_signal="GPIO_EMC_31"/>
                  <pin peripheral="SEMC" signal="DATA, 10" pin_num="D5" pin_signal="GPIO_EMC_32"/>
                  <pin peripheral="SEMC" signal="DATA, 11" pin_num="C4" pin_signal="GPIO_EMC_33"/>
                  <pin peripheral="SEMC" signal="DATA, 12" pin_num="D4" pin_signal="GPIO_EMC_34"/>
                  <pin peripheral="SEMC" signal="DATA, 13" pin_num="E5" pin_signal="GPIO_EMC_35"/>
                  <pin peripheral="SEMC" signal="DATA, 14" pin_num="C3" pin_signal="GPIO_EMC_36"/>
                  <pin peripheral="SEMC" signal="DATA, 15" pin_num="E4" pin_signal="GPIO_EMC_37"/>
                  <pin peripheral="SEMC" signal="DM, 0" pin_num="H3" pin_signal="GPIO_EMC_08"/>
                  <pin peripheral="SEMC" signal="DM, 1" pin_num="D6" pin_signal="GPIO_EMC_38"/>
                  <pin peripheral="SEMC" signal="semc_ras" pin_num="D2" pin_signal="GPIO_EMC_25"/>
                  <pin peripheral="SEMC" signal="semc_rdy" pin_num="A7" pin_signal="GPIO_EMC_40"/>
                  <pin peripheral="SEMC" signal="semc_we" pin_num="D1" pin_signal="GPIO_EMC_28"/>
                  <pin peripheral="LCDIF" signal="lcdif_clk" pin_num="D7" pin_signal="GPIO_B0_00"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 00" pin_num="C8" pin_signal="GPIO_B0_04"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 01" pin_num="B8" pin_signal="GPIO_B0_05"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 02" pin_num="A8" pin_signal="GPIO_B0_06"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 03" pin_num="A9" pin_signal="GPIO_B0_07"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 04" pin_num="B9" pin_signal="GPIO_B0_08"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 05" pin_num="C9" pin_signal="GPIO_B0_09"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 06" pin_num="D9" pin_signal="GPIO_B0_10"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 07" pin_num="A10" pin_signal="GPIO_B0_11"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 08" pin_num="C10" pin_signal="GPIO_B0_12"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 09" pin_num="D10" pin_signal="GPIO_B0_13"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 10" pin_num="E10" pin_signal="GPIO_B0_14"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 11" pin_num="E11" pin_signal="GPIO_B0_15"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 12" pin_num="A11" pin_signal="GPIO_B1_00"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 13" pin_num="B11" pin_signal="GPIO_B1_01"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 14" pin_num="C11" pin_signal="GPIO_B1_02"/>
                  <pin peripheral="LCDIF" signal="lcdif_data, 15" pin_num="D11" pin_signal="GPIO_B1_03"/>
                  <pin peripheral="LCDIF" signal="lcdif_vsync" pin_num="D8" pin_signal="GPIO_B0_03"/>
                  <pin peripheral="LCDIF" signal="lcdif_hsync" pin_num="E8" pin_signal="GPIO_B0_02"/>
                  <pin peripheral="LCDIF" signal="lcdif_enable" pin_num="E7" pin_signal="GPIO_B0_01"/>
                  <pin peripheral="GPIO1" signal="gpio_io, 02" pin_num="M11" pin_signal="GPIO_AD_B0_02">
                     <pin_features>
                        <pin_feature name="identifier" value="LCDIF_RESET"/>
                        <pin_feature name="direction" value="OUTPUT"/>
                        <pin_feature name="gpio_init_state" value="true"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="GPIO1" signal="gpio_io, 10" pin_num="G13" pin_signal="GPIO_AD_B0_10">
                     <pin_features>
                        <pin_feature name="identifier" value="LED_BLUE"/>
                        <pin_feature name="direction" value="OUTPUT"/>
                        <pin_feature name="gpio_init_state" value="true"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="GPIO1" signal="gpio_io, 15" pin_num="L10" pin_signal="GPIO_AD_B0_15">
                     <pin_features>
                        <pin_feature name="identifier" value="LCDIF_BL"/>
                        <pin_feature name="direction" value="OUTPUT"/>
                        <pin_feature name="gpio_init_state" value="true"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="ENET" signal="enet_mdc" pin_num="L12" pin_signal="GPIO_AD_B1_04"/>
                  <pin peripheral="ENET" signal="enet_mdio" pin_num="B14" pin_signal="GPIO_B1_15"/>
                  <pin peripheral="ENET" signal="enet_tx_clk" pin_num="B13" pin_signal="GPIO_B1_10"/>
                  <pin peripheral="ENET" signal="enet_tx_data, 0" pin_num="B12" pin_signal="GPIO_B1_07"/>
                  <pin peripheral="ENET" signal="enet_tx_data, 1" pin_num="A12" pin_signal="GPIO_B1_08"/>
                  <pin peripheral="ENET" signal="enet_rx_er" pin_num="C13" pin_signal="GPIO_B1_11"/>
                  <pin peripheral="ENET" signal="enet_tx_en" pin_num="A13" pin_signal="GPIO_B1_09"/>
                  <pin peripheral="ENET" signal="enet_rx_data, 0" pin_num="E12" pin_signal="GPIO_B1_04"/>
                  <pin peripheral="ENET" signal="enet_rx_data, 1" pin_num="D12" pin_signal="GPIO_B1_05"/>
                  <pin peripheral="ENET" signal="enet_rx_en" pin_num="C12" pin_signal="GPIO_B1_06"/>
                  <pin peripheral="USDHC1" signal="usdhc_vselect" pin_num="C14" pin_signal="GPIO_B1_14"/>
                  <pin peripheral="USDHC1" signal="usdhc_clk" pin_num="J3" pin_signal="GPIO_SD_B0_01"/>
                  <pin peripheral="USDHC1" signal="usdhc_cmd" pin_num="J4" pin_signal="GPIO_SD_B0_00"/>
                  <pin peripheral="USDHC1" signal="usdhc_data, 1" pin_num="K1" pin_signal="GPIO_SD_B0_03"/>
                  <pin peripheral="USDHC1" signal="usdhc_data, 2" pin_num="H2" pin_signal="GPIO_SD_B0_04"/>
                  <pin peripheral="USDHC1" signal="usdhc_data, 3" pin_num="J2" pin_signal="GPIO_SD_B0_05"/>
                  <pin peripheral="USDHC1" signal="usdhc_data, 0" pin_num="J1" pin_signal="GPIO_SD_B0_02"/>
                  <pin peripheral="GPIO1" signal="gpio_io, 03" pin_num="G11" pin_signal="GPIO_AD_B0_03">
                     <pin_features>
                        <pin_feature name="direction" value="INPUT"/>
                        <pin_feature name="gpio_interrupt" value="kGPIO_IntRisingOrFallingEdge"/>
                        <pin_feature name="pull_up_down_config" value="Pull_Up_100K_Ohm"/>
                        <pin_feature name="pull_keeper_select" value="Pull"/>
                     </pin_features>
                  </pin>
               </pins>
            </function>
         </functions_list>
      </pins>
      <clocks name="Clocks" version="7.0" enabled="true" update_project_code="true">
         <generated_project_files>
            <file path="board/clock_config.c" update_enabled="true"/>
            <file path="board/clock_config.h" update_enabled="true"/>
         </generated_project_files>
         <clocks_profile>
            <processor_version>9.0.1</processor_version>
         </clocks_profile>
         <clock_configurations>
            <clock_configuration name="BOARD_BootClockRUN">
               <description></description>
               <options/>
               <dependencies>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.rtc_xtali" description="&apos;RTC_XTALI&apos; (Pins tool id: XTALOSC24M.rtc_xtali, Clocks tool id: XTALOSC24M.RTC_XTALI) needs to be routed" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.rtc_xtali" description="&apos;RTC_XTALI&apos; (Pins tool id: XTALOSC24M.rtc_xtali, Clocks tool id: XTALOSC24M.RTC_XTALI) needs to have &apos;INPUT&apos; direction" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="direction" evaluation="">
                        <data>INPUT</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.rtc_xtalo" description="&apos;RTC_XTALO&apos; (Pins tool id: XTALOSC24M.rtc_xtalo, Clocks tool id: XTALOSC24M.RTC_XTALO) needs to be routed" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.rtc_xtalo" description="&apos;RTC_XTALO&apos; (Pins tool id: XTALOSC24M.rtc_xtalo, Clocks tool id: XTALOSC24M.RTC_XTALO) needs to have &apos;OUTPUT&apos; direction" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="direction" evaluation="">
                        <data>OUTPUT</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.xtali" description="&apos;XTALI&apos; (Pins tool id: XTALOSC24M.xtali, Clocks tool id: XTALOSC24M.XTALI) needs to be routed" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.xtali" description="&apos;XTALI&apos; (Pins tool id: XTALOSC24M.xtali, Clocks tool id: XTALOSC24M.XTALI) needs to have &apos;INPUT&apos; direction" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="direction" evaluation="">
                        <data>INPUT</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.xtalo" description="&apos;XTALO&apos; (Pins tool id: XTALOSC24M.xtalo, Clocks tool id: XTALOSC24M.XTALO) needs to be routed" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.xtalo" description="&apos;XTALO&apos; (Pins tool id: XTALOSC24M.xtalo, Clocks tool id: XTALOSC24M.XTALO) needs to have &apos;OUTPUT&apos; direction" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="direction" evaluation="">
                        <data>OUTPUT</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Clocks initialization requires the COMMON Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockRUN">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Clocks initialization requires the IOMUXC Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockRUN">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <clock_sources>
                  <clock_source id="XTALOSC24M.RTC_OSC.outFreq" value="32.768 kHz" locked="false" enabled="true"/>
               </clock_sources>
               <clock_outputs>
                  <clock_output id="AHB_CLK_ROOT.outFreq" value="600 MHz" locked="false" accuracy=""/>
                  <clock_output id="CAN_CLK_ROOT.outFreq" value="40 MHz" locked="false" accuracy=""/>
                  <clock_output id="CKIL_SYNC_CLK_ROOT.outFreq" value="32.768 kHz" locked="false" accuracy=""/>
                  <clock_output id="CLK_1M.outFreq" value="1 MHz" locked="false" accuracy=""/>
                  <clock_output id="CLK_24M.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="CSI_CLK_ROOT.outFreq" value="12 MHz" locked="false" accuracy=""/>
                  <clock_output id="ENET1_TX_CLK.outFreq" value="125 MHz" locked="false" accuracy=""/>
                  <clock_output id="ENET_125M_CLK.outFreq" value="125 MHz" locked="false" accuracy=""/>
                  <clock_output id="ENET_25M_REF_CLK.outFreq" value="25 MHz" locked="false" accuracy=""/>
                  <clock_output id="FLEXIO1_CLK_ROOT.outFreq" value="30 MHz" locked="false" accuracy=""/>
                  <clock_output id="FLEXIO2_CLK_ROOT.outFreq" value="30 MHz" locked="false" accuracy=""/>
                  <clock_output id="FLEXSPI_CLK_ROOT.outFreq" value="160 MHz" locked="false" accuracy=""/>
                  <clock_output id="GPT1_ipg_clk_highfreq.outFreq" value="75 MHz" locked="false" accuracy=""/>
                  <clock_output id="GPT2_ipg_clk_highfreq.outFreq" value="75 MHz" locked="false" accuracy=""/>
                  <clock_output id="IPG_CLK_ROOT.outFreq" value="150 MHz" locked="false" accuracy=""/>
                  <clock_output id="LCDIF_CLK_ROOT.outFreq" value="33.75 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPI2C_CLK_ROOT.outFreq" value="60 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPSPI_CLK_ROOT.outFreq" value="105.6 MHz" locked="false" accuracy=""/>
                  <clock_output id="LVDS1_CLK.outFreq" value="1.2 GHz" locked="false" accuracy=""/>
                  <clock_output id="MQS_MCLK.outFreq" value="1080/17 MHz" locked="false" accuracy=""/>
                  <clock_output id="PERCLK_CLK_ROOT.outFreq" value="75 MHz" locked="false" accuracy=""/>
                  <clock_output id="PLL7_MAIN_CLK.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI1_CLK_ROOT.outFreq" value="1080/17 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI1_MCLK1.outFreq" value="1080/17 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI1_MCLK2.outFreq" value="1080/17 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI1_MCLK3.outFreq" value="30 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI2_CLK_ROOT.outFreq" value="1080/17 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI2_MCLK1.outFreq" value="1080/17 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI2_MCLK3.outFreq" value="30 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI3_CLK_ROOT.outFreq" value="1080/17 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI3_MCLK1.outFreq" value="1080/17 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI3_MCLK3.outFreq" value="30 MHz" locked="false" accuracy=""/>
                  <clock_output id="SEMC_CLK_ROOT.outFreq" value="150 MHz" locked="false" accuracy=""/>
                  <clock_output id="SPDIF0_CLK_ROOT.outFreq" value="30 MHz" locked="false" accuracy=""/>
                  <clock_output id="TRACE_CLK_ROOT.outFreq" value="132 MHz" locked="false" accuracy=""/>
                  <clock_output id="UART_CLK_ROOT.outFreq" value="80 MHz" locked="false" accuracy=""/>
                  <clock_output id="USDHC1_CLK_ROOT.outFreq" value="198 MHz" locked="false" accuracy=""/>
                  <clock_output id="USDHC2_CLK_ROOT.outFreq" value="198 MHz" locked="false" accuracy=""/>
               </clock_outputs>
               <clock_settings>
                  <setting id="CCM.AHB_PODF.scale" value="1" locked="true"/>
                  <setting id="CCM.ARM_PODF.scale" value="2" locked="true"/>
                  <setting id="CCM.FLEXSPI_PODF.scale" value="3" locked="true"/>
                  <setting id="CCM.FLEXSPI_SEL.sel" value="CCM.PLL3_SW_CLK_SEL" locked="false"/>
                  <setting id="CCM.LCDIF_PODF.scale" value="4" locked="true"/>
                  <setting id="CCM.LCDIF_PRED.scale" value="4" locked="true"/>
                  <setting id="CCM.LPSPI_PODF.scale" value="5" locked="true"/>
                  <setting id="CCM.PERCLK_PODF.scale" value="2" locked="true"/>
                  <setting id="CCM.SEMC_PODF.scale" value="4" locked="true"/>
                  <setting id="CCM.TRACE_CLK_SEL.sel" value="CCM_ANALOG.PLL2_MAIN_CLK" locked="false"/>
                  <setting id="CCM.TRACE_PODF.scale" value="4" locked="true"/>
                  <setting id="CCM_ANALOG.ENET_DIV.scale" value="4" locked="true"/>
                  <setting id="CCM_ANALOG.PLL1_BYPASS.sel" value="CCM_ANALOG.PLL1" locked="false"/>
                  <setting id="CCM_ANALOG.PLL1_PREDIV.scale" value="1" locked="true"/>
                  <setting id="CCM_ANALOG.PLL1_VDIV.scale" value="50" locked="true"/>
                  <setting id="CCM_ANALOG.PLL2.denom" value="1" locked="true"/>
                  <setting id="CCM_ANALOG.PLL2.num" value="0" locked="true"/>
                  <setting id="CCM_ANALOG.PLL2_BYPASS.sel" value="CCM_ANALOG.PLL2_OUT_CLK" locked="false"/>
                  <setting id="CCM_ANALOG.PLL2_PFD0_BYPASS.sel" value="CCM_ANALOG.PLL2_PFD0" locked="false"/>
                  <setting id="CCM_ANALOG.PLL2_PFD1_BYPASS.sel" value="CCM_ANALOG.PLL2_PFD1" locked="false"/>
                  <setting id="CCM_ANALOG.PLL2_PFD2_BYPASS.sel" value="CCM_ANALOG.PLL2_PFD2" locked="false"/>
                  <setting id="CCM_ANALOG.PLL2_PFD3_BYPASS.sel" value="CCM_ANALOG.PLL2_PFD3" locked="false"/>
                  <setting id="CCM_ANALOG.PLL3_BYPASS.sel" value="CCM_ANALOG.PLL3" locked="false"/>
                  <setting id="CCM_ANALOG.PLL3_PFD0_BYPASS.sel" value="CCM_ANALOG.PLL3_PFD0" locked="false"/>
                  <setting id="CCM_ANALOG.PLL3_PFD0_DIV.scale" value="33" locked="true"/>
                  <setting id="CCM_ANALOG.PLL3_PFD0_MUL.scale" value="18" locked="true"/>
                  <setting id="CCM_ANALOG.PLL3_PFD1_BYPASS.sel" value="CCM_ANALOG.PLL3_PFD1" locked="false"/>
                  <setting id="CCM_ANALOG.PLL3_PFD2_BYPASS.sel" value="CCM_ANALOG.PLL3_PFD2" locked="false"/>
                  <setting id="CCM_ANALOG.PLL3_PFD3_BYPASS.sel" value="CCM_ANALOG.PLL3_PFD3" locked="false"/>
                  <setting id="CCM_ANALOG.PLL4.denom" value="50" locked="false"/>
                  <setting id="CCM_ANALOG.PLL4.div" value="47" locked="false"/>
                  <setting id="CCM_ANALOG.PLL5.denom" value="1" locked="false"/>
                  <setting id="CCM_ANALOG.PLL5.div" value="31" locked="true"/>
                  <setting id="CCM_ANALOG.PLL5.num" value="0" locked="false"/>
                  <setting id="CCM_ANALOG.PLL5_BYPASS.sel" value="CCM_ANALOG.PLL5_POST_DIV" locked="false"/>
                  <setting id="CCM_ANALOG.PLL5_POST_DIV.scale" value="2" locked="false"/>
                  <setting id="CCM_ANALOG.PLL6_BYPASS.sel" value="CCM_ANALOG.PLL6" locked="false"/>
                  <setting id="CCM_ANALOG.VIDEO_DIV.scale" value="4" locked="false"/>
                  <setting id="CCM_ANALOG_PLL_USB1_POWER_CFG" value="Yes" locked="false"/>
                  <setting id="CCM_ANALOG_PLL_VIDEO_POWERDOWN_CFG" value="No" locked="false"/>
               </clock_settings>
               <called_from_default_init>true</called_from_default_init>
            </clock_configuration>
         </clock_configurations>
      </clocks>
      <dcdx name="DCDx" version="3.0" enabled="true" update_project_code="true">
         <generated_project_files>
            <file path="board/dcd.c" update_enabled="true"/>
            <file path="board/dcd.h" update_enabled="true"/>
         </generated_project_files>
         <dcdx_profile>
            <processor_version>9.0.1</processor_version>
            <output_format>c_array</output_format>
         </dcdx_profile>
         <dcdx_configurations>
            <dcdx_configuration name="Device_configuration">
               <description></description>
               <options/>
               <command_groups>
                  <command_group name="Imported Commands" enabled="true">
                     <commands>
                        <command type="write_value" address="CCM_CCGR0" value="0xFFFFFFFF" value_width="4"/>
                        <command type="write_value" address="CCM_CCGR1" value="0xFFFFFFFF" value_width="4"/>
                        <command type="write_value" address="CCM_CCGR2" value="0xFFFFFFFF" value_width="4"/>
                        <command type="write_value" address="CCM_CCGR3" value="0xFFFFFFFF" value_width="4"/>
                        <command type="write_value" address="CCM_CCGR4" value="0xFFFFFFFF" value_width="4"/>
                        <command type="write_value" address="CCM_CCGR5" value="0xFFFFFFFF" value_width="4"/>
                        <command type="write_value" address="CCM_CCGR6" value="0xFFFFFFFF" value_width="4"/>
                        <command type="write_value" address="CCM_ANALOG_PLL_SYS" value="0x2001" value_width="4"/>
                        <command type="write_value" address="CCM_ANALOG_PFD_528" value="0x1D0000" value_width="4"/>
                        <command type="write_value" address="CCM_CBCDR" value="0x10D40" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_00" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_01" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_02" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_03" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_04" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_05" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_06" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_07" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_08" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_09" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_10" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_11" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_12" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_13" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_14" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_15" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_16" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_17" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_18" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_19" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_20" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_21" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_22" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_23" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_24" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_25" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_26" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_27" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_28" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_29" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_30" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_31" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_32" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_33" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_34" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_35" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_36" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_37" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_38" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_39" value="0x10" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_00" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_01" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_02" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_03" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_04" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_05" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_06" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_07" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_08" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_09" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_10" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_11" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_12" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_13" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_14" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_15" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_16" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_17" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_18" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_19" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_20" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_21" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_22" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_23" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_24" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_25" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_26" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_27" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_28" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_29" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_30" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_31" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_32" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_33" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_34" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_35" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_36" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_37" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_38" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_39" value="0x110F9" value_width="4"/>
                        <command type="write_value" address="SEMC_MCR" value="0x10000004" value_width="4"/>
                        <command type="write_value" address="SEMC_BMCR0" value="0x81" value_width="4"/>
                        <command type="write_value" address="SEMC_BMCR1" value="0x81" value_width="4"/>
                        <command type="write_value" address="SEMC_BR0" value="0x8000001B" value_width="4"/>
                        <command type="write_value" address="SEMC_BR1" value="0x8200001B" value_width="4"/>
                        <command type="write_value" address="SEMC_BR2" value="0x8400001B" value_width="4"/>
                        <command type="write_value" address="SEMC_BR3" value="0x8600001B" value_width="4"/>
                        <command type="write_value" address="SEMC_BR4" value="0x90000021" value_width="4"/>
                        <command type="write_value" address="SEMC_BR5" value="0xA0000019" value_width="4"/>
                        <command type="write_value" address="SEMC_BR6" value="0xA8000017" value_width="4"/>
                        <command type="write_value" address="SEMC_BR7" value="0xA900001B" value_width="4"/>
                        <command type="write_value" address="SEMC_BR8" value="0x21" value_width="4"/>
                        <command type="write_value" address="SEMC_IOCR" value="0x79A8" value_width="4"/>
                        <command type="write_value" address="SEMC_SDRAMCR0" value="0xF31" value_width="4"/>
                        <command type="write_value" address="SEMC_SDRAMCR1" value="0x652922" value_width="4"/>
                        <command type="write_value" address="SEMC_SDRAMCR2" value="0x10920" value_width="4"/>
                        <command type="write_value" address="SEMC_SDRAMCR3" value="0x50210A08" value_width="4"/>
                        <command type="write_value" address="SEMC_DBICR0" value="0x21" value_width="4"/>
                        <command type="write_value" address="SEMC_DBICR1" value="0x888888" value_width="4"/>
                        <command type="write_value" address="SEMC_IPCR1" value="0x02" value_width="4"/>
                        <command type="write_value" address="SEMC_IPCR2" value="0x00" value_width="4"/>
                        <command type="write_value" address="SEMC_IPCR0" value="0x80000000" value_width="4"/>
                        <command type="write_value" address="SEMC_IPCMD" value="0xA55A000F" value_width="4"/>
                        <command type="check_any_bit_set" address="SEMC_INTR" value="0x01" value_width="4"/>
                        <command type="write_value" address="SEMC_IPCR0" value="0x80000000" value_width="4"/>
                        <command type="write_value" address="SEMC_IPCMD" value="0xA55A000C" value_width="4"/>
                        <command type="check_any_bit_set" address="SEMC_INTR" value="0x01" value_width="4"/>
                        <command type="write_value" address="SEMC_IPCR0" value="0x80000000" value_width="4"/>
                        <command type="write_value" address="SEMC_IPCMD" value="0xA55A000C" value_width="4"/>
                        <command type="check_any_bit_set" address="SEMC_INTR" value="0x01" value_width="4"/>
                        <command type="write_value" address="SEMC_IPTXDAT" value="0x33" value_width="4"/>
                        <command type="write_value" address="SEMC_IPCR0" value="0x80000000" value_width="4"/>
                        <command type="write_value" address="SEMC_IPCMD" value="0xA55A000A" value_width="4"/>
                        <command type="check_any_bit_set" address="SEMC_INTR" value="0x01" value_width="4"/>
                        <command type="write_value" address="SEMC_SDRAMCR3" value="0x50210A09" value_width="4"/>
                     </commands>
                  </command_group>
               </command_groups>
            </dcdx_configuration>
         </dcdx_configurations>
      </dcdx>
      <periphs name="Peripherals" version="9.0" enabled="true" update_project_code="true">
         <dependencies>
            <dependency resourceType="SWComponent" resourceId="platform.drivers.lpuart" description="LPUART Driver not found in the toolchain/IDE project. Project will not compile!" problem_level="2" source="Peripherals">
               <feature name="enabled" evaluation="equal">
                  <data type="Boolean">true</data>
               </feature>
            </dependency>
            <dependency resourceType="SWComponent" resourceId="platform.drivers.lpuart" description="Unsupported version of the LPUART Driver in the toolchain/IDE project. Required: ${required_value}, actual: ${actual_value}. Project might not compile correctly." problem_level="1" source="Peripherals">
               <feature name="version" evaluation="greaterOrEqual">
                  <data type="Version">2.2.8</data>
               </feature>
            </dependency>
            <dependency resourceType="SWComponent" resourceId="platform.drivers.semc" description="SEMC Driver not found in the toolchain/IDE project. Project will not compile!" problem_level="2" source="Peripherals">
               <feature name="enabled" evaluation="equal">
                  <data type="Boolean">true</data>
               </feature>
            </dependency>
            <dependency resourceType="SWComponent" resourceId="platform.drivers.semc" description="Unsupported version of the SEMC Driver in the toolchain/IDE project. Required: ${required_value}, actual: ${actual_value}. Project might not compile correctly." problem_level="1" source="Peripherals">
               <feature name="version" evaluation="equivalent">
                  <data type="Version">2.3.0</data>
               </feature>
            </dependency>
            <dependency resourceType="SWComponent" resourceId="platform.drivers.elcdif" description="elcdif not found in the toolchain/IDE project. Project will not compile!" problem_level="2" source="Peripherals">
               <feature name="enabled" evaluation="equal">
                  <data type="Boolean">true</data>
               </feature>
            </dependency>
            <dependency resourceType="SWComponent" resourceId="platform.drivers.elcdif" description="Unsupported version of the elcdif in the toolchain/IDE project. Required: ${required_value}, actual: ${actual_value}. Project might not compile correctly." problem_level="1" source="Peripherals">
               <feature name="version" evaluation="equivalent">
                  <data type="Version">2.0.0</data>
               </feature>
            </dependency>
            <dependency resourceType="SWComponent" resourceId="middleware.fatfs" description="FAT File System stack not found in the toolchain/IDE project. Project will not compile!" problem_level="2" source="Peripherals">
               <feature name="enabled" evaluation="equal">
                  <data type="Boolean">true</data>
               </feature>
            </dependency>
            <dependency resourceType="SWComponent" resourceId="middleware.fatfs" description="Unsupported version of the FAT File System stack in the toolchain/IDE project. Required: ${required_value}, actual: ${actual_value}. Project might not compile correctly." problem_level="1" source="Peripherals">
               <feature name="version" evaluation="equivalent">
                  <data type="Version">0.14.0</data>
               </feature>
            </dependency>
            <dependency resourceType="SWComponent" resourceId="platform.drivers.igpio" description="igpio not found in the toolchain/IDE project. Project will not compile!" problem_level="2" source="Peripherals">
               <feature name="enabled" evaluation="equal">
                  <data type="Boolean">true</data>
               </feature>
            </dependency>
            <dependency resourceType="SWComponent" resourceId="platform.drivers.igpio" description="Unsupported version of the igpio in the toolchain/IDE project. Required: ${required_value}, actual: ${actual_value}. Project might not compile correctly." problem_level="1" source="Peripherals">
               <feature name="version" evaluation="equivalent">
                  <data type="Version">2.0.1</data>
               </feature>
            </dependency>
         </dependencies>
         <generated_project_files>
            <file path="board/peripherals.c" update_enabled="true"/>
            <file path="board/peripherals.h" update_enabled="true"/>
            <file path="source/ffconf.h" update_enabled="true"/>
         </generated_project_files>
         <peripherals_profile>
            <processor_version>9.0.1</processor_version>
         </peripherals_profile>
         <functional_groups>
            <functional_group name="BOARD_InitPeripherals" uuid="c02f2a7b-0e89-43b6-9488-2b4f58340ab8" called_from_default_init="true" id_prefix="" core="core0">
               <description></description>
               <options/>
               <dependencies>
                  <dependency resourceType="ClockOutput" resourceId="UART_CLK_ROOT" description="UART_CLK_ROOT is inactive." problem_level="2" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="frequency" evaluation="greaterThan">
                        <data type="Frequency" unit="Hz">0</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="LPUART1.uart_tx" description="Signal TX of the peripheral LPUART1 is not routed." problem_level="1" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="routed" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="LPUART1.uart_rx" description="Signal RX of the peripheral LPUART1 is not routed." problem_level="1" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="routed" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="LCDIF.lcdif_clk" description="Signal CLK of the peripheral LCDIF is not routed." problem_level="1" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="routed" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="LCDIF.lcdif_enable" description="Signal ENABLE of the peripheral LCDIF is not routed." problem_level="1" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="routed" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="LCDIF.lcdif_hsync" description="Signal HSYNC of the peripheral LCDIF is not routed." problem_level="1" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="routed" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="LCDIF.lcdif_vsync" description="Signal VSYNC of the peripheral LCDIF is not routed." problem_level="1" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="routed" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="LCDIF.lcdif_data.00" description="Signal DATA of the channel 00 of the peripheral LCDIF is not routed." problem_level="1" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="routed" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="LCDIF.lcdif_data.01" description="Signal DATA of the channel 01 of the peripheral LCDIF is not routed." problem_level="1" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="routed" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="LCDIF.lcdif_data.02" description="Signal DATA of the channel 02 of the peripheral LCDIF is not routed." problem_level="1" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="routed" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="LCDIF.lcdif_data.03" description="Signal DATA of the channel 03 of the peripheral LCDIF is not routed." problem_level="1" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="routed" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="LCDIF.lcdif_data.04" description="Signal DATA of the channel 04 of the peripheral LCDIF is not routed." problem_level="1" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="routed" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="LCDIF.lcdif_data.05" description="Signal DATA of the channel 05 of the peripheral LCDIF is not routed." problem_level="1" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="routed" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="LCDIF.lcdif_data.06" description="Signal DATA of the channel 06 of the peripheral LCDIF is not routed." problem_level="1" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="routed" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="LCDIF.lcdif_data.07" description="Signal DATA of the channel 07 of the peripheral LCDIF is not routed." problem_level="1" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="routed" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="LCDIF.lcdif_data.08" description="Signal DATA of the channel 08 of the peripheral LCDIF is not routed." problem_level="1" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="routed" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="LCDIF.lcdif_data.09" description="Signal DATA of the channel 09 of the peripheral LCDIF is not routed." problem_level="1" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="routed" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="LCDIF.lcdif_data.10" description="Signal DATA of the channel 10 of the peripheral LCDIF is not routed." problem_level="1" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="routed" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="LCDIF.lcdif_data.11" description="Signal DATA of the channel 11 of the peripheral LCDIF is not routed." problem_level="1" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="routed" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="LCDIF.lcdif_data.12" description="Signal DATA of the channel 12 of the peripheral LCDIF is not routed." problem_level="1" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="routed" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="LCDIF.lcdif_data.13" description="Signal DATA of the channel 13 of the peripheral LCDIF is not routed." problem_level="1" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="routed" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="LCDIF.lcdif_data.14" description="Signal DATA of the channel 14 of the peripheral LCDIF is not routed." problem_level="1" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="routed" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="LCDIF.lcdif_data.15" description="Signal DATA of the channel 15 of the peripheral LCDIF is not routed." problem_level="1" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="routed" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="ClockOutput" resourceId="LCDIF_CLK_ROOT" description="LCDIF_CLK_ROOT is inactive." problem_level="1" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="frequency" evaluation="greaterThan">
                        <data type="Frequency" unit="Hz">0</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="middleware.fatfs.sd" description="The fsl_sd_disk driver is missing in the project (required for FATFS)." problem_level="1" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="enabled" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <instances>
                  <instance name="LPUART1" uuid="c4097945-c1a4-4198-901a-11b1297f9b3d" type="lpuart" type_id="lpuart_54a65a580e3462acdbacefd5299e0cac" mode="polling" peripheral="LPUART1" enabled="true" comment="" custom_name_enabled="false" editing_lock="false">
                     <config_set name="lpuartConfig_t">
                        <struct name="lpuartConfig">
                           <setting name="clockSource" value="LpuartClock"/>
                           <setting name="lpuartSrcClkFreq" value="BOARD_BootClockRUN"/>
                           <setting name="baudRate_Bps" value="921600"/>
                           <setting name="parityMode" value="kLPUART_ParityDisabled"/>
                           <setting name="dataBitsCount" value="kLPUART_EightDataBits"/>
                           <setting name="isMsb" value="false"/>
                           <setting name="stopBitCount" value="kLPUART_OneStopBit"/>
                           <setting name="txFifoWatermark" value="0"/>
                           <setting name="rxFifoWatermark" value="1"/>
                           <setting name="enableRxRTS" value="false"/>
                           <setting name="enableTxCTS" value="false"/>
                           <setting name="txCtsSource" value="kLPUART_CtsSourcePin"/>
                           <setting name="txCtsConfig" value="kLPUART_CtsSampleAtStart"/>
                           <setting name="rxIdleType" value="kLPUART_IdleTypeStartBit"/>
                           <setting name="rxIdleConfig" value="kLPUART_IdleCharacter1"/>
                           <setting name="enableTx" value="true"/>
                           <setting name="enableRx" value="true"/>
                        </struct>
                     </config_set>
                  </instance>
                  <instance name="SEMC" uuid="b2d43365-247f-4857-87c6-cf56b5ddcae5" type="semc" type_id="semc_84a769c198c91c527e11dcec2f5b4b81" mode="general" peripheral="SEMC" enabled="true" comment="" custom_name_enabled="false" editing_lock="false">
                     <config_set name="fsl_semc">
                        <setting name="enableDCD" value="false"/>
                        <struct name="clockConfig">
                           <setting name="clockSource" value="kSEMC_ClkSrcPeri"/>
                           <setting name="clockSourceFreq" value="BOARD_BootClockRUN"/>
                        </struct>
                        <struct name="semc_config_t">
                           <setting name="dqsMode" value="kSEMC_Loopbackdqspad"/>
                           <setting name="cmdTimeoutCycles" value="0"/>
                           <setting name="busTimeoutCycles" value="0"/>
                           <struct name="queueWeight">
                              <setting name="queueaEnable" value="false"/>
                              <struct name="queueaWeight">
                                 <setting name="structORvalue" value="structure"/>
                                 <struct name="queueaConfig">
                                    <setting name="qos" value="0"/>
                                    <setting name="aging" value="0"/>
                                    <setting name="slaveHitSwith" value="0"/>
                                    <setting name="slaveHitNoswitch" value="0"/>
                                 </struct>
                              </struct>
                              <setting name="queuebEnable" value="false"/>
                              <struct name="queuebWeight">
                                 <setting name="structORvalue" value="structure"/>
                                 <struct name="queuebConfig">
                                    <setting name="qos" value="0"/>
                                    <setting name="aging" value="0"/>
                                    <setting name="slaveHitSwith" value="0"/>
                                    <setting name="weightPagehit" value="0"/>
                                    <setting name="bankRotation" value="0"/>
                                 </struct>
                              </struct>
                           </struct>
                        </struct>
                        <struct name="semc_sdram_config_t">
                           <setting name="csxPinMux" value="kSEMC_MUXCSX0"/>
                           <setting name="semcSdramCs" value="kSEMC_SDRAM_CS0"/>
                           <setting name="address" value="0x80000000"/>
                           <setting name="memsize_input" value="32MB"/>
                           <setting name="portSize" value="kSEMC_PortSize16Bit"/>
                           <setting name="burstLen" value="kSEMC_Sdram_BurstLen1"/>
                           <setting name="columnAddrBitNum" value="kSEMC_SdramColunm_9bit"/>
                           <setting name="casLatency" value="kSEMC_LatencyThree"/>
                           <setting name="tPrecharge2Act_Ns" value="18"/>
                           <setting name="tAct2ReadWrite_Ns" value="18"/>
                           <setting name="tRefreshRecovery_Ns" value="127"/>
                           <setting name="tWriteRecovery_Ns" value="12"/>
                           <setting name="tCkeOff_Ns" value="42"/>
                           <setting name="tAct2Prechage_Ns" value="42"/>
                           <setting name="tSelfRefRecovery_Ns" value="67"/>
                           <setting name="tRefresh2Refresh_Ns" value="60"/>
                           <setting name="tAct2Act_Ns" value="60"/>
                           <setting name="tPrescalePeriod_Ns" value="160"/>
                           <setting name="tIdleTimeout_Ns" value="0"/>
                           <setting name="refreshPeriod_nsPerRow" value="64"/>
                           <setting name="refreshUrgThreshold" value="64"/>
                           <setting name="refreshBurstLen" value="1"/>
                        </struct>
                        <array name="sdramArray"/>
                     </config_set>
                  </instance>
                  <instance name="LCDIF" uuid="045e7c7e-f29e-4ee1-8f04-e6a3e59eebc4" type="elcdif" type_id="elcdif_1c39bcb43ed1a24bc8980672c7378576" mode="rgbMode" peripheral="LCDIF" enabled="true" comment="" custom_name_enabled="false" editing_lock="false">
                     <config_set name="fsl_elcdif">
                        <struct name="config">
                           <setting name="panelWidthInt" value="800"/>
                           <setting name="panelHeightInt" value="480"/>
                           <setting name="hsw" value="20"/>
                           <setting name="hfp" value="210"/>
                           <setting name="hbp" value="46"/>
                           <setting name="vsw" value="10"/>
                           <setting name="vfp" value="22"/>
                           <setting name="vbp" value="23"/>
                           <setting name="frameRate" value="60 Hz"/>
                           <struct name="polarityFlags_st">
                              <setting name="vSyncActive" value="kELCDIF_VsyncActiveLow"/>
                              <setting name="hSyncActive" value="kELCDIF_HsyncActiveLow"/>
                              <setting name="dataEnableActive" value="kELCDIF_DataEnableActiveHigh"/>
                              <setting name="driveDataClkEdge" value="kELCDIF_DriveDataOnRisingClkEdge"/>
                           </struct>
                           <setting name="bufferName" value="defaultBuffer"/>
                           <setting name="bufferAlign" value="64"/>
                           <setting name="pixelFormat" value="kELCDIF_PixelFormatRGB565"/>
                           <setting name="dataBus" value="kELCDIF_DataBus16Bit"/>
                           <setting name="enablePxpHandShake" value="false"/>
                           <setting name="start" value="true"/>
                        </struct>
                        <setting name="isInterruptEnabled" value="true"/>
                        <set name="elcdifInterruptSources">
                           <selected>
                              <id>kELCDIF_CurFrameDoneInterruptEnable</id>
                           </selected>
                        </set>
                        <struct name="interrupt">
                           <setting name="IRQn" value="LCDIF_IRQn"/>
                           <setting name="enable_interrrupt" value="enabled"/>
                           <setting name="enable_priority" value="true"/>
                           <setting name="priority" value="5"/>
                           <setting name="enable_custom_name" value="false"/>
                        </struct>
                     </config_set>
                  </instance>
                  <instance name="NVIC" uuid="a5c52120-6b10-49fa-9fc7-2ce74d0eb43b" type="nvic" type_id="nvic_57b5eef3774cc60acaede6f5b8bddc67" mode="general" peripheral="NVIC" enabled="true" comment="" custom_name_enabled="false" editing_lock="false">
                     <config_set name="nvic">
                        <array name="interrupt_table">
                           <struct name="0"/>
                           <struct name="1"/>
                           <struct name="2"/>
                        </array>
                        <array name="interrupts"/>
                     </config_set>
                  </instance>
                  <instance name="FATFS" uuid="83afda7c-315e-492e-925e-9c31a4957556" type="fatfs" type_id="fatfs_2f85acf758668258920f70258052a088" mode="general" enabled="true" comment="" custom_name_enabled="false" editing_lock="false">
                     <config_set name="init_config">
                        <struct name="initConfig">
                           <setting name="initPartitionsStr" value="false"/>
                           <array name="multiplePartitions">
                              <struct name="0">
                                 <setting name="Volume" value="0"/>
                                 <setting name="Partition" value="autoDetect"/>
                              </struct>
                              <struct name="1">
                                 <setting name="Volume" value="0"/>
                                 <setting name="Partition" value="autoDetect"/>
                              </struct>
                           </array>
                           <setting name="enablePhysicalLayerInit" value="false"/>
                           <struct name="diskConfig">
                              <setting name="initFunctionID" value="FATFS_DiskInit"/>
                           </struct>
                           <setting name="initResultObject" value="false"/>
                           <setting name="resultName" value="FATFS_Result"/>
                           <array name="fatfsObjects">
                              <struct name="0">
                                 <setting name="objID" value="FATFS_System_0"/>
                                 <setting name="diskMount" value="false"/>
                                 <setting name="mountPath" value="0:"/>
                                 <setting name="mountInitOpt" value="false"/>
                              </struct>
                           </array>
                           <array name="filObjects"/>
                           <array name="filInfoObjects"/>
                           <array name="dirObjects"/>
                        </struct>
                     </config_set>
                     <config_set name="ff_config">
                        <setting name="revisionID" value="rev14_1"/>
                        <setting name="MSDKadaptation" value="SD_DISK_ENABLE"/>
                        <struct name="functionConfig">
                           <setting name="FF_FS_READONLY" value="false"/>
                           <setting name="FF_FS_MINIMIZE" value="level1"/>
                           <setting name="FF_USE_STRFUNC" value="enableWithoutConversion"/>
                           <setting name="FF_USE_FIND" value="disableDirRead"/>
                           <setting name="FF_USE_MKFS" value="true"/>
                           <setting name="FF_USE_FASTSEEK" value="false"/>
                           <setting name="FF_USE_EXPAND" value="false"/>
                           <setting name="FF_USE_CHMOD" value="false"/>
                           <setting name="FF_USE_LABEL" value="false"/>
                           <setting name="FF_USE_FORWARD" value="false"/>
                        </struct>
                        <struct name="namespaceConfig">
                           <setting name="FF_USE_LFN" value="enableLfnStack"/>
                           <setting name="FF_MAX_LFN" value="255"/>
                           <setting name="FF_LFN_BUF" value="LFNID"/>
                           <setting name="FF_SFN_BUF" value="SFNID"/>
                           <setting name="FF_LFN_UNICODE" value="UTF8"/>
                           <setting name="FF_STRF_ENCODE" value="UTF8"/>
                           <setting name="FF_CODE_PAGE" value="cpUS"/>
                           <setting name="FF_FS_RPATH" value="enableRP2"/>
                        </struct>
                        <struct name="driveConfig">
                           <setting name="FF_VOLUMES" value="3"/>
                           <setting name="FF_STR_VOLUME_ID" value="stringIdWindows"/>
                           <array name="volumes">
                              <struct name="0">
                                 <setting name="volumeStr" value="RAM"/>
                              </struct>
                              <struct name="1">
                                 <setting name="volumeStr" value="USB"/>
                              </struct>
                              <struct name="2">
                                 <setting name="volumeStr" value="SD"/>
                              </struct>
                           </array>
                           <setting name="FF_MULTI_PARTITION" value="false"/>
                           <setting name="FF_MIN_SS" value="value512"/>
                           <setting name="FF_MAX_SS" value="value512"/>
                           <setting name="FF_LBA64" value="false"/>
                           <setting name="FF_MIN_GPT" value="0x100000000"/>
                           <setting name="FF_USE_TRIM" value="false"/>
                        </struct>
                        <struct name="systemConfig">
                           <setting name="FF_FS_TINY" value="false"/>
                           <setting name="FF_FS_EXFAT" value="false"/>
                           <setting name="FF_FS_NORTC" value="true"/>
                           <setting name="FF_NORTC_MON" value="1"/>
                           <setting name="FF_NORTC_MDAY" value="1"/>
                           <setting name="FF_NORTC_YEAR" value="2021"/>
                           <set name="FF_FS_NOFSINFO">
                              <selected/>
                           </set>
                           <setting name="FF_FS_LOCK" value="0"/>
                           <setting name="FF_FS_REENTRANT" value="false"/>
                           <setting name="FF_FS_TIMEOUT" value="1000"/>
                           <setting name="FF_SYNC_t" value="HANDLE"/>
                           <setting name="includeOS" value="false"/>
                           <setting name="headerFileName" value="somertos.h"/>
                        </struct>
                        <struct name="fatfs_codegenerator"/>
                     </config_set>
                  </instance>
                  <instance name="GPIO1" uuid="b2f11629-c004-4b09-be3d-36031f49bb87" type="igpio" type_id="igpio_b1c1fa279aa7069dca167502b8589cb7" mode="GPIO" peripheral="GPIO1" enabled="true" comment="" custom_name_enabled="false" editing_lock="false">
                     <config_set name="fsl_gpio">
                        <setting name="enable_irq_comb_0_15" value="true"/>
                        <struct name="gpio_interrupt_comb_0_15">
                           <setting name="IRQn" value="GPIO1_Combined_0_15_IRQn"/>
                           <setting name="enable_interrrupt" value="enabled"/>
                           <setting name="enable_priority" value="true"/>
                           <setting name="priority" value="6"/>
                           <setting name="enable_custom_name" value="false"/>
                        </struct>
                        <setting name="enable_irq_comb_16_31" value="true"/>
                        <struct name="gpio_interrupt_comb_16_31">
                           <setting name="IRQn" value="GPIO1_Combined_16_31_IRQn"/>
                           <setting name="enable_interrrupt" value="noInit"/>
                           <setting name="enable_priority" value="false"/>
                           <setting name="priority" value="0"/>
                           <setting name="enable_custom_name" value="false"/>
                        </struct>
                        <setting name="enable_irq_int0" value="false"/>
                        <struct name="gpio_interrupt_int0">
                           <setting name="IRQn" value="GPIO1_INT0_IRQn"/>
                           <setting name="enable_interrrupt" value="enabled"/>
                           <setting name="enable_priority" value="false"/>
                           <setting name="priority" value="0"/>
                           <setting name="enable_custom_name" value="false"/>
                        </struct>
                        <setting name="enable_irq_int1" value="false"/>
                        <struct name="gpio_interrupt_int1">
                           <setting name="IRQn" value="GPIO1_INT1_IRQn"/>
                           <setting name="enable_interrrupt" value="enabled"/>
                           <setting name="enable_priority" value="false"/>
                           <setting name="priority" value="0"/>
                           <setting name="enable_custom_name" value="false"/>
                        </struct>
                        <setting name="enable_irq_int2" value="false"/>
                        <struct name="gpio_interrupt_int2">
                           <setting name="IRQn" value="GPIO1_INT2_IRQn"/>
                           <setting name="enable_interrrupt" value="enabled"/>
                           <setting name="enable_priority" value="false"/>
                           <setting name="priority" value="0"/>
                           <setting name="enable_custom_name" value="false"/>
                        </struct>
                        <setting name="enable_irq_int3" value="false"/>
                        <struct name="gpio_interrupt_int3">
                           <setting name="IRQn" value="GPIO1_INT3_IRQn"/>
                           <setting name="enable_interrrupt" value="enabled"/>
                           <setting name="enable_priority" value="false"/>
                           <setting name="priority" value="0"/>
                           <setting name="enable_custom_name" value="false"/>
                        </struct>
                        <setting name="enable_irq_int4" value="false"/>
                        <struct name="gpio_interrupt_int4">
                           <setting name="IRQn" value="GPIO1_INT4_IRQn"/>
                           <setting name="enable_interrrupt" value="enabled"/>
                           <setting name="enable_priority" value="false"/>
                           <setting name="priority" value="0"/>
                           <setting name="enable_custom_name" value="false"/>
                        </struct>
                        <setting name="enable_irq_int5" value="false"/>
                        <struct name="gpio_interrupt_int5">
                           <setting name="IRQn" value="GPIO1_INT5_IRQn"/>
                           <setting name="enable_interrrupt" value="enabled"/>
                           <setting name="enable_priority" value="false"/>
                           <setting name="priority" value="0"/>
                           <setting name="enable_custom_name" value="false"/>
                        </struct>
                        <setting name="enable_irq_int6" value="false"/>
                        <struct name="gpio_interrupt_int6">
                           <setting name="IRQn" value="GPIO1_INT6_IRQn"/>
                           <setting name="enable_interrrupt" value="enabled"/>
                           <setting name="enable_priority" value="false"/>
                           <setting name="priority" value="0"/>
                           <setting name="enable_custom_name" value="false"/>
                        </struct>
                        <setting name="enable_irq_int7" value="false"/>
                        <struct name="gpio_interrupt_int7">
                           <setting name="IRQn" value="GPIO1_INT7_IRQn"/>
                           <setting name="enable_interrrupt" value="enabled"/>
                           <setting name="enable_priority" value="false"/>
                           <setting name="priority" value="0"/>
                           <setting name="enable_custom_name" value="false"/>
                        </struct>
                     </config_set>
                  </instance>
               </instances>
            </functional_group>
         </functional_groups>
         <components>
            <component name="system" uuid="383240c7-9862-4363-92a1-9aa1c238f9b3" type_id="system_54b53072540eeeb8f8e9343e71f28176">
               <config_set_global name="global_system_definitions">
                  <setting name="user_definitions" value=""/>
                  <setting name="user_includes" value=""/>
               </config_set_global>
            </component>
            <component name="generic_can" uuid="b5276c55-8985-4981-856b-f8e9a16ab1c5" type_id="generic_can_1bfdd78b1af214566c1f23cf6a582d80">
               <config_set_global name="global_can"/>
            </component>
            <component name="generic_uart" uuid="7f754fae-7869-45e1-a443-bb9c52bfad1a" type_id="generic_uart_8cae00565451cf2346eb1b8c624e73a6">
               <config_set_global name="global_uart"/>
            </component>
            <component name="msg" uuid="7b0c9559-9b86-48e1-82d7-01346a71825a" type_id="msg_6e2baaf3b97dbeef01c0043275f9a0e7">
               <config_set_global name="global_messages"/>
            </component>
         </components>
      </periphs>
      <tee name="TEE" version="3.0" enabled="false" update_project_code="true">
         <generated_project_files/>
         <tee_profile>
            <processor_version>N/A</processor_version>
         </tee_profile>
         <global_options/>
         <user_memory_regions/>
      </tee>
   </tools>
</configuration>