Overview
========
The CRC Example project is a demonstration program that uses the KSDK software to generate checksums
for an ASCII string. Several CRC protocols are implemented using the CRC driver API.

Toolchain supported
===================
- IAR embedded Workbench  8.32.3
- Keil MDK  5.27
- MCUXpresso  11.0.0
- GCC ARM Embedded  8.2.1

Hardware requirements
=====================
- Mini/micro USB cable
- LPCLPCXpresso54102 board
- Personal Computer

Board settings
==============
No special settings are required.

Prepare the Demo
================
1.  Connect a micro USB cable between the PC host and the CMSIS DAP USB port (J6) on the board
2.  Open a serial terminal with the following settings (See Appendix A in Getting started guide for description how to determine serial port number):
    - 115200 baud rate
    - 8 data bits
    - No parity
    - One stop bit
    - No flow control
3.  Download the program to the target board.
4.  Either press the reset button on your board or launch the debugger in your IDE to begin running the demo.

Running the demo
================
The log below shows example output of the CRC driver demo in the terminal window:
~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
CRC Peripheral Driver Example

Test string: 123456789
CRC-16 CCITT FALSE: 0x29b1
CRC-16 ARC: 0xbb3d
CRC-32: 0xcbf43926
~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
Customization options
=====================

