<?xml version="1.0" encoding= "UTF-8" ?>
<configuration name="LPC54102J512" version="1.6" xsi:schemaLocation="http://mcuxpresso.nxp.com/XSD/mex_configuration_1.6 http://mcuxpresso.nxp.com/XSD/mex_configuration_1.6.xsd" uuid="319f76d0-a626-4f16-9afa-d5c3c08da96b" xmlns="http://mcuxpresso.nxp.com/XSD/mex_configuration_1.6" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">
   <common>
      <processor>LPC54102J512</processor>
      <package>LPC54102J512BD64</package>
      <board>LPCXpresso54102</board>
      <mcu_data>ksdk2_0</mcu_data>
      <cores selected="cm4">
         <core name="Cortex-M0P" id="cm0plus" description=""/>
         <core name="Cortex-M4F" id="cm4" description=""/>
      </cores>
      <description>Configuration imported from C:\Users\mcu-sdk-2.0\boards\lpcxpresso54102\demo_apps\led_blinky\cm4\iar</description>
   </common>
   <preferences>
      <validate_boot_init_only>true</validate_boot_init_only>
      <generate_extended_information>false</generate_extended_information>
      <generate_code_modified_registers_only>false</generate_code_modified_registers_only>
   </preferences>
   <tools>
      <pins name="Pins" version="6.0" enabled="true" update_project_code="true">
         <pins_profile>
            <processor_version>6.0.1</processor_version>
         </pins_profile>
         <functions_list>
            <function name="BOARD_InitPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>true</callFromInitBoot>
                  <prefix>BOARD_</prefix>
                  <coreID>cm4</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="SWD" description="Peripheral SWD is not initialized" problem_level="1" source="Pins:BOARD_InitPins">
                     <feature name="initialized" evaluation="equal" configuration="cm4">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitPins">
                     <feature name="enabled" evaluation="equal" configuration="cm4">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.lpc_gpio" description="Pins initialization requires the LPC_GPIO Driver in the project." problem_level="2" source="Pins:BOARD_InitPins">
                     <feature name="enabled" evaluation="equal" configuration="cm4">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.lpc_iocon" description="Pins initialization requires the LPC_IOCON Driver in the project." problem_level="2" source="Pins:BOARD_InitPins">
                     <feature name="enabled" evaluation="equal" configuration="cm4">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="GPIO" signal="PIO0, 29" pin_num="11" pin_signal="PIO0_29/ADC_0/SCT0_OUT2/CT32B0_MAT3/CT32B0_CAP1/CT32B0_MAT1">
                     <pin_features>
                        <pin_feature name="direction" value="OUTPUT"/>
                        <pin_feature name="mode" value="pullUp"/>
                        <pin_feature name="invert" value="disabled"/>
                        <pin_feature name="glitch_filter" value="disabled"/>
                        <pin_feature name="open_drain" value="disabled"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="SWD" signal="SWO" pin_num="50" pin_signal="PIO0_15/SPI0_SSEL1/SWO/CT32B2_MAT2">
                     <pin_features>
                        <pin_feature name="mode" value="inactive"/>
                     </pin_features>
                  </pin>
               </pins>
            </function>
         </functions_list>
      </pins>
      <clocks name="Clocks" version="6.0" enabled="true" update_project_code="true">
         <clocks_profile>
            <processor_version>6.0.1</processor_version>
         </clocks_profile>
         <clock_configurations>
            <clock_configuration name="BOARD_BootClockIRC12M">
               <description></description>
               <options/>
               <dependencies>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Clocks initialization requires the COMMON Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockIRC12M">
                     <feature name="enabled" evaluation="equal" configuration="cm0plus">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Clocks initialization requires the COMMON Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockIRC12M">
                     <feature name="enabled" evaluation="equal" configuration="cm4">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.power" description="Clocks initialization requires the POWER Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockIRC12M">
                     <feature name="enabled" evaluation="equal" configuration="cm0plus">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.power" description="Clocks initialization requires the POWER Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockIRC12M">
                     <feature name="enabled" evaluation="equal" configuration="cm4">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.clock" description="Clocks initialization requires the CLOCK Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockIRC12M">
                     <feature name="enabled" evaluation="equal" configuration="cm0plus">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.clock" description="Clocks initialization requires the CLOCK Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockIRC12M">
                     <feature name="enabled" evaluation="equal" configuration="cm4">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <clock_sources/>
               <clock_outputs>
                  <clock_output id="ASYNCAPB_clock.outFreq" value="12 MHz" locked="false" accuracy=""/>
                  <clock_output id="FRG_clock.outFreq" value="12 MHz" locked="false" accuracy=""/>
                  <clock_output id="MAIN_clock.outFreq" value="12 MHz" locked="false" accuracy=""/>
                  <clock_output id="System_clock.outFreq" value="12 MHz" locked="false" accuracy=""/>
               </clock_outputs>
               <clock_settings/>
               <called_from_default_init>false</called_from_default_init>
            </clock_configuration>
            <clock_configuration name="BOARD_BootClockPLL48M">
               <description></description>
               <options/>
               <dependencies>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Clocks initialization requires the COMMON Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL48M">
                     <feature name="enabled" evaluation="equal" configuration="cm0plus">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Clocks initialization requires the COMMON Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL48M">
                     <feature name="enabled" evaluation="equal" configuration="cm4">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.power" description="Clocks initialization requires the POWER Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL48M">
                     <feature name="enabled" evaluation="equal" configuration="cm0plus">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.power" description="Clocks initialization requires the POWER Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL48M">
                     <feature name="enabled" evaluation="equal" configuration="cm4">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.clock" description="Clocks initialization requires the CLOCK Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL48M">
                     <feature name="enabled" evaluation="equal" configuration="cm0plus">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.clock" description="Clocks initialization requires the CLOCK Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL48M">
                     <feature name="enabled" evaluation="equal" configuration="cm4">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <clock_sources/>
               <clock_outputs>
                  <clock_output id="ASYNCAPB_clock.outFreq" value="48 MHz" locked="false" accuracy=""/>
                  <clock_output id="FRG_clock.outFreq" value="48 MHz" locked="false" accuracy=""/>
                  <clock_output id="MAIN_clock.outFreq" value="48 MHz" locked="false" accuracy=""/>
                  <clock_output id="System_clock.outFreq" value="48 MHz" locked="false" accuracy=""/>
               </clock_outputs>
               <clock_settings>
                  <setting id="PLL_Mode" value="Fractional" locked="false"/>
                  <setting id="SYSCON.MAINCLKSELB.sel" value="SYSCON.PLL_BYPASS" locked="false"/>
                  <setting id="SYSCON.M_MULT.scale" value="49152" locked="true"/>
                  <setting id="SYSCON.N_DIV.scale" value="3" locked="true"/>
                  <setting id="SYSCON.PDEC.scale" value="2" locked="true"/>
                  <setting id="SYSCON.PLL_BYPASS.sel" value="SYSCON.DIRECTO" locked="false"/>
                  <setting id="SYSCON_SYSPLLCTRL_BYPASSCCODIV2_CFG" value="Enabled" locked="false"/>
               </clock_settings>
               <called_from_default_init>false</called_from_default_init>
            </clock_configuration>
            <clock_configuration name="BOARD_BootClockPLL96M">
               <description></description>
               <options/>
               <dependencies>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Clocks initialization requires the COMMON Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL96M">
                     <feature name="enabled" evaluation="equal" configuration="cm0plus">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Clocks initialization requires the COMMON Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL96M">
                     <feature name="enabled" evaluation="equal" configuration="cm4">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.power" description="Clocks initialization requires the POWER Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL96M">
                     <feature name="enabled" evaluation="equal" configuration="cm0plus">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.power" description="Clocks initialization requires the POWER Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL96M">
                     <feature name="enabled" evaluation="equal" configuration="cm4">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.clock" description="Clocks initialization requires the CLOCK Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL96M">
                     <feature name="enabled" evaluation="equal" configuration="cm0plus">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.clock" description="Clocks initialization requires the CLOCK Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL96M">
                     <feature name="enabled" evaluation="equal" configuration="cm4">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <clock_sources/>
               <clock_outputs>
                  <clock_output id="ASYNCAPB_clock.outFreq" value="96 MHz" locked="false" accuracy=""/>
                  <clock_output id="FRG_clock.outFreq" value="96 MHz" locked="false" accuracy=""/>
                  <clock_output id="MAIN_clock.outFreq" value="96 MHz" locked="false" accuracy=""/>
                  <clock_output id="System_clock.outFreq" value="96 MHz" locked="false" accuracy=""/>
               </clock_outputs>
               <clock_settings>
                  <setting id="PLL_Mode" value="Fractional" locked="false"/>
                  <setting id="SYSCON.DIRECTO.sel" value="SYSCON.PLL" locked="false"/>
                  <setting id="SYSCON.MAINCLKSELB.sel" value="SYSCON.PLL_BYPASS" locked="false"/>
                  <setting id="SYSCON.M_MULT.scale" value="49152" locked="true"/>
                  <setting id="SYSCON.N_DIV.scale" value="3" locked="true"/>
                  <setting id="SYSCON.PDEC.scale" value="2" locked="true"/>
                  <setting id="SYSCON.PLL_BYPASS.sel" value="SYSCON.DIRECTO" locked="false"/>
                  <setting id="SYSCON_SYSPLLCTRL_BYPASSCCODIV2_CFG" value="Enabled" locked="false"/>
               </clock_settings>
               <called_from_default_init>true</called_from_default_init>
            </clock_configuration>
            <clock_configuration name="BOARD_BootClockPLL100M">
               <description></description>
               <options/>
               <dependencies>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Clocks initialization requires the COMMON Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL100M">
                     <feature name="enabled" evaluation="equal" configuration="cm0plus">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Clocks initialization requires the COMMON Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL100M">
                     <feature name="enabled" evaluation="equal" configuration="cm4">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.power" description="Clocks initialization requires the POWER Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL100M">
                     <feature name="enabled" evaluation="equal" configuration="cm0plus">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.power" description="Clocks initialization requires the POWER Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL100M">
                     <feature name="enabled" evaluation="equal" configuration="cm4">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.clock" description="Clocks initialization requires the CLOCK Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL100M">
                     <feature name="enabled" evaluation="equal" configuration="cm0plus">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.clock" description="Clocks initialization requires the CLOCK Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL100M">
                     <feature name="enabled" evaluation="equal" configuration="cm4">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <clock_sources/>
               <clock_outputs>
                  <clock_output id="ASYNCAPB_clock.outFreq" value="100 MHz" locked="false" accuracy=""/>
                  <clock_output id="FRG_clock.outFreq" value="100 MHz" locked="false" accuracy=""/>
                  <clock_output id="MAIN_clock.outFreq" value="100 MHz" locked="false" accuracy=""/>
                  <clock_output id="System_clock.outFreq" value="100 MHz" locked="false" accuracy=""/>
               </clock_outputs>
               <clock_settings>
                  <setting id="PLL_Mode" value="Fractional" locked="false"/>
                  <setting id="SYSCON.DIRECTO.sel" value="SYSCON.PLL" locked="false"/>
                  <setting id="SYSCON.MAINCLKSELB.sel" value="SYSCON.PLL_BYPASS" locked="false"/>
                  <setting id="SYSCON.M_MULT.scale" value="102400" locked="true"/>
                  <setting id="SYSCON.N_DIV.scale" value="6" locked="true"/>
                  <setting id="SYSCON.PDEC.scale" value="2" locked="true"/>
                  <setting id="SYSCON.PLL_BYPASS.sel" value="SYSCON.DIRECTO" locked="false"/>
               </clock_settings>
               <called_from_default_init>false</called_from_default_init>
            </clock_configuration>
         </clock_configurations>
      </clocks>
      <dcdx name="DCDx" version="2.0" enabled="false" update_project_code="true">
         <dcdx_profile>
            <processor_version>N/A</processor_version>
         </dcdx_profile>
         <dcdx_configurations/>
      </dcdx>
      <periphs name="Peripherals" version="6.0" enabled="false" update_project_code="true">
         <peripherals_profile>
            <processor_version>N/A</processor_version>
         </peripherals_profile>
         <functional_groups/>
         <components/>
      </periphs>
      <tee name="TEE" version="1.0" enabled="false" update_project_code="true">
         <tee_profile>
            <processor_version>N/A</processor_version>
         </tee_profile>
         <global_options/>
         <user_memory_regions/>
      </tee>
   </tools>
</configuration>