<?xml version="1.0" encoding= "UTF-8" ?>
<configuration name="" version="1.6" xsi:schemaLocation="http://mcuxpresso.nxp.com/XSD/mex_configuration_1.6 http://mcuxpresso.nxp.com/XSD/mex_configuration_1.6.xsd" uuid="935550d9-8bef-441f-85f2-e3d88ca98182" xmlns="http://mcuxpresso.nxp.com/XSD/mex_configuration_1.6" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">
   <common>
      <processor>LPC804</processor>
      <package>LPC804M101JDH24</package>
      <board>LPCXpresso804</board>
      <mcu_data>ksdk2_0</mcu_data>
      <cores selected="core0">
         <core name="Cortex-M0P" id="core0" description="M0P core"/>
      </cores>
      <description></description>
   </common>
   <preferences>
      <validate_boot_init_only>true</validate_boot_init_only>
      <generate_extended_information>false</generate_extended_information>
      <generate_code_modified_registers_only>false</generate_code_modified_registers_only>
   </preferences>
   <tools>
      <pins name="Pins" version="6.0" enabled="true" update_project_code="true">
         <pins_profile>
            <processor_version>0.2.7</processor_version>
         </pins_profile>
         <functions_list>
            <function name="BOARD_InitPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>true</callFromInitBoot>
                  <prefix>BOARD_</prefix>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="USART0" description="Peripheral USART0 is not initialized" problem_level="1" source="Pins:BOARD_InitPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.swm" description="Pins initialization requires the SWM Driver in the project." problem_level="2" source="Pins:BOARD_InitPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="USART0" signal="RXD" pin_num="22" pin_signal="PIO0_0/ACMP_I1">
                     <pin_features>
                        <pin_feature name="identifier" value=""/>
                     </pin_features>
                  </pin>
                  <pin peripheral="USART0" signal="TXD" pin_num="7" pin_signal="PIO0_4/ADC_11"/>
               </pins>
            </function>
         </functions_list>
      </pins>
      <clocks name="Clocks" version="6.0" enabled="true" update_project_code="true">
         <clocks_profile>
            <processor_version>0.2.7</processor_version>
         </clocks_profile>
         <clock_configurations>
            <clock_configuration name="BOARD_BootClockRUN">
               <description></description>
               <options/>
               <dependencies>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Clocks initialization requires the COMMON Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockRUN">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.power_no_lib" description="Clocks initialization requires the POWER_NO_LIB Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockRUN">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.clock" description="Clocks initialization requires the CLOCK Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockRUN">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <clock_sources/>
               <clock_outputs>
                  <clock_output id="FROHF_clock.outFreq" value="30 MHz" locked="false" accuracy=""/>
                  <clock_output id="LowPower_clock.outFreq" value="1 MHz" locked="false" accuracy=""/>
                  <clock_output id="System_clock.outFreq" value="15 MHz" locked="false" accuracy=""/>
                  <clock_output id="WWDT_clock.outFreq" value="1 MHz" locked="false" accuracy=""/>
                  <clock_output id="divto750k_clock.outFreq" value="750 kHz" locked="false" accuracy=""/>
               </clock_outputs>
               <clock_settings/>
               <called_from_default_init>true</called_from_default_init>
            </clock_configuration>
            <clock_configuration name="BOARD_BootClockFRO18M">
               <description></description>
               <options/>
               <dependencies>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Clocks initialization requires the COMMON Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockFRO18M">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.power_no_lib" description="Clocks initialization requires the POWER_NO_LIB Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockFRO18M">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.clock" description="Clocks initialization requires the CLOCK Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockFRO18M">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <clock_sources>
                  <clock_source id="SYSCON.fro_osc.outFreq" value="18 MHz" locked="false" enabled="false"/>
               </clock_sources>
               <clock_outputs>
                  <clock_output id="FROHF_clock.outFreq" value="18 MHz" locked="false" accuracy=""/>
                  <clock_output id="LowPower_clock.outFreq" value="1 MHz" locked="false" accuracy=""/>
                  <clock_output id="System_clock.outFreq" value="9 MHz" locked="false" accuracy=""/>
                  <clock_output id="WWDT_clock.outFreq" value="1 MHz" locked="false" accuracy=""/>
                  <clock_output id="divto750k_clock.outFreq" value="750 kHz" locked="false" accuracy=""/>
               </clock_outputs>
               <clock_settings/>
               <called_from_default_init>false</called_from_default_init>
            </clock_configuration>
            <clock_configuration name="BOARD_BootClockFRO24M">
               <description></description>
               <options/>
               <dependencies>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Clocks initialization requires the COMMON Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockFRO24M">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.power_no_lib" description="Clocks initialization requires the POWER_NO_LIB Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockFRO24M">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.clock" description="Clocks initialization requires the CLOCK Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockFRO24M">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <clock_sources>
                  <clock_source id="SYSCON.fro_osc.outFreq" value="24 MHz" locked="false" enabled="false"/>
               </clock_sources>
               <clock_outputs>
                  <clock_output id="FROHF_clock.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="LowPower_clock.outFreq" value="1 MHz" locked="false" accuracy=""/>
                  <clock_output id="System_clock.outFreq" value="12 MHz" locked="false" accuracy=""/>
                  <clock_output id="WWDT_clock.outFreq" value="1 MHz" locked="false" accuracy=""/>
                  <clock_output id="divto750k_clock.outFreq" value="750 kHz" locked="false" accuracy=""/>
               </clock_outputs>
               <clock_settings/>
               <called_from_default_init>false</called_from_default_init>
            </clock_configuration>
            <clock_configuration name="BOARD_BootClockFRO30M">
               <description></description>
               <options/>
               <dependencies>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Clocks initialization requires the COMMON Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockFRO30M">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.power_no_lib" description="Clocks initialization requires the POWER_NO_LIB Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockFRO30M">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.clock" description="Clocks initialization requires the CLOCK Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockFRO30M">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <clock_sources/>
               <clock_outputs>
                  <clock_output id="FROHF_clock.outFreq" value="30 MHz" locked="false" accuracy=""/>
                  <clock_output id="LowPower_clock.outFreq" value="1 MHz" locked="false" accuracy=""/>
                  <clock_output id="System_clock.outFreq" value="15 MHz" locked="false" accuracy=""/>
                  <clock_output id="WWDT_clock.outFreq" value="1 MHz" locked="false" accuracy=""/>
                  <clock_output id="divto750k_clock.outFreq" value="750 kHz" locked="false" accuracy=""/>
               </clock_outputs>
               <clock_settings/>
               <called_from_default_init>false</called_from_default_init>
            </clock_configuration>
         </clock_configurations>
      </clocks>
      <periphs name="Peripherals" version="6.0" enabled="true" update_project_code="true">
         <peripherals_profile>
            <processor_version>0.2.7</processor_version>
         </peripherals_profile>
         <functional_groups>
            <functional_group name="BOARD_InitPeripherals" uuid="dcb1516e-c6df-4d3e-932b-d56d355c5970" called_from_default_init="true" id_prefix="" core="core0">
               <description></description>
               <options/>
               <dependencies/>
               <instances/>
            </functional_group>
         </functional_groups>
         <components>
            <component name="system" type_id="system_54b53072540eeeb8f8e9343e71f28176">
               <config_set_global name="global_system_definitions"/>
            </component>
            <component name="msg" type_id="msg_6e2baaf3b97dbeef01c0043275f9a0e7">
               <config_set_global name="global_messages"/>
            </component>
         </components>
      </periphs>
   </tools>
</configuration>